(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(title_block
		(title "\"Slow\" GPIO pins")
	)
	(lib_symbols
		(symbol "Capacitors SMD:CC0402_100NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_100NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" "100nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/05/13 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_100NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_33R_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_33R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "33"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "33"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270673309L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_33R_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Standard Logic:SN74LV166ANS"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 7.62 1.27 0)
			)
			(property "Value" "SN74LV166ANS"
				(at 0 -50.165 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOIC127P780X200-16N"
				(at 0 -52.07 0)
			)
			(property "Datasheet" ""
				(at 0 -53.975 0)
			)
			(property "Description" "SN74LV166ANS"
				(at 0 -55.88 0)
			)
			(property "Library Ref" "74166"
				(at 0 -57.785 0)
			)
			(property "Library Path" "SchLib\\Standard Logic.SchLib"
				(at 0 -59.69 0)
			)
			(property "Comment" "SN74LV166ANS"
				(at 0 -61.595 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -63.5 0)
			)
			(property "Component Type" "Standard"
				(at 0 -65.405 0)
			)
			(property "Device" "SN74LV166ANS"
				(at 0 -67.31 0)
			)
			(property "PackageDescription" "SOIC, 1.27mm Pitch; 16 Pin, 5.30mm W X 10.2mm L X 2.00mm H body, IPC Medium Density"
				(at 0 -69.215 0)
			)
			(property "Status" " "
				(at 0 -71.12 0)
			)
			(property "Part Description" "8-Bit Parallel-Load  Shift Register"
				(at 0 -73.025 0)
			)
			(property "Manufacturer" "TEXAS INSTRUMENTS"
				(at 0 -74.93 0)
			)
			(property "Manufacturer Part Number" "SN74LV166ANS"
				(at 0 -76.835 0)
			)
			(property "Pin Count" "16"
				(at 0 -78.74 0)
			)
			(property "Case" "SOIC16"
				(at 0 -80.645 0)
			)
			(property "Mounted" "Yes"
				(at 0 -82.55 0)
			)
			(property "Socket" "No"
				(at 0 -84.455 0)
			)
			(property "SMD" "Yes"
				(at 0 -86.36 0)
			)
			(property "PressFit" "No"
				(at 0 -88.265 0)
			)
			(property "Sense" "No"
				(at 0 -90.17 0)
			)
			(property "Sense Comment" " "
				(at 0 -92.075 0)
			)
			(property "Bonding" "No"
				(at 0 -93.98 0)
			)
			(property "Status Comment" " "
				(at 0 -95.885 0)
			)
			(property "ComponentHeight" "2mm"
				(at 0 -97.79 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -99.695 0)
			)
			(property "Footprint Ref" "SOIC127P780X200-16N"
				(at 0 -101.6 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -103.505 0)
			)
			(property "HelpURL" ""
				(at 0 -105.41 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -107.315 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -109.22 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -111.125 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -113.03 0)
			)
			(property "CreateDate" "04/29/20 00:00:00"
				(at 0 -114.935 0)
			)
			(property "LatestRevisionDate" "04/29/20 00:00:00"
				(at 0 -116.84 0)
			)
			(property "SCEM" " "
				(at 0 -118.745 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -120.65 0)
			)
			(property "Library Name" "Standard Logic"
				(at 0 -122.555 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -124.46 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -126.365 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "SN74LV166ANS_0_1"
				(rectangle
					(start 0 -45.72)
					(end 15.24 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "SH/~{LD}")
					(number "15")
				)
				(pin input line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "SER")
					(number "1")
				)
				(pin input line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "CLK_INH")
					(number "6")
				)
				(pin input line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "CLK")
					(number "7")
				)
				(pin input line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "~{CLR}")
					(number "9")
				)
				(pin input line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "A")
					(number "2")
				)
				(pin input line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "B")
					(number "3")
				)
				(pin input line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "C")
					(number "4")
				)
				(pin input line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "D")
					(number "5")
				)
				(pin input line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "E")
					(number "10")
				)
				(pin input line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "F")
					(number "11")
				)
				(pin input line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "G")
					(number "12")
				)
				(pin input line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "H")
					(number "14")
				)
				(pin power_in line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "VCC")
					(number "16")
				)
				(pin output line
					(at 20.32 -25.4 180)
					(length 5.08)
					(name "QH")
					(number "13")
				)
				(pin power_in line
					(at 20.32 -43.18 180)
					(length 5.08)
					(name "GND")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Standard Logic:SN74LV595ARGYR"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 10.16 1.27 0)
			)
			(property "Value" "SN74LV595ARGYR"
				(at 0 -37.465 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:TEXAS_RGY (R-PVQFN-N16)"
				(at 0 -39.37 0)
			)
			(property "Datasheet" ""
				(at 0 -41.275 0)
			)
			(property "Description" "SN74LV595ARGYR"
				(at 0 -43.18 0)
			)
			(property "Library Ref" "74595_a"
				(at 0 -45.085 0)
			)
			(property "Library Path" "SchLib\\Standard Logic.SchLib"
				(at 0 -46.99 0)
			)
			(property "Comment" "SN74LV595ARGY"
				(at 0 -48.895 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -50.8 0)
			)
			(property "Component Type" "Standard"
				(at 0 -52.705 0)
			)
			(property "Device" "SN74LV595ARGY"
				(at 0 -54.61 0)
			)
			(property "PackageDescription" "TEXAS Case Style RGY (R-PVQFN-N16), QFN, 0.50mm Pitch, Rect.; 16 Pin, 4.00mm L X 3.50mm W X 1mm H body (w/Thermal Tab 2.65 X 2.15mm)"
				(at 0 -56.515 0)
			)
			(property "Status" " "
				(at 0 -58.42 0)
			)
			(property "Part Description" "8-Bit Shift Register with 3-State Output Registers"
				(at 0 -60.325 0)
			)
			(property "Manufacturer" "TEXAS INSTRUMENTS"
				(at 0 -62.23 0)
			)
			(property "Manufacturer Part Number" "SN74LV595ARGY"
				(at 0 -64.135 0)
			)
			(property "Pin Count" "17"
				(at 0 -66.04 0)
			)
			(property "Case" "QFN16"
				(at 0 -67.945 0)
			)
			(property "Mounted" "Yes"
				(at 0 -69.85 0)
			)
			(property "Socket" "No"
				(at 0 -71.755 0)
			)
			(property "SMD" "Yes"
				(at 0 -73.66 0)
			)
			(property "PressFit" "No"
				(at 0 -75.565 0)
			)
			(property "Sense" "No"
				(at 0 -77.47 0)
			)
			(property "Sense Comment" " "
				(at 0 -79.375 0)
			)
			(property "Bonding" "No"
				(at 0 -81.28 0)
			)
			(property "Status Comment" " "
				(at 0 -83.185 0)
			)
			(property "ComponentHeight" "1mm"
				(at 0 -85.09 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -86.995 0)
			)
			(property "Footprint Ref" "TEXAS_RGY (R-PVQFN-N16)"
				(at 0 -88.9 0)
			)
			(property "Author" "CERN DEM MR"
				(at 0 -90.805 0)
			)
			(property "HelpURL" ""
				(at 0 -92.71 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -94.615 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -96.52 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -98.425 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -100.33 0)
			)
			(property "CreateDate" "10/10/17 00:00:00"
				(at 0 -102.235 0)
			)
			(property "LatestRevisionDate" "10/10/17 00:00:00"
				(at 0 -104.14 0)
			)
			(property "SCEM" " "
				(at 0 -106.045 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -107.95 0)
			)
			(property "Library Name" "Standard Logic"
				(at 0 -109.855 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -111.76 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -113.665 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "SN74LV595ARGYR_0_1"
				(rectangle
					(start 0 -33.02)
					(end 20.32 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 19.812 -31.623)
					(end 20.32 -29.337)
					(fill
						(type outline)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "~{OE}")
					(number "13")
				)
				(pin input clock
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "RCLK")
					(number "12")
				)
				(pin input line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "~{SRCLR}")
					(number "10")
				)
				(pin input line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "SRCLK")
					(number "11")
				)
				(pin input line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "SER")
					(number "14")
				)
				(pin power_in line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "VCC")
					(number "16")
				)
				(pin tri_state line
					(at 25.4 -2.54 180)
					(length 5.08)
					(name "QA")
					(number "15")
				)
				(pin tri_state line
					(at 25.4 -5.08 180)
					(length 5.08)
					(name "QB")
					(number "1")
				)
				(pin tri_state line
					(at 25.4 -7.62 180)
					(length 5.08)
					(name "QC")
					(number "2")
				)
				(pin tri_state line
					(at 25.4 -10.16 180)
					(length 5.08)
					(name "QD")
					(number "3")
				)
				(pin tri_state line
					(at 25.4 -12.7 180)
					(length 5.08)
					(name "QE")
					(number "4")
				)
				(pin tri_state line
					(at 25.4 -15.24 180)
					(length 5.08)
					(name "QF")
					(number "5")
				)
				(pin tri_state line
					(at 25.4 -17.78 180)
					(length 5.08)
					(name "QG")
					(number "6")
				)
				(pin tri_state line
					(at 25.4 -20.32 180)
					(length 5.08)
					(name "QH")
					(number "7")
				)
				(pin output line
					(at 25.4 -22.86 180)
					(length 5.08)
					(name "QH'")
					(number "9")
				)
				(pin power_in line
					(at 25.4 -27.94 180)
					(length 5.08)
					(name "GND")
					(number "8")
				)
				(pin power_in line
					(at 25.4 -30.48 180)
					(length 5.08)
					(name "EP")
					(number "17")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P3V3"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0202"
				(at 0 0 0)
			)
			(property "Value" "P3V3"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P3V3_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P3V3")
					(number "")
				)
			)
			(embedded_fonts no)
		)
	)
	(text_box "Place series termination resistors close to FPGA."
		(exclude_from_sim no)
		(at 64.77 71.12 0)
		(size 24.13 8.89)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 194 1)
		)
	)
	(junction
		(at 193.04 148.59)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 193.04 72.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 110.49 76.2)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 242.57 72.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 144.78 78.74)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 142.24 71.12)
	)
	(wire
		(pts
			(xy 241.3 64.77) (xy 243.84 64.77)
		)
	)
	(wire
		(pts
			(xy 219.71 72.39) (xy 222.25 72.39)
		)
	)
	(wire
		(pts
			(xy 241.3 54.61) (xy 243.84 54.61)
		)
	)
	(wire
		(pts
			(xy 85.09 60.96) (xy 111.76 60.96)
		)
	)
	(wire
		(pts
			(xy 189.23 72.39) (xy 193.04 72.39)
		)
	)
	(wire
		(pts
			(xy 142.24 76.2) (xy 144.78 76.2)
		)
	)
	(wire
		(pts
			(xy 144.78 78.74) (xy 144.78 86.36)
		)
	)
	(wire
		(pts
			(xy 241.3 52.07) (xy 243.84 52.07)
		)
	)
	(wire
		(pts
			(xy 142.24 78.74) (xy 144.78 78.74)
		)
	)
	(wire
		(pts
			(xy 278.13 54.61) (xy 269.24 54.61)
		)
	)
	(wire
		(pts
			(xy 142.24 66.04) (xy 144.78 66.04)
		)
	)
	(wire
		(pts
			(xy 142.24 68.58) (xy 144.78 68.58)
		)
	)
	(wire
		(pts
			(xy 226.06 44.45) (xy 243.84 44.45)
		)
	)
	(wire
		(pts
			(xy 242.57 72.39) (xy 242.57 74.93)
		)
	)
	(wire
		(pts
			(xy 176.53 31.75) (xy 194.31 31.75)
		)
	)
	(wire
		(pts
			(xy 176.53 120.65) (xy 194.31 120.65)
		)
	)
	(wire
		(pts
			(xy 191.77 64.77) (xy 194.31 64.77)
		)
	)
	(wire
		(pts
			(xy 73.66 53.34) (xy 77.47 53.34)
		)
	)
	(wire
		(pts
			(xy 191.77 140.97) (xy 194.31 140.97)
		)
	)
	(wire
		(pts
			(xy 193.04 148.59) (xy 193.04 151.13)
		)
	)
	(wire
		(pts
			(xy 242.57 72.39) (xy 243.84 72.39)
		)
	)
	(wire
		(pts
			(xy 194.31 110.49) (xy 191.77 110.49)
		)
	)
	(wire
		(pts
			(xy 193.04 148.59) (xy 194.31 148.59)
		)
	)
	(wire
		(pts
			(xy 222.25 148.59) (xy 222.25 158.75)
		)
	)
	(wire
		(pts
			(xy 191.77 133.35) (xy 194.31 133.35)
		)
	)
	(wire
		(pts
			(xy 191.77 52.07) (xy 194.31 52.07)
		)
	)
	(wire
		(pts
			(xy 73.66 66.04) (xy 77.47 66.04)
		)
	)
	(wire
		(pts
			(xy 142.24 60.96) (xy 144.78 60.96)
		)
	)
	(wire
		(pts
			(xy 142.24 50.8) (xy 144.78 50.8)
		)
	)
	(wire
		(pts
			(xy 73.66 58.42) (xy 111.76 58.42)
		)
	)
	(wire
		(pts
			(xy 193.04 72.39) (xy 194.31 72.39)
		)
	)
	(wire
		(pts
			(xy 191.77 128.27) (xy 194.31 128.27)
		)
	)
	(wire
		(pts
			(xy 176.53 118.11) (xy 194.31 118.11)
		)
	)
	(wire
		(pts
			(xy 142.24 58.42) (xy 144.78 58.42)
		)
	)
	(wire
		(pts
			(xy 191.77 67.31) (xy 194.31 67.31)
		)
	)
	(wire
		(pts
			(xy 278.13 95.25) (xy 278.13 54.61)
		)
	)
	(wire
		(pts
			(xy 191.77 130.81) (xy 194.31 130.81)
		)
	)
	(wire
		(pts
			(xy 226.06 31.75) (xy 243.84 31.75)
		)
	)
	(wire
		(pts
			(xy 219.71 54.61) (xy 223.52 54.61)
		)
	)
	(wire
		(pts
			(xy 110.49 76.2) (xy 111.76 76.2)
		)
	)
	(wire
		(pts
			(xy 106.68 76.2) (xy 110.49 76.2)
		)
	)
	(wire
		(pts
			(xy 191.77 54.61) (xy 194.31 54.61)
		)
	)
	(wire
		(pts
			(xy 189.23 148.59) (xy 193.04 148.59)
		)
	)
	(wire
		(pts
			(xy 219.71 130.81) (xy 232.41 130.81)
		)
	)
	(wire
		(pts
			(xy 176.53 44.45) (xy 194.31 44.45)
		)
	)
	(wire
		(pts
			(xy 144.78 76.2) (xy 144.78 78.74)
		)
	)
	(wire
		(pts
			(xy 191.77 49.53) (xy 194.31 49.53)
		)
	)
	(wire
		(pts
			(xy 191.77 59.69) (xy 194.31 59.69)
		)
	)
	(wire
		(pts
			(xy 191.77 135.89) (xy 194.31 135.89)
		)
	)
	(wire
		(pts
			(xy 176.53 41.91) (xy 194.31 41.91)
		)
	)
	(wire
		(pts
			(xy 223.52 34.29) (xy 243.84 34.29)
		)
	)
	(wire
		(pts
			(xy 271.78 72.39) (xy 271.78 82.55)
		)
	)
	(wire
		(pts
			(xy 73.66 60.96) (xy 77.47 60.96)
		)
	)
	(wire
		(pts
			(xy 191.77 138.43) (xy 194.31 138.43)
		)
	)
	(wire
		(pts
			(xy 219.71 148.59) (xy 222.25 148.59)
		)
	)
	(wire
		(pts
			(xy 241.3 59.69) (xy 243.84 59.69)
		)
	)
	(wire
		(pts
			(xy 191.77 125.73) (xy 194.31 125.73)
		)
	)
	(wire
		(pts
			(xy 142.24 55.88) (xy 144.78 55.88)
		)
	)
	(wire
		(pts
			(xy 241.3 67.31) (xy 243.84 67.31)
		)
	)
	(wire
		(pts
			(xy 241.3 49.53) (xy 243.84 49.53)
		)
	)
	(wire
		(pts
			(xy 85.09 53.34) (xy 111.76 53.34)
		)
	)
	(wire
		(pts
			(xy 223.52 54.61) (xy 223.52 34.29)
		)
	)
	(wire
		(pts
			(xy 142.24 63.5) (xy 144.78 63.5)
		)
	)
	(wire
		(pts
			(xy 193.04 72.39) (xy 193.04 74.93)
		)
	)
	(wire
		(pts
			(xy 191.77 57.15) (xy 194.31 57.15)
		)
	)
	(wire
		(pts
			(xy 191.77 95.25) (xy 278.13 95.25)
		)
	)
	(wire
		(pts
			(xy 73.66 50.8) (xy 111.76 50.8)
		)
	)
	(wire
		(pts
			(xy 222.25 72.39) (xy 222.25 82.55)
		)
	)
	(wire
		(pts
			(xy 241.3 57.15) (xy 243.84 57.15)
		)
	)
	(wire
		(pts
			(xy 110.49 76.2) (xy 110.49 78.74)
		)
	)
	(wire
		(pts
			(xy 191.77 110.49) (xy 191.77 95.25)
		)
	)
	(wire
		(pts
			(xy 142.24 53.34) (xy 144.78 53.34)
		)
	)
	(wire
		(pts
			(xy 269.24 72.39) (xy 271.78 72.39)
		)
	)
	(wire
		(pts
			(xy 238.76 72.39) (xy 242.57 72.39)
		)
	)
	(wire
		(pts
			(xy 191.77 143.51) (xy 194.31 143.51)
		)
	)
	(wire
		(pts
			(xy 191.77 62.23) (xy 194.31 62.23)
		)
	)
	(wire
		(pts
			(xy 226.06 41.91) (xy 243.84 41.91)
		)
	)
	(wire
		(pts
			(xy 241.3 62.23) (xy 243.84 62.23)
		)
	)
	(wire
		(pts
			(xy 85.09 66.04) (xy 111.76 66.04)
		)
	)
	(wire
		(pts
			(xy 176.53 107.95) (xy 194.31 107.95)
		)
	)
	(label "I_IOEXP_RCLK"
		(at 92.71 53.34 0)
	)
	(label "IOEXP_RST_N"
		(at 179.07 120.65 0)
	)
	(label "I_IOEXP_RCLK"
		(at 179.07 31.75 0)
	)
	(label "I_IOEXP_SCLK"
		(at 177.8 118.11 0)
	)
	(label "I_IOEXP_RCLK"
		(at 228.6 31.75 0)
	)
	(label "IOEXP_RST_N"
		(at 228.6 44.45 0)
	)
	(label "I_IOEXP_SCLK"
		(at 179.07 41.91 0)
	)
	(label "IOEXP_RST_N"
		(at 179.07 44.45 0)
	)
	(label "I_IOEXP_SCLK"
		(at 92.71 60.96 0)
	)
	(label "I_IOEXP_RCLK"
		(at 177.8 107.95 0)
	)
	(label "I_IOEXP_SCLK"
		(at 227.33 41.91 0)
	)
	(hierarchical_label "IOEXP_Q"
		(shape output)
		(at 232.41 130.81 0)
	)
	(hierarchical_label "GPIO_OUT1"
		(shape output)
		(at 144.78 53.34 0)
	)
	(hierarchical_label "GPIO_IN1"
		(shape input)
		(at 191.77 52.07 180)
	)
	(hierarchical_label "GPIO_OUT5"
		(shape output)
		(at 144.78 63.5 0)
	)
	(hierarchical_label "GPIO_OUT2"
		(shape output)
		(at 144.78 55.88 0)
	)
	(hierarchical_label "IOEXP_SCLK"
		(shape input)
		(at 73.66 60.96 180)
	)
	(hierarchical_label "GPIO_IN10"
		(shape input)
		(at 241.3 54.61 180)
	)
	(hierarchical_label "GPIO_IN11"
		(shape input)
		(at 241.3 57.15 180)
	)
	(hierarchical_label "IOEXP_D"
		(shape input)
		(at 73.66 66.04 180)
	)
	(hierarchical_label "GPIO_IN13"
		(shape input)
		(at 241.3 62.23 180)
	)
	(hierarchical_label "GPIO_IN16"
		(shape input)
		(at 191.77 125.73 180)
	)
	(hierarchical_label "GPIO_OUT6"
		(shape output)
		(at 144.78 66.04 0)
	)
	(hierarchical_label "GPIO_IN6"
		(shape input)
		(at 191.77 64.77 180)
	)
	(hierarchical_label "GPIO_IN0"
		(shape input)
		(at 191.77 49.53 180)
	)
	(hierarchical_label "GPIO_IN9"
		(shape input)
		(at 241.3 52.07 180)
	)
	(hierarchical_label "GPIO_IN19"
		(shape input)
		(at 191.77 133.35 180)
	)
	(hierarchical_label "GPIO_IN18"
		(shape input)
		(at 191.77 130.81 180)
	)
	(hierarchical_label "GPIO_IN15"
		(shape input)
		(at 241.3 67.31 180)
	)
	(hierarchical_label "GPIO_IN22"
		(shape input)
		(at 191.77 140.97 180)
	)
	(hierarchical_label "GPIO_OUT7"
		(shape output)
		(at 144.78 68.58 0)
	)
	(hierarchical_label "GPIO_IN3"
		(shape input)
		(at 191.77 57.15 180)
	)
	(hierarchical_label "GPIO_IN7"
		(shape input)
		(at 191.77 67.31 180)
	)
	(hierarchical_label "GPIO_OUT4"
		(shape output)
		(at 144.78 60.96 0)
	)
	(hierarchical_label "GPIO_IN21"
		(shape input)
		(at 191.77 138.43 180)
	)
	(hierarchical_label "GPIO_OUT0"
		(shape output)
		(at 144.78 50.8 0)
	)
	(hierarchical_label "GPIO_IN4"
		(shape input)
		(at 191.77 59.69 180)
	)
	(hierarchical_label "GPIO_IN12"
		(shape input)
		(at 241.3 59.69 180)
	)
	(hierarchical_label "IOEXP_RCLK"
		(shape input)
		(at 73.66 53.34 180)
	)
	(hierarchical_label "GPIO_IN2"
		(shape input)
		(at 191.77 54.61 180)
	)
	(hierarchical_label "GPIO_IN20"
		(shape input)
		(at 191.77 135.89 180)
	)
	(hierarchical_label "GPIO_IN8"
		(shape input)
		(at 241.3 49.53 180)
	)
	(hierarchical_label "IOEXP_RST_N"
		(shape input)
		(at 73.66 58.42 180)
	)
	(hierarchical_label "IOEXP_OE_N"
		(shape input)
		(at 73.66 50.8 180)
	)
	(hierarchical_label "GPIO_OUT3"
		(shape output)
		(at 144.78 58.42 0)
	)
	(hierarchical_label "GPIO_IN14"
		(shape input)
		(at 241.3 64.77 180)
	)
	(hierarchical_label "GPIO_IN23"
		(shape input)
		(at 191.77 143.51 180)
	)
	(hierarchical_label "GPIO_IN5"
		(shape input)
		(at 191.77 62.23 180)
	)
	(hierarchical_label "GPIO_IN17"
		(shape input)
		(at 191.77 128.27 180)
	)
	(symbol
		(lib_id "power:GND")
		(at 110.49 86.36 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0537"
			(at 110.49 86.36 0)
		)
		(property "Value" "GND"
			(at 110.49 91.44 0)
		)
		(property "Footprint" ""
			(at 110.49 86.36 0)
		)
		(property "Datasheet" ""
			(at 110.49 86.36 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 110.49 86.36 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0537")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_33R_1%_0.0625W_100PPM")
		(at 77.47 66.04 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R463"
			(at 78.74 44.704 0)
		)
		(property "Value" "R0402_33R_1%_0.0625W_100PPM"
			(at 77.47 70.993 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 77.47 72.898 0)
		)
		(property "Datasheet" ""
			(at 77.47 74.803 0)
		)
		(property "Description" "±1%"
			(at 81.28 60.96 0)
		)
		(property "Val" "33"
			(at 83.566 44.704 0)
		)
		(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 77.47 76.708 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 77.47 78.613 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 77.47 80.518 0)
		)
		(property "Comment" "33"
			(at 77.47 82.423 0)
		)
		(property "Component Kind" "Standard"
			(at 77.47 84.328 0)
		)
		(property "Component Type" "Standard"
			(at 77.47 86.233 0)
		)
		(property "PackageDescription" " "
			(at 77.47 88.138 0)
		)
		(property "Pin Count" "2"
			(at 77.47 90.043 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 77.47 91.948 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 77.47 93.853 0)
		)
		(property "Status" "Not Recommended"
			(at 77.47 95.758 0)
		)
		(property "Power" "0.0625W"
			(at 77.47 97.663 0)
		)
		(property "Voltage" " "
			(at 77.47 101.473 0)
		)
		(property "Tolerance" "±1%"
			(at 77.47 103.378 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 77.47 105.283 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 77.47 107.188 0)
		)
		(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 77.47 109.093 0)
		)
		(property "Case" "0402"
			(at 77.47 110.998 0)
		)
		(property "PressFit" "No"
			(at 77.47 112.903 0)
		)
		(property "Mounted" "Yes"
			(at 77.47 114.808 0)
		)
		(property "Sense Comment" " "
			(at 77.47 116.713 0)
		)
		(property "Sense" "No"
			(at 77.47 118.618 0)
		)
		(property "Status Comment" " "
			(at 77.47 120.523 0)
		)
		(property "Socket" "No"
			(at 77.47 122.428 0)
		)
		(property "SMD" "Yes"
			(at 77.47 124.333 0)
		)
		(property "ComponentHeight" " "
			(at 77.47 126.238 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 77.47 128.143 0)
		)
		(property "Manufacturer1 Part Number" "232270673309L"
			(at 77.47 130.048 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 77.47 131.953 0)
		)
		(property "HelpURL" ""
			(at 77.47 133.858 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 77.47 135.763 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 77.47 137.668 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 77.47 139.573 0)
		)
		(property "Database Table Name" "Resistors"
			(at 77.47 141.478 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 77.47 143.383 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 77.47 145.288 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 77.47 147.193 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R463")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 106.68 76.2 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0536"
			(at 106.68 76.2 0)
		)
		(property "Value" "P3V3"
			(at 105.41 72.39 90)
		)
		(property "Footprint" ""
			(at 106.68 76.2 0)
		)
		(property "Datasheet" ""
			(at 106.68 76.2 0)
		)
		(property "Description" ""
			(at 106.68 76.2 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0536")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 193.04 74.93 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C277"
			(at 196.85 77.4699 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 186.817 74.93 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 184.912 74.93 0)
		)
		(property "Datasheet" ""
			(at 183.007 74.93 0)
		)
		(property "Description" "100nF"
			(at 193.04 74.93 0)
		)
		(property "SMD" "Yes"
			(at 141.097 74.93 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 181.102 74.93 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 179.197 74.93 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 177.292 74.93 0)
		)
		(property "Comment" "100nF"
			(at 175.387 74.93 0)
		)
		(property "Component Kind" "Standard"
			(at 173.482 74.93 0)
		)
		(property "Component Type" "Standard"
			(at 171.577 74.93 0)
		)
		(property "Pin Count" "2"
			(at 169.672 74.93 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 167.767 74.93 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 165.862 74.93 0)
		)
		(property "PackageDescription" " "
			(at 163.957 74.93 0)
		)
		(property "Status" "Not Recommended"
			(at 162.052 74.93 0)
		)
		(property "Status Comment" " "
			(at 160.147 74.93 0)
		)
		(property "Voltage" "16V"
			(at 158.242 74.93 0)
		)
		(property "Tolerance" "±10%"
			(at 154.432 74.93 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 152.527 74.93 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 150.622 74.93 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 148.717 74.93 0)
		)
		(property "Case" "0402"
			(at 146.812 74.93 0)
		)
		(property "Mounted" "Yes"
			(at 144.907 74.93 0)
		)
		(property "Socket" "No"
			(at 143.002 74.93 0)
		)
		(property "PressFit" " "
			(at 139.192 74.93 0)
		)
		(property "Sense" "No"
			(at 137.287 74.93 0)
		)
		(property "Sense Comment" " "
			(at 135.382 74.93 0)
		)
		(property "ComponentHeight" " "
			(at 133.477 74.93 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 131.572 74.93 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 129.667 74.93 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 127.762 74.93 0)
		)
		(property "HelpURL" ""
			(at 125.857 74.93 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 123.952 74.93 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 122.047 74.93 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 120.142 74.93 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 118.237 74.93 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 116.332 74.93 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 114.427 74.93 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 112.522 74.93 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C277")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_33R_1%_0.0625W_100PPM")
		(at 77.47 60.96 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R462"
			(at 78.74 42.418 0)
		)
		(property "Value" "R0402_33R_1%_0.0625W_100PPM"
			(at 77.47 65.913 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 77.47 67.818 0)
		)
		(property "Datasheet" ""
			(at 77.47 69.723 0)
		)
		(property "Description" "±1%"
			(at 81.28 55.88 0)
		)
		(property "Val" "33"
			(at 83.566 42.418 0)
		)
		(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 77.47 71.628 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 77.47 73.533 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 77.47 75.438 0)
		)
		(property "Comment" "33"
			(at 77.47 77.343 0)
		)
		(property "Component Kind" "Standard"
			(at 77.47 79.248 0)
		)
		(property "Component Type" "Standard"
			(at 77.47 81.153 0)
		)
		(property "PackageDescription" " "
			(at 77.47 83.058 0)
		)
		(property "Pin Count" "2"
			(at 77.47 84.963 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 77.47 86.868 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 77.47 88.773 0)
		)
		(property "Status" "Not Recommended"
			(at 77.47 90.678 0)
		)
		(property "Power" "0.0625W"
			(at 77.47 92.583 0)
		)
		(property "Voltage" " "
			(at 77.47 96.393 0)
		)
		(property "Tolerance" "±1%"
			(at 77.47 98.298 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 77.47 100.203 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 77.47 102.108 0)
		)
		(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 77.47 104.013 0)
		)
		(property "Case" "0402"
			(at 77.47 105.918 0)
		)
		(property "PressFit" "No"
			(at 77.47 107.823 0)
		)
		(property "Mounted" "Yes"
			(at 77.47 109.728 0)
		)
		(property "Sense Comment" " "
			(at 77.47 111.633 0)
		)
		(property "Sense" "No"
			(at 77.47 113.538 0)
		)
		(property "Status Comment" " "
			(at 77.47 115.443 0)
		)
		(property "Socket" "No"
			(at 77.47 117.348 0)
		)
		(property "SMD" "Yes"
			(at 77.47 119.253 0)
		)
		(property "ComponentHeight" " "
			(at 77.47 121.158 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 77.47 123.063 0)
		)
		(property "Manufacturer1 Part Number" "232270673309L"
			(at 77.47 124.968 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 77.47 126.873 0)
		)
		(property "HelpURL" ""
			(at 77.47 128.778 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 77.47 130.683 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 77.47 132.588 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 77.47 134.493 0)
		)
		(property "Database Table Name" "Resistors"
			(at 77.47 136.398 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 77.47 138.303 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 77.47 140.208 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 77.47 142.113 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R462")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 144.78 86.36 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0538"
			(at 144.78 86.36 0)
		)
		(property "Value" "GND"
			(at 147.32 87.6299 0)
		)
		(property "Footprint" ""
			(at 144.78 86.36 0)
		)
		(property "Datasheet" ""
			(at 144.78 86.36 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 144.78 86.36 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0538")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 193.04 158.75 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01036"
			(at 193.04 158.75 0)
		)
		(property "Value" "GND"
			(at 193.04 163.83 0)
		)
		(property "Footprint" ""
			(at 193.04 158.75 0)
		)
		(property "Datasheet" ""
			(at 193.04 158.75 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 193.04 158.75 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01036")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 222.25 158.75 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01041"
			(at 222.25 158.75 0)
		)
		(property "Value" "GND"
			(at 222.25 163.83 0)
		)
		(property "Footprint" ""
			(at 222.25 158.75 0)
		)
		(property "Datasheet" ""
			(at 222.25 158.75 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 222.25 158.75 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01041")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 189.23 148.59 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01035"
			(at 189.23 148.59 0)
		)
		(property "Value" "P3V3"
			(at 185.42 148.5899 90)
		)
		(property "Footprint" ""
			(at 189.23 148.59 0)
		)
		(property "Datasheet" ""
			(at 189.23 148.59 0)
		)
		(property "Description" ""
			(at 189.23 148.59 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01035")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 243.84 39.37 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01126"
			(at 243.84 39.37 0)
		)
		(property "Value" "GND"
			(at 240.03 39.3699 90)
		)
		(property "Footprint" ""
			(at 243.84 39.37 0)
		)
		(property "Datasheet" ""
			(at 243.84 39.37 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 243.84 39.37 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01126")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 193.04 151.13 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C278"
			(at 196.85 153.6699 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 186.817 151.13 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 184.912 151.13 0)
		)
		(property "Datasheet" ""
			(at 183.007 151.13 0)
		)
		(property "Description" "100nF"
			(at 193.04 151.13 0)
		)
		(property "SMD" "Yes"
			(at 141.097 151.13 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 181.102 151.13 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 179.197 151.13 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 177.292 151.13 0)
		)
		(property "Comment" "100nF"
			(at 175.387 151.13 0)
		)
		(property "Component Kind" "Standard"
			(at 173.482 151.13 0)
		)
		(property "Component Type" "Standard"
			(at 171.577 151.13 0)
		)
		(property "Pin Count" "2"
			(at 169.672 151.13 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 167.767 151.13 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 165.862 151.13 0)
		)
		(property "PackageDescription" " "
			(at 163.957 151.13 0)
		)
		(property "Status" "Not Recommended"
			(at 162.052 151.13 0)
		)
		(property "Status Comment" " "
			(at 160.147 151.13 0)
		)
		(property "Voltage" "16V"
			(at 158.242 151.13 0)
		)
		(property "Tolerance" "±10%"
			(at 154.432 151.13 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 152.527 151.13 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 150.622 151.13 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 148.717 151.13 0)
		)
		(property "Case" "0402"
			(at 146.812 151.13 0)
		)
		(property "Mounted" "Yes"
			(at 144.907 151.13 0)
		)
		(property "Socket" "No"
			(at 143.002 151.13 0)
		)
		(property "PressFit" " "
			(at 139.192 151.13 0)
		)
		(property "Sense" "No"
			(at 137.287 151.13 0)
		)
		(property "Sense Comment" " "
			(at 135.382 151.13 0)
		)
		(property "ComponentHeight" " "
			(at 133.477 151.13 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 131.572 151.13 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 129.667 151.13 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 127.762 151.13 0)
		)
		(property "HelpURL" ""
			(at 125.857 151.13 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 123.952 151.13 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 122.047 151.13 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 120.142 151.13 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 118.237 151.13 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 116.332 151.13 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 114.427 151.13 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 112.522 151.13 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C278")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Standard Logic:SN74LV595ARGYR")
		(at 116.84 48.26 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC51"
			(at 127 43.18 0)
		)
		(property "Value" "SN74LV595ARGYR"
			(at 127 45.72 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:TEXAS_RGY (R-PVQFN-N16)"
			(at 116.84 87.63 0)
		)
		(property "Datasheet" ""
			(at 116.84 89.535 0)
		)
		(property "Description" "SN74LV595ARGYR"
			(at 116.84 91.44 0)
		)
		(property "Library Ref" "74595_a"
			(at 116.84 93.345 0)
		)
		(property "Library Path" "SchLib\\Standard Logic.SchLib"
			(at 116.84 95.25 0)
		)
		(property "Comment" "SN74LV595ARGY"
			(at 116.84 97.155 0)
		)
		(property "Component Kind" "Standard"
			(at 116.84 99.06 0)
		)
		(property "Component Type" "Standard"
			(at 116.84 100.965 0)
		)
		(property "Device" "SN74LV595ARGY"
			(at 116.84 102.87 0)
		)
		(property "PackageDescription" "TEXAS Case Style RGY (R-PVQFN-N16), QFN, 0.50mm Pitch, Rect.; 16 Pin, 4.00mm L X 3.50mm W X 1mm H body (w/Thermal Tab 2.65 X 2.15mm)"
			(at 116.84 104.775 0)
		)
		(property "Status" " "
			(at 116.84 106.68 0)
		)
		(property "Part Description" "8-Bit Shift Register with 3-State Output Registers"
			(at 116.84 108.585 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 116.84 110.49 0)
		)
		(property "Manufacturer Part Number" "SN74LV595ARGY"
			(at 116.84 112.395 0)
		)
		(property "Pin Count" "17"
			(at 116.84 114.3 0)
		)
		(property "Case" "QFN16"
			(at 116.84 116.205 0)
		)
		(property "Mounted" "Yes"
			(at 116.84 118.11 0)
		)
		(property "Socket" "No"
			(at 116.84 120.015 0)
		)
		(property "SMD" "Yes"
			(at 116.84 121.92 0)
		)
		(property "PressFit" "No"
			(at 116.84 123.825 0)
		)
		(property "Sense" "No"
			(at 116.84 125.73 0)
		)
		(property "Sense Comment" " "
			(at 116.84 127.635 0)
		)
		(property "Bonding" "No"
			(at 116.84 129.54 0)
		)
		(property "Status Comment" " "
			(at 116.84 131.445 0)
		)
		(property "ComponentHeight" "1mm"
			(at 116.84 133.35 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 116.84 135.255 0)
		)
		(property "Footprint Ref" "TEXAS_RGY (R-PVQFN-N16)"
			(at 116.84 137.16 0)
		)
		(property "Author" "CERN DEM MR"
			(at 116.84 139.065 0)
		)
		(property "HelpURL" ""
			(at 116.84 140.97 0)
		)
		(property "ComponentLink1URL" " "
			(at 116.84 142.875 0)
		)
		(property "ComponentLink1Description" " "
			(at 116.84 144.78 0)
		)
		(property "ComponentLink2URL" " "
			(at 116.84 146.685 0)
		)
		(property "ComponentLink2Description" " "
			(at 116.84 148.59 0)
		)
		(property "CreateDate" "10/10/17 00:00:00"
			(at 116.84 150.495 0)
		)
		(property "LatestRevisionDate" "10/10/17 00:00:00"
			(at 116.84 152.4 0)
		)
		(property "SCEM" " "
			(at 116.84 154.305 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 116.84 156.21 0)
		)
		(property "Library Name" "Standard Logic"
			(at 116.84 158.115 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 116.84 160.02 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 116.84 161.925 0)
		)
		(pin "15")
		(pin "9")
		(pin "4")
		(pin "10")
		(pin "2")
		(pin "12")
		(pin "16")
		(pin "11")
		(pin "6")
		(pin "5")
		(pin "17")
		(pin "8")
		(pin "1")
		(pin "13")
		(pin "14")
		(pin "3")
		(pin "7")
		(instances
			(project "vme-wren"
				(path
					(reference "IC51")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 194.31 39.37 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01125"
			(at 194.31 39.37 0)
		)
		(property "Value" "GND"
			(at 190.5 39.3699 90)
		)
		(property "Footprint" ""
			(at 194.31 39.37 0)
		)
		(property "Datasheet" ""
			(at 194.31 39.37 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 194.31 39.37 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01125")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 194.31 115.57 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01127"
			(at 194.31 115.57 0)
		)
		(property "Value" "GND"
			(at 190.5 115.5699 90)
		)
		(property "Footprint" ""
			(at 194.31 115.57 0)
		)
		(property "Datasheet" ""
			(at 194.31 115.57 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 194.31 115.57 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01127")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 193.04 82.55 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01034"
			(at 193.04 82.55 0)
		)
		(property "Value" "GND"
			(at 193.04 87.63 0)
		)
		(property "Footprint" ""
			(at 193.04 82.55 0)
		)
		(property "Datasheet" ""
			(at 193.04 82.55 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 193.04 82.55 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01034")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_33R_1%_0.0625W_100PPM")
		(at 77.47 53.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R460"
			(at 78.74 37.338 0)
		)
		(property "Value" "R0402_33R_1%_0.0625W_100PPM"
			(at 77.47 58.293 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 77.47 60.198 0)
		)
		(property "Datasheet" ""
			(at 77.47 62.103 0)
		)
		(property "Description" "±1%"
			(at 81.28 48.26 0)
		)
		(property "Val" "33"
			(at 83.566 37.338 0)
		)
		(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 77.47 64.008 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 77.47 65.913 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 77.47 67.818 0)
		)
		(property "Comment" "33"
			(at 77.47 69.723 0)
		)
		(property "Component Kind" "Standard"
			(at 77.47 71.628 0)
		)
		(property "Component Type" "Standard"
			(at 77.47 73.533 0)
		)
		(property "PackageDescription" " "
			(at 77.47 75.438 0)
		)
		(property "Pin Count" "2"
			(at 77.47 77.343 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 77.47 79.248 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 77.47 81.153 0)
		)
		(property "Status" "Not Recommended"
			(at 77.47 83.058 0)
		)
		(property "Power" "0.0625W"
			(at 77.47 84.963 0)
		)
		(property "Voltage" " "
			(at 77.47 88.773 0)
		)
		(property "Tolerance" "±1%"
			(at 77.47 90.678 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 77.47 92.583 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 77.47 94.488 0)
		)
		(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 77.47 96.393 0)
		)
		(property "Case" "0402"
			(at 77.47 98.298 0)
		)
		(property "PressFit" "No"
			(at 77.47 100.203 0)
		)
		(property "Mounted" "Yes"
			(at 77.47 102.108 0)
		)
		(property "Sense Comment" " "
			(at 77.47 104.013 0)
		)
		(property "Sense" "No"
			(at 77.47 105.918 0)
		)
		(property "Status Comment" " "
			(at 77.47 107.823 0)
		)
		(property "Socket" "No"
			(at 77.47 109.728 0)
		)
		(property "SMD" "Yes"
			(at 77.47 111.633 0)
		)
		(property "ComponentHeight" " "
			(at 77.47 113.538 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 77.47 115.443 0)
		)
		(property "Manufacturer1 Part Number" "232270673309L"
			(at 77.47 117.348 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 77.47 119.253 0)
		)
		(property "HelpURL" ""
			(at 77.47 121.158 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 77.47 123.063 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 77.47 124.968 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 77.47 126.873 0)
		)
		(property "Database Table Name" "Resistors"
			(at 77.47 128.778 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 77.47 130.683 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 77.47 132.588 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 77.47 134.493 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R460")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 271.78 82.55 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01040"
			(at 271.78 82.55 0)
		)
		(property "Value" "GND"
			(at 271.78 87.63 0)
		)
		(property "Footprint" ""
			(at 271.78 82.55 0)
		)
		(property "Datasheet" ""
			(at 271.78 82.55 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 271.78 82.55 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01040")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 222.25 82.55 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01039"
			(at 222.25 82.55 0)
		)
		(property "Value" "GND"
			(at 222.25 87.63 0)
		)
		(property "Footprint" ""
			(at 222.25 82.55 0)
		)
		(property "Datasheet" ""
			(at 222.25 82.55 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 222.25 82.55 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01039")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 189.23 72.39 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0564"
			(at 189.23 72.39 0)
		)
		(property "Value" "P3V3"
			(at 185.42 72.3899 90)
		)
		(property "Footprint" ""
			(at 189.23 72.39 0)
		)
		(property "Datasheet" ""
			(at 189.23 72.39 0)
		)
		(property "Description" ""
			(at 189.23 72.39 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0564")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 238.76 72.39 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01037"
			(at 238.76 72.39 0)
		)
		(property "Value" "P3V3"
			(at 234.95 72.3899 90)
		)
		(property "Footprint" ""
			(at 238.76 72.39 0)
		)
		(property "Datasheet" ""
			(at 238.76 72.39 0)
		)
		(property "Description" ""
			(at 238.76 72.39 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01037")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 242.57 82.55 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01038"
			(at 242.57 82.55 0)
		)
		(property "Value" "GND"
			(at 242.57 87.63 0)
		)
		(property "Footprint" ""
			(at 242.57 82.55 0)
		)
		(property "Datasheet" ""
			(at 242.57 82.55 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 242.57 82.55 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01038")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Standard Logic:SN74LV166ANS")
		(at 199.39 29.21 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC52"
			(at 207.01 24.13 0)
		)
		(property "Value" "SN74LV166ANS"
			(at 207.01 26.67 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOIC127P780X200-16N"
			(at 199.39 81.28 0)
		)
		(property "Datasheet" ""
			(at 199.39 83.185 0)
		)
		(property "Description" "SN74LV166ANS"
			(at 199.39 85.09 0)
		)
		(property "Library Ref" "74166"
			(at 199.39 86.995 0)
		)
		(property "Library Path" "SchLib\\Standard Logic.SchLib"
			(at 199.39 88.9 0)
		)
		(property "Comment" "SN74LV166ANS"
			(at 199.39 90.805 0)
		)
		(property "Component Kind" "Standard"
			(at 199.39 92.71 0)
		)
		(property "Component Type" "Standard"
			(at 199.39 94.615 0)
		)
		(property "Device" "SN74LV166ANS"
			(at 199.39 96.52 0)
		)
		(property "PackageDescription" "SOIC, 1.27mm Pitch; 16 Pin, 5.30mm W X 10.2mm L X 2.00mm H body, IPC Medium Density"
			(at 199.39 98.425 0)
		)
		(property "Status" " "
			(at 199.39 100.33 0)
		)
		(property "Part Description" "8-Bit Parallel-Load  Shift Register"
			(at 199.39 102.235 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 199.39 104.14 0)
		)
		(property "Manufacturer Part Number" "SN74LV166ANS"
			(at 199.39 106.045 0)
		)
		(property "Pin Count" "16"
			(at 199.39 107.95 0)
		)
		(property "Case" "SOIC16"
			(at 199.39 109.855 0)
		)
		(property "Mounted" "Yes"
			(at 199.39 111.76 0)
		)
		(property "Socket" "No"
			(at 199.39 113.665 0)
		)
		(property "SMD" "Yes"
			(at 199.39 115.57 0)
		)
		(property "PressFit" "No"
			(at 199.39 117.475 0)
		)
		(property "Sense" "No"
			(at 199.39 119.38 0)
		)
		(property "Sense Comment" " "
			(at 199.39 121.285 0)
		)
		(property "Bonding" "No"
			(at 199.39 123.19 0)
		)
		(property "Status Comment" " "
			(at 199.39 125.095 0)
		)
		(property "ComponentHeight" "2mm"
			(at 199.39 127 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 199.39 128.905 0)
		)
		(property "Footprint Ref" "SOIC127P780X200-16N"
			(at 199.39 130.81 0)
		)
		(property "Author" "CERN DEM BC"
			(at 199.39 132.715 0)
		)
		(property "HelpURL" ""
			(at 199.39 134.62 0)
		)
		(property "ComponentLink1URL" " "
			(at 199.39 136.525 0)
		)
		(property "ComponentLink1Description" " "
			(at 199.39 138.43 0)
		)
		(property "ComponentLink2URL" " "
			(at 199.39 140.335 0)
		)
		(property "ComponentLink2Description" " "
			(at 199.39 142.24 0)
		)
		(property "CreateDate" "04/29/20 00:00:00"
			(at 199.39 144.145 0)
		)
		(property "LatestRevisionDate" "04/29/20 00:00:00"
			(at 199.39 146.05 0)
		)
		(property "SCEM" " "
			(at 199.39 147.955 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 199.39 149.86 0)
		)
		(property "Library Name" "Standard Logic"
			(at 199.39 151.765 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 199.39 153.67 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 199.39 155.575 0)
		)
		(pin "16")
		(pin "10")
		(pin "5")
		(pin "15")
		(pin "7")
		(pin "9")
		(pin "6")
		(pin "4")
		(pin "8")
		(pin "3")
		(pin "13")
		(pin "1")
		(pin "12")
		(pin "11")
		(pin "14")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "IC52")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 242.57 74.93 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C279"
			(at 246.38 77.4699 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 236.347 74.93 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 234.442 74.93 0)
		)
		(property "Datasheet" ""
			(at 232.537 74.93 0)
		)
		(property "Description" "100nF"
			(at 242.57 74.93 0)
		)
		(property "SMD" "Yes"
			(at 190.627 74.93 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 230.632 74.93 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 228.727 74.93 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 226.822 74.93 0)
		)
		(property "Comment" "100nF"
			(at 224.917 74.93 0)
		)
		(property "Component Kind" "Standard"
			(at 223.012 74.93 0)
		)
		(property "Component Type" "Standard"
			(at 221.107 74.93 0)
		)
		(property "Pin Count" "2"
			(at 219.202 74.93 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 217.297 74.93 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 215.392 74.93 0)
		)
		(property "PackageDescription" " "
			(at 213.487 74.93 0)
		)
		(property "Status" "Not Recommended"
			(at 211.582 74.93 0)
		)
		(property "Status Comment" " "
			(at 209.677 74.93 0)
		)
		(property "Voltage" "16V"
			(at 207.772 74.93 0)
		)
		(property "Tolerance" "±10%"
			(at 203.962 74.93 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 202.057 74.93 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 200.152 74.93 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 198.247 74.93 0)
		)
		(property "Case" "0402"
			(at 196.342 74.93 0)
		)
		(property "Mounted" "Yes"
			(at 194.437 74.93 0)
		)
		(property "Socket" "No"
			(at 192.532 74.93 0)
		)
		(property "PressFit" " "
			(at 188.722 74.93 0)
		)
		(property "Sense" "No"
			(at 186.817 74.93 0)
		)
		(property "Sense Comment" " "
			(at 184.912 74.93 0)
		)
		(property "ComponentHeight" " "
			(at 183.007 74.93 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 181.102 74.93 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 179.197 74.93 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 177.292 74.93 0)
		)
		(property "HelpURL" ""
			(at 175.387 74.93 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 173.482 74.93 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 171.577 74.93 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 169.672 74.93 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 167.767 74.93 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 165.862 74.93 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 163.957 74.93 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 162.052 74.93 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C279")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Standard Logic:SN74LV166ANS")
		(at 248.92 29.21 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC56"
			(at 256.54 24.13 0)
		)
		(property "Value" "SN74LV166ANS"
			(at 256.54 26.67 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOIC127P780X200-16N"
			(at 248.92 81.28 0)
		)
		(property "Datasheet" ""
			(at 248.92 83.185 0)
		)
		(property "Description" "SN74LV166ANS"
			(at 248.92 85.09 0)
		)
		(property "Library Ref" "74166"
			(at 248.92 86.995 0)
		)
		(property "Library Path" "SchLib\\Standard Logic.SchLib"
			(at 248.92 88.9 0)
		)
		(property "Comment" "SN74LV166ANS"
			(at 248.92 90.805 0)
		)
		(property "Component Kind" "Standard"
			(at 248.92 92.71 0)
		)
		(property "Component Type" "Standard"
			(at 248.92 94.615 0)
		)
		(property "Device" "SN74LV166ANS"
			(at 248.92 96.52 0)
		)
		(property "PackageDescription" "SOIC, 1.27mm Pitch; 16 Pin, 5.30mm W X 10.2mm L X 2.00mm H body, IPC Medium Density"
			(at 248.92 98.425 0)
		)
		(property "Status" " "
			(at 248.92 100.33 0)
		)
		(property "Part Description" "8-Bit Parallel-Load  Shift Register"
			(at 248.92 102.235 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 248.92 104.14 0)
		)
		(property "Manufacturer Part Number" "SN74LV166ANS"
			(at 248.92 106.045 0)
		)
		(property "Pin Count" "16"
			(at 248.92 107.95 0)
		)
		(property "Case" "SOIC16"
			(at 248.92 109.855 0)
		)
		(property "Mounted" "Yes"
			(at 248.92 111.76 0)
		)
		(property "Socket" "No"
			(at 248.92 113.665 0)
		)
		(property "SMD" "Yes"
			(at 248.92 115.57 0)
		)
		(property "PressFit" "No"
			(at 248.92 117.475 0)
		)
		(property "Sense" "No"
			(at 248.92 119.38 0)
		)
		(property "Sense Comment" " "
			(at 248.92 121.285 0)
		)
		(property "Bonding" "No"
			(at 248.92 123.19 0)
		)
		(property "Status Comment" " "
			(at 248.92 125.095 0)
		)
		(property "ComponentHeight" "2mm"
			(at 248.92 127 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 248.92 128.905 0)
		)
		(property "Footprint Ref" "SOIC127P780X200-16N"
			(at 248.92 130.81 0)
		)
		(property "Author" "CERN DEM BC"
			(at 248.92 132.715 0)
		)
		(property "HelpURL" ""
			(at 248.92 134.62 0)
		)
		(property "ComponentLink1URL" " "
			(at 248.92 136.525 0)
		)
		(property "ComponentLink1Description" " "
			(at 248.92 138.43 0)
		)
		(property "ComponentLink2URL" " "
			(at 248.92 140.335 0)
		)
		(property "ComponentLink2Description" " "
			(at 248.92 142.24 0)
		)
		(property "CreateDate" "04/29/20 00:00:00"
			(at 248.92 144.145 0)
		)
		(property "LatestRevisionDate" "04/29/20 00:00:00"
			(at 248.92 146.05 0)
		)
		(property "SCEM" " "
			(at 248.92 147.955 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 248.92 149.86 0)
		)
		(property "Library Name" "Standard Logic"
			(at 248.92 151.765 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 248.92 153.67 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 248.92 155.575 0)
		)
		(pin "16")
		(pin "10")
		(pin "5")
		(pin "15")
		(pin "7")
		(pin "9")
		(pin "6")
		(pin "4")
		(pin "8")
		(pin "3")
		(pin "13")
		(pin "1")
		(pin "12")
		(pin "11")
		(pin "14")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "IC56")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 110.49 78.74 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C345"
			(at 106.68 81.2799 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 104.267 78.74 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 102.362 78.74 0)
		)
		(property "Datasheet" ""
			(at 100.457 78.74 0)
		)
		(property "Description" "100nF"
			(at 110.49 78.74 0)
		)
		(property "SMD" "Yes"
			(at 58.547 78.74 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 98.552 78.74 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 96.647 78.74 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 94.742 78.74 0)
		)
		(property "Comment" "100nF"
			(at 92.837 78.74 0)
		)
		(property "Component Kind" "Standard"
			(at 90.932 78.74 0)
		)
		(property "Component Type" "Standard"
			(at 89.027 78.74 0)
		)
		(property "Pin Count" "2"
			(at 87.122 78.74 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 85.217 78.74 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 83.312 78.74 0)
		)
		(property "PackageDescription" " "
			(at 81.407 78.74 0)
		)
		(property "Status" "Not Recommended"
			(at 79.502 78.74 0)
		)
		(property "Status Comment" " "
			(at 77.597 78.74 0)
		)
		(property "Voltage" "16V"
			(at 75.692 78.74 0)
		)
		(property "Tolerance" "±10%"
			(at 71.882 78.74 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 69.977 78.74 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 68.072 78.74 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 66.167 78.74 0)
		)
		(property "Case" "0402"
			(at 64.262 78.74 0)
		)
		(property "Mounted" "Yes"
			(at 62.357 78.74 0)
		)
		(property "Socket" "No"
			(at 60.452 78.74 0)
		)
		(property "PressFit" " "
			(at 56.642 78.74 0)
		)
		(property "Sense" "No"
			(at 54.737 78.74 0)
		)
		(property "Sense Comment" " "
			(at 52.832 78.74 0)
		)
		(property "ComponentHeight" " "
			(at 50.927 78.74 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 49.022 78.74 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 47.117 78.74 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 45.212 78.74 0)
		)
		(property "HelpURL" ""
			(at 43.307 78.74 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 41.402 78.74 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 39.497 78.74 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 37.592 78.74 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 35.687 78.74 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 33.782 78.74 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 31.877 78.74 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 29.972 78.74 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C345")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 194.31 34.29 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01042"
			(at 194.31 34.29 0)
		)
		(property "Value" "GND"
			(at 190.5 34.2899 90)
		)
		(property "Footprint" ""
			(at 194.31 34.29 0)
		)
		(property "Datasheet" ""
			(at 194.31 34.29 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 194.31 34.29 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01042")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Standard Logic:SN74LV166ANS")
		(at 199.39 105.41 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC55"
			(at 207.01 100.33 0)
		)
		(property "Value" "SN74LV166ANS"
			(at 207.01 102.87 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOIC127P780X200-16N"
			(at 199.39 157.48 0)
		)
		(property "Datasheet" ""
			(at 199.39 159.385 0)
		)
		(property "Description" "SN74LV166ANS"
			(at 199.39 161.29 0)
		)
		(property "Library Ref" "74166"
			(at 199.39 163.195 0)
		)
		(property "Library Path" "SchLib\\Standard Logic.SchLib"
			(at 199.39 165.1 0)
		)
		(property "Comment" "SN74LV166ANS"
			(at 199.39 167.005 0)
		)
		(property "Component Kind" "Standard"
			(at 199.39 168.91 0)
		)
		(property "Component Type" "Standard"
			(at 199.39 170.815 0)
		)
		(property "Device" "SN74LV166ANS"
			(at 199.39 172.72 0)
		)
		(property "PackageDescription" "SOIC, 1.27mm Pitch; 16 Pin, 5.30mm W X 10.2mm L X 2.00mm H body, IPC Medium Density"
			(at 199.39 174.625 0)
		)
		(property "Status" " "
			(at 199.39 176.53 0)
		)
		(property "Part Description" "8-Bit Parallel-Load  Shift Register"
			(at 199.39 178.435 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 199.39 180.34 0)
		)
		(property "Manufacturer Part Number" "SN74LV166ANS"
			(at 199.39 182.245 0)
		)
		(property "Pin Count" "16"
			(at 199.39 184.15 0)
		)
		(property "Case" "SOIC16"
			(at 199.39 186.055 0)
		)
		(property "Mounted" "Yes"
			(at 199.39 187.96 0)
		)
		(property "Socket" "No"
			(at 199.39 189.865 0)
		)
		(property "SMD" "Yes"
			(at 199.39 191.77 0)
		)
		(property "PressFit" "No"
			(at 199.39 193.675 0)
		)
		(property "Sense" "No"
			(at 199.39 195.58 0)
		)
		(property "Sense Comment" " "
			(at 199.39 197.485 0)
		)
		(property "Bonding" "No"
			(at 199.39 199.39 0)
		)
		(property "Status Comment" " "
			(at 199.39 201.295 0)
		)
		(property "ComponentHeight" "2mm"
			(at 199.39 203.2 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 199.39 205.105 0)
		)
		(property "Footprint Ref" "SOIC127P780X200-16N"
			(at 199.39 207.01 0)
		)
		(property "Author" "CERN DEM BC"
			(at 199.39 208.915 0)
		)
		(property "HelpURL" ""
			(at 199.39 210.82 0)
		)
		(property "ComponentLink1URL" " "
			(at 199.39 212.725 0)
		)
		(property "ComponentLink1Description" " "
			(at 199.39 214.63 0)
		)
		(property "ComponentLink2URL" " "
			(at 199.39 216.535 0)
		)
		(property "ComponentLink2Description" " "
			(at 199.39 218.44 0)
		)
		(property "CreateDate" "04/29/20 00:00:00"
			(at 199.39 220.345 0)
		)
		(property "LatestRevisionDate" "04/29/20 00:00:00"
			(at 199.39 222.25 0)
		)
		(property "SCEM" " "
			(at 199.39 224.155 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 199.39 226.06 0)
		)
		(property "Library Name" "Standard Logic"
			(at 199.39 227.965 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 199.39 229.87 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 199.39 231.775 0)
		)
		(pin "16")
		(pin "10")
		(pin "5")
		(pin "15")
		(pin "7")
		(pin "9")
		(pin "6")
		(pin "4")
		(pin "8")
		(pin "3")
		(pin "13")
		(pin "1")
		(pin "12")
		(pin "11")
		(pin "14")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "IC55")
					(unit 1)
				)
			)
		)
	)
)
