(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A3")
	(title_block
		(title "User Interface")
		(rev "-")
	)
	(lib_symbols
		(symbol "Analog & Interface:CP2105-F01-GM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 20.32 1.27 0)
			)
			(property "Value" "CP2105-F01-GM"
				(at 0 -65.405 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:QFN50P400X400X80-25N-S280"
				(at 0 -67.31 0)
			)
			(property "Datasheet" ""
				(at 0 -69.215 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "CP2105-F01-GM"
				(at 0 -71.12 0)
			)
			(property "Library Ref" "CP2105-F01-GM"
				(at 0 -73.025 0)
			)
			(property "Library Path" "SchLib\\Analog & Interface.SchLib"
				(at 0 -74.93 0)
			)
			(property "Comment" "CP2105-F01-GM"
				(at 0 -76.835 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -78.74 0)
			)
			(property "Component Type" "Standard"
				(at 0 -80.645 0)
			)
			(property "Device" "CP2105-F01-GM"
				(at 0 -82.55 0)
			)
			(property "PackageDescription" "QFN, 0.50mm Pitch, Square; 24 Pin, 4.00mm L X 4.00mm W X 0.80mm H body (w/Thermal Tab 2.80 X 2.80mm), IPC Medium Density"
				(at 0 -84.455 0)
			)
			(property "Status" " "
				(at 0 -86.36 0)
			)
			(property "Part Description" "Single-Chip USB to Dual UART Bridge"
				(at 0 -88.265 0)
			)
			(property "Manufacturer" "SILICON LABS"
				(at 0 -90.17 0)
			)
			(property "Manufacturer Part Number" "CP2105-F01-GM"
				(at 0 -92.075 0)
			)
			(property "Pin Count" "25"
				(at 0 -93.98 0)
			)
			(property "Case" "QFN24"
				(at 0 -95.885 0)
			)
			(property "Mounted" "Yes"
				(at 0 -97.79 0)
			)
			(property "Socket" "No"
				(at 0 -99.695 0)
			)
			(property "SMD" "Yes"
				(at 0 -101.6 0)
			)
			(property "PressFit" "No"
				(at 0 -103.505 0)
			)
			(property "Sense" "No"
				(at 0 -105.41 0)
			)
			(property "Sense Comment" " "
				(at 0 -107.315 0)
			)
			(property "Bonding" "No"
				(at 0 -109.22 0)
			)
			(property "Status Comment" " "
				(at 0 -111.125 0)
			)
			(property "ComponentHeight" "0.8mm"
				(at 0 -113.03 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -114.935 0)
			)
			(property "Footprint Ref" "QFN50P400X400X80-25N-S280"
				(at 0 -116.84 0)
			)
			(property "Author" "CERN DEM MR"
				(at 0 -118.745 0)
			)
			(property "HelpURL" ""
				(at 0 -120.65 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -122.555 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -124.46 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -126.365 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -128.27 0)
			)
			(property "CreateDate" "10/12/16 00:00:00"
				(at 0 -130.175 0)
			)
			(property "LatestRevisionDate" "10/12/16 00:00:00"
				(at 0 -132.08 0)
			)
			(property "SCEM" " "
				(at 0 -133.985 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -135.89 0)
			)
			(property "Library Name" "Analog & Interface"
				(at 0 -137.795 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -139.7 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -141.605 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CP2105-F01-GM_0_1"
				(rectangle
					(start 0 -59.69)
					(end 0.508 -57.404)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0 -60.96)
					(end 40.64 0)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "REGIN")
					(number "7")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "VBUS")
					(number "8")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "D+")
					(number "3")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "D-")
					(number "4")
				)
				(pin power_in line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "VDD")
					(number "6")
				)
				(pin power_in line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "VIO")
					(number "5")
				)
				(pin power_in line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "GND")
					(number "2")
				)
				(pin power_in line
					(at -5.08 -58.42 0)
					(length 5.08)
					(name "EP")
					(number "25")
				)
				(pin bidirectional line
					(at 45.72 -2.54 180)
					(length 5.08)
					(name "~{RST}")
					(number "9")
				)
				(pin input line
					(at 45.72 -12.7 180)
					(length 5.08)
					(name "~{SUSPEND/}RI_SCI")
					(number "1")
				)
				(pin bidirectional line
					(at 45.72 -15.24 180)
					(length 5.08)
					(name "GPIO.0_SCI/DCD_SCI")
					(number "24")
				)
				(pin bidirectional line
					(at 45.72 -17.78 180)
					(length 5.08)
					(name "GPIO.1_SCI/DTR_SCI")
					(number "23")
				)
				(pin bidirectional line
					(at 45.72 -20.32 180)
					(length 5.08)
					(name "GPIO.2_SCI/DSR_SCI")
					(number "22")
				)
				(pin output line
					(at 45.72 -22.86 180)
					(length 5.08)
					(name "TXD_SCI")
					(number "21")
				)
				(pin input line
					(at 45.72 -25.4 180)
					(length 5.08)
					(name "RXD_SCI")
					(number "20")
				)
				(pin output line
					(at 45.72 -27.94 180)
					(length 5.08)
					(name "RTS_SCI")
					(number "19")
				)
				(pin input line
					(at 45.72 -30.48 180)
					(length 5.08)
					(name "CTS_SCI")
					(number "18")
				)
				(pin input line
					(at 45.72 -40.64 180)
					(length 5.08)
					(name "~{SUSPEND/}RI_ECI")
					(number "17")
				)
				(pin input line
					(at 45.72 -43.18 180)
					(length 5.08)
					(name "NC/VPP/DCD_ECI")
					(number "16")
				)
				(pin bidirectional line
					(at 45.72 -45.72 180)
					(length 5.08)
					(name "GPIO.0_ECI/DTR_ECI")
					(number "15")
				)
				(pin bidirectional line
					(at 45.72 -48.26 180)
					(length 5.08)
					(name "GPIO.1_ECI/DSR_ECI")
					(number "14")
				)
				(pin output line
					(at 45.72 -50.8 180)
					(length 5.08)
					(name "TXD_ECI")
					(number "13")
				)
				(pin input line
					(at 45.72 -53.34 180)
					(length 5.08)
					(name "RXD_ECI")
					(number "12")
				)
				(pin output line
					(at 45.72 -55.88 180)
					(length 5.08)
					(name "RTS_ECI")
					(number "11")
				)
				(pin input line
					(at 45.72 -58.42 180)
					(length 5.08)
					(name "CTS_ECI")
					(number "10")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_100NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_100NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" "100nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/05/13 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_100NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_1UF_25V_10%_X5R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_1UF_25V_10%_X5R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Val" "1uF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_1UF_25V_10%_X5R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "1uF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Preferred"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "25V"
				(at 0 -34.798 0)
			)
			(property "TC" "X5R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "TDK"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "02/17/20 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "02/17/20 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_1UF_25V_10%_X5R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Diodes:PRTR5V0U2X"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 5.08 1.27 0)
			)
			(property "Value" "PRTR5V0U2X"
				(at 0 -17.145 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOT190P230X110-4N"
				(at 0 -19.05 0)
			)
			(property "Datasheet" ""
				(at 0 -20.955 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "PRTR5V0U2X"
				(at 0 -22.86 0)
			)
			(property "Library Ref" "PRTR5V0U2X"
				(at 0 -24.765 0)
			)
			(property "Library Path" "SchLib\\Diodes.SchLib"
				(at 0 -26.67 0)
			)
			(property "Comment" "PRTR5V0U2X"
				(at 0 -28.575 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -30.48 0)
			)
			(property "Component Type" "Standard"
				(at 0 -32.385 0)
			)
			(property "Device" "PRTR5V0U2X"
				(at 0 -34.29 0)
			)
			(property "PackageDescription" "SOT143B, SOT, 1.90mm Pitch; 4 Pin, 1.30mm W X 2.90mm L X 1.10mm H body, IPC Medium Density"
				(at 0 -36.195 0)
			)
			(property "Voltage" "5.5V"
				(at 0 -38.1 0)
			)
			(property "Power" " "
				(at 0 -40.005 0)
			)
			(property "Status" " "
				(at 0 -41.91 0)
			)
			(property "Part Description" "Ultra Low Capacitance (1pF) Double Rail-to-Rail ESD Protection Diode (8kV)"
				(at 0 -43.815 0)
			)
			(property "Manufacturer" "NXP SEMICONDUCTORS"
				(at 0 -45.72 0)
			)
			(property "Manufacturer Part Number" "PRTR5V0U2X"
				(at 0 -47.625 0)
			)
			(property "Pin Count" "4"
				(at 0 -49.53 0)
			)
			(property "Case" "SOT143B"
				(at 0 -51.435 0)
			)
			(property "Mounted" "Yes"
				(at 0 -53.34 0)
			)
			(property "Socket" "No"
				(at 0 -55.245 0)
			)
			(property "SMD" "Yes"
				(at 0 -57.15 0)
			)
			(property "PressFit" "No"
				(at 0 -59.055 0)
			)
			(property "Sense" "No"
				(at 0 -60.96 0)
			)
			(property "Sense Comment" " "
				(at 0 -62.865 0)
			)
			(property "Bonding" "No"
				(at 0 -64.77 0)
			)
			(property "Status Comment" " "
				(at 0 -66.675 0)
			)
			(property "ComponentHeight" "1.1mm"
				(at 0 -68.58 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -70.485 0)
			)
			(property "Footprint Ref" "SOT190P230X110-4N"
				(at 0 -72.39 0)
			)
			(property "HelpURL" ""
				(at 0 -74.295 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -76.2 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -78.105 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -80.01 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -81.915 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -83.82 0)
			)
			(property "CreateDate" "03/22/11 00:00:00"
				(at 0 -85.725 0)
			)
			(property "LatestRevisionDate" "03/22/11 00:00:00"
				(at 0 -87.63 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -89.535 0)
			)
			(property "Library Name" "Diodes"
				(at 0 -91.44 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -93.345 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -95.25 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "PRTR5V0U2X_0_1"
				(polyline
					(pts
						(xy 0 -2.54) (xy 10.16 -2.54)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0 -12.7)
					(end 10.16 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 1.27 -2.54) (xy 1.27 -7.62)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 1.27 -2.54)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -5.08) (xy 8.89 -5.08)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 1.27 -5.08)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -7.62) (xy 8.89 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 -6.096) (xy 3.302 -5.08) (xy 2.286 -4.064) (xy 2.286 -6.096)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 2.286 -8.636) (xy 3.302 -7.62) (xy 2.286 -6.604) (xy 2.286 -8.636)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 3.302 -4.064) (xy 3.302 -6.096)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -6.604) (xy 3.302 -8.636)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.064 -3.556) (xy 5.08 -2.54) (xy 4.064 -1.524) (xy 4.064 -3.556)
					)
					(fill
						(type outline)
					)
				)
				(circle
					(center 4.318 -5.08)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 -10.16) (xy 0 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 -10.16) (xy 4.318 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.572 -1.524) (xy 5.08 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -1.524) (xy 5.08 -3.556)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -7.62) (xy 5.08 -10.16)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 5.08 -7.62)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -6.096) (xy 7.112 -5.08) (xy 6.096 -4.064) (xy 6.096 -6.096)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 6.096 -8.636) (xy 7.112 -7.62) (xy 6.096 -6.604) (xy 6.096 -8.636)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 7.112 -4.064) (xy 7.112 -6.096)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.112 -6.604) (xy 7.112 -8.636)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.89 -2.54) (xy 8.89 -7.62)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 8.89 -2.54)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(circle
					(center 8.89 -5.08)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 10.16 -10.16) (xy 5.08 -10.16)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "GND")
					(number "1")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "I/O1")
					(number "2")
				)
				(pin power_in line
					(at 15.24 -2.54 180)
					(length 5.08)
					(name "VCC")
					(number "4")
				)
				(pin bidirectional line
					(at 15.24 -10.16 180)
					(length 5.08)
					(name "I/O2")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "MOLEX:MOLEX_500075-1517"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 7.62 1.27 0)
			)
			(property "Value" "MOLEX_500075-1517"
				(at 0 -24.765 0)
			)
			(property "Footprint" "MOLEX THD:MOLEX_500075-1517"
				(at 0 -26.67 0)
			)
			(property "Datasheet" ""
				(at 0 -28.575 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Family" "USB"
				(at 7.62 -21.59 0)
			)
			(property "Part Number" "MOLEX_500075-1517"
				(at 0 -30.48 0)
			)
			(property "Library Ref" "Connector USB 5 Pin + 1Shield"
				(at 0 -32.385 0)
			)
			(property "Library Path" "SchLib\\Connectors.SchLib"
				(at 0 -34.29 0)
			)
			(property "Comment" " "
				(at 0 -36.195 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -38.1 0)
			)
			(property "Component Type" "Standard"
				(at 0 -40.005 0)
			)
			(property "PackageDescription" " "
				(at 0 -41.91 0)
			)
			(property "Pin Count" "6"
				(at 0 -43.815 0)
			)
			(property "Case" " "
				(at 0 -45.72 0)
			)
			(property "Footprint Path" "PcbLib\\MOLEX THD.PcbLib"
				(at 0 -47.625 0)
			)
			(property "Footprint Ref" "MOLEX_500075-1517"
				(at 0 -49.53 0)
			)
			(property "Family_1" "USB"
				(at 0 -51.435 0)
			)
			(property "Mounted" "Yes"
				(at 0 -53.34 0)
			)
			(property "Socket" "No"
				(at 0 -55.245 0)
			)
			(property "SMD" "No"
				(at 0 -57.15 0)
			)
			(property "PressFit" "No"
				(at 0 -59.055 0)
			)
			(property "Sense" "No"
				(at 0 -60.96 0)
			)
			(property "Sense Comment" " "
				(at 0 -62.865 0)
			)
			(property "Status" "None"
				(at 0 -64.77 0)
			)
			(property "Status Comment" " "
				(at 0 -66.675 0)
			)
			(property "SCEM" " "
				(at 0 -68.58 0)
			)
			(property "Device" " "
				(at 0 -70.485 0)
			)
			(property "Part Description" "USB Mini-B Serie Type 2, Through Hole Straight Receptacle"
				(at 0 -72.39 0)
			)
			(property "Manufacturer" "MOLEX"
				(at 0 -74.295 0)
			)
			(property "Manufacturer Part Number" "500075-1517"
				(at 0 -76.2 0)
			)
			(property "ComponentHeight" "7.7mm"
				(at 0 -78.105 0)
			)
			(property "HelpURL" ""
				(at 0 -80.01 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -81.915 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -83.82 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -85.725 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -87.63 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -89.535 0)
			)
			(property "CreateDate" "07/25/12 00:00:00"
				(at 0 -91.44 0)
			)
			(property "LatestRevisionDate" "07/25/12 00:00:00"
				(at 0 -93.345 0)
			)
			(property "Database Table Name" "Connectors"
				(at 0 -95.25 0)
			)
			(property "Library Name" "MOLEX"
				(at 0 -97.155 0)
			)
			(property "Footprint Library" "MOLEX THD"
				(at 0 -99.06 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -100.965 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "MOLEX_500075-1517_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 15.24 0)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 0 -17.78)
					(radius 0.508)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 0 -20.32) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -20.32) (xy 15.24 -20.32)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0 -20.32)
					(end 15.24 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 8.89 -3.81) (xy 13.97 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.89 -5.08) (xy 11.43 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.89 -7.62) (xy 11.43 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.89 -10.16) (xy 11.43 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.89 -12.7) (xy 11.43 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.89 -15.24) (xy 11.43 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.89 -16.51) (xy 13.97 -16.51)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 10.414 -5.461)
					(end 13.462 -4.699)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 10.414 -8.001)
					(end 13.462 -7.239)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 10.414 -10.541)
					(end 13.462 -9.779)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 10.414 -13.081)
					(end 13.462 -12.319)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 10.414 -15.621)
					(end 13.462 -14.859)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 13.97 -16.51) (xy 13.97 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 15.24 0) (xy 15.24 -20.32)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "VBUS")
					(number "1")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "-D")
					(number "2")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "+D")
					(number "3")
				)
				(pin passive line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "ID")
					(number "4")
				)
				(pin power_in line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "GND")
					(number "5")
				)
				(pin power_in line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "SH")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_10K_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "10k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "10k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671003L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_10K_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Switches:SW_TYCO_1-1571983-0"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 5.08 1.27 0)
			)
			(property "Value" "SW_TYCO_1-1571983-0"
				(at 0 -24.765 0)
			)
			(property "Footprint" "Switches:SW_TYCO_1-1571983-0"
				(at 0 -26.67 0)
			)
			(property "Datasheet" ""
				(at 0 -28.575 0)
			)
			(property "Description" "Switch"
				(at 5.08 -2.032 0)
			)
			(property "Part Number" "SW_TYCO_1-1571983-0"
				(at 0 -30.48 0)
			)
			(property "Library Ref" "SW 8x SPST DIP Switch"
				(at 0 -32.385 0)
			)
			(property "Library Path" "SchLib\\Switches.SchLib"
				(at 0 -34.29 0)
			)
			(property "Comment" " "
				(at 0 -36.195 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -38.1 0)
			)
			(property "Component Type" "Standard"
				(at 0 -40.005 0)
			)
			(property "Pin Count" "16"
				(at 0 -41.91 0)
			)
			(property "Case" " "
				(at 0 -43.815 0)
			)
			(property "Footprint Path" "PcbLib\\Switches.PcbLib"
				(at 0 -45.72 0)
			)
			(property "Footprint Ref" "SW_TYCO_1-1571983-0"
				(at 0 -47.625 0)
			)
			(property "PackageDescription" "Pitch 1.27mm,  Body 11.28x6.2mm, 8 Ways SPST Surface-Mount DIP Switch,TYCO GDH Series"
				(at 0 -49.53 0)
			)
			(property "Family" "Switch"
				(at 0 -51.435 0)
			)
			(property "Mounted" "Yes"
				(at 0 -53.34 0)
			)
			(property "Socket" "No"
				(at 0 -55.245 0)
			)
			(property "SMD" "Yes"
				(at 0 -57.15 0)
			)
			(property "PressFit" "No"
				(at 0 -59.055 0)
			)
			(property "Sense" "No"
				(at 0 -60.96 0)
			)
			(property "Sense Comment" " "
				(at 0 -62.865 0)
			)
			(property "Status" "None"
				(at 0 -64.77 0)
			)
			(property "Status Comment" " "
				(at 0 -66.675 0)
			)
			(property "SCEM" " "
				(at 0 -68.58 0)
			)
			(property "Part Description" "8 Way SPST SMD DIP Switch, Latched, Contact Rating 0.025A 24VDC"
				(at 0 -70.485 0)
			)
			(property "Manufacturer" "TYCO"
				(at 0 -72.39 0)
			)
			(property "Manufacturer Part Number" "1-1571983-0 or GDH08S04"
				(at 0 -74.295 0)
			)
			(property "ComponentHeight" "2.31mm"
				(at 0 -76.2 0)
			)
			(property "Manufacturer1 Example" " "
				(at 0 -78.105 0)
			)
			(property "Manufacturer1 Part Number" " "
				(at 0 -80.01 0)
			)
			(property "Manufacturer1 ComponentHeight" " "
				(at 0 -81.915 0)
			)
			(property "HelpURL" ""
				(at 0 -83.82 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -85.725 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -87.63 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -89.535 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -91.44 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -93.345 0)
			)
			(property "CreateDate" "01/08/09 00:00:00"
				(at 0 -95.25 0)
			)
			(property "LatestRevisionDate" "01/08/09 00:00:00"
				(at 0 -97.155 0)
			)
			(property "Database Table Name" "Eletro-mechanical"
				(at 0 -99.06 0)
			)
			(property "Library Name" "Switches"
				(at 0 -100.965 0)
			)
			(property "Footprint Library" "Switches"
				(at 0 -102.87 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -104.775 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "SW_TYCO_1-1571983-0_0_1"
				(polyline
					(pts
						(xy 0 -2.54) (xy 2.032 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -5.08) (xy 2.032 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -7.62) (xy 2.032 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -10.16) (xy 2.032 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -12.7) (xy 2.032 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -15.24) (xy 2.032 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -17.78) (xy 2.032 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -20.32) (xy 2.032 -20.32)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0 -22.86)
					(end 10.16 0)
					(fill
						(type background)
					)
				)
				(circle
					(center 2.54 -2.54)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -5.08)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -7.62)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -10.16)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -12.7)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -15.24)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -17.78)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 -20.32)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.112 -1.27) (xy 3.048 -2.286)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.112 -3.81) (xy 3.048 -4.826)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.112 -6.35) (xy 3.048 -7.366)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.112 -8.89) (xy 3.048 -9.906)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.112 -11.43) (xy 3.048 -12.446)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.112 -13.97) (xy 3.048 -14.986)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.112 -16.51) (xy 3.048 -17.526)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.112 -19.05) (xy 3.048 -20.066)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 7.62 -2.54)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 7.62 -5.08)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 7.62 -7.62)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 7.62 -10.16)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 7.62 -12.7)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 7.62 -15.24)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 7.62 -17.78)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 7.62 -20.32)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.128 -2.54) (xy 10.16 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.128 -5.08) (xy 10.16 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.128 -7.62) (xy 10.16 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.128 -10.16) (xy 10.16 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.128 -12.7) (xy 10.16 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.128 -15.24) (xy 10.16 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.128 -17.78) (xy 10.16 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.128 -20.32) (xy 10.16 -20.32)
					)
					(fill
						(type none)
					)
				)
				(text "1"
					(at 4.826 -1.016 0)
				)
				(text "2"
					(at 4.826 -3.302 0)
				)
				(text "3"
					(at 4.826 -5.842 0)
				)
				(text "4"
					(at 4.826 -8.382 0)
				)
				(text "5"
					(at 5.08 -10.922 0)
				)
				(text "6"
					(at 5.08 -13.462 0)
				)
				(text "7"
					(at 5.08 -16.002 0)
				)
				(text "8"
					(at 5.08 -18.542 0)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "1")
					(number "1")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "2")
					(number "2")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "3")
					(number "3")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "4")
					(number "4")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "5")
					(number "5")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "6")
					(number "6")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "7")
					(number "7")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "8")
					(number "8")
				)
				(pin bidirectional line
					(at 15.24 -2.54 180)
					(length 5.08)
					(name "16")
					(number "16")
				)
				(pin bidirectional line
					(at 15.24 -5.08 180)
					(length 5.08)
					(name "15")
					(number "15")
				)
				(pin bidirectional line
					(at 15.24 -7.62 180)
					(length 5.08)
					(name "14")
					(number "14")
				)
				(pin bidirectional line
					(at 15.24 -10.16 180)
					(length 5.08)
					(name "13")
					(number "13")
				)
				(pin bidirectional line
					(at 15.24 -12.7 180)
					(length 5.08)
					(name "12")
					(number "12")
				)
				(pin bidirectional line
					(at 15.24 -15.24 180)
					(length 5.08)
					(name "11")
					(number "11")
				)
				(pin bidirectional line
					(at 15.24 -17.78 180)
					(length 5.08)
					(name "10")
					(number "10")
				)
				(pin bidirectional line
					(at 15.24 -20.32 180)
					(length 5.08)
					(name "9")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:PWR_FLAG"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#FLG"
				(at 0 1.905 0)
			)
			(property "Value" "PWR_FLAG"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "general power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "PWR_FLAG_0_0"
				(pin power_out line
					(at 0 0 90)
					(length 0)
					(name "pwr")
					(number "1")
				)
			)
			(symbol "PWR_FLAG_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 1.27) (xy -1.016 1.905) (xy 0 2.54) (xy 1.016 1.905) (xy 0 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P3V3"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0202"
				(at 0 0 0)
			)
			(property "Value" "P3V3"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P3V3_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P3V3")
					(number "")
				)
			)
			(embedded_fonts no)
		)
	)
	(text_box "Manual VME base address switch."
		(exclude_from_sim no)
		(at 236.22 138.43 0)
		(size 40.64 20.32)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 194 1)
		)
	)
	(junction
		(at 215.9 151.13)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 154.94 57.15)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 215.9 158.75)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 148.59 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 128.27 69.85)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 186.69 85.09)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 186.69 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 142.24 156.21)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 180.34 140.97)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 154.94 151.13)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 162.56 59.69)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 215.9 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 186.69 82.55)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 215.9 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 215.9 156.21)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 135.89 158.75)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 176.53 49.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 177.8 85.09)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 187.96 49.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 173.99 143.51)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 186.69 100.33)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 215.9 143.51)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 167.64 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 168.91 62.23)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 215.9 148.59)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 161.29 148.59)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 240.03 69.85)
	)
	(no_connect
		(at 240.03 85.09)
	)
	(no_connect
		(at 240.03 72.39)
	)
	(no_connect
		(at 240.03 82.55)
	)
	(no_connect
		(at 240.03 59.69)
	)
	(no_connect
		(at 240.03 44.45)
	)
	(no_connect
		(at 240.03 97.79)
	)
	(no_connect
		(at 240.03 90.17)
	)
	(no_connect
		(at 240.03 57.15)
	)
	(no_connect
		(at 240.03 87.63)
	)
	(no_connect
		(at 127 64.77)
	)
	(no_connect
		(at 240.03 54.61)
	)
	(no_connect
		(at 240.03 62.23)
	)
	(no_connect
		(at 240.03 100.33)
	)
	(bus_entry
		(at 115.57 148.59)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 115.57 138.43)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 115.57 146.05)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 115.57 140.97)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 115.57 143.51)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 115.57 151.13)
		(size 2.54 2.54)
	)
	(wire
		(pts
			(xy 142.24 135.89) (xy 142.24 156.21)
		)
	)
	(wire
		(pts
			(xy 189.23 100.33) (xy 186.69 100.33)
		)
	)
	(wire
		(pts
			(xy 215.9 148.59) (xy 215.9 151.13)
		)
	)
	(wire
		(pts
			(xy 127 69.85) (xy 128.27 69.85)
		)
	)
	(wire
		(pts
			(xy 186.69 82.55) (xy 186.69 62.23)
		)
	)
	(wire
		(pts
			(xy 177.8 85.09) (xy 186.69 85.09)
		)
	)
	(wire
		(pts
			(xy 167.64 146.05) (xy 193.04 146.05)
		)
	)
	(bus
		(pts
			(xy 115.57 143.51) (xy 115.57 146.05)
		)
	)
	(wire
		(pts
			(xy 161.29 148.59) (xy 193.04 148.59)
		)
	)
	(wire
		(pts
			(xy 240.03 95.25) (xy 250.19 95.25)
		)
	)
	(bus
		(pts
			(xy 115.57 148.59) (xy 115.57 151.13)
		)
	)
	(wire
		(pts
			(xy 173.99 143.51) (xy 173.99 135.89)
		)
	)
	(wire
		(pts
			(xy 162.56 59.69) (xy 162.56 71.12)
		)
	)
	(wire
		(pts
			(xy 182.88 57.15) (xy 189.23 57.15)
		)
	)
	(wire
		(pts
			(xy 193.04 140.97) (xy 180.34 140.97)
		)
	)
	(wire
		(pts
			(xy 186.69 86.36) (xy 186.69 85.09)
		)
	)
	(wire
		(pts
			(xy 215.9 156.21) (xy 213.36 156.21)
		)
	)
	(wire
		(pts
			(xy 148.59 135.89) (xy 148.59 153.67)
		)
	)
	(bus
		(pts
			(xy 110.49 137.16) (xy 115.57 137.16)
		)
	)
	(wire
		(pts
			(xy 177.8 93.98) (xy 177.8 100.33)
		)
	)
	(wire
		(pts
			(xy 215.9 153.67) (xy 215.9 156.21)
		)
	)
	(wire
		(pts
			(xy 154.94 135.89) (xy 154.94 151.13)
		)
	)
	(wire
		(pts
			(xy 154.94 151.13) (xy 193.04 151.13)
		)
	)
	(wire
		(pts
			(xy 118.11 151.13) (xy 154.94 151.13)
		)
	)
	(wire
		(pts
			(xy 148.59 153.67) (xy 193.04 153.67)
		)
	)
	(wire
		(pts
			(xy 189.23 97.79) (xy 186.69 97.79)
		)
	)
	(wire
		(pts
			(xy 128.27 67.31) (xy 128.27 69.85)
		)
	)
	(wire
		(pts
			(xy 213.36 143.51) (xy 215.9 143.51)
		)
	)
	(wire
		(pts
			(xy 168.91 62.23) (xy 180.34 62.23)
		)
	)
	(wire
		(pts
			(xy 154.94 71.12) (xy 154.94 57.15)
		)
	)
	(wire
		(pts
			(xy 127 67.31) (xy 128.27 67.31)
		)
	)
	(wire
		(pts
			(xy 118.11 153.67) (xy 148.59 153.67)
		)
	)
	(wire
		(pts
			(xy 215.9 158.75) (xy 213.36 158.75)
		)
	)
	(wire
		(pts
			(xy 240.03 67.31) (xy 250.19 67.31)
		)
	)
	(wire
		(pts
			(xy 215.9 153.67) (xy 213.36 153.67)
		)
	)
	(wire
		(pts
			(xy 180.34 140.97) (xy 180.34 135.89)
		)
	)
	(wire
		(pts
			(xy 118.11 146.05) (xy 167.64 146.05)
		)
	)
	(bus
		(pts
			(xy 115.57 140.97) (xy 115.57 143.51)
		)
	)
	(wire
		(pts
			(xy 186.69 93.98) (xy 186.69 97.79)
		)
	)
	(wire
		(pts
			(xy 127 62.23) (xy 168.91 62.23)
		)
	)
	(wire
		(pts
			(xy 130.81 158.75) (xy 135.89 158.75)
		)
	)
	(wire
		(pts
			(xy 118.11 140.97) (xy 180.34 140.97)
		)
	)
	(wire
		(pts
			(xy 186.69 97.79) (xy 186.69 100.33)
		)
	)
	(wire
		(pts
			(xy 215.9 143.51) (xy 215.9 140.97)
		)
	)
	(wire
		(pts
			(xy 176.53 57.15) (xy 176.53 49.53)
		)
	)
	(wire
		(pts
			(xy 215.9 156.21) (xy 215.9 158.75)
		)
	)
	(wire
		(pts
			(xy 186.69 85.09) (xy 186.69 82.55)
		)
	)
	(bus
		(pts
			(xy 115.57 137.16) (xy 115.57 138.43)
		)
	)
	(wire
		(pts
			(xy 127 59.69) (xy 162.56 59.69)
		)
	)
	(wire
		(pts
			(xy 215.9 151.13) (xy 215.9 153.67)
		)
	)
	(wire
		(pts
			(xy 154.94 57.15) (xy 176.53 57.15)
		)
	)
	(wire
		(pts
			(xy 130.81 156.21) (xy 142.24 156.21)
		)
	)
	(wire
		(pts
			(xy 135.89 135.89) (xy 135.89 158.75)
		)
	)
	(wire
		(pts
			(xy 166.37 49.53) (xy 176.53 49.53)
		)
	)
	(wire
		(pts
			(xy 215.9 146.05) (xy 215.9 148.59)
		)
	)
	(wire
		(pts
			(xy 213.36 140.97) (xy 215.9 140.97)
		)
	)
	(wire
		(pts
			(xy 182.88 59.69) (xy 182.88 57.15)
		)
	)
	(wire
		(pts
			(xy 162.56 59.69) (xy 182.88 59.69)
		)
	)
	(wire
		(pts
			(xy 215.9 151.13) (xy 213.36 151.13)
		)
	)
	(wire
		(pts
			(xy 215.9 158.75) (xy 215.9 161.29)
		)
	)
	(wire
		(pts
			(xy 167.64 135.89) (xy 167.64 146.05)
		)
	)
	(wire
		(pts
			(xy 180.34 62.23) (xy 180.34 54.61)
		)
	)
	(wire
		(pts
			(xy 168.91 62.23) (xy 168.91 91.44)
		)
	)
	(wire
		(pts
			(xy 142.24 156.21) (xy 193.04 156.21)
		)
	)
	(wire
		(pts
			(xy 162.56 91.44) (xy 168.91 91.44)
		)
	)
	(bus
		(pts
			(xy 115.57 146.05) (xy 115.57 148.59)
		)
	)
	(wire
		(pts
			(xy 215.9 148.59) (xy 213.36 148.59)
		)
	)
	(wire
		(pts
			(xy 118.11 143.51) (xy 173.99 143.51)
		)
	)
	(wire
		(pts
			(xy 187.96 44.45) (xy 187.96 49.53)
		)
	)
	(wire
		(pts
			(xy 128.27 69.85) (xy 128.27 72.39)
		)
	)
	(wire
		(pts
			(xy 189.23 44.45) (xy 187.96 44.45)
		)
	)
	(wire
		(pts
			(xy 173.99 143.51) (xy 193.04 143.51)
		)
	)
	(wire
		(pts
			(xy 250.19 64.77) (xy 240.03 64.77)
		)
	)
	(wire
		(pts
			(xy 135.89 158.75) (xy 193.04 158.75)
		)
	)
	(wire
		(pts
			(xy 215.9 143.51) (xy 215.9 146.05)
		)
	)
	(bus
		(pts
			(xy 115.57 138.43) (xy 115.57 140.97)
		)
	)
	(wire
		(pts
			(xy 186.69 62.23) (xy 189.23 62.23)
		)
	)
	(wire
		(pts
			(xy 180.34 54.61) (xy 189.23 54.61)
		)
	)
	(wire
		(pts
			(xy 127 57.15) (xy 154.94 57.15)
		)
	)
	(wire
		(pts
			(xy 215.9 146.05) (xy 213.36 146.05)
		)
	)
	(wire
		(pts
			(xy 176.53 49.53) (xy 187.96 49.53)
		)
	)
	(wire
		(pts
			(xy 186.69 82.55) (xy 189.23 82.55)
		)
	)
	(wire
		(pts
			(xy 177.8 100.33) (xy 186.69 100.33)
		)
	)
	(wire
		(pts
			(xy 118.11 148.59) (xy 161.29 148.59)
		)
	)
	(wire
		(pts
			(xy 187.96 49.53) (xy 189.23 49.53)
		)
	)
	(wire
		(pts
			(xy 177.8 86.36) (xy 177.8 85.09)
		)
	)
	(wire
		(pts
			(xy 250.19 92.71) (xy 240.03 92.71)
		)
	)
	(wire
		(pts
			(xy 161.29 135.89) (xy 161.29 148.59)
		)
	)
	(label "VMEF.NOGA_N2"
		(at 119.38 146.05 0)
	)
	(label "VMEF.NOGA_N1"
		(at 119.38 143.51 0)
	)
	(label "USB_D_P"
		(at 129.54 62.23 0)
	)
	(label "VMEF.NOGA_N3"
		(at 119.38 148.59 0)
	)
	(label "VMEF.NOGA_N0"
		(at 119.38 140.97 0)
	)
	(label "USB_VBUS"
		(at 129.54 57.15 0)
	)
	(label "USB_D_N"
		(at 129.54 59.69 0)
	)
	(label "VMEF.NOGA_N4"
		(at 119.38 151.13 0)
	)
	(label "VMEF.USEGA_N"
		(at 119.38 153.67 0)
	)
	(hierarchical_label "PL_UART_RXD"
		(shape input)
		(at 250.19 95.25 0)
	)
	(hierarchical_label "PS_UART_RXD"
		(shape input)
		(at 250.19 67.31 0)
	)
	(hierarchical_label "PS_UART_TXD"
		(shape output)
		(at 250.19 64.77 0)
	)
	(hierarchical_label "PL_UART_TXD"
		(shape output)
		(at 250.19 92.71 0)
	)
	(hierarchical_label "SWITCH1_N"
		(shape output)
		(at 130.81 158.75 180)
	)
	(hierarchical_label "{VMEF}"
		(shape bidirectional)
		(at 110.49 137.16 180)
	)
	(hierarchical_label "SWITCH0_N"
		(shape output)
		(at 130.81 156.21 180)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 167.64 128.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R371"
			(at 167.64 115.316 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 162.687 128.27 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 160.782 128.27 0)
		)
		(property "Datasheet" ""
			(at 158.877 128.27 0)
		)
		(property "Description" "±1%"
			(at 172.72 132.08 0)
		)
		(property "Val" "10k"
			(at 167.64 117.348 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 156.972 128.27 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 155.067 128.27 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 153.162 128.27 0)
		)
		(property "Comment" "10k"
			(at 151.257 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 149.352 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 147.447 128.27 0)
		)
		(property "PackageDescription" " "
			(at 145.542 128.27 0)
		)
		(property "Pin Count" "2"
			(at 143.637 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 141.732 128.27 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 139.827 128.27 0)
		)
		(property "Status" "Not Recommended"
			(at 137.922 128.27 0)
		)
		(property "Power" "0.0625W"
			(at 136.017 128.27 0)
		)
		(property "Voltage" " "
			(at 132.207 128.27 0)
		)
		(property "Tolerance" "±1%"
			(at 130.302 128.27 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 128.397 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 126.492 128.27 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 124.587 128.27 0)
		)
		(property "Case" "0402"
			(at 122.682 128.27 0)
		)
		(property "PressFit" "No"
			(at 120.777 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 118.872 128.27 0)
		)
		(property "Sense Comment" " "
			(at 116.967 128.27 0)
		)
		(property "Sense" "No"
			(at 115.062 128.27 0)
		)
		(property "Status Comment" " "
			(at 113.157 128.27 0)
		)
		(property "Socket" "No"
			(at 111.252 128.27 0)
		)
		(property "SMD" "Yes"
			(at 109.347 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 107.442 128.27 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 105.537 128.27 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 103.632 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 101.727 128.27 0)
		)
		(property "HelpURL" ""
			(at 99.822 128.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 97.917 128.27 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 96.012 128.27 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 94.107 128.27 0)
		)
		(property "Database Table Name" "Resistors"
			(at 92.202 128.27 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 90.297 128.27 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 88.392 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 86.487 128.27 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R371")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 177.8 85.09 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG026"
			(at 177.8 83.185 0)
		)
		(property "Value" "PWR_FLAG"
			(at 177.8 80.01 0)
		)
		(property "Footprint" ""
			(at 177.8 85.09 0)
		)
		(property "Datasheet" ""
			(at 177.8 85.09 0)
		)
		(property "Description" "general power-flag symbol"
			(at 177.8 85.09 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG026")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 154.94 57.15 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG027"
			(at 154.94 55.245 0)
		)
		(property "Value" "PWR_FLAG"
			(at 154.94 52.07 0)
		)
		(property "Footprint" ""
			(at 154.94 57.15 0)
		)
		(property "Datasheet" ""
			(at 154.94 57.15 0)
		)
		(property "Description" "general power-flag symbol"
			(at 154.94 57.15 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#FLG027")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 173.99 128.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0700"
			(at 173.99 128.27 0)
		)
		(property "Value" "P3V3"
			(at 173.99 124.46 90)
		)
		(property "Footprint" ""
			(at 173.99 128.27 0)
		)
		(property "Datasheet" ""
			(at 173.99 128.27 0)
		)
		(property "Description" ""
			(at 173.99 128.27 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0700")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diodes:PRTR5V0U2X")
		(at 152.4 86.36 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC4"
			(at 151.13 81.026 0)
		)
		(property "Value" "PRTR5V0U2X"
			(at 169.545 86.36 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOT190P230X110-4N"
			(at 171.45 86.36 0)
		)
		(property "Datasheet" ""
			(at 173.355 86.36 0)
		)
		(property "Description" ""
			(at 152.4 86.36 0)
		)
		(property "SMD" "Yes"
			(at 209.55 86.36 0)
		)
		(property "Part Number" "PRTR5V0U2X"
			(at 175.26 86.36 0)
		)
		(property "Library Ref" "PRTR5V0U2X"
			(at 177.165 86.36 0)
		)
		(property "Library Path" "SchLib\\Diodes.SchLib"
			(at 179.07 86.36 0)
		)
		(property "Comment" "PRTR5V0U2X"
			(at 180.975 86.36 0)
		)
		(property "Component Kind" "Standard"
			(at 182.88 86.36 0)
		)
		(property "Component Type" "Standard"
			(at 184.785 86.36 0)
		)
		(property "Device" "PRTR5V0U2X"
			(at 186.69 86.36 0)
		)
		(property "PackageDescription" "SOT143B, SOT, 1.90mm Pitch; 4 Pin, 1.30mm W X 2.90mm L X 1.10mm H body, IPC Medium Density"
			(at 188.595 86.36 0)
		)
		(property "Voltage" "5.5V"
			(at 190.5 86.36 0)
		)
		(property "Power" " "
			(at 192.405 86.36 0)
		)
		(property "Status" " "
			(at 194.31 86.36 0)
		)
		(property "Part Description" "Ultra Low Capacitance (1pF) Double Rail-to-Rail ESD Protection Diode (8kV)"
			(at 196.215 86.36 0)
		)
		(property "Manufacturer" "NXP SEMICONDUCTORS"
			(at 198.12 86.36 0)
		)
		(property "Manufacturer Part Number" "PRTR5V0U2X"
			(at 200.025 86.36 0)
		)
		(property "Pin Count" "4"
			(at 201.93 86.36 0)
		)
		(property "Case" "SOT143B"
			(at 203.835 86.36 0)
		)
		(property "Mounted" "Yes"
			(at 205.74 86.36 0)
		)
		(property "Socket" "No"
			(at 207.645 86.36 0)
		)
		(property "PressFit" "No"
			(at 211.455 86.36 0)
		)
		(property "Sense" "No"
			(at 213.36 86.36 0)
		)
		(property "Sense Comment" " "
			(at 215.265 86.36 0)
		)
		(property "Bonding" "No"
			(at 217.17 86.36 0)
		)
		(property "Status Comment" " "
			(at 219.075 86.36 0)
		)
		(property "ComponentHeight" "1.1mm"
			(at 220.98 86.36 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 222.885 86.36 0)
		)
		(property "Footprint Ref" "SOT190P230X110-4N"
			(at 224.79 86.36 0)
		)
		(property "HelpURL" ""
			(at 226.695 86.36 0)
		)
		(property "ComponentLink1URL" " "
			(at 228.6 86.36 0)
		)
		(property "ComponentLink1Description" " "
			(at 230.505 86.36 0)
		)
		(property "ComponentLink2URL" " "
			(at 232.41 86.36 0)
		)
		(property "ComponentLink2Description" " "
			(at 234.315 86.36 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 236.22 86.36 0)
		)
		(property "CreateDate" "03/22/11 00:00:00"
			(at 238.125 86.36 0)
		)
		(property "LatestRevisionDate" "03/22/11 00:00:00"
			(at 240.03 86.36 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 241.935 86.36 0)
		)
		(property "Library Name" "Diodes"
			(at 243.84 86.36 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 245.745 86.36 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 247.65 86.36 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(instances
			(project "vme-wren"
				(path
					(reference "IC4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 186.69 100.33 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0384"
			(at 186.69 100.33 0)
		)
		(property "Value" "GND"
			(at 186.69 104.14 0)
		)
		(property "Footprint" ""
			(at 186.69 100.33 0)
		)
		(property "Datasheet" ""
			(at 186.69 100.33 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 186.69 100.33 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0384")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Analog & Interface:CP2105-F01-GM")
		(at 194.31 41.91 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "IC3"
			(at 214.63 40.64 0)
		)
		(property "Value" "CP2105-F01-GM"
			(at 206.248 104.394 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:QFN50P400X400X80-25N-S280"
			(at 194.31 109.22 0)
		)
		(property "Datasheet" ""
			(at 194.31 111.125 0)
		)
		(property "Description" ""
			(at 194.31 41.91 0)
		)
		(property "SMD" "Yes"
			(at 194.31 143.51 0)
		)
		(property "SCEM" " "
			(at 194.31 175.895 0)
		)
		(property "Part Number" "CP2105-F01-GM"
			(at 194.31 113.03 0)
		)
		(property "Library Ref" "CP2105-F01-GM"
			(at 194.31 114.935 0)
		)
		(property "Library Path" "SchLib\\Analog & Interface.SchLib"
			(at 194.31 116.84 0)
		)
		(property "Comment" "CP2105-F01-GM"
			(at 194.31 118.745 0)
		)
		(property "Component Kind" "Standard"
			(at 194.31 120.65 0)
		)
		(property "Component Type" "Standard"
			(at 194.31 122.555 0)
		)
		(property "Device" "CP2105-F01-GM"
			(at 194.31 124.46 0)
		)
		(property "PackageDescription" "QFN, 0.50mm Pitch, Square; 24 Pin, 4.00mm L X 4.00mm W X 0.80mm H body (w/Thermal Tab 2.80 X 2.80mm), IPC Medium Density"
			(at 194.31 126.365 0)
		)
		(property "Status" " "
			(at 194.31 128.27 0)
		)
		(property "Part Description" "Single-Chip USB to Dual UART Bridge"
			(at 194.31 130.175 0)
		)
		(property "Manufacturer" "SILICON LABS"
			(at 194.31 132.08 0)
		)
		(property "Manufacturer Part Number" "CP2105-F01-GM"
			(at 194.31 133.985 0)
		)
		(property "Pin Count" "25"
			(at 194.31 135.89 0)
		)
		(property "Case" "QFN24"
			(at 194.31 137.795 0)
		)
		(property "Mounted" "Yes"
			(at 194.31 139.7 0)
		)
		(property "Socket" "No"
			(at 194.31 141.605 0)
		)
		(property "PressFit" "No"
			(at 194.31 145.415 0)
		)
		(property "Sense" "No"
			(at 194.31 147.32 0)
		)
		(property "Sense Comment" " "
			(at 194.31 149.225 0)
		)
		(property "Bonding" "No"
			(at 194.31 151.13 0)
		)
		(property "Status Comment" " "
			(at 194.31 153.035 0)
		)
		(property "ComponentHeight" "0.8mm"
			(at 194.31 154.94 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 194.31 156.845 0)
		)
		(property "Footprint Ref" "QFN50P400X400X80-25N-S280"
			(at 194.31 158.75 0)
		)
		(property "Author" "CERN DEM MR"
			(at 194.31 160.655 0)
		)
		(property "HelpURL" ""
			(at 194.31 162.56 0)
		)
		(property "ComponentLink1URL" " "
			(at 194.31 164.465 0)
		)
		(property "ComponentLink2URL" " "
			(at 194.31 166.37 0)
		)
		(property "ComponentLink2Description" " "
			(at 194.31 168.275 0)
		)
		(property "ComponentLink1Description" " "
			(at 194.31 170.18 0)
		)
		(property "CreateDate" "10/12/16 00:00:00"
			(at 194.31 172.085 0)
		)
		(property "LatestRevisionDate" "10/12/16 00:00:00"
			(at 194.31 173.99 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 194.31 177.8 0)
		)
		(property "Library Name" "Analog & Interface"
			(at 194.31 179.705 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 194.31 181.61 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 194.31 183.515 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "18")
		(pin "19")
		(pin "2")
		(pin "20")
		(pin "21")
		(pin "22")
		(pin "23")
		(pin "24")
		(pin "25")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 135.89 128.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0659"
			(at 135.89 128.27 0)
		)
		(property "Value" "P3V3"
			(at 135.89 124.46 90)
		)
		(property "Footprint" ""
			(at 135.89 128.27 0)
		)
		(property "Datasheet" ""
			(at 135.89 128.27 0)
		)
		(property "Description" ""
			(at 135.89 128.27 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0659")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 177.8 86.36 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C53"
			(at 181.102 90.17 0)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 171.577 86.36 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 169.672 86.36 0)
		)
		(property "Datasheet" ""
			(at 167.767 86.36 0)
		)
		(property "Description" "100nF"
			(at 177.8 86.36 0)
		)
		(property "SMD" "Yes"
			(at 125.857 86.36 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 165.862 86.36 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 163.957 86.36 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 162.052 86.36 0)
		)
		(property "Comment" "100nF"
			(at 160.147 86.36 0)
		)
		(property "Component Kind" "Standard"
			(at 158.242 86.36 0)
		)
		(property "Component Type" "Standard"
			(at 156.337 86.36 0)
		)
		(property "Pin Count" "2"
			(at 154.432 86.36 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 152.527 86.36 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 150.622 86.36 0)
		)
		(property "PackageDescription" " "
			(at 148.717 86.36 0)
		)
		(property "Status" "Not Recommended"
			(at 146.812 86.36 0)
		)
		(property "Status Comment" " "
			(at 144.907 86.36 0)
		)
		(property "Voltage" "16V"
			(at 143.002 86.36 0)
		)
		(property "Tolerance" "±10%"
			(at 139.192 86.36 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 137.287 86.36 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 135.382 86.36 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 133.477 86.36 0)
		)
		(property "Case" "0402"
			(at 131.572 86.36 0)
		)
		(property "Mounted" "Yes"
			(at 129.667 86.36 0)
		)
		(property "Socket" "No"
			(at 127.762 86.36 0)
		)
		(property "PressFit" " "
			(at 123.952 86.36 0)
		)
		(property "Sense" "No"
			(at 122.047 86.36 0)
		)
		(property "Sense Comment" " "
			(at 120.142 86.36 0)
		)
		(property "ComponentHeight" " "
			(at 118.237 86.36 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 116.332 86.36 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 114.427 86.36 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 112.522 86.36 0)
		)
		(property "HelpURL" ""
			(at 110.617 86.36 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 108.712 86.36 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 106.807 86.36 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 104.902 86.36 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 102.997 86.36 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 101.092 86.36 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 99.187 86.36 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 97.282 86.36 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C53")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 148.59 128.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R344"
			(at 148.59 115.316 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 143.637 128.27 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 141.732 128.27 0)
		)
		(property "Datasheet" ""
			(at 139.827 128.27 0)
		)
		(property "Description" "±1%"
			(at 153.67 132.08 0)
		)
		(property "Val" "10k"
			(at 148.59 117.348 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 137.922 128.27 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 136.017 128.27 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 134.112 128.27 0)
		)
		(property "Comment" "10k"
			(at 132.207 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 130.302 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 128.397 128.27 0)
		)
		(property "PackageDescription" " "
			(at 126.492 128.27 0)
		)
		(property "Pin Count" "2"
			(at 124.587 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 122.682 128.27 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 120.777 128.27 0)
		)
		(property "Status" "Not Recommended"
			(at 118.872 128.27 0)
		)
		(property "Power" "0.0625W"
			(at 116.967 128.27 0)
		)
		(property "Voltage" " "
			(at 113.157 128.27 0)
		)
		(property "Tolerance" "±1%"
			(at 111.252 128.27 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 109.347 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 107.442 128.27 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 105.537 128.27 0)
		)
		(property "Case" "0402"
			(at 103.632 128.27 0)
		)
		(property "PressFit" "No"
			(at 101.727 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 99.822 128.27 0)
		)
		(property "Sense Comment" " "
			(at 97.917 128.27 0)
		)
		(property "Sense" "No"
			(at 96.012 128.27 0)
		)
		(property "Status Comment" " "
			(at 94.107 128.27 0)
		)
		(property "Socket" "No"
			(at 92.202 128.27 0)
		)
		(property "SMD" "Yes"
			(at 90.297 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 88.392 128.27 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 86.487 128.27 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 84.582 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 82.677 128.27 0)
		)
		(property "HelpURL" ""
			(at 80.772 128.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 78.867 128.27 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 76.962 128.27 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 75.057 128.27 0)
		)
		(property "Database Table Name" "Resistors"
			(at 73.152 128.27 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 71.247 128.27 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 69.342 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 67.437 128.27 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R344")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 180.34 128.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R385"
			(at 180.34 115.316 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 175.387 128.27 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 173.482 128.27 0)
		)
		(property "Datasheet" ""
			(at 171.577 128.27 0)
		)
		(property "Description" "±1%"
			(at 185.42 132.08 0)
		)
		(property "Val" "10k"
			(at 180.34 117.348 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 169.672 128.27 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 167.767 128.27 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 165.862 128.27 0)
		)
		(property "Comment" "10k"
			(at 163.957 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 162.052 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 160.147 128.27 0)
		)
		(property "PackageDescription" " "
			(at 158.242 128.27 0)
		)
		(property "Pin Count" "2"
			(at 156.337 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 154.432 128.27 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 152.527 128.27 0)
		)
		(property "Status" "Not Recommended"
			(at 150.622 128.27 0)
		)
		(property "Power" "0.0625W"
			(at 148.717 128.27 0)
		)
		(property "Voltage" " "
			(at 144.907 128.27 0)
		)
		(property "Tolerance" "±1%"
			(at 143.002 128.27 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 141.097 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 139.192 128.27 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 137.287 128.27 0)
		)
		(property "Case" "0402"
			(at 135.382 128.27 0)
		)
		(property "PressFit" "No"
			(at 133.477 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 131.572 128.27 0)
		)
		(property "Sense Comment" " "
			(at 129.667 128.27 0)
		)
		(property "Sense" "No"
			(at 127.762 128.27 0)
		)
		(property "Status Comment" " "
			(at 125.857 128.27 0)
		)
		(property "Socket" "No"
			(at 123.952 128.27 0)
		)
		(property "SMD" "Yes"
			(at 122.047 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 120.142 128.27 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 118.237 128.27 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 116.332 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 114.427 128.27 0)
		)
		(property "HelpURL" ""
			(at 112.522 128.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 110.617 128.27 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 108.712 128.27 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 106.807 128.27 0)
		)
		(property "Database Table Name" "Resistors"
			(at 104.902 128.27 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 102.997 128.27 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 101.092 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 99.187 128.27 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R385")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 158.75 49.53 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0387"
			(at 158.75 49.53 0)
		)
		(property "Value" "GND"
			(at 154.94 49.53 90)
		)
		(property "Footprint" ""
			(at 158.75 49.53 0)
		)
		(property "Datasheet" ""
			(at 158.75 49.53 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 158.75 49.53 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0387")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 161.29 128.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R358"
			(at 161.29 115.316 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 156.337 128.27 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 154.432 128.27 0)
		)
		(property "Datasheet" ""
			(at 152.527 128.27 0)
		)
		(property "Description" "±1%"
			(at 166.37 132.08 0)
		)
		(property "Val" "10k"
			(at 161.29 117.348 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 150.622 128.27 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 148.717 128.27 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 146.812 128.27 0)
		)
		(property "Comment" "10k"
			(at 144.907 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 143.002 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 141.097 128.27 0)
		)
		(property "PackageDescription" " "
			(at 139.192 128.27 0)
		)
		(property "Pin Count" "2"
			(at 137.287 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 135.382 128.27 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 133.477 128.27 0)
		)
		(property "Status" "Not Recommended"
			(at 131.572 128.27 0)
		)
		(property "Power" "0.0625W"
			(at 129.667 128.27 0)
		)
		(property "Voltage" " "
			(at 125.857 128.27 0)
		)
		(property "Tolerance" "±1%"
			(at 123.952 128.27 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 122.047 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 120.142 128.27 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 118.237 128.27 0)
		)
		(property "Case" "0402"
			(at 116.332 128.27 0)
		)
		(property "PressFit" "No"
			(at 114.427 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 112.522 128.27 0)
		)
		(property "Sense Comment" " "
			(at 110.617 128.27 0)
		)
		(property "Sense" "No"
			(at 108.712 128.27 0)
		)
		(property "Status Comment" " "
			(at 106.807 128.27 0)
		)
		(property "Socket" "No"
			(at 104.902 128.27 0)
		)
		(property "SMD" "Yes"
			(at 102.997 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 101.092 128.27 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 99.187 128.27 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 97.282 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 95.377 128.27 0)
		)
		(property "HelpURL" ""
			(at 93.472 128.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 91.567 128.27 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 89.662 128.27 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 87.757 128.27 0)
		)
		(property "Database Table Name" "Resistors"
			(at 85.852 128.27 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 83.947 128.27 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 82.042 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 80.137 128.27 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R358")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 161.29 128.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0697"
			(at 161.29 128.27 0)
		)
		(property "Value" "P3V3"
			(at 161.29 124.46 90)
		)
		(property "Footprint" ""
			(at 161.29 128.27 0)
		)
		(property "Datasheet" ""
			(at 161.29 128.27 0)
		)
		(property "Description" ""
			(at 161.29 128.27 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0697")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switches:SW_TYCO_1-1571983-0")
		(at 198.12 138.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW2"
			(at 203.2 135.89 0)
		)
		(property "Value" "SW_TYCO_1-1571983-0"
			(at 198.12 163.195 0)
		)
		(property "Footprint" "Switches:SW_TYCO_1-1571983-0"
			(at 198.12 165.1 0)
		)
		(property "Datasheet" ""
			(at 198.12 167.005 0)
		)
		(property "Description" "Switch"
			(at 203.2 140.462 0)
		)
		(property "Part Number" "SW_TYCO_1-1571983-0"
			(at 198.12 168.91 0)
		)
		(property "Library Ref" "SW 8x SPST DIP Switch"
			(at 198.12 170.815 0)
		)
		(property "Library Path" "SchLib\\Switches.SchLib"
			(at 198.12 172.72 0)
		)
		(property "Comment" " "
			(at 198.12 174.625 0)
		)
		(property "Component Kind" "Standard"
			(at 198.12 176.53 0)
		)
		(property "Component Type" "Standard"
			(at 198.12 178.435 0)
		)
		(property "Pin Count" "16"
			(at 198.12 180.34 0)
		)
		(property "Case" " "
			(at 198.12 182.245 0)
		)
		(property "Footprint Path" "PcbLib\\Switches.PcbLib"
			(at 198.12 184.15 0)
		)
		(property "Footprint Ref" "SW_TYCO_1-1571983-0"
			(at 198.12 186.055 0)
		)
		(property "PackageDescription" "Pitch 1.27mm,  Body 11.28x6.2mm, 8 Ways SPST Surface-Mount DIP Switch,TYCO GDH Series"
			(at 198.12 187.96 0)
		)
		(property "Family" "Switch"
			(at 198.12 189.865 0)
		)
		(property "Mounted" "Yes"
			(at 198.12 191.77 0)
		)
		(property "Socket" "No"
			(at 198.12 193.675 0)
		)
		(property "SMD" "Yes"
			(at 198.12 195.58 0)
		)
		(property "PressFit" "No"
			(at 198.12 197.485 0)
		)
		(property "Sense" "No"
			(at 198.12 199.39 0)
		)
		(property "Sense Comment" " "
			(at 198.12 201.295 0)
		)
		(property "Status" "None"
			(at 198.12 203.2 0)
		)
		(property "Status Comment" " "
			(at 198.12 205.105 0)
		)
		(property "SCEM" " "
			(at 198.12 207.01 0)
		)
		(property "Part Description" "8 Way SPST SMD DIP Switch, Latched, Contact Rating 0.025A 24VDC"
			(at 198.12 208.915 0)
		)
		(property "Manufacturer" "TYCO"
			(at 198.12 210.82 0)
		)
		(property "Manufacturer Part Number" "1-1571983-0 or GDH08S04"
			(at 198.12 212.725 0)
		)
		(property "ComponentHeight" "2.31mm"
			(at 198.12 214.63 0)
		)
		(property "Manufacturer1 Example" " "
			(at 198.12 216.535 0)
		)
		(property "Manufacturer1 Part Number" " "
			(at 198.12 218.44 0)
		)
		(property "Manufacturer1 ComponentHeight" " "
			(at 198.12 220.345 0)
		)
		(property "HelpURL" ""
			(at 198.12 222.25 0)
		)
		(property "ComponentLink1URL" " "
			(at 198.12 224.155 0)
		)
		(property "ComponentLink1Description" " "
			(at 198.12 226.06 0)
		)
		(property "ComponentLink2URL" " "
			(at 198.12 227.965 0)
		)
		(property "ComponentLink2Description" " "
			(at 198.12 229.87 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 198.12 231.775 0)
		)
		(property "CreateDate" "01/08/09 00:00:00"
			(at 198.12 233.68 0)
		)
		(property "LatestRevisionDate" "01/08/09 00:00:00"
			(at 198.12 235.585 0)
		)
		(property "Database Table Name" "Eletro-mechanical"
			(at 198.12 237.49 0)
		)
		(property "Library Name" "Switches"
			(at 198.12 239.395 0)
		)
		(property "Footprint Library" "Switches"
			(at 198.12 241.3 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 198.12 243.205 0)
		)
		(pin "14")
		(pin "12")
		(pin "6")
		(pin "3")
		(pin "16")
		(pin "5")
		(pin "8")
		(pin "13")
		(pin "2")
		(pin "7")
		(pin "15")
		(pin "1")
		(pin "9")
		(pin "10")
		(pin "11")
		(pin "4")
		(instances
			(project "vme-wren"
				(path
					(reference "SW2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 173.99 128.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R372"
			(at 173.99 115.316 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 169.037 128.27 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 167.132 128.27 0)
		)
		(property "Datasheet" ""
			(at 165.227 128.27 0)
		)
		(property "Description" "±1%"
			(at 179.07 132.08 0)
		)
		(property "Val" "10k"
			(at 173.99 117.348 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 163.322 128.27 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 161.417 128.27 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 159.512 128.27 0)
		)
		(property "Comment" "10k"
			(at 157.607 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 155.702 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 153.797 128.27 0)
		)
		(property "PackageDescription" " "
			(at 151.892 128.27 0)
		)
		(property "Pin Count" "2"
			(at 149.987 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 148.082 128.27 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 146.177 128.27 0)
		)
		(property "Status" "Not Recommended"
			(at 144.272 128.27 0)
		)
		(property "Power" "0.0625W"
			(at 142.367 128.27 0)
		)
		(property "Voltage" " "
			(at 138.557 128.27 0)
		)
		(property "Tolerance" "±1%"
			(at 136.652 128.27 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 134.747 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 132.842 128.27 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 130.937 128.27 0)
		)
		(property "Case" "0402"
			(at 129.032 128.27 0)
		)
		(property "PressFit" "No"
			(at 127.127 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 125.222 128.27 0)
		)
		(property "Sense Comment" " "
			(at 123.317 128.27 0)
		)
		(property "Sense" "No"
			(at 121.412 128.27 0)
		)
		(property "Status Comment" " "
			(at 119.507 128.27 0)
		)
		(property "Socket" "No"
			(at 117.602 128.27 0)
		)
		(property "SMD" "Yes"
			(at 115.697 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 113.792 128.27 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 111.887 128.27 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 109.982 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 108.077 128.27 0)
		)
		(property "HelpURL" ""
			(at 106.172 128.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 104.267 128.27 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 102.362 128.27 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 100.457 128.27 0)
		)
		(property "Database Table Name" "Resistors"
			(at 98.552 128.27 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 96.647 128.27 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 94.742 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 92.837 128.27 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R372")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 154.94 91.44 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0388"
			(at 154.94 91.44 0)
		)
		(property "Value" "GND"
			(at 154.94 95.25 0)
		)
		(property "Footprint" ""
			(at 154.94 91.44 0)
		)
		(property "Datasheet" ""
			(at 154.94 91.44 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 154.94 91.44 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0388")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 142.24 128.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0660"
			(at 142.24 128.27 0)
		)
		(property "Value" "P3V3"
			(at 142.24 124.46 90)
		)
		(property "Footprint" ""
			(at 142.24 128.27 0)
		)
		(property "Datasheet" ""
			(at 142.24 128.27 0)
		)
		(property "Description" ""
			(at 142.24 128.27 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0660")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 135.89 128.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R330"
			(at 135.89 115.316 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 130.937 128.27 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 129.032 128.27 0)
		)
		(property "Datasheet" ""
			(at 127.127 128.27 0)
		)
		(property "Description" "±1%"
			(at 140.97 132.08 0)
		)
		(property "Val" "10k"
			(at 135.89 117.348 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 125.222 128.27 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 123.317 128.27 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 121.412 128.27 0)
		)
		(property "Comment" "10k"
			(at 119.507 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 117.602 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 115.697 128.27 0)
		)
		(property "PackageDescription" " "
			(at 113.792 128.27 0)
		)
		(property "Pin Count" "2"
			(at 111.887 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 109.982 128.27 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 108.077 128.27 0)
		)
		(property "Status" "Not Recommended"
			(at 106.172 128.27 0)
		)
		(property "Power" "0.0625W"
			(at 104.267 128.27 0)
		)
		(property "Voltage" " "
			(at 100.457 128.27 0)
		)
		(property "Tolerance" "±1%"
			(at 98.552 128.27 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 96.647 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 94.742 128.27 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 92.837 128.27 0)
		)
		(property "Case" "0402"
			(at 90.932 128.27 0)
		)
		(property "PressFit" "No"
			(at 89.027 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 87.122 128.27 0)
		)
		(property "Sense Comment" " "
			(at 85.217 128.27 0)
		)
		(property "Sense" "No"
			(at 83.312 128.27 0)
		)
		(property "Status Comment" " "
			(at 81.407 128.27 0)
		)
		(property "Socket" "No"
			(at 79.502 128.27 0)
		)
		(property "SMD" "Yes"
			(at 77.597 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 75.692 128.27 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 73.787 128.27 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 71.882 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 69.977 128.27 0)
		)
		(property "HelpURL" ""
			(at 68.072 128.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 66.167 128.27 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 64.262 128.27 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 62.357 128.27 0)
		)
		(property "Database Table Name" "Resistors"
			(at 60.452 128.27 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 58.547 128.27 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 56.642 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 54.737 128.27 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R330")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 154.94 128.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0662"
			(at 154.94 128.27 0)
		)
		(property "Value" "P3V3"
			(at 154.94 124.46 90)
		)
		(property "Footprint" ""
			(at 154.94 128.27 0)
		)
		(property "Datasheet" ""
			(at 154.94 128.27 0)
		)
		(property "Description" ""
			(at 154.94 128.27 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0662")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 154.94 128.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R357"
			(at 154.94 115.316 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 149.987 128.27 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 148.082 128.27 0)
		)
		(property "Datasheet" ""
			(at 146.177 128.27 0)
		)
		(property "Description" "±1%"
			(at 160.02 132.08 0)
		)
		(property "Val" "10k"
			(at 154.94 117.348 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 144.272 128.27 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 142.367 128.27 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 140.462 128.27 0)
		)
		(property "Comment" "10k"
			(at 138.557 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 136.652 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 134.747 128.27 0)
		)
		(property "PackageDescription" " "
			(at 132.842 128.27 0)
		)
		(property "Pin Count" "2"
			(at 130.937 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 129.032 128.27 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 127.127 128.27 0)
		)
		(property "Status" "Not Recommended"
			(at 125.222 128.27 0)
		)
		(property "Power" "0.0625W"
			(at 123.317 128.27 0)
		)
		(property "Voltage" " "
			(at 119.507 128.27 0)
		)
		(property "Tolerance" "±1%"
			(at 117.602 128.27 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 115.697 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 113.792 128.27 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 111.887 128.27 0)
		)
		(property "Case" "0402"
			(at 109.982 128.27 0)
		)
		(property "PressFit" "No"
			(at 108.077 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 106.172 128.27 0)
		)
		(property "Sense Comment" " "
			(at 104.267 128.27 0)
		)
		(property "Sense" "No"
			(at 102.362 128.27 0)
		)
		(property "Status Comment" " "
			(at 100.457 128.27 0)
		)
		(property "Socket" "No"
			(at 98.552 128.27 0)
		)
		(property "SMD" "Yes"
			(at 96.647 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 94.742 128.27 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 92.837 128.27 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 90.932 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 89.027 128.27 0)
		)
		(property "HelpURL" ""
			(at 87.122 128.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 85.217 128.27 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 83.312 128.27 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 81.407 128.27 0)
		)
		(property "Database Table Name" "Resistors"
			(at 79.502 128.27 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 77.597 128.27 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 75.692 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 73.787 128.27 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R357")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 215.9 161.29 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0658"
			(at 215.9 161.29 0)
		)
		(property "Value" "GND"
			(at 215.9 165.1 0)
		)
		(property "Footprint" ""
			(at 215.9 161.29 0)
		)
		(property "Datasheet" ""
			(at 215.9 161.29 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 215.9 161.29 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0658")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "MOLEX:MOLEX_500075-1517")
		(at 121.92 52.07 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J2"
			(at 114.3 50.8 0)
		)
		(property "Value" "MOLEX_500075-1517"
			(at 121.92 76.835 0)
		)
		(property "Footprint" "MOLEX THD:MOLEX_500075-1517"
			(at 121.92 78.74 0)
		)
		(property "Datasheet" ""
			(at 121.92 80.645 0)
		)
		(property "Description" ""
			(at 121.92 52.07 0)
		)
		(property "SMD" "No"
			(at 121.92 109.22 0)
		)
		(property "SCEM" " "
			(at 121.92 120.65 0)
		)
		(property "Family" "USB"
			(at 114.3 73.66 0)
		)
		(property "Part Number" "MOLEX_500075-1517"
			(at 121.92 82.55 0)
		)
		(property "Library Ref" "Connector USB 5 Pin + 1Shield"
			(at 121.92 84.455 0)
		)
		(property "Library Path" "SchLib\\Connectors.SchLib"
			(at 121.92 86.36 0)
		)
		(property "Comment" " "
			(at 121.92 88.265 0)
		)
		(property "Component Kind" "Standard"
			(at 121.92 90.17 0)
		)
		(property "Component Type" "Standard"
			(at 121.92 92.075 0)
		)
		(property "PackageDescription" " "
			(at 121.92 93.98 0)
		)
		(property "Pin Count" "6"
			(at 121.92 95.885 0)
		)
		(property "Case" " "
			(at 121.92 97.79 0)
		)
		(property "Footprint Path" "PcbLib\\MOLEX THD.PcbLib"
			(at 121.92 99.695 0)
		)
		(property "Footprint Ref" "MOLEX_500075-1517"
			(at 121.92 101.6 0)
		)
		(property "Mounted" "Yes"
			(at 121.92 105.41 0)
		)
		(property "Socket" "No"
			(at 121.92 107.315 0)
		)
		(property "PressFit" "No"
			(at 121.92 111.125 0)
		)
		(property "Sense" "No"
			(at 121.92 113.03 0)
		)
		(property "Sense Comment" " "
			(at 121.92 114.935 0)
		)
		(property "Status" "None"
			(at 121.92 116.84 0)
		)
		(property "Status Comment" " "
			(at 121.92 118.745 0)
		)
		(property "Device" " "
			(at 121.92 122.555 0)
		)
		(property "Part Description" "USB Mini-B Serie Type 2, Through Hole Straight Receptacle"
			(at 121.92 124.46 0)
		)
		(property "Manufacturer" "MOLEX"
			(at 121.92 126.365 0)
		)
		(property "Manufacturer Part Number" "500075-1517"
			(at 121.92 128.27 0)
		)
		(property "ComponentHeight" "7.7mm"
			(at 121.92 130.175 0)
		)
		(property "HelpURL" ""
			(at 121.92 132.08 0)
		)
		(property "ComponentLink1URL" " "
			(at 121.92 133.985 0)
		)
		(property "ComponentLink1Description" " "
			(at 121.92 135.89 0)
		)
		(property "ComponentLink2URL" " "
			(at 121.92 137.795 0)
		)
		(property "ComponentLink2Description" " "
			(at 121.92 139.7 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 121.92 141.605 0)
		)
		(property "CreateDate" "07/25/12 00:00:00"
			(at 121.92 143.51 0)
		)
		(property "LatestRevisionDate" "07/25/12 00:00:00"
			(at 121.92 145.415 0)
		)
		(property "Database Table Name" "Connectors"
			(at 121.92 147.32 0)
		)
		(property "Library Name" "MOLEX"
			(at 121.92 149.225 0)
		)
		(property "Footprint Library" "MOLEX THD"
			(at 121.92 151.13 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 121.92 153.035 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(instances
			(project "vme-wren"
				(path
					(reference "J2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 166.37 49.53 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C148"
			(at 162.56 46.228 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 166.37 55.753 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 166.37 57.658 0)
		)
		(property "Datasheet" ""
			(at 166.37 59.563 0)
		)
		(property "Description" ""
			(at 166.37 49.53 0)
		)
		(property "SMD" "Yes"
			(at 166.37 101.473 0)
		)
		(property "Val" "1uF"
			(at 162.56 52.578 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 166.37 61.468 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 166.37 63.373 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 166.37 65.278 0)
		)
		(property "Comment" "1uF"
			(at 166.37 67.183 0)
		)
		(property "Component Kind" "Standard"
			(at 166.37 69.088 0)
		)
		(property "Component Type" "Standard"
			(at 166.37 70.993 0)
		)
		(property "Pin Count" "2"
			(at 166.37 72.898 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 166.37 74.803 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 166.37 76.708 0)
		)
		(property "PackageDescription" " "
			(at 166.37 78.613 0)
		)
		(property "Status" "Preferred"
			(at 166.37 80.518 0)
		)
		(property "Status Comment" " "
			(at 166.37 82.423 0)
		)
		(property "Voltage" "25V"
			(at 166.37 84.328 0)
		)
		(property "Tolerance" "±10%"
			(at 166.37 88.138 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 166.37 90.043 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 166.37 91.948 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 166.37 93.853 0)
		)
		(property "Case" "0402"
			(at 166.37 95.758 0)
		)
		(property "Mounted" "Yes"
			(at 166.37 97.663 0)
		)
		(property "Socket" "No"
			(at 166.37 99.568 0)
		)
		(property "PressFit" " "
			(at 166.37 103.378 0)
		)
		(property "Sense" "No"
			(at 166.37 105.283 0)
		)
		(property "Sense Comment" " "
			(at 166.37 107.188 0)
		)
		(property "ComponentHeight" " "
			(at 166.37 109.093 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 166.37 110.998 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 166.37 112.903 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 166.37 114.808 0)
		)
		(property "HelpURL" ""
			(at 166.37 116.713 0)
		)
		(property "Author" "CERN DEM BC"
			(at 166.37 118.618 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 166.37 120.523 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 166.37 122.428 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 166.37 124.333 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 166.37 126.238 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 166.37 128.143 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 166.37 130.048 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C148")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 142.24 128.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R343"
			(at 142.24 115.316 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 137.287 128.27 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 135.382 128.27 0)
		)
		(property "Datasheet" ""
			(at 133.477 128.27 0)
		)
		(property "Description" "±1%"
			(at 147.32 132.08 0)
		)
		(property "Val" "10k"
			(at 142.24 117.348 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 131.572 128.27 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 129.667 128.27 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 127.762 128.27 0)
		)
		(property "Comment" "10k"
			(at 125.857 128.27 0)
		)
		(property "Component Kind" "Standard"
			(at 123.952 128.27 0)
		)
		(property "Component Type" "Standard"
			(at 122.047 128.27 0)
		)
		(property "PackageDescription" " "
			(at 120.142 128.27 0)
		)
		(property "Pin Count" "2"
			(at 118.237 128.27 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 116.332 128.27 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 114.427 128.27 0)
		)
		(property "Status" "Not Recommended"
			(at 112.522 128.27 0)
		)
		(property "Power" "0.0625W"
			(at 110.617 128.27 0)
		)
		(property "Voltage" " "
			(at 106.807 128.27 0)
		)
		(property "Tolerance" "±1%"
			(at 104.902 128.27 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 102.997 128.27 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 101.092 128.27 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 99.187 128.27 0)
		)
		(property "Case" "0402"
			(at 97.282 128.27 0)
		)
		(property "PressFit" "No"
			(at 95.377 128.27 0)
		)
		(property "Mounted" "Yes"
			(at 93.472 128.27 0)
		)
		(property "Sense Comment" " "
			(at 91.567 128.27 0)
		)
		(property "Sense" "No"
			(at 89.662 128.27 0)
		)
		(property "Status Comment" " "
			(at 87.757 128.27 0)
		)
		(property "Socket" "No"
			(at 85.852 128.27 0)
		)
		(property "SMD" "Yes"
			(at 83.947 128.27 0)
		)
		(property "ComponentHeight" " "
			(at 82.042 128.27 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 80.137 128.27 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 78.232 128.27 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 76.327 128.27 0)
		)
		(property "HelpURL" ""
			(at 74.422 128.27 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 72.517 128.27 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 70.612 128.27 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 68.707 128.27 0)
		)
		(property "Database Table Name" "Resistors"
			(at 66.802 128.27 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 64.897 128.27 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 62.992 128.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 61.087 128.27 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R343")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 128.27 72.39 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0383"
			(at 128.27 72.39 0)
		)
		(property "Value" "GND"
			(at 128.27 76.2 0)
		)
		(property "Footprint" ""
			(at 128.27 72.39 0)
		)
		(property "Datasheet" ""
			(at 128.27 72.39 0)
		)
		(property "Description" "GROUND power-flag symbol"
			(at 128.27 72.39 0)
		)
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR0383")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 167.64 128.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0699"
			(at 167.64 128.27 0)
		)
		(property "Value" "P3V3"
			(at 167.64 124.46 90)
		)
		(property "Footprint" ""
			(at 167.64 128.27 0)
		)
		(property "Datasheet" ""
			(at 167.64 128.27 0)
		)
		(property "Description" ""
			(at 167.64 128.27 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0699")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 180.34 128.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0706"
			(at 180.34 128.27 0)
		)
		(property "Value" "P3V3"
			(at 180.34 124.46 90)
		)
		(property "Footprint" ""
			(at 180.34 128.27 0)
		)
		(property "Datasheet" ""
			(at 180.34 128.27 0)
		)
		(property "Description" ""
			(at 180.34 128.27 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0706")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 148.59 128.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0661"
			(at 148.59 128.27 0)
		)
		(property "Value" "P3V3"
			(at 148.59 124.46 90)
		)
		(property "Footprint" ""
			(at 148.59 128.27 0)
		)
		(property "Datasheet" ""
			(at 148.59 128.27 0)
		)
		(property "Description" ""
			(at 148.59 128.27 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0661")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_1UF_25V_10%_X5R")
		(at 186.69 86.36 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C52"
			(at 189.738 90.17 0)
		)
		(property "Value" "CC0402_1UF_25V_10%_X5R"
			(at 180.467 86.36 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 178.562 86.36 0)
		)
		(property "Datasheet" ""
			(at 176.657 86.36 0)
		)
		(property "Description" ""
			(at 186.69 86.36 0)
		)
		(property "SMD" "Yes"
			(at 134.747 86.36 0)
		)
		(property "Val" "1uF"
			(at 183.642 90.17 0)
		)
		(property "Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 174.752 86.36 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 172.847 86.36 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 170.942 86.36 0)
		)
		(property "Comment" "1uF"
			(at 169.037 86.36 0)
		)
		(property "Component Kind" "Standard"
			(at 167.132 86.36 0)
		)
		(property "Component Type" "Standard"
			(at 165.227 86.36 0)
		)
		(property "Pin Count" "2"
			(at 163.322 86.36 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 161.417 86.36 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 159.512 86.36 0)
		)
		(property "PackageDescription" " "
			(at 157.607 86.36 0)
		)
		(property "Status" "Preferred"
			(at 155.702 86.36 0)
		)
		(property "Status Comment" " "
			(at 153.797 86.36 0)
		)
		(property "Voltage" "25V"
			(at 151.892 86.36 0)
		)
		(property "Tolerance" "±10%"
			(at 148.082 86.36 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 146.177 86.36 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 144.272 86.36 0)
		)
		(property "Manufacturer Part Number" "CC0402_1UF_25V_10%_X5R"
			(at 142.367 86.36 0)
		)
		(property "Case" "0402"
			(at 140.462 86.36 0)
		)
		(property "Mounted" "Yes"
			(at 138.557 86.36 0)
		)
		(property "Socket" "No"
			(at 136.652 86.36 0)
		)
		(property "PressFit" " "
			(at 132.842 86.36 0)
		)
		(property "Sense" "No"
			(at 130.937 86.36 0)
		)
		(property "Sense Comment" " "
			(at 129.032 86.36 0)
		)
		(property "ComponentHeight" " "
			(at 127.127 86.36 0)
		)
		(property "Manufacturer1 Example" "TDK"
			(at 125.222 86.36 0)
		)
		(property "Manufacturer1 Part Number" "C1005X5R1E105K050"
			(at 123.317 86.36 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 121.412 86.36 0)
		)
		(property "HelpURL" ""
			(at 119.507 86.36 0)
		)
		(property "Author" "CERN DEM BC"
			(at 117.602 86.36 0)
		)
		(property "CreateDate" "02/17/20 00:00:00"
			(at 115.697 86.36 0)
		)
		(property "LatestRevisionDate" "02/17/20 00:00:00"
			(at 113.792 86.36 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 111.887 86.36 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 109.982 86.36 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 108.077 86.36 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 106.172 86.36 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C52")
					(unit 1)
				)
			)
		)
	)
)
