(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A3")
	(title_block
		(title "VME buffers - P2 row A timing I/O")
	)
	(lib_symbols
		(symbol "Capacitors SMD:CC0402_100NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_100NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" "100nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/05/13 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_100NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Standard Logic:SN74LVCH16T245DGG"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 11.43 1.27 0)
			)
			(property "Value" "SN74LVCH16T245DGG"
				(at 0 -75.565 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOP50P810X120-48N"
				(at 0 -77.47 0)
			)
			(property "Datasheet" ""
				(at 0 -79.375 0)
			)
			(property "Description" "SN74LVCH16T245DGG"
				(at 0 -81.28 0)
			)
			(property "Library Ref" "7416T245"
				(at 0 -83.185 0)
			)
			(property "Library Path" "SchLib\\Standard Logic.SchLib"
				(at 0 -85.09 0)
			)
			(property "Comment" "SN74LVCH16T245DGG"
				(at 0 -86.995 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -88.9 0)
			)
			(property "Component Type" "Standard"
				(at 0 -90.805 0)
			)
			(property "Device" "SN74LVCH16T245DGG"
				(at 0 -92.71 0)
			)
			(property "PackageDescription" "SOP, 48-Leads, Body 12.6x6.2mm (max), Pitch 0.50mm, IPC Medium Density"
				(at 0 -94.615 0)
			)
			(property "Status" " "
				(at 0 -96.52 0)
			)
			(property "Part Description" "16-Bit Dual-Supply Bus Transceiver with Configurable Voltage Translation and 3-State Outputs"
				(at 0 -98.425 0)
			)
			(property "Manufacturer" "TEXAS INSTRUMENTS"
				(at 0 -100.33 0)
			)
			(property "Manufacturer Part Number" "SN74LVCH16T245DGG"
				(at 0 -102.235 0)
			)
			(property "Pin Count" "48"
				(at 0 -104.14 0)
			)
			(property "Case" "TSSOP48"
				(at 0 -106.045 0)
			)
			(property "Mounted" "Yes"
				(at 0 -107.95 0)
			)
			(property "Socket" "No"
				(at 0 -109.855 0)
			)
			(property "SMD" "Yes"
				(at 0 -111.76 0)
			)
			(property "PressFit" "No"
				(at 0 -113.665 0)
			)
			(property "Sense" "No"
				(at 0 -115.57 0)
			)
			(property "Sense Comment" " "
				(at 0 -117.475 0)
			)
			(property "Bonding" "No"
				(at 0 -119.38 0)
			)
			(property "Status Comment" " "
				(at 0 -121.285 0)
			)
			(property "ComponentHeight" "1.2mm"
				(at 0 -123.19 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -125.095 0)
			)
			(property "Footprint Ref" "SOP50P810X120-48N"
				(at 0 -127 0)
			)
			(property "Author" "CERN DEM HF"
				(at 0 -128.905 0)
			)
			(property "HelpURL" ""
				(at 0 -130.81 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -132.715 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -134.62 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -136.525 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -138.43 0)
			)
			(property "CreateDate" "03/29/22 00:00:00"
				(at 0 -140.335 0)
			)
			(property "LatestRevisionDate" "03/29/22 00:00:00"
				(at 0 -142.24 0)
			)
			(property "SCEM" " "
				(at 0 -144.145 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -146.05 0)
			)
			(property "Library Name" "Standard Logic"
				(at 0 -147.955 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -149.86 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -151.765 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "SN74LVCH16T245DGG_0_1"
				(rectangle
					(start 0 -71.12)
					(end 22.86 0)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "1A1")
					(number "47")
				)
				(pin bidirectional line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "1A2")
					(number "46")
				)
				(pin bidirectional line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "1A3")
					(number "44")
				)
				(pin bidirectional line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "1A4")
					(number "43")
				)
				(pin bidirectional line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "1A5")
					(number "41")
				)
				(pin bidirectional line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "1A6")
					(number "40")
				)
				(pin bidirectional line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "1A7")
					(number "38")
				)
				(pin bidirectional line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "1A8")
					(number "37")
				)
				(pin bidirectional line
					(at -5.08 -25.4 0)
					(length 5.08)
					(name "2A1")
					(number "36")
				)
				(pin bidirectional line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "2A2")
					(number "35")
				)
				(pin bidirectional line
					(at -5.08 -30.48 0)
					(length 5.08)
					(name "2A3")
					(number "33")
				)
				(pin bidirectional line
					(at -5.08 -33.02 0)
					(length 5.08)
					(name "2A4")
					(number "32")
				)
				(pin bidirectional line
					(at -5.08 -35.56 0)
					(length 5.08)
					(name "2A5")
					(number "30")
				)
				(pin bidirectional line
					(at -5.08 -38.1 0)
					(length 5.08)
					(name "2A6")
					(number "29")
				)
				(pin bidirectional line
					(at -5.08 -40.64 0)
					(length 5.08)
					(name "2A7")
					(number "27")
				)
				(pin bidirectional line
					(at -5.08 -43.18 0)
					(length 5.08)
					(name "2A8")
					(number "26")
				)
				(pin input line
					(at -5.08 -48.26 0)
					(length 5.08)
					(name "1~{OE}")
					(number "48")
				)
				(pin input line
					(at -5.08 -50.8 0)
					(length 5.08)
					(name "1DIR")
					(number "1")
				)
				(pin input line
					(at -5.08 -53.34 0)
					(length 5.08)
					(name "2~{OE}")
					(number "25")
				)
				(pin input line
					(at -5.08 -55.88 0)
					(length 5.08)
					(name "2DIR")
					(number "24")
				)
				(pin power_in line
					(at -5.08 -60.96 0)
					(length 5.08)
					(name "VCCA")
					(number "31")
				)
				(pin power_in line
					(at -5.08 -63.5 0)
					(length 5.08)
					(name "VCCA")
					(number "42")
				)
				(pin power_in line
					(at -5.08 -66.04 0)
					(length 5.08)
					(name "VCCB")
					(number "7")
				)
				(pin power_in line
					(at -5.08 -68.58 0)
					(length 5.08)
					(name "VCCB")
					(number "18")
				)
				(pin bidirectional line
					(at 27.94 -2.54 180)
					(length 5.08)
					(name "1B1")
					(number "2")
				)
				(pin bidirectional line
					(at 27.94 -5.08 180)
					(length 5.08)
					(name "1B2")
					(number "3")
				)
				(pin bidirectional line
					(at 27.94 -7.62 180)
					(length 5.08)
					(name "1B3")
					(number "5")
				)
				(pin bidirectional line
					(at 27.94 -10.16 180)
					(length 5.08)
					(name "1B4")
					(number "6")
				)
				(pin bidirectional line
					(at 27.94 -12.7 180)
					(length 5.08)
					(name "1B5")
					(number "8")
				)
				(pin bidirectional line
					(at 27.94 -15.24 180)
					(length 5.08)
					(name "1B6")
					(number "9")
				)
				(pin bidirectional line
					(at 27.94 -17.78 180)
					(length 5.08)
					(name "1B7")
					(number "11")
				)
				(pin bidirectional line
					(at 27.94 -20.32 180)
					(length 5.08)
					(name "1B8")
					(number "12")
				)
				(pin bidirectional line
					(at 27.94 -25.4 180)
					(length 5.08)
					(name "2B1")
					(number "13")
				)
				(pin bidirectional line
					(at 27.94 -27.94 180)
					(length 5.08)
					(name "2B2")
					(number "14")
				)
				(pin bidirectional line
					(at 27.94 -30.48 180)
					(length 5.08)
					(name "2B3")
					(number "16")
				)
				(pin bidirectional line
					(at 27.94 -33.02 180)
					(length 5.08)
					(name "2B4")
					(number "17")
				)
				(pin bidirectional line
					(at 27.94 -35.56 180)
					(length 5.08)
					(name "2B5")
					(number "19")
				)
				(pin bidirectional line
					(at 27.94 -38.1 180)
					(length 5.08)
					(name "2B6")
					(number "20")
				)
				(pin bidirectional line
					(at 27.94 -40.64 180)
					(length 5.08)
					(name "2B7")
					(number "22")
				)
				(pin bidirectional line
					(at 27.94 -43.18 180)
					(length 5.08)
					(name "2B8")
					(number "23")
				)
				(pin power_in line
					(at 27.94 -50.8 180)
					(length 5.08)
					(name "GND")
					(number "4")
				)
				(pin power_in line
					(at 27.94 -53.34 180)
					(length 5.08)
					(name "GND")
					(number "10")
				)
				(pin power_in line
					(at 27.94 -55.88 180)
					(length 5.08)
					(name "GND")
					(number "15")
				)
				(pin power_in line
					(at 27.94 -58.42 180)
					(length 5.08)
					(name "GND")
					(number "21")
				)
				(pin power_in line
					(at 27.94 -60.96 180)
					(length 5.08)
					(name "GND")
					(number "28")
				)
				(pin power_in line
					(at 27.94 -63.5 180)
					(length 5.08)
					(name "GND")
					(number "34")
				)
				(pin power_in line
					(at 27.94 -66.04 180)
					(length 5.08)
					(name "GND")
					(number "39")
				)
				(pin power_in line
					(at 27.94 -68.58 180)
					(length 5.08)
					(name "GND")
					(number "45")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P3V3"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0202"
				(at 0 0 0)
			)
			(property "Value" "P3V3"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P3V3_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P3V3")
					(number "")
				)
			)
			(embedded_fonts no)
		)
	)
	(bus_alias "USERIO_A"
		(members "USERIO_A.IO[0..31]" "USERIO_A.DIR[0..3]" "USERIO_A.OE_N[0..3]")
	)
	(junction
		(at 101.6 171.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 139.7 158.75)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 102.87 214.63)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 139.7 173.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 285.75 170.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 285.75 172.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 102.87 207.01)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 247.65 165.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 139.7 163.83)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 285.75 165.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 285.75 160.02)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 207.01)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 240.03 224.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 139.7 161.29)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 285.75 162.56)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 240.03 217.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 139.7 166.37)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 129.54 214.63)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 247.65 170.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 285.75 157.48)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 285.75 167.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 266.7 224.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 266.7 217.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 101.6 166.37)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 139.7 168.91)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 139.7 171.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(bus_entry
		(at 163.83 110.49)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 222.25 147.32)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 134.62)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 113.03)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 163.83 148.59)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 76.2 140.97)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 163.83 138.43)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 222.25 160.02)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 138.43)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 148.59)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 309.88 106.68)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 76.2 120.65)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 143.51)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 139.7)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 309.88 114.3)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 222.25 121.92)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 149.86)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 135.89)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 146.05)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 146.05)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 161.29)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 137.16)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 163.83 120.65)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 222.25 160.02)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 149.86)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 157.48)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 163.83 135.89)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 309.88 142.24)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 222.25 154.94)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 138.43)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 309.88 129.54)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 222.25 116.84)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 309.88 124.46)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 163.83 125.73)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 222.25 142.24)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 132.08)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 309.88 116.84)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 76.2 133.35)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 163.83)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 119.38)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 118.11)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 139.7)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 163.83 143.51)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 76.2 143.51)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 109.22)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 110.49)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 162.56)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 115.57)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 161.29)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 151.13)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 127)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 111.76)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 144.78)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 163.83 146.05)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 163.83 115.57)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 76.2 148.59)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 163.83 123.19)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 309.88 147.32)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 222.25 134.62)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 162.56)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 163.83 118.11)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 76.2 163.83)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 140.97)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 309.88 134.62)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 309.88 121.92)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 76.2 158.75)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 124.46)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 309.88 119.38)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 76.2 151.13)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 156.21)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 128.27)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 309.88 144.78)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 163.83 107.95)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 222.25 137.16)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 125.73)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 163.83 133.35)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 222.25 142.24)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 309.88 111.76)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 163.83 130.81)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 163.83 140.97)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 222.25 132.08)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 144.78)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 309.88 132.08)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 309.88 139.7)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 76.2 135.89)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 114.3)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 309.88 109.22)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 163.83 113.03)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 309.88 137.16)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 76.2 123.19)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 76.2 133.35)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 222.25 147.32)
		(size 2.54 -2.54)
	)
	(bus
		(pts
			(xy 312.42 139.7) (xy 312.42 142.24)
		)
	)
	(wire
		(pts
			(xy 224.79 160.02) (xy 250.19 160.02)
		)
	)
	(wire
		(pts
			(xy 224.79 152.4) (xy 250.19 152.4)
		)
	)
	(bus
		(pts
			(xy 76.2 158.75) (xy 76.2 161.29)
		)
	)
	(wire
		(pts
			(xy 285.75 154.94) (xy 285.75 157.48)
		)
	)
	(wire
		(pts
			(xy 224.79 157.48) (xy 250.19 157.48)
		)
	)
	(wire
		(pts
			(xy 137.16 107.95) (xy 163.83 107.95)
		)
	)
	(wire
		(pts
			(xy 285.75 162.56) (xy 285.75 165.1)
		)
	)
	(wire
		(pts
			(xy 137.16 115.57) (xy 163.83 115.57)
		)
	)
	(wire
		(pts
			(xy 224.79 119.38) (xy 250.19 119.38)
		)
	)
	(bus
		(pts
			(xy 312.42 132.08) (xy 312.42 134.62)
		)
	)
	(wire
		(pts
			(xy 137.16 161.29) (xy 139.7 161.29)
		)
	)
	(bus
		(pts
			(xy 312.42 144.78) (xy 312.42 147.32)
		)
	)
	(bus
		(pts
			(xy 222.25 147.32) (xy 222.25 149.86)
		)
	)
	(wire
		(pts
			(xy 101.6 168.91) (xy 101.6 166.37)
		)
	)
	(bus
		(pts
			(xy 166.37 138.43) (xy 166.37 140.97)
		)
	)
	(bus
		(pts
			(xy 222.25 109.22) (xy 222.25 111.76)
		)
	)
	(wire
		(pts
			(xy 283.21 116.84) (xy 309.88 116.84)
		)
	)
	(wire
		(pts
			(xy 283.21 121.92) (xy 309.88 121.92)
		)
	)
	(wire
		(pts
			(xy 283.21 167.64) (xy 285.75 167.64)
		)
	)
	(wire
		(pts
			(xy 285.75 160.02) (xy 285.75 162.56)
		)
	)
	(wire
		(pts
			(xy 78.74 120.65) (xy 104.14 120.65)
		)
	)
	(bus
		(pts
			(xy 312.42 111.76) (xy 312.42 114.3)
		)
	)
	(wire
		(pts
			(xy 137.16 138.43) (xy 163.83 138.43)
		)
	)
	(bus
		(pts
			(xy 222.25 137.16) (xy 222.25 139.7)
		)
	)
	(wire
		(pts
			(xy 224.79 121.92) (xy 250.19 121.92)
		)
	)
	(bus
		(pts
			(xy 166.37 125.73) (xy 166.37 128.27)
		)
	)
	(bus
		(pts
			(xy 166.37 118.11) (xy 166.37 120.65)
		)
	)
	(wire
		(pts
			(xy 101.6 171.45) (xy 101.6 173.99)
		)
	)
	(wire
		(pts
			(xy 283.21 170.18) (xy 285.75 170.18)
		)
	)
	(wire
		(pts
			(xy 283.21 111.76) (xy 309.88 111.76)
		)
	)
	(wire
		(pts
			(xy 137.16 133.35) (xy 163.83 133.35)
		)
	)
	(bus
		(pts
			(xy 222.25 154.94) (xy 222.25 157.48)
		)
	)
	(wire
		(pts
			(xy 139.7 168.91) (xy 139.7 171.45)
		)
	)
	(wire
		(pts
			(xy 78.74 143.51) (xy 104.14 143.51)
		)
	)
	(wire
		(pts
			(xy 224.79 106.68) (xy 250.19 106.68)
		)
	)
	(bus
		(pts
			(xy 76.2 138.43) (xy 76.2 140.97)
		)
	)
	(wire
		(pts
			(xy 283.21 124.46) (xy 309.88 124.46)
		)
	)
	(bus
		(pts
			(xy 166.37 123.19) (xy 166.37 125.73)
		)
	)
	(wire
		(pts
			(xy 224.79 142.24) (xy 250.19 142.24)
		)
	)
	(wire
		(pts
			(xy 266.7 217.17) (xy 278.13 217.17)
		)
	)
	(wire
		(pts
			(xy 137.16 158.75) (xy 139.7 158.75)
		)
	)
	(wire
		(pts
			(xy 101.6 166.37) (xy 104.14 166.37)
		)
	)
	(bus
		(pts
			(xy 76.2 123.19) (xy 76.2 125.73)
		)
	)
	(wire
		(pts
			(xy 137.16 168.91) (xy 139.7 168.91)
		)
	)
	(wire
		(pts
			(xy 283.21 119.38) (xy 309.88 119.38)
		)
	)
	(wire
		(pts
			(xy 224.79 139.7) (xy 250.19 139.7)
		)
	)
	(wire
		(pts
			(xy 137.16 143.51) (xy 163.83 143.51)
		)
	)
	(bus
		(pts
			(xy 222.25 119.38) (xy 222.25 121.92)
		)
	)
	(bus
		(pts
			(xy 222.25 149.86) (xy 222.25 154.94)
		)
	)
	(wire
		(pts
			(xy 78.74 110.49) (xy 104.14 110.49)
		)
	)
	(bus
		(pts
			(xy 312.42 149.86) (xy 334.01 149.86)
		)
	)
	(wire
		(pts
			(xy 78.74 123.19) (xy 104.14 123.19)
		)
	)
	(wire
		(pts
			(xy 283.21 162.56) (xy 285.75 162.56)
		)
	)
	(bus
		(pts
			(xy 166.37 110.49) (xy 166.37 113.03)
		)
	)
	(wire
		(pts
			(xy 137.16 118.11) (xy 163.83 118.11)
		)
	)
	(wire
		(pts
			(xy 139.7 163.83) (xy 139.7 166.37)
		)
	)
	(wire
		(pts
			(xy 137.16 113.03) (xy 163.83 113.03)
		)
	)
	(bus
		(pts
			(xy 312.42 119.38) (xy 312.42 121.92)
		)
	)
	(wire
		(pts
			(xy 139.7 166.37) (xy 139.7 168.91)
		)
	)
	(bus
		(pts
			(xy 166.37 135.89) (xy 166.37 138.43)
		)
	)
	(wire
		(pts
			(xy 283.21 106.68) (xy 309.88 106.68)
		)
	)
	(wire
		(pts
			(xy 137.16 110.49) (xy 163.83 110.49)
		)
	)
	(wire
		(pts
			(xy 224.79 132.08) (xy 250.19 132.08)
		)
	)
	(bus
		(pts
			(xy 222.25 160.02) (xy 222.25 162.56)
		)
	)
	(bus
		(pts
			(xy 166.37 113.03) (xy 166.37 115.57)
		)
	)
	(bus
		(pts
			(xy 222.25 142.24) (xy 222.25 144.78)
		)
	)
	(wire
		(pts
			(xy 224.79 137.16) (xy 250.19 137.16)
		)
	)
	(wire
		(pts
			(xy 137.16 125.73) (xy 163.83 125.73)
		)
	)
	(bus
		(pts
			(xy 76.2 143.51) (xy 76.2 146.05)
		)
	)
	(wire
		(pts
			(xy 283.21 109.22) (xy 309.88 109.22)
		)
	)
	(bus
		(pts
			(xy 222.25 124.46) (xy 222.25 127)
		)
	)
	(wire
		(pts
			(xy 137.16 135.89) (xy 163.83 135.89)
		)
	)
	(wire
		(pts
			(xy 78.74 113.03) (xy 104.14 113.03)
		)
	)
	(bus
		(pts
			(xy 217.17 194.31) (xy 254 194.31)
		)
	)
	(wire
		(pts
			(xy 137.16 130.81) (xy 163.83 130.81)
		)
	)
	(wire
		(pts
			(xy 224.79 111.76) (xy 250.19 111.76)
		)
	)
	(wire
		(pts
			(xy 240.03 217.17) (xy 251.46 217.17)
		)
	)
	(bus
		(pts
			(xy 166.37 140.97) (xy 166.37 143.51)
		)
	)
	(wire
		(pts
			(xy 139.7 156.21) (xy 139.7 158.75)
		)
	)
	(bus
		(pts
			(xy 166.37 146.05) (xy 166.37 148.59)
		)
	)
	(wire
		(pts
			(xy 139.7 161.29) (xy 139.7 163.83)
		)
	)
	(bus
		(pts
			(xy 312.42 109.22) (xy 312.42 111.76)
		)
	)
	(wire
		(pts
			(xy 285.75 167.64) (xy 285.75 170.18)
		)
	)
	(wire
		(pts
			(xy 240.03 224.79) (xy 251.46 224.79)
		)
	)
	(wire
		(pts
			(xy 137.16 163.83) (xy 139.7 163.83)
		)
	)
	(wire
		(pts
			(xy 283.21 114.3) (xy 309.88 114.3)
		)
	)
	(wire
		(pts
			(xy 78.74 107.95) (xy 104.14 107.95)
		)
	)
	(bus
		(pts
			(xy 76.2 115.57) (xy 76.2 118.11)
		)
	)
	(wire
		(pts
			(xy 283.21 144.78) (xy 309.88 144.78)
		)
	)
	(bus
		(pts
			(xy 76.2 120.65) (xy 76.2 123.19)
		)
	)
	(bus
		(pts
			(xy 76.2 125.73) (xy 76.2 128.27)
		)
	)
	(wire
		(pts
			(xy 266.7 224.79) (xy 278.13 224.79)
		)
	)
	(bus
		(pts
			(xy 312.42 116.84) (xy 312.42 119.38)
		)
	)
	(wire
		(pts
			(xy 247.65 172.72) (xy 250.19 172.72)
		)
	)
	(wire
		(pts
			(xy 285.75 165.1) (xy 285.75 167.64)
		)
	)
	(wire
		(pts
			(xy 78.74 148.59) (xy 104.14 148.59)
		)
	)
	(wire
		(pts
			(xy 78.74 140.97) (xy 104.14 140.97)
		)
	)
	(bus
		(pts
			(xy 222.25 157.48) (xy 222.25 160.02)
		)
	)
	(wire
		(pts
			(xy 78.74 146.05) (xy 104.14 146.05)
		)
	)
	(wire
		(pts
			(xy 129.54 207.01) (xy 140.97 207.01)
		)
	)
	(wire
		(pts
			(xy 224.79 116.84) (xy 250.19 116.84)
		)
	)
	(wire
		(pts
			(xy 104.14 171.45) (xy 101.6 171.45)
		)
	)
	(bus
		(pts
			(xy 312.42 142.24) (xy 312.42 144.78)
		)
	)
	(wire
		(pts
			(xy 137.16 140.97) (xy 163.83 140.97)
		)
	)
	(wire
		(pts
			(xy 78.74 130.81) (xy 104.14 130.81)
		)
	)
	(bus
		(pts
			(xy 222.25 132.08) (xy 222.25 134.62)
		)
	)
	(wire
		(pts
			(xy 224.79 114.3) (xy 250.19 114.3)
		)
	)
	(bus
		(pts
			(xy 76.2 113.03) (xy 76.2 115.57)
		)
	)
	(wire
		(pts
			(xy 137.16 171.45) (xy 139.7 171.45)
		)
	)
	(bus
		(pts
			(xy 76.2 135.89) (xy 76.2 138.43)
		)
	)
	(wire
		(pts
			(xy 283.21 137.16) (xy 309.88 137.16)
		)
	)
	(bus
		(pts
			(xy 222.25 134.62) (xy 222.25 137.16)
		)
	)
	(bus
		(pts
			(xy 312.42 134.62) (xy 312.42 137.16)
		)
	)
	(bus
		(pts
			(xy 76.2 128.27) (xy 76.2 133.35)
		)
	)
	(wire
		(pts
			(xy 78.74 153.67) (xy 104.14 153.67)
		)
	)
	(bus
		(pts
			(xy 222.25 139.7) (xy 222.25 142.24)
		)
	)
	(wire
		(pts
			(xy 137.16 120.65) (xy 163.83 120.65)
		)
	)
	(wire
		(pts
			(xy 283.21 132.08) (xy 309.88 132.08)
		)
	)
	(bus
		(pts
			(xy 76.2 133.35) (xy 76.2 135.89)
		)
	)
	(bus
		(pts
			(xy 222.25 144.78) (xy 222.25 147.32)
		)
	)
	(wire
		(pts
			(xy 137.16 156.21) (xy 139.7 156.21)
		)
	)
	(wire
		(pts
			(xy 285.75 157.48) (xy 285.75 160.02)
		)
	)
	(wire
		(pts
			(xy 129.54 214.63) (xy 140.97 214.63)
		)
	)
	(bus
		(pts
			(xy 217.17 201.93) (xy 254 201.93)
		)
	)
	(wire
		(pts
			(xy 137.16 146.05) (xy 163.83 146.05)
		)
	)
	(wire
		(pts
			(xy 283.21 147.32) (xy 309.88 147.32)
		)
	)
	(wire
		(pts
			(xy 283.21 172.72) (xy 285.75 172.72)
		)
	)
	(wire
		(pts
			(xy 247.65 170.18) (xy 247.65 172.72)
		)
	)
	(bus
		(pts
			(xy 222.25 111.76) (xy 222.25 114.3)
		)
	)
	(bus
		(pts
			(xy 76.2 148.59) (xy 76.2 151.13)
		)
	)
	(bus
		(pts
			(xy 312.42 121.92) (xy 312.42 124.46)
		)
	)
	(wire
		(pts
			(xy 283.21 154.94) (xy 285.75 154.94)
		)
	)
	(bus
		(pts
			(xy 76.2 151.13) (xy 76.2 156.21)
		)
	)
	(bus
		(pts
			(xy 312.42 147.32) (xy 312.42 149.86)
		)
	)
	(wire
		(pts
			(xy 139.7 171.45) (xy 139.7 173.99)
		)
	)
	(bus
		(pts
			(xy 76.2 156.21) (xy 76.2 158.75)
		)
	)
	(wire
		(pts
			(xy 283.21 134.62) (xy 309.88 134.62)
		)
	)
	(wire
		(pts
			(xy 285.75 170.18) (xy 285.75 172.72)
		)
	)
	(bus
		(pts
			(xy 166.37 143.51) (xy 166.37 146.05)
		)
	)
	(wire
		(pts
			(xy 283.21 157.48) (xy 285.75 157.48)
		)
	)
	(wire
		(pts
			(xy 283.21 129.54) (xy 309.88 129.54)
		)
	)
	(wire
		(pts
			(xy 78.74 115.57) (xy 104.14 115.57)
		)
	)
	(bus
		(pts
			(xy 222.25 116.84) (xy 222.25 119.38)
		)
	)
	(bus
		(pts
			(xy 222.25 114.3) (xy 222.25 116.84)
		)
	)
	(bus
		(pts
			(xy 166.37 133.35) (xy 166.37 135.89)
		)
	)
	(wire
		(pts
			(xy 137.16 148.59) (xy 163.83 148.59)
		)
	)
	(wire
		(pts
			(xy 137.16 166.37) (xy 139.7 166.37)
		)
	)
	(wire
		(pts
			(xy 137.16 173.99) (xy 139.7 173.99)
		)
	)
	(bus
		(pts
			(xy 76.2 140.97) (xy 76.2 143.51)
		)
	)
	(bus
		(pts
			(xy 76.2 161.29) (xy 76.2 163.83)
		)
	)
	(bus
		(pts
			(xy 76.2 118.11) (xy 76.2 120.65)
		)
	)
	(wire
		(pts
			(xy 78.74 133.35) (xy 104.14 133.35)
		)
	)
	(wire
		(pts
			(xy 224.79 124.46) (xy 250.19 124.46)
		)
	)
	(wire
		(pts
			(xy 78.74 118.11) (xy 104.14 118.11)
		)
	)
	(wire
		(pts
			(xy 78.74 135.89) (xy 104.14 135.89)
		)
	)
	(wire
		(pts
			(xy 250.19 167.64) (xy 247.65 167.64)
		)
	)
	(bus
		(pts
			(xy 76.2 110.49) (xy 76.2 113.03)
		)
	)
	(wire
		(pts
			(xy 224.79 154.94) (xy 250.19 154.94)
		)
	)
	(wire
		(pts
			(xy 101.6 173.99) (xy 104.14 173.99)
		)
	)
	(bus
		(pts
			(xy 166.37 120.65) (xy 166.37 123.19)
		)
	)
	(bus
		(pts
			(xy 222.25 99.06) (xy 222.25 109.22)
		)
	)
	(wire
		(pts
			(xy 250.19 170.18) (xy 247.65 170.18)
		)
	)
	(wire
		(pts
			(xy 224.79 144.78) (xy 250.19 144.78)
		)
	)
	(wire
		(pts
			(xy 283.21 165.1) (xy 285.75 165.1)
		)
	)
	(bus
		(pts
			(xy 166.37 148.59) (xy 166.37 151.13)
		)
	)
	(wire
		(pts
			(xy 139.7 173.99) (xy 139.7 179.07)
		)
	)
	(bus
		(pts
			(xy 312.42 137.16) (xy 312.42 139.7)
		)
	)
	(wire
		(pts
			(xy 139.7 158.75) (xy 139.7 161.29)
		)
	)
	(wire
		(pts
			(xy 285.75 172.72) (xy 285.75 177.8)
		)
	)
	(bus
		(pts
			(xy 166.37 128.27) (xy 166.37 133.35)
		)
	)
	(bus
		(pts
			(xy 312.42 124.46) (xy 312.42 127)
		)
	)
	(bus
		(pts
			(xy 76.2 100.33) (xy 76.2 110.49)
		)
	)
	(wire
		(pts
			(xy 78.74 158.75) (xy 104.14 158.75)
		)
	)
	(wire
		(pts
			(xy 78.74 138.43) (xy 104.14 138.43)
		)
	)
	(wire
		(pts
			(xy 78.74 156.21) (xy 104.14 156.21)
		)
	)
	(wire
		(pts
			(xy 137.16 123.19) (xy 163.83 123.19)
		)
	)
	(bus
		(pts
			(xy 222.25 121.92) (xy 222.25 124.46)
		)
	)
	(wire
		(pts
			(xy 247.65 165.1) (xy 250.19 165.1)
		)
	)
	(wire
		(pts
			(xy 224.79 147.32) (xy 250.19 147.32)
		)
	)
	(wire
		(pts
			(xy 78.74 161.29) (xy 104.14 161.29)
		)
	)
	(bus
		(pts
			(xy 312.42 114.3) (xy 312.42 116.84)
		)
	)
	(wire
		(pts
			(xy 224.79 129.54) (xy 250.19 129.54)
		)
	)
	(bus
		(pts
			(xy 166.37 151.13) (xy 187.96 151.13)
		)
	)
	(bus
		(pts
			(xy 76.2 146.05) (xy 76.2 148.59)
		)
	)
	(wire
		(pts
			(xy 224.79 109.22) (xy 250.19 109.22)
		)
	)
	(wire
		(pts
			(xy 102.87 207.01) (xy 114.3 207.01)
		)
	)
	(wire
		(pts
			(xy 102.87 214.63) (xy 114.3 214.63)
		)
	)
	(wire
		(pts
			(xy 283.21 142.24) (xy 309.88 142.24)
		)
	)
	(wire
		(pts
			(xy 78.74 125.73) (xy 104.14 125.73)
		)
	)
	(wire
		(pts
			(xy 247.65 167.64) (xy 247.65 165.1)
		)
	)
	(bus
		(pts
			(xy 166.37 115.57) (xy 166.37 118.11)
		)
	)
	(wire
		(pts
			(xy 283.21 160.02) (xy 285.75 160.02)
		)
	)
	(bus
		(pts
			(xy 222.25 127) (xy 222.25 132.08)
		)
	)
	(wire
		(pts
			(xy 104.14 168.91) (xy 101.6 168.91)
		)
	)
	(wire
		(pts
			(xy 283.21 139.7) (xy 309.88 139.7)
		)
	)
	(bus
		(pts
			(xy 312.42 127) (xy 312.42 132.08)
		)
	)
	(wire
		(pts
			(xy 224.79 134.62) (xy 250.19 134.62)
		)
	)
	(label "VMEPX_USERIO_A.IO26"
		(at 140.97 120.65 0)
	)
	(label "VMEPX_USERIO_A.IO31"
		(at 140.97 107.95 0)
	)
	(label "{VMEPX_USERIO_A}"
		(at 226.06 194.31 0)
	)
	(label "USERIO_A.IO14"
		(at 224.79 144.78 0)
	)
	(label "VMEPX_USERIO_A.IO2"
		(at 285.75 142.24 0)
	)
	(label "VMEPX_USERIO_A.IO16"
		(at 140.97 148.59 0)
	)
	(label "VMEPX_USERIO_A.IO19"
		(at 140.97 140.97 0)
	)
	(label "{USERIO_A}"
		(at 76.2 100.33 0)
	)
	(label "USERIO_A.IO16"
		(at 81.28 110.49 0)
	)
	(label "VMEPX_USERIO_A.IO14"
		(at 285.75 109.22 0)
	)
	(label "VMEPX_USERIO_A.IO30"
		(at 140.97 110.49 0)
	)
	(label "USERIO_A.IO13"
		(at 224.79 142.24 0)
	)
	(label "USERIO_A.IO26"
		(at 81.28 135.89 0)
	)
	(label "USERIO_A.IO21"
		(at 81.28 120.65 0)
	)
	(label "USERIO_A.IO6"
		(at 224.79 121.92 0)
	)
	(label "USERIO_A.IO5"
		(at 224.79 119.38 0)
	)
	(label "USERIO_A.IO10"
		(at 224.79 134.62 0)
	)
	(label "USERIO_A.IO4"
		(at 224.79 116.84 0)
	)
	(label "USERIO_A.IO30"
		(at 81.28 146.05 0)
	)
	(label "VMEPX_USERIO_A.IO18"
		(at 140.97 143.51 0)
	)
	(label "USERIO_A.IO25"
		(at 81.28 130.81 0)
	)
	(label "USERIO_A.IO17"
		(at 81.28 107.95 0)
	)
	(label "USERIO_A.IO18"
		(at 81.28 113.03 0)
	)
	(label "VMEPX_USERIO_A.IO23"
		(at 140.97 130.81 0)
	)
	(label "USERIO_A.IO24"
		(at 81.28 133.35 0)
	)
	(label "VMEPX_USERIO_A.IO29"
		(at 140.97 113.03 0)
	)
	(label "USERIO_A.IO1"
		(at 224.79 106.68 0)
	)
	(label "USERIO_A.IO28"
		(at 81.28 140.97 0)
	)
	(label "USERIO_A.IO27"
		(at 81.28 138.43 0)
	)
	(label "USERIO_A.IO12"
		(at 224.79 139.7 0)
	)
	(label "VMEPX_USERIO_A.IO17"
		(at 140.97 146.05 0)
	)
	(label "USERIO_A.IO2"
		(at 224.79 111.76 0)
	)
	(label "USERIO_A.IO22"
		(at 81.28 123.19 0)
	)
	(label "VMEPX_USERIO_A.IO9"
		(at 285.75 121.92 0)
	)
	(label "{VMEPX_USERIO_A}"
		(at 317.5 149.86 0)
	)
	(label "{VMEPX_USERIO_A}"
		(at 170.18 151.13 0)
	)
	(label "VMEPX_USERIO_A.IO15"
		(at 285.75 106.68 0)
	)
	(label "USERIO_A.IO31"
		(at 81.28 148.59 0)
	)
	(label "VMEPX_USERIO_A.IO21"
		(at 140.97 135.89 0)
	)
	(label "VMEPX_USERIO_A.IO4"
		(at 285.75 137.16 0)
	)
	(label "VMEPX_USERIO_A.IO11"
		(at 285.75 116.84 0)
	)
	(label "USERIO_A.IO7"
		(at 224.79 124.46 0)
	)
	(label "USERIO_A.IO29"
		(at 81.28 143.51 0)
	)
	(label "VMEPX_USERIO_A.IO1"
		(at 285.75 144.78 0)
	)
	(label "USERIO_A.IO8"
		(at 224.79 132.08 0)
	)
	(label "USERIO_A.DIR0"
		(at 224.79 154.94 0)
	)
	(label "VMEPX_USERIO_A.IO6"
		(at 285.75 132.08 0)
	)
	(label "{USERIO_A}"
		(at 226.06 201.93 0)
	)
	(label "VMEPX_USERIO_A.IO8"
		(at 285.75 124.46 0)
	)
	(label "{USERIO_A}"
		(at 222.25 99.06 0)
	)
	(label "VMEPX_USERIO_A.IO7"
		(at 285.75 129.54 0)
	)
	(label "VMEPX_USERIO_A.IO10"
		(at 285.75 119.38 0)
	)
	(label "USERIO_A.IO0"
		(at 224.79 109.22 0)
	)
	(label "VMEPX_USERIO_A.IO5"
		(at 285.75 134.62 0)
	)
	(label "USERIO_A.IO23"
		(at 81.28 125.73 0)
	)
	(label "USERIO_A.DIR1"
		(at 224.79 160.02 0)
	)
	(label "VMEPX_USERIO_A.IO12"
		(at 285.75 114.3 0)
	)
	(label "VMEPX_USERIO_A.IO22"
		(at 140.97 133.35 0)
	)
	(label "USERIO_A.OE_N1"
		(at 224.79 157.48 0)
	)
	(label "VMEPX_USERIO_A.IO20"
		(at 140.97 138.43 0)
	)
	(label "USERIO_A.IO11"
		(at 224.79 137.16 0)
	)
	(label "USERIO_A.DIR3"
		(at 81.28 161.29 0)
	)
	(label "USERIO_A.OE_N2"
		(at 81.28 153.67 0)
	)
	(label "USERIO_A.OE_N0"
		(at 224.79 152.4 0)
	)
	(label "VMEPX_USERIO_A.IO27"
		(at 140.97 118.11 0)
	)
	(label "USERIO_A.IO15"
		(at 224.79 147.32 0)
	)
	(label "USERIO_A.IO3"
		(at 224.79 114.3 0)
	)
	(label "VMEPX_USERIO_A.IO0"
		(at 285.75 147.32 0)
	)
	(label "VMEPX_USERIO_A.IO13"
		(at 285.75 111.76 0)
	)
	(label "VMEPX_USERIO_A.IO25"
		(at 140.97 123.19 0)
	)
	(label "USERIO_A.DIR2"
		(at 81.28 156.21 0)
	)
	(label "USERIO_A.IO20"
		(at 81.28 118.11 0)
	)
	(label "VMEPX_USERIO_A.IO24"
		(at 140.97 125.73 0)
	)
	(label "VMEPX_USERIO_A.IO3"
		(at 285.75 139.7 0)
	)
	(label "VMEPX_USERIO_A.IO28"
		(at 140.97 115.57 0)
	)
	(label "USERIO_A.IO19"
		(at 81.28 115.57 0)
	)
	(label "USERIO_A.OE_N3"
		(at 81.28 158.75 0)
	)
	(label "USERIO_A.IO9"
		(at 224.79 129.54 0)
	)
	(hierarchical_label "{VMEPX_USERIO_A}"
		(shape bidirectional)
		(at 254 194.31 0)
	)
	(hierarchical_label "{USERIO_A}"
		(shape bidirectional)
		(at 254 201.93 0)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 102.87 207.01 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR08"
			(at 102.87 207.01 0)
		)
		(property "Value" "P3V3"
			(at 102.87 201.93 0)
		)
		(property "Footprint" ""
			(at 102.87 207.01 0)
		)
		(property "Datasheet" ""
			(at 102.87 207.01 0)
		)
		(property "Description" ""
			(at 102.87 207.01 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR08")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 251.46 224.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C72"
			(at 255.27 222.2501 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 256.54 219.71 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 251.46 224.79 0)
		)
		(property "Datasheet" ""
			(at 251.46 224.79 0)
		)
		(property "Description" "100nF"
			(at 255.27 219.7101 90)
		)
		(property "SMD" "Yes"
			(at 250.952 227.076 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 263.398 224.79 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 265.303 224.79 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 267.208 224.79 0)
		)
		(property "Comment" "100nF"
			(at 269.113 224.79 0)
		)
		(property "Component Kind" "Standard"
			(at 271.018 224.79 0)
		)
		(property "Component Type" "Standard"
			(at 272.923 224.79 0)
		)
		(property "Pin Count" "2"
			(at 274.828 224.79 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 276.733 224.79 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 278.638 224.79 0)
		)
		(property "PackageDescription" " "
			(at 280.543 224.79 0)
		)
		(property "Status" "Not Recommended"
			(at 282.448 224.79 0)
		)
		(property "Status Comment" " "
			(at 284.353 224.79 0)
		)
		(property "Voltage" "16V"
			(at 286.258 224.79 0)
		)
		(property "Tolerance" "±10%"
			(at 290.068 224.79 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 291.973 224.79 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 293.878 224.79 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 295.783 224.79 0)
		)
		(property "Case" "0402"
			(at 297.688 224.79 0)
		)
		(property "Mounted" "Yes"
			(at 299.593 224.79 0)
		)
		(property "Socket" "No"
			(at 301.498 224.79 0)
		)
		(property "PressFit" " "
			(at 305.308 224.79 0)
		)
		(property "Sense" "No"
			(at 307.213 224.79 0)
		)
		(property "Sense Comment" " "
			(at 309.118 224.79 0)
		)
		(property "ComponentHeight" " "
			(at 311.023 224.79 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 312.928 224.79 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 314.833 224.79 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 316.738 224.79 0)
		)
		(property "HelpURL" ""
			(at 318.643 224.79 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 320.548 224.79 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 322.453 224.79 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 324.358 224.79 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 326.263 224.79 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 328.168 224.79 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 330.073 224.79 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 331.978 224.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C72")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 129.54 214.63 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C111"
			(at 133.35 212.0901 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 134.62 209.55 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 129.54 214.63 0)
		)
		(property "Datasheet" ""
			(at 129.54 214.63 0)
		)
		(property "Description" "100nF"
			(at 133.35 209.5501 90)
		)
		(property "SMD" "Yes"
			(at 129.032 216.916 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 141.478 214.63 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 143.383 214.63 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 145.288 214.63 0)
		)
		(property "Comment" "100nF"
			(at 147.193 214.63 0)
		)
		(property "Component Kind" "Standard"
			(at 149.098 214.63 0)
		)
		(property "Component Type" "Standard"
			(at 151.003 214.63 0)
		)
		(property "Pin Count" "2"
			(at 152.908 214.63 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 154.813 214.63 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 156.718 214.63 0)
		)
		(property "PackageDescription" " "
			(at 158.623 214.63 0)
		)
		(property "Status" "Not Recommended"
			(at 160.528 214.63 0)
		)
		(property "Status Comment" " "
			(at 162.433 214.63 0)
		)
		(property "Voltage" "16V"
			(at 164.338 214.63 0)
		)
		(property "Tolerance" "±10%"
			(at 168.148 214.63 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 170.053 214.63 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 171.958 214.63 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 173.863 214.63 0)
		)
		(property "Case" "0402"
			(at 175.768 214.63 0)
		)
		(property "Mounted" "Yes"
			(at 177.673 214.63 0)
		)
		(property "Socket" "No"
			(at 179.578 214.63 0)
		)
		(property "PressFit" " "
			(at 183.388 214.63 0)
		)
		(property "Sense" "No"
			(at 185.293 214.63 0)
		)
		(property "Sense Comment" " "
			(at 187.198 214.63 0)
		)
		(property "ComponentHeight" " "
			(at 189.103 214.63 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 191.008 214.63 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 192.913 214.63 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 194.818 214.63 0)
		)
		(property "HelpURL" ""
			(at 196.723 214.63 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 198.628 214.63 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 200.533 214.63 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 202.438 214.63 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 204.343 214.63 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 206.248 214.63 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 208.153 214.63 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 210.058 214.63 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C111")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 266.7 224.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C87"
			(at 270.51 222.2501 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 271.78 219.71 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 266.7 224.79 0)
		)
		(property "Datasheet" ""
			(at 266.7 224.79 0)
		)
		(property "Description" "100nF"
			(at 270.51 219.7101 90)
		)
		(property "SMD" "Yes"
			(at 266.192 227.076 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 278.638 224.79 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 280.543 224.79 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 282.448 224.79 0)
		)
		(property "Comment" "100nF"
			(at 284.353 224.79 0)
		)
		(property "Component Kind" "Standard"
			(at 286.258 224.79 0)
		)
		(property "Component Type" "Standard"
			(at 288.163 224.79 0)
		)
		(property "Pin Count" "2"
			(at 290.068 224.79 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 291.973 224.79 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 293.878 224.79 0)
		)
		(property "PackageDescription" " "
			(at 295.783 224.79 0)
		)
		(property "Status" "Not Recommended"
			(at 297.688 224.79 0)
		)
		(property "Status Comment" " "
			(at 299.593 224.79 0)
		)
		(property "Voltage" "16V"
			(at 301.498 224.79 0)
		)
		(property "Tolerance" "±10%"
			(at 305.308 224.79 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 307.213 224.79 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 309.118 224.79 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 311.023 224.79 0)
		)
		(property "Case" "0402"
			(at 312.928 224.79 0)
		)
		(property "Mounted" "Yes"
			(at 314.833 224.79 0)
		)
		(property "Socket" "No"
			(at 316.738 224.79 0)
		)
		(property "PressFit" " "
			(at 320.548 224.79 0)
		)
		(property "Sense" "No"
			(at 322.453 224.79 0)
		)
		(property "Sense Comment" " "
			(at 324.358 224.79 0)
		)
		(property "ComponentHeight" " "
			(at 326.263 224.79 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 328.168 224.79 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 330.073 224.79 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 331.978 224.79 0)
		)
		(property "HelpURL" ""
			(at 333.883 224.79 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 335.788 224.79 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 337.693 224.79 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 339.598 224.79 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 341.503 224.79 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 343.408 224.79 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 345.313 224.79 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 347.218 224.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C87")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 240.03 217.17 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR059"
			(at 240.03 217.17 0)
		)
		(property "Value" "P3V3"
			(at 240.03 212.09 0)
		)
		(property "Footprint" ""
			(at 240.03 217.17 0)
		)
		(property "Datasheet" ""
			(at 240.03 217.17 0)
		)
		(property "Description" ""
			(at 240.03 217.17 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR059")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 139.7 179.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR09"
			(at 139.7 179.07 0)
		)
		(property "Value" "GND"
			(at 139.7 182.88 0)
		)
		(property "Footprint" ""
			(at 139.7 179.07 0)
		)
		(property "Datasheet" ""
			(at 139.7 179.07 0)
		)
		(property "Description" ""
			(at 139.7 179.07 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR09")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 101.6 171.45 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR07"
			(at 101.6 171.45 0)
		)
		(property "Value" "P3V3"
			(at 97.79 171.45 90)
		)
		(property "Footprint" ""
			(at 101.6 171.45 0)
		)
		(property "Datasheet" ""
			(at 101.6 171.45 0)
		)
		(property "Description" ""
			(at 101.6 171.45 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR07")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 129.54 207.01 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR012"
			(at 129.54 207.01 0)
		)
		(property "Value" "P1V8"
			(at 129.54 201.93 0)
		)
		(property "Footprint" ""
			(at 129.54 207.01 0)
		)
		(property "Datasheet" ""
			(at 129.54 207.01 0)
		)
		(property "Description" ""
			(at 129.54 207.01 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR012")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 114.3 214.63 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C88"
			(at 118.11 212.0901 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 119.38 209.55 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 114.3 214.63 0)
		)
		(property "Datasheet" ""
			(at 114.3 214.63 0)
		)
		(property "Description" "100nF"
			(at 118.11 209.5501 90)
		)
		(property "SMD" "Yes"
			(at 113.792 216.916 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 126.238 214.63 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 128.143 214.63 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 130.048 214.63 0)
		)
		(property "Comment" "100nF"
			(at 131.953 214.63 0)
		)
		(property "Component Kind" "Standard"
			(at 133.858 214.63 0)
		)
		(property "Component Type" "Standard"
			(at 135.763 214.63 0)
		)
		(property "Pin Count" "2"
			(at 137.668 214.63 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 139.573 214.63 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 141.478 214.63 0)
		)
		(property "PackageDescription" " "
			(at 143.383 214.63 0)
		)
		(property "Status" "Not Recommended"
			(at 145.288 214.63 0)
		)
		(property "Status Comment" " "
			(at 147.193 214.63 0)
		)
		(property "Voltage" "16V"
			(at 149.098 214.63 0)
		)
		(property "Tolerance" "±10%"
			(at 152.908 214.63 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 154.813 214.63 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 156.718 214.63 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 158.623 214.63 0)
		)
		(property "Case" "0402"
			(at 160.528 214.63 0)
		)
		(property "Mounted" "Yes"
			(at 162.433 214.63 0)
		)
		(property "Socket" "No"
			(at 164.338 214.63 0)
		)
		(property "PressFit" " "
			(at 168.148 214.63 0)
		)
		(property "Sense" "No"
			(at 170.053 214.63 0)
		)
		(property "Sense Comment" " "
			(at 171.958 214.63 0)
		)
		(property "ComponentHeight" " "
			(at 173.863 214.63 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 175.768 214.63 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 177.673 214.63 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 179.578 214.63 0)
		)
		(property "HelpURL" ""
			(at 181.483 214.63 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 183.388 214.63 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 185.293 214.63 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 187.198 214.63 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 189.103 214.63 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 191.008 214.63 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 192.913 214.63 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 194.818 214.63 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C88")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 247.65 165.1 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR014"
			(at 247.65 165.1 0)
		)
		(property "Value" "P1V8"
			(at 243.84 165.1 90)
		)
		(property "Footprint" ""
			(at 247.65 165.1 0)
		)
		(property "Datasheet" ""
			(at 247.65 165.1 0)
		)
		(property "Description" ""
			(at 247.65 165.1 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR014")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 240.03 224.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C73"
			(at 243.84 222.2501 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 245.11 219.71 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 240.03 224.79 0)
		)
		(property "Datasheet" ""
			(at 240.03 224.79 0)
		)
		(property "Description" "100nF"
			(at 243.84 219.7101 90)
		)
		(property "SMD" "Yes"
			(at 239.522 227.076 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 251.968 224.79 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 253.873 224.79 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 255.778 224.79 0)
		)
		(property "Comment" "100nF"
			(at 257.683 224.79 0)
		)
		(property "Component Kind" "Standard"
			(at 259.588 224.79 0)
		)
		(property "Component Type" "Standard"
			(at 261.493 224.79 0)
		)
		(property "Pin Count" "2"
			(at 263.398 224.79 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 265.303 224.79 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 267.208 224.79 0)
		)
		(property "PackageDescription" " "
			(at 269.113 224.79 0)
		)
		(property "Status" "Not Recommended"
			(at 271.018 224.79 0)
		)
		(property "Status Comment" " "
			(at 272.923 224.79 0)
		)
		(property "Voltage" "16V"
			(at 274.828 224.79 0)
		)
		(property "Tolerance" "±10%"
			(at 278.638 224.79 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 280.543 224.79 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 282.448 224.79 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 284.353 224.79 0)
		)
		(property "Case" "0402"
			(at 286.258 224.79 0)
		)
		(property "Mounted" "Yes"
			(at 288.163 224.79 0)
		)
		(property "Socket" "No"
			(at 290.068 224.79 0)
		)
		(property "PressFit" " "
			(at 293.878 224.79 0)
		)
		(property "Sense" "No"
			(at 295.783 224.79 0)
		)
		(property "Sense Comment" " "
			(at 297.688 224.79 0)
		)
		(property "ComponentHeight" " "
			(at 299.593 224.79 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 301.498 224.79 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 303.403 224.79 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 305.308 224.79 0)
		)
		(property "HelpURL" ""
			(at 307.213 224.79 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 309.118 224.79 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 311.023 224.79 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 312.928 224.79 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 314.833 224.79 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 316.738 224.79 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 318.643 224.79 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 320.548 224.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C73")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 129.54 214.63 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR013"
			(at 129.54 214.63 0)
		)
		(property "Value" "GND"
			(at 129.54 219.71 0)
		)
		(property "Footprint" ""
			(at 129.54 214.63 0)
		)
		(property "Datasheet" ""
			(at 129.54 214.63 0)
		)
		(property "Description" ""
			(at 129.54 214.63 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR013")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 240.03 224.79 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR064"
			(at 240.03 224.79 0)
		)
		(property "Value" "GND"
			(at 240.03 229.87 0)
		)
		(property "Footprint" ""
			(at 240.03 224.79 0)
		)
		(property "Datasheet" ""
			(at 240.03 224.79 0)
		)
		(property "Description" ""
			(at 240.03 224.79 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR064")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 102.87 214.63 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C109"
			(at 106.68 212.0901 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 107.95 209.55 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 102.87 214.63 0)
		)
		(property "Datasheet" ""
			(at 102.87 214.63 0)
		)
		(property "Description" "100nF"
			(at 106.68 209.5501 90)
		)
		(property "SMD" "Yes"
			(at 102.362 216.916 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 114.808 214.63 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 116.713 214.63 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 118.618 214.63 0)
		)
		(property "Comment" "100nF"
			(at 120.523 214.63 0)
		)
		(property "Component Kind" "Standard"
			(at 122.428 214.63 0)
		)
		(property "Component Type" "Standard"
			(at 124.333 214.63 0)
		)
		(property "Pin Count" "2"
			(at 126.238 214.63 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 128.143 214.63 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 130.048 214.63 0)
		)
		(property "PackageDescription" " "
			(at 131.953 214.63 0)
		)
		(property "Status" "Not Recommended"
			(at 133.858 214.63 0)
		)
		(property "Status Comment" " "
			(at 135.763 214.63 0)
		)
		(property "Voltage" "16V"
			(at 137.668 214.63 0)
		)
		(property "Tolerance" "±10%"
			(at 141.478 214.63 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 143.383 214.63 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 145.288 214.63 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 147.193 214.63 0)
		)
		(property "Case" "0402"
			(at 149.098 214.63 0)
		)
		(property "Mounted" "Yes"
			(at 151.003 214.63 0)
		)
		(property "Socket" "No"
			(at 152.908 214.63 0)
		)
		(property "PressFit" " "
			(at 156.718 214.63 0)
		)
		(property "Sense" "No"
			(at 158.623 214.63 0)
		)
		(property "Sense Comment" " "
			(at 160.528 214.63 0)
		)
		(property "ComponentHeight" " "
			(at 162.433 214.63 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 164.338 214.63 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 166.243 214.63 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 168.148 214.63 0)
		)
		(property "HelpURL" ""
			(at 170.053 214.63 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 171.958 214.63 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 173.863 214.63 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 175.768 214.63 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 177.673 214.63 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 179.578 214.63 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 181.483 214.63 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 183.388 214.63 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C109")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 101.6 166.37 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR06"
			(at 101.6 166.37 0)
		)
		(property "Value" "P1V8"
			(at 97.79 166.37 90)
		)
		(property "Footprint" ""
			(at 101.6 166.37 0)
		)
		(property "Datasheet" ""
			(at 101.6 166.37 0)
		)
		(property "Description" ""
			(at 101.6 166.37 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 285.75 177.8 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR04"
			(at 285.75 177.8 0)
		)
		(property "Value" "GND"
			(at 285.75 181.61 0)
		)
		(property "Footprint" ""
			(at 285.75 177.8 0)
		)
		(property "Datasheet" ""
			(at 285.75 177.8 0)
		)
		(property "Description" ""
			(at 285.75 177.8 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 266.7 224.79 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR010"
			(at 266.7 224.79 0)
		)
		(property "Value" "GND"
			(at 266.7 229.87 0)
		)
		(property "Footprint" ""
			(at 266.7 224.79 0)
		)
		(property "Datasheet" ""
			(at 266.7 224.79 0)
		)
		(property "Description" ""
			(at 266.7 224.79 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR010")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 278.13 224.79 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C74"
			(at 281.94 222.2501 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 283.21 219.71 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 278.13 224.79 0)
		)
		(property "Datasheet" ""
			(at 278.13 224.79 0)
		)
		(property "Description" "100nF"
			(at 281.94 219.7101 90)
		)
		(property "SMD" "Yes"
			(at 277.622 227.076 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 290.068 224.79 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 291.973 224.79 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 293.878 224.79 0)
		)
		(property "Comment" "100nF"
			(at 295.783 224.79 0)
		)
		(property "Component Kind" "Standard"
			(at 297.688 224.79 0)
		)
		(property "Component Type" "Standard"
			(at 299.593 224.79 0)
		)
		(property "Pin Count" "2"
			(at 301.498 224.79 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 303.403 224.79 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 305.308 224.79 0)
		)
		(property "PackageDescription" " "
			(at 307.213 224.79 0)
		)
		(property "Status" "Not Recommended"
			(at 309.118 224.79 0)
		)
		(property "Status Comment" " "
			(at 311.023 224.79 0)
		)
		(property "Voltage" "16V"
			(at 312.928 224.79 0)
		)
		(property "Tolerance" "±10%"
			(at 316.738 224.79 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 318.643 224.79 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 320.548 224.79 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 322.453 224.79 0)
		)
		(property "Case" "0402"
			(at 324.358 224.79 0)
		)
		(property "Mounted" "Yes"
			(at 326.263 224.79 0)
		)
		(property "Socket" "No"
			(at 328.168 224.79 0)
		)
		(property "PressFit" " "
			(at 331.978 224.79 0)
		)
		(property "Sense" "No"
			(at 333.883 224.79 0)
		)
		(property "Sense Comment" " "
			(at 335.788 224.79 0)
		)
		(property "ComponentHeight" " "
			(at 337.693 224.79 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 339.598 224.79 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 341.503 224.79 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 343.408 224.79 0)
		)
		(property "HelpURL" ""
			(at 345.313 224.79 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 347.218 224.79 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 349.123 224.79 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 351.028 224.79 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 352.933 224.79 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 354.838 224.79 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 356.743 224.79 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 358.648 224.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C74")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Standard Logic:SN74LVCH16T245DGG")
		(at 255.27 104.14 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC42"
			(at 266.7 99.06 0)
		)
		(property "Value" "SN74LVCH16T245DGG"
			(at 266.7 101.6 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOP50P810X120-48N"
			(at 255.27 181.61 0)
		)
		(property "Datasheet" ""
			(at 255.27 183.515 0)
		)
		(property "Description" "SN74LVCH16T245DGG"
			(at 255.27 185.42 0)
		)
		(property "Library Ref" "7416T245"
			(at 255.27 187.325 0)
		)
		(property "Library Path" "SchLib\\Standard Logic.SchLib"
			(at 255.27 189.23 0)
		)
		(property "Comment" "SN74LVCH16T245DGG"
			(at 255.27 191.135 0)
		)
		(property "Component Kind" "Standard"
			(at 255.27 193.04 0)
		)
		(property "Component Type" "Standard"
			(at 255.27 194.945 0)
		)
		(property "Device" "SN74LVCH16T245DGG"
			(at 255.27 196.85 0)
		)
		(property "PackageDescription" "SOP, 48-Leads, Body 12.6x6.2mm (max), Pitch 0.50mm, IPC Medium Density"
			(at 255.27 198.755 0)
		)
		(property "Status" " "
			(at 255.27 200.66 0)
		)
		(property "Part Description" "16-Bit Dual-Supply Bus Transceiver with Configurable Voltage Translation and 3-State Outputs"
			(at 255.27 202.565 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 255.27 204.47 0)
		)
		(property "Manufacturer Part Number" "SN74LVCH16T245DGG"
			(at 255.27 206.375 0)
		)
		(property "Pin Count" "48"
			(at 255.27 208.28 0)
		)
		(property "Case" "TSSOP48"
			(at 255.27 210.185 0)
		)
		(property "Mounted" "Yes"
			(at 255.27 212.09 0)
		)
		(property "Socket" "No"
			(at 255.27 213.995 0)
		)
		(property "SMD" "Yes"
			(at 255.27 215.9 0)
		)
		(property "PressFit" "No"
			(at 255.27 217.805 0)
		)
		(property "Sense" "No"
			(at 255.27 219.71 0)
		)
		(property "Sense Comment" " "
			(at 255.27 221.615 0)
		)
		(property "Bonding" "No"
			(at 255.27 223.52 0)
		)
		(property "Status Comment" " "
			(at 255.27 225.425 0)
		)
		(property "ComponentHeight" "1.2mm"
			(at 255.27 227.33 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 255.27 229.235 0)
		)
		(property "Footprint Ref" "SOP50P810X120-48N"
			(at 255.27 231.14 0)
		)
		(property "Author" "CERN DEM HF"
			(at 255.27 233.045 0)
		)
		(property "HelpURL" ""
			(at 255.27 234.95 0)
		)
		(property "ComponentLink1URL" " "
			(at 255.27 236.855 0)
		)
		(property "ComponentLink1Description" " "
			(at 255.27 238.76 0)
		)
		(property "ComponentLink2URL" " "
			(at 255.27 240.665 0)
		)
		(property "ComponentLink2Description" " "
			(at 255.27 242.57 0)
		)
		(property "CreateDate" "03/29/22 00:00:00"
			(at 255.27 244.475 0)
		)
		(property "LatestRevisionDate" "03/29/22 00:00:00"
			(at 255.27 246.38 0)
		)
		(property "SCEM" " "
			(at 255.27 248.285 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 255.27 250.19 0)
		)
		(property "Library Name" "Standard Logic"
			(at 255.27 252.095 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 255.27 254 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 255.27 255.905 0)
		)
		(pin "25")
		(pin "18")
		(pin "22")
		(pin "32")
		(pin "16")
		(pin "20")
		(pin "14")
		(pin "27")
		(pin "33")
		(pin "5")
		(pin "44")
		(pin "30")
		(pin "48")
		(pin "34")
		(pin "23")
		(pin "46")
		(pin "3")
		(pin "37")
		(pin "43")
		(pin "47")
		(pin "41")
		(pin "38")
		(pin "2")
		(pin "40")
		(pin "31")
		(pin "15")
		(pin "1")
		(pin "8")
		(pin "42")
		(pin "12")
		(pin "10")
		(pin "39")
		(pin "21")
		(pin "4")
		(pin "11")
		(pin "9")
		(pin "26")
		(pin "24")
		(pin "45")
		(pin "36")
		(pin "35")
		(pin "19")
		(pin "6")
		(pin "28")
		(pin "29")
		(pin "17")
		(pin "7")
		(pin "13")
		(instances
			(project "vme-wren"
				(path
					(reference "IC42")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 247.65 170.18 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR076"
			(at 247.65 170.18 0)
		)
		(property "Value" "P3V3"
			(at 243.84 170.18 90)
		)
		(property "Footprint" ""
			(at 247.65 170.18 0)
		)
		(property "Datasheet" ""
			(at 247.65 170.18 0)
		)
		(property "Description" ""
			(at 247.65 170.18 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR076")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 266.7 217.17 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR05"
			(at 266.7 217.17 0)
		)
		(property "Value" "P1V8"
			(at 266.7 212.09 0)
		)
		(property "Footprint" ""
			(at 266.7 217.17 0)
		)
		(property "Datasheet" ""
			(at 266.7 217.17 0)
		)
		(property "Description" ""
			(at 266.7 217.17 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Standard Logic:SN74LVCH16T245DGG")
		(at 109.22 105.41 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC16"
			(at 120.65 100.33 0)
		)
		(property "Value" "SN74LVCH16T245DGG"
			(at 120.65 102.87 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOP50P810X120-48N"
			(at 109.22 182.88 0)
		)
		(property "Datasheet" ""
			(at 109.22 184.785 0)
		)
		(property "Description" "SN74LVCH16T245DGG"
			(at 109.22 186.69 0)
		)
		(property "Library Ref" "7416T245"
			(at 109.22 188.595 0)
		)
		(property "Library Path" "SchLib\\Standard Logic.SchLib"
			(at 109.22 190.5 0)
		)
		(property "Comment" "SN74LVCH16T245DGG"
			(at 109.22 192.405 0)
		)
		(property "Component Kind" "Standard"
			(at 109.22 194.31 0)
		)
		(property "Component Type" "Standard"
			(at 109.22 196.215 0)
		)
		(property "Device" "SN74LVCH16T245DGG"
			(at 109.22 198.12 0)
		)
		(property "PackageDescription" "SOP, 48-Leads, Body 12.6x6.2mm (max), Pitch 0.50mm, IPC Medium Density"
			(at 109.22 200.025 0)
		)
		(property "Status" " "
			(at 109.22 201.93 0)
		)
		(property "Part Description" "16-Bit Dual-Supply Bus Transceiver with Configurable Voltage Translation and 3-State Outputs"
			(at 109.22 203.835 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 109.22 205.74 0)
		)
		(property "Manufacturer Part Number" "SN74LVCH16T245DGG"
			(at 109.22 207.645 0)
		)
		(property "Pin Count" "48"
			(at 109.22 209.55 0)
		)
		(property "Case" "TSSOP48"
			(at 109.22 211.455 0)
		)
		(property "Mounted" "Yes"
			(at 109.22 213.36 0)
		)
		(property "Socket" "No"
			(at 109.22 215.265 0)
		)
		(property "SMD" "Yes"
			(at 109.22 217.17 0)
		)
		(property "PressFit" "No"
			(at 109.22 219.075 0)
		)
		(property "Sense" "No"
			(at 109.22 220.98 0)
		)
		(property "Sense Comment" " "
			(at 109.22 222.885 0)
		)
		(property "Bonding" "No"
			(at 109.22 224.79 0)
		)
		(property "Status Comment" " "
			(at 109.22 226.695 0)
		)
		(property "ComponentHeight" "1.2mm"
			(at 109.22 228.6 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 109.22 230.505 0)
		)
		(property "Footprint Ref" "SOP50P810X120-48N"
			(at 109.22 232.41 0)
		)
		(property "Author" "CERN DEM HF"
			(at 109.22 234.315 0)
		)
		(property "HelpURL" ""
			(at 109.22 236.22 0)
		)
		(property "ComponentLink1URL" " "
			(at 109.22 238.125 0)
		)
		(property "ComponentLink1Description" " "
			(at 109.22 240.03 0)
		)
		(property "ComponentLink2URL" " "
			(at 109.22 241.935 0)
		)
		(property "ComponentLink2Description" " "
			(at 109.22 243.84 0)
		)
		(property "CreateDate" "03/29/22 00:00:00"
			(at 109.22 245.745 0)
		)
		(property "LatestRevisionDate" "03/29/22 00:00:00"
			(at 109.22 247.65 0)
		)
		(property "SCEM" " "
			(at 109.22 249.555 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 109.22 251.46 0)
		)
		(property "Library Name" "Standard Logic"
			(at 109.22 253.365 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 109.22 255.27 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 109.22 257.175 0)
		)
		(pin "25")
		(pin "18")
		(pin "22")
		(pin "32")
		(pin "16")
		(pin "20")
		(pin "14")
		(pin "27")
		(pin "33")
		(pin "5")
		(pin "44")
		(pin "30")
		(pin "48")
		(pin "34")
		(pin "23")
		(pin "46")
		(pin "3")
		(pin "37")
		(pin "43")
		(pin "47")
		(pin "41")
		(pin "38")
		(pin "2")
		(pin "40")
		(pin "31")
		(pin "15")
		(pin "1")
		(pin "8")
		(pin "42")
		(pin "12")
		(pin "10")
		(pin "39")
		(pin "21")
		(pin "4")
		(pin "11")
		(pin "9")
		(pin "26")
		(pin "24")
		(pin "45")
		(pin "36")
		(pin "35")
		(pin "19")
		(pin "6")
		(pin "28")
		(pin "29")
		(pin "17")
		(pin "7")
		(pin "13")
		(instances
			(project "vme-wren"
				(path
					(reference "IC16")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 140.97 214.63 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C110"
			(at 144.78 212.0901 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 146.05 209.55 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 140.97 214.63 0)
		)
		(property "Datasheet" ""
			(at 140.97 214.63 0)
		)
		(property "Description" "100nF"
			(at 144.78 209.5501 90)
		)
		(property "SMD" "Yes"
			(at 140.462 216.916 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 152.908 214.63 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 154.813 214.63 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 156.718 214.63 0)
		)
		(property "Comment" "100nF"
			(at 158.623 214.63 0)
		)
		(property "Component Kind" "Standard"
			(at 160.528 214.63 0)
		)
		(property "Component Type" "Standard"
			(at 162.433 214.63 0)
		)
		(property "Pin Count" "2"
			(at 164.338 214.63 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 166.243 214.63 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 168.148 214.63 0)
		)
		(property "PackageDescription" " "
			(at 170.053 214.63 0)
		)
		(property "Status" "Not Recommended"
			(at 171.958 214.63 0)
		)
		(property "Status Comment" " "
			(at 173.863 214.63 0)
		)
		(property "Voltage" "16V"
			(at 175.768 214.63 0)
		)
		(property "Tolerance" "±10%"
			(at 179.578 214.63 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 181.483 214.63 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 183.388 214.63 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 185.293 214.63 0)
		)
		(property "Case" "0402"
			(at 187.198 214.63 0)
		)
		(property "Mounted" "Yes"
			(at 189.103 214.63 0)
		)
		(property "Socket" "No"
			(at 191.008 214.63 0)
		)
		(property "PressFit" " "
			(at 194.818 214.63 0)
		)
		(property "Sense" "No"
			(at 196.723 214.63 0)
		)
		(property "Sense Comment" " "
			(at 198.628 214.63 0)
		)
		(property "ComponentHeight" " "
			(at 200.533 214.63 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 202.438 214.63 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 204.343 214.63 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 206.248 214.63 0)
		)
		(property "HelpURL" ""
			(at 208.153 214.63 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 210.058 214.63 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 211.963 214.63 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 213.868 214.63 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 215.773 214.63 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 217.678 214.63 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 219.583 214.63 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 221.488 214.63 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C110")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 102.87 214.63 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR011"
			(at 102.87 214.63 0)
		)
		(property "Value" "GND"
			(at 102.87 219.71 0)
		)
		(property "Footprint" ""
			(at 102.87 214.63 0)
		)
		(property "Datasheet" ""
			(at 102.87 214.63 0)
		)
		(property "Description" ""
			(at 102.87 214.63 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR011")
					(unit 1)
				)
			)
		)
	)
)
