(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A3")
	(title_block
		(title "VME interface connections - top level")
	)
	(lib_symbols
		(symbol "Analog & Interface:DS90LV027AQMA_NOPB"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 7.62 1.27 0)
			)
			(property "Value" "DS90LV027AQMA_NOPB"
				(at 0 -29.845 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOIC127P600X175-8N"
				(at 0 -31.75 0)
			)
			(property "Datasheet" ""
				(at 0 -33.655 0)
			)
			(property "Description" "DS90LV027AQMA_NOPB"
				(at 0 -35.56 0)
			)
			(property "Library Ref" "DS90LV027AQ"
				(at 0 -37.465 0)
			)
			(property "Library Path" "SchLib\\Analog & Interface.SchLib"
				(at 0 -39.37 0)
			)
			(property "Comment" "DS90LV027AQMA/NOPB"
				(at 0 -41.275 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -43.18 0)
			)
			(property "Component Type" "Standard"
				(at 0 -45.085 0)
			)
			(property "Device" "DS90LV027AQMA/NOPB"
				(at 0 -46.99 0)
			)
			(property "PackageDescription" "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density"
				(at 0 -48.895 0)
			)
			(property "Status" " "
				(at 0 -50.8 0)
			)
			(property "Part Description" "Automotive LVDS Dual Differential Driver"
				(at 0 -52.705 0)
			)
			(property "Manufacturer" "TEXAS INSTRUMENTS"
				(at 0 -54.61 0)
			)
			(property "Manufacturer Part Number" "DS90LV027AQMA"
				(at 0 -56.515 0)
			)
			(property "Pin Count" "8"
				(at 0 -58.42 0)
			)
			(property "Case" "SOIC8"
				(at 0 -60.325 0)
			)
			(property "Mounted" "Yes"
				(at 0 -62.23 0)
			)
			(property "Socket" "No"
				(at 0 -64.135 0)
			)
			(property "SMD" "Yes"
				(at 0 -66.04 0)
			)
			(property "PressFit" "No"
				(at 0 -67.945 0)
			)
			(property "Sense" "No"
				(at 0 -69.85 0)
			)
			(property "Sense Comment" " "
				(at 0 -71.755 0)
			)
			(property "Bonding" "No"
				(at 0 -73.66 0)
			)
			(property "Status Comment" " "
				(at 0 -75.565 0)
			)
			(property "ComponentHeight" "1.75mm"
				(at 0 -77.47 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -79.375 0)
			)
			(property "Footprint Ref" "SOIC127P600X175-8N"
				(at 0 -81.28 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -83.185 0)
			)
			(property "HelpURL" ""
				(at 0 -85.09 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -86.995 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -88.9 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -90.805 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -92.71 0)
			)
			(property "CreateDate" "01/11/17 00:00:00"
				(at 0 -94.615 0)
			)
			(property "LatestRevisionDate" "06/01/22 00:00:00"
				(at 0 -96.52 0)
			)
			(property "SCEM" " "
				(at 0 -98.425 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -100.33 0)
			)
			(property "Library Name" "Analog & Interface"
				(at 0 -102.235 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -104.14 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -106.045 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "DS90LV027AQMA_NOPB_0_1"
				(rectangle
					(start 0 -25.4)
					(end 15.24 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 5.334 -5.08) (xy 0 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.334 -15.24) (xy 0 -15.24)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 8.382 -6.35)
					(radius 0.4572)
					(fill
						(type none)
					)
				)
				(circle
					(center 8.382 -16.51)
					(radius 0.4572)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.89 -6.35) (xy 9.906 -6.35) (xy 9.906 -7.62) (xy 15.24 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 8.89 -16.51) (xy 9.906 -16.51) (xy 9.906 -17.78) (xy 15.24 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 9.398 -5.08) (xy 5.334 -7.62) (xy 5.334 -2.54) (xy 9.398 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 9.398 -15.24) (xy 5.334 -17.78) (xy 5.334 -12.7) (xy 9.398 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 15.24 -2.54) (xy 9.906 -2.54) (xy 9.906 -3.81) (xy 7.366 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 15.24 -12.7) (xy 9.906 -12.7) (xy 9.906 -13.97) (xy 7.366 -13.97)
					)
					(fill
						(type none)
					)
				)
				(text "D"
					(at 7.112 -5.842 0)
				)
				(text "D"
					(at 7.112 -16.002 0)
				)
				(pin input line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "DI1")
					(number "2")
				)
				(pin input line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "DI2")
					(number "3")
				)
				(pin power_in line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "VCC")
					(number "1")
				)
				(pin output line
					(at 20.32 -2.54 180)
					(length 5.08)
					(name "DO1+")
					(number "7")
				)
				(pin output line
					(at 20.32 -7.62 180)
					(length 5.08)
					(name "DO1-")
					(number "8")
				)
				(pin output line
					(at 20.32 -12.7 180)
					(length 5.08)
					(name "DO2+")
					(number "6")
				)
				(pin output line
					(at 20.32 -17.78 180)
					(length 5.08)
					(name "DO2-")
					(number "5")
				)
				(pin power_in line
					(at 20.32 -22.86 180)
					(length 5.08)
					(name "GND")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Analog & Interface:MAX3430ESA"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 8.89 1.27 0)
			)
			(property "Value" "MAX3430ESA"
				(at 0 -29.845 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOIC127P600X175-8N"
				(at 0 -31.75 0)
			)
			(property "Datasheet" ""
				(at 0 -33.655 0)
			)
			(property "Description" "MAX3430ESA"
				(at 0 -35.56 0)
			)
			(property "Library Ref" "MAX3430"
				(at 0 -37.465 0)
			)
			(property "Library Path" "SchLib\\Analog & Interface.SchLib"
				(at 0 -39.37 0)
			)
			(property "Comment" "MAX3430ESA"
				(at 0 -41.275 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -43.18 0)
			)
			(property "Component Type" "Standard"
				(at 0 -45.085 0)
			)
			(property "Device" "MAX3430ESA"
				(at 0 -46.99 0)
			)
			(property "PackageDescription" "SOIC, 1.27mm Pitch; 8 Pin, 3.90mm W X 4.90mm L X 1.75mm H body, IPC Medium Density"
				(at 0 -48.895 0)
			)
			(property "Status" " "
				(at 0 -50.8 0)
			)
			(property "Part Description" "±80V Fault-Protected, Fail-Safe, 1/4-Unit Load, +3.3V RS-485 Transceiver (-40°C to +85°C)"
				(at 0 -52.705 0)
			)
			(property "Manufacturer" "MAXIM"
				(at 0 -54.61 0)
			)
			(property "Manufacturer Part Number" "MAX3430ESA"
				(at 0 -56.515 0)
			)
			(property "Pin Count" "8"
				(at 0 -58.42 0)
			)
			(property "Case" "SOIC8"
				(at 0 -60.325 0)
			)
			(property "Mounted" "Yes"
				(at 0 -62.23 0)
			)
			(property "Socket" "No"
				(at 0 -64.135 0)
			)
			(property "SMD" "Yes"
				(at 0 -66.04 0)
			)
			(property "PressFit" "No"
				(at 0 -67.945 0)
			)
			(property "Sense" "No"
				(at 0 -69.85 0)
			)
			(property "Sense Comment" " "
				(at 0 -71.755 0)
			)
			(property "Bonding" "No"
				(at 0 -73.66 0)
			)
			(property "Status Comment" " "
				(at 0 -75.565 0)
			)
			(property "ComponentHeight" "1.75mm"
				(at 0 -77.47 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -79.375 0)
			)
			(property "Footprint Ref" "SOIC127P600X175-8N"
				(at 0 -81.28 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -83.185 0)
			)
			(property "HelpURL" ""
				(at 0 -85.09 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -86.995 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -88.9 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -90.805 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -92.71 0)
			)
			(property "CreateDate" "02/10/20 00:00:00"
				(at 0 -94.615 0)
			)
			(property "LatestRevisionDate" "02/10/20 00:00:00"
				(at 0 -96.52 0)
			)
			(property "SCEM" " "
				(at 0 -98.425 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -100.33 0)
			)
			(property "Library Name" "Analog & Interface"
				(at 0 -102.235 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -104.14 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -106.045 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "MAX3430ESA_0_1"
				(rectangle
					(start 0 -25.4)
					(end 17.78 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 5.08 -17.78) (xy 6.35 -17.78)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.35 -7.62) (xy 5.08 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.35 -7.62) (xy 10.414 -10.16) (xy 10.414 -5.08) (xy 6.35 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.35 -12.7) (xy 7.874 -12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.874 -5.588) (xy 7.874 -2.54) (xy 6.35 -2.54)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 7.874 -6.096)
					(radius 0.4572)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.874 -12.7) (xy 7.874 -16.129)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 9.398 -16.51)
					(radius 0.4572)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 9.906 -16.51) (xy 12.7 -16.51)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 10.414 -6.35) (xy 13.97 -6.35)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 10.414 -17.78) (xy 6.35 -15.24) (xy 6.35 -20.32) (xy 10.414 -17.78)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 10.922 -8.89)
					(radius 0.4572)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 11.43 -8.89) (xy 12.7 -8.89)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 12.7 -15.24)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 12.7 -16.51) (xy 12.7 -8.89)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 13.97 -6.35) (xy 13.97 -19.05)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 13.97 -10.16)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 13.97 -19.05) (xy 8.382 -19.05)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 17.78 -10.16) (xy 13.97 -10.16)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 17.78 -15.24) (xy 12.7 -15.24)
					)
					(fill
						(type none)
					)
				)
				(text "D"
					(at 7.62 -17.78 0)
				)
				(text "R"
					(at 9.144 -7.62 0)
				)
				(text "A"
					(at 16.51 -8.89 0)
				)
				(text "B"
					(at 16.51 -13.97 0)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "~{RE}")
					(number "2")
				)
				(pin output line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "RO")
					(number "1")
				)
				(pin input line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "DE")
					(number "3")
				)
				(pin input line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "DI")
					(number "4")
				)
				(pin power_in line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "VCC")
					(number "8")
				)
				(pin input line
					(at 22.86 -10.16 180)
					(length 5.08)
					(name "A")
					(number "6")
				)
				(pin input line
					(at 22.86 -15.24 180)
					(length 5.08)
					(name "B")
					(number "7")
				)
				(pin power_in line
					(at 22.86 -22.86 180)
					(length 5.08)
					(name "GND")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Capacitors SMD:CC0402_100NF_16V_10%_X7R"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 3.048 0)
			)
			(property "Value" "CC0402_100NF_16V_10%_X7R"
				(at 0 -6.223 0)
			)
			(property "Footprint" "Capacitors SMD:CAPC1005X55N"
				(at 0 -8.128 0)
			)
			(property "Datasheet" ""
				(at 0 -10.033 0)
			)
			(property "Description" "100nF"
				(at 3.81 -3.048 0)
			)
			(property "Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -11.938 0)
			)
			(property "Library Ref" "Capacitor - non polarized"
				(at 0 -13.843 0)
			)
			(property "Library Path" "SchLib\\Capacitors.SchLib"
				(at 0 -15.748 0)
			)
			(property "Comment" "100nF"
				(at 0 -17.653 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -19.558 0)
			)
			(property "Component Type" "Standard"
				(at 0 -21.463 0)
			)
			(property "Pin Count" "2"
				(at 0 -23.368 0)
			)
			(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
				(at 0 -25.273 0)
			)
			(property "Footprint Ref" "CAPC1005X55N"
				(at 0 -27.178 0)
			)
			(property "PackageDescription" " "
				(at 0 -29.083 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -30.988 0)
			)
			(property "Status Comment" " "
				(at 0 -32.893 0)
			)
			(property "Voltage" "16V"
				(at 0 -34.798 0)
			)
			(property "TC" "X7R"
				(at 0 -36.703 0)
			)
			(property "Tolerance" "±10%"
				(at 0 -38.608 0)
			)
			(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
				(at 0 -40.513 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -42.418 0)
			)
			(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
				(at 0 -44.323 0)
			)
			(property "Case" "0402"
				(at 0 -46.228 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.133 0)
			)
			(property "Socket" "No"
				(at 0 -50.038 0)
			)
			(property "SMD" "Yes"
				(at 0 -51.943 0)
			)
			(property "PressFit" " "
				(at 0 -53.848 0)
			)
			(property "Sense" "No"
				(at 0 -55.753 0)
			)
			(property "Sense Comment" " "
				(at 0 -57.658 0)
			)
			(property "ComponentHeight" " "
				(at 0 -59.563 0)
			)
			(property "Manufacturer1 Example" "MURATA"
				(at 0 -61.468 0)
			)
			(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
				(at 0 -63.373 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.278 0)
			)
			(property "HelpURL" ""
				(at 0 -67.183 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.088 0)
			)
			(property "CreateDate" "12/05/13 00:00:00"
				(at 0 -70.993 0)
			)
			(property "LatestRevisionDate" "12/03/07 00:00:00"
				(at 0 -72.898 0)
			)
			(property "Database Table Name" "Capacitors"
				(at 0 -74.803 0)
			)
			(property "Library Name" "Capacitors SMD"
				(at 0 -76.708 0)
			)
			(property "Footprint Library" "Capacitors SMD"
				(at 0 -78.613 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -80.518 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "CC0402_100NF_16V_10%_X7R_0_1"
				(polyline
					(pts
						(xy 2.54 0) (xy 3.302 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -2.032) (xy 3.302 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.318 2.032) (xy 4.318 -2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 4.318 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Diodes:SM712.TCT"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 3.81 1.27 0)
			)
			(property "Value" "SM712.TCT"
				(at 0 -14.605 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:SOT95P237X112-3N"
				(at 0 -16.51 0)
			)
			(property "Datasheet" ""
				(at 0 -18.415 0)
			)
			(property "Description" "SM712.TCT"
				(at 0 -20.32 0)
			)
			(property "Library Ref" "SM712"
				(at 0 -22.225 0)
			)
			(property "Library Path" "SchLib\\Diodes.SchLib"
				(at 0 -24.13 0)
			)
			(property "Comment" "SM712.TCT"
				(at 0 -26.035 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -27.94 0)
			)
			(property "Component Type" "Standard"
				(at 0 -29.845 0)
			)
			(property "Device" "SM712.TCT"
				(at 0 -31.75 0)
			)
			(property "PackageDescription" "SOT, 0.95mm Pitch; 3 Pin, 1.30mm W X 2.92mm L X 1.12mm H body, IPC Medium Density"
				(at 0 -33.655 0)
			)
			(property "Voltage" "12V/-7V"
				(at 0 -35.56 0)
			)
			(property "Power" "400W"
				(at 0 -37.465 0)
			)
			(property "Status" " "
				(at 0 -39.37 0)
			)
			(property "Part Description" "Asymmetrical TVS Diode for Extended Common-Mode RS-485"
				(at 0 -41.275 0)
			)
			(property "Manufacturer" "SEMTECH"
				(at 0 -43.18 0)
			)
			(property "Manufacturer Part Number" "SM712.TCT"
				(at 0 -45.085 0)
			)
			(property "Pin Count" "3"
				(at 0 -46.99 0)
			)
			(property "Case" "SOT23-3"
				(at 0 -48.895 0)
			)
			(property "Mounted" "Yes"
				(at 0 -50.8 0)
			)
			(property "Socket" "No"
				(at 0 -52.705 0)
			)
			(property "SMD" "Yes"
				(at 0 -54.61 0)
			)
			(property "PressFit" "No"
				(at 0 -56.515 0)
			)
			(property "Sense" "No"
				(at 0 -58.42 0)
			)
			(property "Sense Comment" " "
				(at 0 -60.325 0)
			)
			(property "Bonding" "No"
				(at 0 -62.23 0)
			)
			(property "Status Comment" " "
				(at 0 -64.135 0)
			)
			(property "ComponentHeight" "1.12mm"
				(at 0 -66.04 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -67.945 0)
			)
			(property "Footprint Ref" "SOT95P237X112-3N"
				(at 0 -69.85 0)
			)
			(property "HelpURL" ""
				(at 0 -71.755 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -73.66 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -75.565 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -77.47 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -79.375 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -81.28 0)
			)
			(property "CreateDate" "09/03/14 00:00:00"
				(at 0 -83.185 0)
			)
			(property "LatestRevisionDate" "01/13/15 00:00:00"
				(at 0 -85.09 0)
			)
			(property "Field1" " "
				(at 0 -86.995 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -88.9 0)
			)
			(property "Library Name" "Diodes"
				(at 0 -90.805 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -92.71 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -94.615 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "SM712.TCT_0_1"
				(polyline
					(pts
						(xy 0 -2.54) (xy 6.858 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -7.62) (xy 6.858 -7.62)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0 -10.16)
					(end 7.62 0)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 1.524 -1.27) (xy 1.778 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -6.35) (xy 1.778 -6.604)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.778 -1.524) (xy 1.778 -3.556)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.778 -3.556) (xy 2.032 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.778 -6.604) (xy 1.778 -8.636)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.778 -8.636) (xy 2.032 -8.89)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.794 -3.556) (xy 1.778 -2.54) (xy 2.794 -1.524) (xy 2.794 -3.556)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 2.794 -8.636) (xy 1.778 -7.62) (xy 2.794 -6.604) (xy 2.794 -8.636)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 4.572 -3.556) (xy 5.588 -2.54) (xy 4.572 -1.524) (xy 4.572 -3.556)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 4.572 -8.636) (xy 5.588 -7.62) (xy 4.572 -6.604) (xy 4.572 -8.636)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 5.334 -1.27) (xy 5.588 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.334 -6.35) (xy 5.588 -6.604)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.588 -1.524) (xy 5.588 -3.556)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.588 -3.556) (xy 5.842 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.588 -6.604) (xy 5.588 -8.636)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.588 -8.636) (xy 5.842 -8.89)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.858 -2.54) (xy 6.858 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.858 -5.08) (xy 6.858 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.858 -5.08) (xy 7.62 -5.08)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 6.858 -5.08)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(text "12V"
					(at 1.016 -5.842 0)
				)
				(text "7V"
					(at 4.318 -5.842 0)
				)
				(pin passive line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "I/O1")
					(number "1")
				)
				(pin passive line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "I/O2")
					(number "2")
				)
				(pin passive line
					(at 12.7 -5.08 180)
					(length 5.08)
					(name "GND")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_10K_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "10k"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "10k"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270671003L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_10K_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0402_33R_1%_0.0625W_100PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0402_33R_1%_0.0625W_100PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1005X40N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "33"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "33"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1005X40N"
				(at 0 -27.813 0)
			)
			(property "Status" "Not Recommended"
				(at 0 -29.718 0)
			)
			(property "Power" "0.0625W"
				(at 0 -31.623 0)
			)
			(property "TC" "±100ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0402"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "YAGEO PHYCOMP"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "232270673309L"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.4mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM JLC"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "12/03/07 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "10/17/12 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0402_33R_1%_0.0625W_100PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Resistors SMD:R0603_120R_1%_0.2W_200PPM"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 3.81 1.778 0)
			)
			(property "Value" "R0603_120R_1%_0.2W_200PPM"
				(at 0 -4.953 0)
			)
			(property "Footprint" "Resistors SMD:RESC1608X55N"
				(at 0 -6.858 0)
			)
			(property "Datasheet" ""
				(at 0 -8.763 0)
			)
			(property "Description" "±1%"
				(at 3.81 0 0)
			)
			(property "Val" "120"
				(at 3.81 -1.778 0)
			)
			(property "Part Number" "R0603_120R_1%_0.2W_200PPM"
				(at 0 -10.668 0)
			)
			(property "Library Ref" "Resistor - 1%"
				(at 0 -12.573 0)
			)
			(property "Library Path" "SchLib\\Resistors.SchLib"
				(at 0 -14.478 0)
			)
			(property "Comment" "120"
				(at 0 -16.383 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -18.288 0)
			)
			(property "Component Type" "Standard"
				(at 0 -20.193 0)
			)
			(property "PackageDescription" " "
				(at 0 -22.098 0)
			)
			(property "Pin Count" "2"
				(at 0 -24.003 0)
			)
			(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
				(at 0 -25.908 0)
			)
			(property "Footprint Ref" "RESC1608X55N"
				(at 0 -27.813 0)
			)
			(property "Status" "Preferred"
				(at 0 -29.718 0)
			)
			(property "Power" "0.2W"
				(at 0 -31.623 0)
			)
			(property "TC" "±200ppm/°C"
				(at 0 -33.528 0)
			)
			(property "Voltage" " "
				(at 0 -35.433 0)
			)
			(property "Tolerance" "±1%"
				(at 0 -37.338 0)
			)
			(property "Part Description" "General Purpose Thick Film Chip Resistor"
				(at 0 -39.243 0)
			)
			(property "Manufacturer" "GENERIC"
				(at 0 -41.148 0)
			)
			(property "Manufacturer Part Number" "R0603_120R_1%_0.2W_200PPM"
				(at 0 -43.053 0)
			)
			(property "Case" "0603"
				(at 0 -44.958 0)
			)
			(property "PressFit" "No"
				(at 0 -46.863 0)
			)
			(property "Mounted" "Yes"
				(at 0 -48.768 0)
			)
			(property "Sense Comment" " "
				(at 0 -50.673 0)
			)
			(property "Sense" "No"
				(at 0 -52.578 0)
			)
			(property "Status Comment" " "
				(at 0 -54.483 0)
			)
			(property "Socket" "No"
				(at 0 -56.388 0)
			)
			(property "SMD" "Yes"
				(at 0 -58.293 0)
			)
			(property "ComponentHeight" " "
				(at 0 -60.198 0)
			)
			(property "Manufacturer1 Example" "TE CONNECTIVITY"
				(at 0 -62.103 0)
			)
			(property "Manufacturer1 Part Number" "CRGH0603F120R"
				(at 0 -64.008 0)
			)
			(property "Manufacturer1 ComponentHeight" "0.55mm"
				(at 0 -65.913 0)
			)
			(property "HelpURL" ""
				(at 0 -67.818 0)
			)
			(property "Author" "CERN DEM HF"
				(at 0 -69.723 0)
			)
			(property "CreateDate" "02/24/23 00:00:00"
				(at 0 -71.628 0)
			)
			(property "LatestRevisionDate" "02/24/23 00:00:00"
				(at 0 -73.533 0)
			)
			(property "Database Table Name" "Resistors"
				(at 0 -75.438 0)
			)
			(property "Library Name" "Resistors SMD"
				(at 0 -77.343 0)
			)
			(property "Footprint Library" "Resistors SMD"
				(at 0 -79.248 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -81.153 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "R0603_120R_1%_0.2W_200PPM_0_1"
				(polyline
					(pts
						(xy 1.524 0.762) (xy 1.524 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 -0.762) (xy 6.096 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 0.762) (xy 1.524 0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.096 -0.762) (xy 6.096 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 0 0)
					(length 1.524)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 1.524)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Standard Logic:SN74LV595ARGYR"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 10.16 1.27 0)
			)
			(property "Value" "SN74LV595ARGYR"
				(at 0 -37.465 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:TEXAS_RGY (R-PVQFN-N16)"
				(at 0 -39.37 0)
			)
			(property "Datasheet" ""
				(at 0 -41.275 0)
			)
			(property "Description" "SN74LV595ARGYR"
				(at 0 -43.18 0)
			)
			(property "Library Ref" "74595_a"
				(at 0 -45.085 0)
			)
			(property "Library Path" "SchLib\\Standard Logic.SchLib"
				(at 0 -46.99 0)
			)
			(property "Comment" "SN74LV595ARGY"
				(at 0 -48.895 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -50.8 0)
			)
			(property "Component Type" "Standard"
				(at 0 -52.705 0)
			)
			(property "Device" "SN74LV595ARGY"
				(at 0 -54.61 0)
			)
			(property "PackageDescription" "TEXAS Case Style RGY (R-PVQFN-N16), QFN, 0.50mm Pitch, Rect.; 16 Pin, 4.00mm L X 3.50mm W X 1mm H body (w/Thermal Tab 2.65 X 2.15mm)"
				(at 0 -56.515 0)
			)
			(property "Status" " "
				(at 0 -58.42 0)
			)
			(property "Part Description" "8-Bit Shift Register with 3-State Output Registers"
				(at 0 -60.325 0)
			)
			(property "Manufacturer" "TEXAS INSTRUMENTS"
				(at 0 -62.23 0)
			)
			(property "Manufacturer Part Number" "SN74LV595ARGY"
				(at 0 -64.135 0)
			)
			(property "Pin Count" "17"
				(at 0 -66.04 0)
			)
			(property "Case" "QFN16"
				(at 0 -67.945 0)
			)
			(property "Mounted" "Yes"
				(at 0 -69.85 0)
			)
			(property "Socket" "No"
				(at 0 -71.755 0)
			)
			(property "SMD" "Yes"
				(at 0 -73.66 0)
			)
			(property "PressFit" "No"
				(at 0 -75.565 0)
			)
			(property "Sense" "No"
				(at 0 -77.47 0)
			)
			(property "Sense Comment" " "
				(at 0 -79.375 0)
			)
			(property "Bonding" "No"
				(at 0 -81.28 0)
			)
			(property "Status Comment" " "
				(at 0 -83.185 0)
			)
			(property "ComponentHeight" "1mm"
				(at 0 -85.09 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -86.995 0)
			)
			(property "Footprint Ref" "TEXAS_RGY (R-PVQFN-N16)"
				(at 0 -88.9 0)
			)
			(property "Author" "CERN DEM MR"
				(at 0 -90.805 0)
			)
			(property "HelpURL" ""
				(at 0 -92.71 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -94.615 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -96.52 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -98.425 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -100.33 0)
			)
			(property "CreateDate" "10/10/17 00:00:00"
				(at 0 -102.235 0)
			)
			(property "LatestRevisionDate" "10/10/17 00:00:00"
				(at 0 -104.14 0)
			)
			(property "SCEM" " "
				(at 0 -106.045 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -107.95 0)
			)
			(property "Library Name" "Standard Logic"
				(at 0 -109.855 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -111.76 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -113.665 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "SN74LV595ARGYR_0_1"
				(rectangle
					(start 0 -33.02)
					(end 20.32 0)
					(fill
						(type background)
					)
				)
				(rectangle
					(start 19.812 -31.623)
					(end 20.32 -29.337)
					(fill
						(type outline)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "~{OE}")
					(number "13")
				)
				(pin input clock
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "RCLK")
					(number "12")
				)
				(pin input line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "~{SRCLR}")
					(number "10")
				)
				(pin input line
					(at -5.08 -12.7 0)
					(length 5.08)
					(name "SRCLK")
					(number "11")
				)
				(pin input line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "SER")
					(number "14")
				)
				(pin power_in line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "VCC")
					(number "16")
				)
				(pin tri_state line
					(at 25.4 -2.54 180)
					(length 5.08)
					(name "QA")
					(number "15")
				)
				(pin tri_state line
					(at 25.4 -5.08 180)
					(length 5.08)
					(name "QB")
					(number "1")
				)
				(pin tri_state line
					(at 25.4 -7.62 180)
					(length 5.08)
					(name "QC")
					(number "2")
				)
				(pin tri_state line
					(at 25.4 -10.16 180)
					(length 5.08)
					(name "QD")
					(number "3")
				)
				(pin tri_state line
					(at 25.4 -12.7 180)
					(length 5.08)
					(name "QE")
					(number "4")
				)
				(pin tri_state line
					(at 25.4 -15.24 180)
					(length 5.08)
					(name "QF")
					(number "5")
				)
				(pin tri_state line
					(at 25.4 -17.78 180)
					(length 5.08)
					(name "QG")
					(number "6")
				)
				(pin tri_state line
					(at 25.4 -20.32 180)
					(length 5.08)
					(name "QH")
					(number "7")
				)
				(pin output line
					(at 25.4 -22.86 180)
					(length 5.08)
					(name "QH'")
					(number "9")
				)
				(pin power_in line
					(at 25.4 -27.94 180)
					(length 5.08)
					(name "GND")
					(number "8")
				)
				(pin power_in line
					(at 25.4 -30.48 180)
					(length 5.08)
					(name "EP")
					(number "17")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Standard Logic:SN74LVTH125RGY"
			(pin_names
				(offset 1.27)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "IC"
				(at 7.62 1.27 0)
			)
			(property "Value" "SN74LVTH125RGY"
				(at 0 -34.925 0)
			)
			(property "Footprint" "ICs And Semiconductors SMD:TEXAS_RGY (S-PVQFN-N14)"
				(at 0 -36.83 0)
			)
			(property "Datasheet" ""
				(at 0 -38.735 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Part Number" "SN74LVTH125RGY"
				(at 0 -40.64 0)
			)
			(property "Library Ref" "74125"
				(at 0 -42.545 0)
			)
			(property "Library Path" "SchLib\\Standard Logic.SchLib"
				(at 0 -44.45 0)
			)
			(property "Comment" "SN74LVTH125RGY"
				(at 0 -46.355 0)
			)
			(property "Component Kind" "Standard"
				(at 0 -48.26 0)
			)
			(property "Component Type" "Standard"
				(at 0 -50.165 0)
			)
			(property "Device" "SN74LVTH125RGY"
				(at 0 -52.07 0)
			)
			(property "PackageDescription" "TEXAS Case Style RGY (S-PVQFN-N14), QFN, 0.50mm Pitch, Rect.; 14 Pin, 3.50mm L X 3.50mm W X 1mm H body (w/Thermal Tab 2.15 X 2.15mm)"
				(at 0 -53.975 0)
			)
			(property "Status" " "
				(at 0 -55.88 0)
			)
			(property "Part Description" "3.3V ABT Quadruple Bus Buffer with 3-State Outputs"
				(at 0 -57.785 0)
			)
			(property "Manufacturer" "TEXAS INSTRUMENTS"
				(at 0 -59.69 0)
			)
			(property "Manufacturer Part Number" "SN74LVTH125RGY"
				(at 0 -61.595 0)
			)
			(property "Pin Count" "15"
				(at 0 -63.5 0)
			)
			(property "Case" "QFN14"
				(at 0 -65.405 0)
			)
			(property "Mounted" "Yes"
				(at 0 -67.31 0)
			)
			(property "Socket" "No"
				(at 0 -69.215 0)
			)
			(property "SMD" "Yes"
				(at 0 -71.12 0)
			)
			(property "PressFit" "No"
				(at 0 -73.025 0)
			)
			(property "Sense" "No"
				(at 0 -74.93 0)
			)
			(property "Sense Comment" " "
				(at 0 -76.835 0)
			)
			(property "Bonding" "No"
				(at 0 -78.74 0)
			)
			(property "Status Comment" " "
				(at 0 -80.645 0)
			)
			(property "ComponentHeight" "1mm"
				(at 0 -82.55 0)
			)
			(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
				(at 0 -84.455 0)
			)
			(property "Footprint Ref" "TEXAS_RGY (S-PVQFN-N14)"
				(at 0 -86.36 0)
			)
			(property "Author" "CERN DEM BC"
				(at 0 -88.265 0)
			)
			(property "HelpURL" ""
				(at 0 -90.17 0)
			)
			(property "ComponentLink1URL" " "
				(at 0 -92.075 0)
			)
			(property "ComponentLink1Description" " "
				(at 0 -93.98 0)
			)
			(property "ComponentLink2URL" " "
				(at 0 -95.885 0)
			)
			(property "ComponentLink2Description" " "
				(at 0 -97.79 0)
			)
			(property "CreateDate" "04/22/20 00:00:00"
				(at 0 -99.695 0)
			)
			(property "LatestRevisionDate" "04/22/20 00:00:00"
				(at 0 -101.6 0)
			)
			(property "SCEM" " "
				(at 0 -103.505 0)
			)
			(property "Database Table Name" "ICs And Semiconductors"
				(at 0 -105.41 0)
			)
			(property "Library Name" "Standard Logic"
				(at 0 -107.315 0)
			)
			(property "Footprint Library" "ICs And Semiconductors SMD"
				(at 0 -109.22 0)
			)
			(property "License" "CC-BY-SA 4.0"
				(at 0 -111.125 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(symbol "SN74LVTH125RGY_0_1"
				(rectangle
					(start 0 -30.48)
					(end 15.24 0)
					(fill
						(type background)
					)
				)
				(pin input line
					(at -5.08 -2.54 0)
					(length 5.08)
					(name "1~{OE}")
					(number "1")
				)
				(pin input line
					(at -5.08 -5.08 0)
					(length 5.08)
					(name "2~{OE}")
					(number "4")
				)
				(pin input line
					(at -5.08 -7.62 0)
					(length 5.08)
					(name "3~{OE}")
					(number "10")
				)
				(pin input line
					(at -5.08 -10.16 0)
					(length 5.08)
					(name "4~{OE}")
					(number "13")
				)
				(pin input line
					(at -5.08 -15.24 0)
					(length 5.08)
					(name "1A")
					(number "2")
				)
				(pin input line
					(at -5.08 -17.78 0)
					(length 5.08)
					(name "2A")
					(number "5")
				)
				(pin input line
					(at -5.08 -20.32 0)
					(length 5.08)
					(name "3A")
					(number "9")
				)
				(pin input line
					(at -5.08 -22.86 0)
					(length 5.08)
					(name "4A")
					(number "12")
				)
				(pin power_in line
					(at -5.08 -27.94 0)
					(length 5.08)
					(name "VCC")
					(number "14")
				)
				(pin tri_state line
					(at 20.32 -15.24 180)
					(length 5.08)
					(name "1Y")
					(number "3")
				)
				(pin tri_state line
					(at 20.32 -17.78 180)
					(length 5.08)
					(name "2Y")
					(number "6")
				)
				(pin tri_state line
					(at 20.32 -20.32 180)
					(length 5.08)
					(name "3Y")
					(number "8")
				)
				(pin tri_state line
					(at 20.32 -22.86 180)
					(length 5.08)
					(name "4Y")
					(number "11")
				)
				(pin power_in line
					(at 20.32 -27.94 180)
					(length 5.08)
					(name "GND")
					(number "7")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "GROUND power-flag symbol"
				(at 0 0 0)
			)
			(property "ki_keywords" "Power Flag Symbol"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "vme-wren:P3V3"
			(power)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR0202"
				(at 0 0 0)
			)
			(property "Value" "P3V3"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "P3V3_0_0"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin power_in line
					(at 0 0 0)
					(length 0)
					(hide yes)
					(name "P3V3")
					(number "")
				)
			)
			(embedded_fonts no)
		)
	)
	(bus_alias "F_P0"
		(members "F_P0.RS485_DATA0" "F_P0.RS485_DATA1" "F_P0.TURNCLK[1..2]" "F_P0.BUNCHCLK[1..2]"
			"F_P0.TTC_DATA1" "F_P0.TTC_DATA0"
		)
	)
	(bus_alias "HWBYTE"
		(members "HWBYTE.H1_[0..7]" "HWBYTE.H2_[0..7]" "HWBYTE.L1_[0..7]" "HWBYTE.L2_[0..7]")
	)
	(bus_alias "VMEPX_USERIO_A"
		(members "VMEPX_USERIO_A.IO[0..31]")
	)
	(text_box "Place series termination resistors close to FPGA."
		(exclude_from_sim no)
		(at 17.78 255.27 0)
		(size 24.13 8.89)
		(margins 0.9525 0.9525 0.9525 0.9525)
		(fill
			(type color)
			(color 255 255 194 1)
		)
	)
	(junction
		(at 78.74 95.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 168.91 260.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 31.75 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 46.99 87.63)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 31.75 175.26)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 54.61 257.81)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 38.1 135.89)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 31.75 43.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 401.32 189.23)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 269.24 167.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 327.66 189.23)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 52.07 193.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 166.37 147.32)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 30.48 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 257.81 226.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 386.08 172.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 270.51 224.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 91.44 40.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 54.61 240.03)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 344.17 223.52)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 52.07 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 184.15 226.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 96.52 260.35)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 46.99 38.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 311.15 170.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 31.75 82.55)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 166.37 149.86)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 96.52 45.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 344.17 170.18)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 83.82 40.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 82.55 90.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 335.28 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 80.01 45.72)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 127 257.81)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 91.44 90.17)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 242.57 259.08)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 25.4 123.19)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 39.37 185.42)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 96.52 95.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 166.37 144.78)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 383.54 44.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 312.42 227.33)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 200.66 256.54)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 383.54 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 335.28 44.45)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 31.75 33.02)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 165.1 205.74)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 386.08 226.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 60.96 232.41)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 190.5 24.13)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 382.27 165.1)
	)
	(no_connect
		(at 382.27 218.44)
	)
	(no_connect
		(at 307.34 152.4)
	)
	(no_connect
		(at 308.61 219.71)
	)
	(no_connect
		(at 307.34 160.02)
	)
	(no_connect
		(at 307.34 157.48)
	)
	(no_connect
		(at 307.34 154.94)
	)
	(no_connect
		(at 92.71 245.11)
	)
	(bus_entry
		(at 181.61 242.57)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 255.27 236.22)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 323.85 144.78)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 255.27 243.84)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 181.61 245.11)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 255.27 241.3)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 25.4 182.88)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 398.78 152.4)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 398.78 157.48)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 190.5 66.04)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 255.27 238.76)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 255.27 231.14)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 181.61 234.95)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 181.61 237.49)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 398.78 213.36)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 255.27 233.68)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 398.78 208.28)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 398.78 160.02)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 325.12 207.01)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 398.78 144.78)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 398.78 210.82)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 181.61 232.41)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 25.4 172.72)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 181.61 240.03)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 398.78 200.66)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 398.78 162.56)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 323.85 149.86)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 25.4 133.35)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 325.12 199.39)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 398.78 149.86)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 398.78 147.32)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 398.78 154.94)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 398.78 215.9)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 255.27 248.92)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 25.4 35.56)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 181.61 250.19)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 25.4 85.09)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 325.12 212.09)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 325.12 217.17)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 25.4 143.51)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 323.85 142.24)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 398.78 198.12)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 325.12 209.55)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 325.12 214.63)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 323.85 147.32)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 325.12 204.47)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 181.61 247.65)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 398.78 205.74)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 255.27 246.38)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 398.78 203.2)
		(size 2.54 -2.54)
	)
	(bus_entry
		(at 325.12 201.93)
		(size 2.54 -2.54)
	)
	(bus
		(pts
			(xy 327.66 201.93) (xy 327.66 204.47)
		)
	)
	(wire
		(pts
			(xy 83.82 40.64) (xy 91.44 40.64)
		)
	)
	(bus
		(pts
			(xy 257.81 236.22) (xy 257.81 238.76)
		)
	)
	(wire
		(pts
			(xy 382.27 170.18) (xy 386.08 170.18)
		)
	)
	(wire
		(pts
			(xy 189.23 238.76) (xy 208.28 238.76)
		)
	)
	(wire
		(pts
			(xy 92.71 240.03) (xy 113.03 240.03)
		)
	)
	(wire
		(pts
			(xy 259.08 201.93) (xy 278.13 201.93)
		)
	)
	(wire
		(pts
			(xy 238.76 248.92) (xy 255.27 248.92)
		)
	)
	(wire
		(pts
			(xy 270.51 224.79) (xy 278.13 224.79)
		)
	)
	(wire
		(pts
			(xy 27.94 43.18) (xy 31.75 43.18)
		)
	)
	(wire
		(pts
			(xy 31.75 21.59) (xy 31.75 20.32)
		)
	)
	(wire
		(pts
			(xy 82.55 88.9) (xy 82.55 90.17)
		)
	)
	(wire
		(pts
			(xy 307.34 167.64) (xy 311.15 167.64)
		)
	)
	(wire
		(pts
			(xy 60.96 232.41) (xy 60.96 229.87)
		)
	)
	(wire
		(pts
			(xy 189.23 241.3) (xy 208.28 241.3)
		)
	)
	(wire
		(pts
			(xy 262.89 219.71) (xy 246.38 219.71)
		)
	)
	(bus
		(pts
			(xy 190.5 66.04) (xy 190.5 68.58)
		)
	)
	(wire
		(pts
			(xy 140.97 198.12) (xy 168.91 198.12)
		)
	)
	(wire
		(pts
			(xy 213.36 135.89) (xy 234.95 135.89)
		)
	)
	(wire
		(pts
			(xy 154.94 144.78) (xy 166.37 144.78)
		)
	)
	(wire
		(pts
			(xy 92.71 237.49) (xy 113.03 237.49)
		)
	)
	(bus
		(pts
			(xy 327.66 196.85) (xy 327.66 199.39)
		)
	)
	(bus
		(pts
			(xy 118.11 92.71) (xy 129.54 92.71)
		)
	)
	(wire
		(pts
			(xy 213.36 123.19) (xy 234.95 123.19)
		)
	)
	(wire
		(pts
			(xy 151.13 165.1) (xy 168.91 165.1)
		)
	)
	(wire
		(pts
			(xy 120.65 218.44) (xy 142.24 218.44)
		)
	)
	(wire
		(pts
			(xy 213.36 128.27) (xy 234.95 128.27)
		)
	)
	(wire
		(pts
			(xy 307.34 144.78) (xy 323.85 144.78)
		)
	)
	(bus
		(pts
			(xy 257.81 226.06) (xy 257.81 228.6)
		)
	)
	(wire
		(pts
			(xy 92.71 257.81) (xy 96.52 257.81)
		)
	)
	(wire
		(pts
			(xy 238.76 259.08) (xy 242.57 259.08)
		)
	)
	(wire
		(pts
			(xy 307.34 170.18) (xy 311.15 170.18)
		)
	)
	(wire
		(pts
			(xy 31.75 175.26) (xy 31.75 191.77)
		)
	)
	(wire
		(pts
			(xy 31.75 199.39) (xy 31.75 200.66)
		)
	)
	(wire
		(pts
			(xy 259.08 199.39) (xy 278.13 199.39)
		)
	)
	(wire
		(pts
			(xy 382.27 223.52) (xy 386.08 223.52)
		)
	)
	(wire
		(pts
			(xy 238.76 256.54) (xy 242.57 256.54)
		)
	)
	(wire
		(pts
			(xy 382.27 208.28) (xy 398.78 208.28)
		)
	)
	(bus
		(pts
			(xy 257.81 233.68) (xy 257.81 236.22)
		)
	)
	(wire
		(pts
			(xy 81.28 177.8) (xy 100.33 177.8)
		)
	)
	(wire
		(pts
			(xy 151.13 157.48) (xy 168.91 157.48)
		)
	)
	(wire
		(pts
			(xy 332.74 208.28) (xy 351.79 208.28)
		)
	)
	(wire
		(pts
			(xy 386.08 172.72) (xy 386.08 180.34)
		)
	)
	(bus
		(pts
			(xy 184.15 229.87) (xy 184.15 232.41)
		)
	)
	(wire
		(pts
			(xy 172.72 278.13) (xy 176.53 278.13)
		)
	)
	(wire
		(pts
			(xy 27.94 92.71) (xy 31.75 92.71)
		)
	)
	(wire
		(pts
			(xy 54.61 229.87) (xy 54.61 240.03)
		)
	)
	(wire
		(pts
			(xy 91.44 40.64) (xy 105.41 40.64)
		)
	)
	(wire
		(pts
			(xy 332.74 213.36) (xy 351.79 213.36)
		)
	)
	(wire
		(pts
			(xy 91.44 90.17) (xy 105.41 90.17)
		)
	)
	(wire
		(pts
			(xy 109.22 223.52) (xy 113.03 223.52)
		)
	)
	(wire
		(pts
			(xy 31.75 33.02) (xy 48.26 33.02)
		)
	)
	(bus
		(pts
			(xy 257.81 243.84) (xy 257.81 246.38)
		)
	)
	(wire
		(pts
			(xy 54.61 222.25) (xy 54.61 220.98)
		)
	)
	(bus
		(pts
			(xy 375.92 44.45) (xy 383.54 44.45)
		)
	)
	(bus
		(pts
			(xy 383.54 88.9) (xy 375.92 88.9)
		)
	)
	(wire
		(pts
			(xy 92.71 247.65) (xy 113.03 247.65)
		)
	)
	(wire
		(pts
			(xy 91.44 40.64) (xy 91.44 48.26)
		)
	)
	(bus
		(pts
			(xy 317.5 44.45) (xy 335.28 44.45)
		)
	)
	(wire
		(pts
			(xy 213.36 125.73) (xy 234.95 125.73)
		)
	)
	(wire
		(pts
			(xy 382.27 213.36) (xy 398.78 213.36)
		)
	)
	(wire
		(pts
			(xy 82.55 157.48) (xy 82.55 153.67)
		)
	)
	(wire
		(pts
			(xy 386.08 226.06) (xy 386.08 233.68)
		)
	)
	(wire
		(pts
			(xy 257.81 82.55) (xy 279.4 82.55)
		)
	)
	(wire
		(pts
			(xy 382.27 172.72) (xy 386.08 172.72)
		)
	)
	(wire
		(pts
			(xy 213.36 115.57) (xy 234.95 115.57)
		)
	)
	(wire
		(pts
			(xy 31.75 175.26) (xy 55.88 175.26)
		)
	)
	(wire
		(pts
			(xy 257.81 85.09) (xy 279.4 85.09)
		)
	)
	(wire
		(pts
			(xy 213.36 110.49) (xy 234.95 110.49)
		)
	)
	(wire
		(pts
			(xy 382.27 162.56) (xy 398.78 162.56)
		)
	)
	(wire
		(pts
			(xy 93.98 278.13) (xy 97.79 278.13)
		)
	)
	(bus
		(pts
			(xy 257.81 189.23) (xy 327.66 189.23)
		)
	)
	(bus
		(pts
			(xy 326.39 152.4) (xy 326.39 149.86)
		)
	)
	(wire
		(pts
			(xy 27.94 82.55) (xy 31.75 82.55)
		)
	)
	(bus
		(pts
			(xy 25.4 143.51) (xy 25.4 172.72)
		)
	)
	(bus
		(pts
			(xy 196.85 100.33) (xy 234.95 100.33)
		)
	)
	(wire
		(pts
			(xy 133.35 187.96) (xy 132.08 187.96)
		)
	)
	(bus
		(pts
			(xy 190.5 24.13) (xy 190.5 66.04)
		)
	)
	(wire
		(pts
			(xy 269.24 168.91) (xy 269.24 167.64)
		)
	)
	(wire
		(pts
			(xy 82.55 196.85) (xy 82.55 193.04)
		)
	)
	(wire
		(pts
			(xy 105.41 278.13) (xy 115.57 278.13)
		)
	)
	(wire
		(pts
			(xy 124.46 257.81) (xy 127 257.81)
		)
	)
	(wire
		(pts
			(xy 168.91 260.35) (xy 168.91 267.97)
		)
	)
	(bus
		(pts
			(xy 118.11 92.71) (xy 118.11 123.19)
		)
	)
	(wire
		(pts
			(xy 39.37 185.42) (xy 55.88 185.42)
		)
	)
	(wire
		(pts
			(xy 92.71 234.95) (xy 113.03 234.95)
		)
	)
	(wire
		(pts
			(xy 166.37 147.32) (xy 166.37 149.86)
		)
	)
	(wire
		(pts
			(xy 382.27 154.94) (xy 398.78 154.94)
		)
	)
	(bus
		(pts
			(xy 257.81 189.23) (xy 257.81 226.06)
		)
	)
	(wire
		(pts
			(xy 81.28 133.35) (xy 100.33 133.35)
		)
	)
	(wire
		(pts
			(xy 30.48 234.95) (xy 34.29 234.95)
		)
	)
	(bus
		(pts
			(xy 335.28 88.9) (xy 341.63 88.9)
		)
	)
	(wire
		(pts
			(xy 270.51 226.06) (xy 270.51 224.79)
		)
	)
	(wire
		(pts
			(xy 96.52 95.25) (xy 105.41 95.25)
		)
	)
	(wire
		(pts
			(xy 31.75 102.87) (xy 31.75 104.14)
		)
	)
	(wire
		(pts
			(xy 48.26 193.04) (xy 52.07 193.04)
		)
	)
	(wire
		(pts
			(xy 81.28 182.88) (xy 100.33 182.88)
		)
	)
	(wire
		(pts
			(xy 344.17 171.45) (xy 344.17 170.18)
		)
	)
	(bus
		(pts
			(xy 327.66 199.39) (xy 327.66 201.93)
		)
	)
	(wire
		(pts
			(xy 81.28 153.67) (xy 82.55 153.67)
		)
	)
	(bus
		(pts
			(xy 25.4 123.19) (xy 118.11 123.19)
		)
	)
	(bus
		(pts
			(xy 327.66 209.55) (xy 327.66 212.09)
		)
	)
	(wire
		(pts
			(xy 78.74 95.25) (xy 96.52 95.25)
		)
	)
	(wire
		(pts
			(xy 194.31 205.74) (xy 195.58 205.74)
		)
	)
	(wire
		(pts
			(xy 39.37 185.42) (xy 39.37 191.77)
		)
	)
	(bus
		(pts
			(xy 375.92 66.04) (xy 383.54 66.04)
		)
	)
	(bus
		(pts
			(xy 383.54 24.13) (xy 383.54 44.45)
		)
	)
	(bus
		(pts
			(xy 25.4 85.09) (xy 25.4 123.19)
		)
	)
	(bus
		(pts
			(xy 326.39 144.78) (xy 326.39 135.89)
		)
	)
	(wire
		(pts
			(xy 257.81 73.66) (xy 279.4 73.66)
		)
	)
	(wire
		(pts
			(xy 200.66 256.54) (xy 200.66 255.27)
		)
	)
	(wire
		(pts
			(xy 194.31 190.5) (xy 213.36 190.5)
		)
	)
	(wire
		(pts
			(xy 127 257.81) (xy 134.62 257.81)
		)
	)
	(bus
		(pts
			(xy 327.66 204.47) (xy 327.66 207.01)
		)
	)
	(wire
		(pts
			(xy 168.91 147.32) (xy 166.37 147.32)
		)
	)
	(wire
		(pts
			(xy 166.37 147.32) (xy 166.37 144.78)
		)
	)
	(wire
		(pts
			(xy 82.55 90.17) (xy 91.44 90.17)
		)
	)
	(wire
		(pts
			(xy 308.61 204.47) (xy 325.12 204.47)
		)
	)
	(wire
		(pts
			(xy 165.1 245.11) (xy 181.61 245.11)
		)
	)
	(wire
		(pts
			(xy 382.27 226.06) (xy 386.08 226.06)
		)
	)
	(wire
		(pts
			(xy 110.49 252.73) (xy 110.49 281.94)
		)
	)
	(wire
		(pts
			(xy 238.76 243.84) (xy 255.27 243.84)
		)
	)
	(wire
		(pts
			(xy 246.38 157.48) (xy 246.38 219.71)
		)
	)
	(wire
		(pts
			(xy 115.57 247.65) (xy 134.62 247.65)
		)
	)
	(wire
		(pts
			(xy 238.76 238.76) (xy 255.27 238.76)
		)
	)
	(wire
		(pts
			(xy 307.34 162.56) (xy 326.39 162.56)
		)
	)
	(wire
		(pts
			(xy 194.31 157.48) (xy 212.09 157.48)
		)
	)
	(wire
		(pts
			(xy 196.85 170.18) (xy 196.85 172.72)
		)
	)
	(wire
		(pts
			(xy 115.57 240.03) (xy 134.62 240.03)
		)
	)
	(wire
		(pts
			(xy 31.75 53.34) (xy 31.75 54.61)
		)
	)
	(wire
		(pts
			(xy 165.1 260.35) (xy 168.91 260.35)
		)
	)
	(wire
		(pts
			(xy 168.91 257.81) (xy 168.91 260.35)
		)
	)
	(wire
		(pts
			(xy 308.61 214.63) (xy 325.12 214.63)
		)
	)
	(wire
		(pts
			(xy 133.35 198.12) (xy 132.08 198.12)
		)
	)
	(wire
		(pts
			(xy 151.13 162.56) (xy 168.91 162.56)
		)
	)
	(wire
		(pts
			(xy 332.74 152.4) (xy 351.79 152.4)
		)
	)
	(wire
		(pts
			(xy 92.71 232.41) (xy 113.03 232.41)
		)
	)
	(bus
		(pts
			(xy 401.32 200.66) (xy 401.32 198.12)
		)
	)
	(bus
		(pts
			(xy 401.32 189.23) (xy 401.32 195.58)
		)
	)
	(wire
		(pts
			(xy 127 259.08) (xy 127 257.81)
		)
	)
	(bus
		(pts
			(xy 257.81 241.3) (xy 257.81 243.84)
		)
	)
	(wire
		(pts
			(xy 38.1 156.21) (xy 38.1 157.48)
		)
	)
	(wire
		(pts
			(xy 213.36 102.87) (xy 234.95 102.87)
		)
	)
	(bus
		(pts
			(xy 401.32 154.94) (xy 401.32 152.4)
		)
	)
	(wire
		(pts
			(xy 382.27 144.78) (xy 398.78 144.78)
		)
	)
	(wire
		(pts
			(xy 31.75 29.21) (xy 31.75 33.02)
		)
	)
	(wire
		(pts
			(xy 27.94 185.42) (xy 39.37 185.42)
		)
	)
	(wire
		(pts
			(xy 257.81 142.24) (xy 276.86 142.24)
		)
	)
	(wire
		(pts
			(xy 344.17 170.18) (xy 344.17 167.64)
		)
	)
	(bus
		(pts
			(xy 184.15 242.57) (xy 184.15 245.11)
		)
	)
	(wire
		(pts
			(xy 213.36 105.41) (xy 234.95 105.41)
		)
	)
	(wire
		(pts
			(xy 257.81 76.2) (xy 279.4 76.2)
		)
	)
	(wire
		(pts
			(xy 332.74 198.12) (xy 351.79 198.12)
		)
	)
	(wire
		(pts
			(xy 30.48 156.21) (xy 30.48 157.48)
		)
	)
	(bus
		(pts
			(xy 327.66 189.23) (xy 401.32 189.23)
		)
	)
	(bus
		(pts
			(xy 184.15 226.06) (xy 184.15 229.87)
		)
	)
	(wire
		(pts
			(xy 307.34 147.32) (xy 323.85 147.32)
		)
	)
	(wire
		(pts
			(xy 242.57 259.08) (xy 242.57 266.7)
		)
	)
	(bus
		(pts
			(xy 180.34 226.06) (xy 184.15 226.06)
		)
	)
	(wire
		(pts
			(xy 48.26 87.63) (xy 46.99 87.63)
		)
	)
	(wire
		(pts
			(xy 54.61 257.81) (xy 62.23 257.81)
		)
	)
	(bus
		(pts
			(xy 401.32 208.28) (xy 401.32 210.82)
		)
	)
	(wire
		(pts
			(xy 189.23 233.68) (xy 208.28 233.68)
		)
	)
	(wire
		(pts
			(xy 166.37 149.86) (xy 166.37 152.4)
		)
	)
	(wire
		(pts
			(xy 213.36 130.81) (xy 234.95 130.81)
		)
	)
	(bus
		(pts
			(xy 327.66 207.01) (xy 327.66 209.55)
		)
	)
	(wire
		(pts
			(xy 27.94 135.89) (xy 38.1 135.89)
		)
	)
	(wire
		(pts
			(xy 60.96 232.41) (xy 62.23 232.41)
		)
	)
	(wire
		(pts
			(xy 46.99 48.26) (xy 48.26 48.26)
		)
	)
	(wire
		(pts
			(xy 115.57 234.95) (xy 134.62 234.95)
		)
	)
	(wire
		(pts
			(xy 238.76 231.14) (xy 255.27 231.14)
		)
	)
	(bus
		(pts
			(xy 172.72 40.64) (xy 198.12 40.64)
		)
	)
	(wire
		(pts
			(xy 41.91 234.95) (xy 62.23 234.95)
		)
	)
	(wire
		(pts
			(xy 46.99 87.63) (xy 46.99 97.79)
		)
	)
	(wire
		(pts
			(xy 311.15 167.64) (xy 311.15 170.18)
		)
	)
	(wire
		(pts
			(xy 52.07 153.67) (xy 55.88 153.67)
		)
	)
	(wire
		(pts
			(xy 238.76 246.38) (xy 255.27 246.38)
		)
	)
	(wire
		(pts
			(xy 76.2 95.25) (xy 78.74 95.25)
		)
	)
	(wire
		(pts
			(xy 60.96 222.25) (xy 60.96 220.98)
		)
	)
	(bus
		(pts
			(xy 401.32 200.66) (xy 401.32 203.2)
		)
	)
	(wire
		(pts
			(xy 81.28 187.96) (xy 100.33 187.96)
		)
	)
	(bus
		(pts
			(xy 326.39 135.89) (xy 401.32 135.89)
		)
	)
	(wire
		(pts
			(xy 308.61 199.39) (xy 325.12 199.39)
		)
	)
	(wire
		(pts
			(xy 165.1 252.73) (xy 186.69 252.73)
		)
	)
	(wire
		(pts
			(xy 332.74 144.78) (xy 351.79 144.78)
		)
	)
	(wire
		(pts
			(xy 165.1 257.81) (xy 168.91 257.81)
		)
	)
	(bus
		(pts
			(xy 25.4 123.19) (xy 25.4 133.35)
		)
	)
	(wire
		(pts
			(xy 307.34 142.24) (xy 323.85 142.24)
		)
	)
	(bus
		(pts
			(xy 401.32 152.4) (xy 401.32 149.86)
		)
	)
	(wire
		(pts
			(xy 200.66 256.54) (xy 208.28 256.54)
		)
	)
	(wire
		(pts
			(xy 27.94 87.63) (xy 46.99 87.63)
		)
	)
	(bus
		(pts
			(xy 383.54 66.04) (xy 383.54 88.9)
		)
	)
	(wire
		(pts
			(xy 30.48 242.57) (xy 34.29 242.57)
		)
	)
	(bus
		(pts
			(xy 184.15 240.03) (xy 184.15 242.57)
		)
	)
	(bus
		(pts
			(xy 401.32 210.82) (xy 401.32 213.36)
		)
	)
	(wire
		(pts
			(xy 213.36 107.95) (xy 234.95 107.95)
		)
	)
	(bus
		(pts
			(xy 184.15 226.06) (xy 257.81 226.06)
		)
	)
	(bus
		(pts
			(xy 184.15 245.11) (xy 184.15 247.65)
		)
	)
	(bus
		(pts
			(xy 257.81 238.76) (xy 257.81 241.3)
		)
	)
	(wire
		(pts
			(xy 386.08 223.52) (xy 386.08 226.06)
		)
	)
	(wire
		(pts
			(xy 83.82 39.37) (xy 83.82 40.64)
		)
	)
	(wire
		(pts
			(xy 382.27 210.82) (xy 398.78 210.82)
		)
	)
	(wire
		(pts
			(xy 165.1 237.49) (xy 181.61 237.49)
		)
	)
	(wire
		(pts
			(xy 189.23 246.38) (xy 189.23 278.13)
		)
	)
	(wire
		(pts
			(xy 110.49 281.94) (xy 262.89 281.94)
		)
	)
	(wire
		(pts
			(xy 269.24 167.64) (xy 269.24 165.1)
		)
	)
	(wire
		(pts
			(xy 92.71 260.35) (xy 96.52 260.35)
		)
	)
	(bus
		(pts
			(xy 401.32 198.12) (xy 401.32 195.58)
		)
	)
	(wire
		(pts
			(xy 92.71 250.19) (xy 113.03 250.19)
		)
	)
	(bus
		(pts
			(xy 335.28 44.45) (xy 335.28 66.04)
		)
	)
	(wire
		(pts
			(xy 246.38 157.48) (xy 276.86 157.48)
		)
	)
	(wire
		(pts
			(xy 194.31 162.56) (xy 212.09 162.56)
		)
	)
	(bus
		(pts
			(xy 25.4 133.35) (xy 25.4 143.51)
		)
	)
	(wire
		(pts
			(xy 30.48 146.05) (xy 30.48 148.59)
		)
	)
	(wire
		(pts
			(xy 27.94 33.02) (xy 31.75 33.02)
		)
	)
	(wire
		(pts
			(xy 96.52 257.81) (xy 96.52 260.35)
		)
	)
	(wire
		(pts
			(xy 81.28 138.43) (xy 100.33 138.43)
		)
	)
	(wire
		(pts
			(xy 48.26 153.67) (xy 52.07 153.67)
		)
	)
	(wire
		(pts
			(xy 82.55 81.28) (xy 82.55 80.01)
		)
	)
	(wire
		(pts
			(xy 259.08 209.55) (xy 278.13 209.55)
		)
	)
	(bus
		(pts
			(xy 326.39 147.32) (xy 326.39 144.78)
		)
	)
	(wire
		(pts
			(xy 31.75 78.74) (xy 31.75 82.55)
		)
	)
	(wire
		(pts
			(xy 382.27 149.86) (xy 398.78 149.86)
		)
	)
	(bus
		(pts
			(xy 335.28 44.45) (xy 341.63 44.45)
		)
	)
	(wire
		(pts
			(xy 257.81 149.86) (xy 276.86 149.86)
		)
	)
	(bus
		(pts
			(xy 383.54 44.45) (xy 383.54 66.04)
		)
	)
	(wire
		(pts
			(xy 311.15 170.18) (xy 311.15 177.8)
		)
	)
	(wire
		(pts
			(xy 92.71 252.73) (xy 110.49 252.73)
		)
	)
	(wire
		(pts
			(xy 308.61 212.09) (xy 325.12 212.09)
		)
	)
	(wire
		(pts
			(xy 262.89 281.94) (xy 262.89 219.71)
		)
	)
	(wire
		(pts
			(xy 382.27 198.12) (xy 398.78 198.12)
		)
	)
	(wire
		(pts
			(xy 167.64 170.18) (xy 168.91 170.18)
		)
	)
	(wire
		(pts
			(xy 30.48 240.03) (xy 54.61 240.03)
		)
	)
	(wire
		(pts
			(xy 80.01 45.72) (xy 96.52 45.72)
		)
	)
	(bus
		(pts
			(xy 184.15 234.95) (xy 184.15 237.49)
		)
	)
	(wire
		(pts
			(xy 39.37 199.39) (xy 39.37 200.66)
		)
	)
	(bus
		(pts
			(xy 190.5 24.13) (xy 383.54 24.13)
		)
	)
	(wire
		(pts
			(xy 165.1 240.03) (xy 181.61 240.03)
		)
	)
	(wire
		(pts
			(xy 382.27 200.66) (xy 398.78 200.66)
		)
	)
	(wire
		(pts
			(xy 41.91 242.57) (xy 62.23 242.57)
		)
	)
	(wire
		(pts
			(xy 115.57 232.41) (xy 134.62 232.41)
		)
	)
	(wire
		(pts
			(xy 344.17 223.52) (xy 351.79 223.52)
		)
	)
	(wire
		(pts
			(xy 109.22 218.44) (xy 113.03 218.44)
		)
	)
	(wire
		(pts
			(xy 27.94 175.26) (xy 31.75 175.26)
		)
	)
	(wire
		(pts
			(xy 382.27 205.74) (xy 398.78 205.74)
		)
	)
	(bus
		(pts
			(xy 335.28 66.04) (xy 341.63 66.04)
		)
	)
	(wire
		(pts
			(xy 238.76 241.3) (xy 255.27 241.3)
		)
	)
	(wire
		(pts
			(xy 242.57 256.54) (xy 242.57 259.08)
		)
	)
	(wire
		(pts
			(xy 78.74 80.01) (xy 78.74 95.25)
		)
	)
	(wire
		(pts
			(xy 76.2 45.72) (xy 80.01 45.72)
		)
	)
	(wire
		(pts
			(xy 386.08 170.18) (xy 386.08 172.72)
		)
	)
	(wire
		(pts
			(xy 238.76 236.22) (xy 255.27 236.22)
		)
	)
	(wire
		(pts
			(xy 308.61 207.01) (xy 325.12 207.01)
		)
	)
	(bus
		(pts
			(xy 401.32 189.23) (xy 401.32 165.1)
		)
	)
	(wire
		(pts
			(xy 166.37 149.86) (xy 168.91 149.86)
		)
	)
	(bus
		(pts
			(xy 25.4 35.56) (xy 25.4 85.09)
		)
	)
	(wire
		(pts
			(xy 31.75 92.71) (xy 48.26 92.71)
		)
	)
	(wire
		(pts
			(xy 259.08 207.01) (xy 278.13 207.01)
		)
	)
	(wire
		(pts
			(xy 332.74 147.32) (xy 351.79 147.32)
		)
	)
	(wire
		(pts
			(xy 27.94 38.1) (xy 46.99 38.1)
		)
	)
	(wire
		(pts
			(xy 46.99 97.79) (xy 48.26 97.79)
		)
	)
	(wire
		(pts
			(xy 76.2 90.17) (xy 82.55 90.17)
		)
	)
	(wire
		(pts
			(xy 257.81 144.78) (xy 276.86 144.78)
		)
	)
	(wire
		(pts
			(xy 30.48 146.05) (xy 55.88 146.05)
		)
	)
	(wire
		(pts
			(xy 382.27 160.02) (xy 398.78 160.02)
		)
	)
	(wire
		(pts
			(xy 81.28 148.59) (xy 100.33 148.59)
		)
	)
	(wire
		(pts
			(xy 344.17 223.52) (xy 344.17 220.98)
		)
	)
	(wire
		(pts
			(xy 257.81 87.63) (xy 279.4 87.63)
		)
	)
	(wire
		(pts
			(xy 96.52 45.72) (xy 105.41 45.72)
		)
	)
	(wire
		(pts
			(xy 238.76 233.68) (xy 255.27 233.68)
		)
	)
	(wire
		(pts
			(xy 189.23 246.38) (xy 208.28 246.38)
		)
	)
	(wire
		(pts
			(xy 92.71 242.57) (xy 113.03 242.57)
		)
	)
	(bus
		(pts
			(xy 120.65 118.11) (xy 143.51 118.11)
		)
	)
	(bus
		(pts
			(xy 327.66 212.09) (xy 327.66 214.63)
		)
	)
	(wire
		(pts
			(xy 31.75 95.25) (xy 31.75 92.71)
		)
	)
	(bus
		(pts
			(xy 401.32 205.74) (xy 401.32 208.28)
		)
	)
	(wire
		(pts
			(xy 38.1 135.89) (xy 38.1 148.59)
		)
	)
	(wire
		(pts
			(xy 308.61 217.17) (xy 325.12 217.17)
		)
	)
	(wire
		(pts
			(xy 194.31 170.18) (xy 196.85 170.18)
		)
	)
	(bus
		(pts
			(xy 257.81 231.14) (xy 257.81 233.68)
		)
	)
	(wire
		(pts
			(xy 48.26 38.1) (xy 46.99 38.1)
		)
	)
	(wire
		(pts
			(xy 308.61 224.79) (xy 312.42 224.79)
		)
	)
	(wire
		(pts
			(xy 165.1 250.19) (xy 181.61 250.19)
		)
	)
	(wire
		(pts
			(xy 194.31 200.66) (xy 213.36 200.66)
		)
	)
	(wire
		(pts
			(xy 46.99 38.1) (xy 46.99 48.26)
		)
	)
	(wire
		(pts
			(xy 115.57 278.13) (xy 115.57 247.65)
		)
	)
	(bus
		(pts
			(xy 401.32 165.1) (xy 401.32 162.56)
		)
	)
	(wire
		(pts
			(xy 76.2 40.64) (xy 83.82 40.64)
		)
	)
	(bus
		(pts
			(xy 257.81 228.6) (xy 257.81 231.14)
		)
	)
	(wire
		(pts
			(xy 332.74 154.94) (xy 351.79 154.94)
		)
	)
	(wire
		(pts
			(xy 257.81 90.17) (xy 279.4 90.17)
		)
	)
	(wire
		(pts
			(xy 96.52 45.72) (xy 96.52 48.26)
		)
	)
	(wire
		(pts
			(xy 166.37 144.78) (xy 168.91 144.78)
		)
	)
	(wire
		(pts
			(xy 382.27 203.2) (xy 398.78 203.2)
		)
	)
	(wire
		(pts
			(xy 332.74 205.74) (xy 351.79 205.74)
		)
	)
	(wire
		(pts
			(xy 151.13 160.02) (xy 168.91 160.02)
		)
	)
	(wire
		(pts
			(xy 259.08 214.63) (xy 278.13 214.63)
		)
	)
	(wire
		(pts
			(xy 213.36 113.03) (xy 234.95 113.03)
		)
	)
	(wire
		(pts
			(xy 165.1 232.41) (xy 181.61 232.41)
		)
	)
	(wire
		(pts
			(xy 307.34 149.86) (xy 323.85 149.86)
		)
	)
	(bus
		(pts
			(xy 241.3 44.45) (xy 279.4 44.45)
		)
	)
	(wire
		(pts
			(xy 165.1 247.65) (xy 181.61 247.65)
		)
	)
	(wire
		(pts
			(xy 31.75 71.12) (xy 31.75 69.85)
		)
	)
	(bus
		(pts
			(xy 184.15 232.41) (xy 184.15 234.95)
		)
	)
	(wire
		(pts
			(xy 308.61 227.33) (xy 312.42 227.33)
		)
	)
	(wire
		(pts
			(xy 115.57 242.57) (xy 134.62 242.57)
		)
	)
	(wire
		(pts
			(xy 54.61 259.08) (xy 54.61 257.81)
		)
	)
	(wire
		(pts
			(xy 54.61 257.81) (xy 54.61 256.54)
		)
	)
	(wire
		(pts
			(xy 165.1 205.74) (xy 168.91 205.74)
		)
	)
	(wire
		(pts
			(xy 165.1 242.57) (xy 181.61 242.57)
		)
	)
	(wire
		(pts
			(xy 140.97 187.96) (xy 168.91 187.96)
		)
	)
	(bus
		(pts
			(xy 401.32 160.02) (xy 401.32 157.48)
		)
	)
	(wire
		(pts
			(xy 312.42 224.79) (xy 312.42 227.33)
		)
	)
	(wire
		(pts
			(xy 195.58 209.55) (xy 195.58 205.74)
		)
	)
	(wire
		(pts
			(xy 382.27 215.9) (xy 398.78 215.9)
		)
	)
	(wire
		(pts
			(xy 184.15 278.13) (xy 189.23 278.13)
		)
	)
	(wire
		(pts
			(xy 166.37 152.4) (xy 168.91 152.4)
		)
	)
	(wire
		(pts
			(xy 308.61 201.93) (xy 325.12 201.93)
		)
	)
	(wire
		(pts
			(xy 200.66 257.81) (xy 200.66 256.54)
		)
	)
	(wire
		(pts
			(xy 308.61 209.55) (xy 325.12 209.55)
		)
	)
	(wire
		(pts
			(xy 31.75 45.72) (xy 31.75 43.18)
		)
	)
	(bus
		(pts
			(xy 25.4 172.72) (xy 25.4 182.88)
		)
	)
	(wire
		(pts
			(xy 30.48 232.41) (xy 60.96 232.41)
		)
	)
	(wire
		(pts
			(xy 382.27 147.32) (xy 398.78 147.32)
		)
	)
	(wire
		(pts
			(xy 82.55 80.01) (xy 78.74 80.01)
		)
	)
	(bus
		(pts
			(xy 184.15 237.49) (xy 184.15 240.03)
		)
	)
	(wire
		(pts
			(xy 194.31 165.1) (xy 212.09 165.1)
		)
	)
	(wire
		(pts
			(xy 91.44 90.17) (xy 91.44 97.79)
		)
	)
	(wire
		(pts
			(xy 27.94 146.05) (xy 30.48 146.05)
		)
	)
	(wire
		(pts
			(xy 30.48 247.65) (xy 34.29 247.65)
		)
	)
	(wire
		(pts
			(xy 194.31 185.42) (xy 213.36 185.42)
		)
	)
	(wire
		(pts
			(xy 161.29 205.74) (xy 165.1 205.74)
		)
	)
	(bus
		(pts
			(xy 327.66 189.23) (xy 327.66 196.85)
		)
	)
	(wire
		(pts
			(xy 344.17 170.18) (xy 351.79 170.18)
		)
	)
	(bus
		(pts
			(xy 172.72 24.13) (xy 190.5 24.13)
		)
	)
	(wire
		(pts
			(xy 96.52 95.25) (xy 96.52 97.79)
		)
	)
	(wire
		(pts
			(xy 96.52 260.35) (xy 96.52 267.97)
		)
	)
	(wire
		(pts
			(xy 81.28 172.72) (xy 100.33 172.72)
		)
	)
	(wire
		(pts
			(xy 326.39 162.56) (xy 326.39 160.02)
		)
	)
	(wire
		(pts
			(xy 38.1 135.89) (xy 55.88 135.89)
		)
	)
	(bus
		(pts
			(xy 326.39 149.86) (xy 326.39 147.32)
		)
	)
	(wire
		(pts
			(xy 165.1 234.95) (xy 181.61 234.95)
		)
	)
	(wire
		(pts
			(xy 147.32 144.78) (xy 146.05 144.78)
		)
	)
	(wire
		(pts
			(xy 238.76 251.46) (xy 257.81 251.46)
		)
	)
	(wire
		(pts
			(xy 54.61 240.03) (xy 62.23 240.03)
		)
	)
	(wire
		(pts
			(xy 382.27 152.4) (xy 398.78 152.4)
		)
	)
	(bus
		(pts
			(xy 335.28 66.04) (xy 335.28 88.9)
		)
	)
	(wire
		(pts
			(xy 81.28 193.04) (xy 82.55 193.04)
		)
	)
	(wire
		(pts
			(xy 257.81 78.74) (xy 279.4 78.74)
		)
	)
	(wire
		(pts
			(xy 194.31 195.58) (xy 213.36 195.58)
		)
	)
	(wire
		(pts
			(xy 52.07 193.04) (xy 55.88 193.04)
		)
	)
	(wire
		(pts
			(xy 257.81 152.4) (xy 276.86 152.4)
		)
	)
	(wire
		(pts
			(xy 344.17 224.79) (xy 344.17 223.52)
		)
	)
	(wire
		(pts
			(xy 80.01 30.48) (xy 80.01 45.72)
		)
	)
	(wire
		(pts
			(xy 41.91 247.65) (xy 62.23 247.65)
		)
	)
	(wire
		(pts
			(xy 81.28 143.51) (xy 100.33 143.51)
		)
	)
	(wire
		(pts
			(xy 312.42 227.33) (xy 312.42 234.95)
		)
	)
	(wire
		(pts
			(xy 31.75 82.55) (xy 48.26 82.55)
		)
	)
	(wire
		(pts
			(xy 193.04 68.58) (xy 217.17 68.58)
		)
	)
	(wire
		(pts
			(xy 326.39 160.02) (xy 351.79 160.02)
		)
	)
	(bus
		(pts
			(xy 401.32 149.86) (xy 401.32 147.32)
		)
	)
	(wire
		(pts
			(xy 31.75 43.18) (xy 48.26 43.18)
		)
	)
	(wire
		(pts
			(xy 194.31 160.02) (xy 212.09 160.02)
		)
	)
	(wire
		(pts
			(xy 83.82 30.48) (xy 80.01 30.48)
		)
	)
	(bus
		(pts
			(xy 401.32 147.32) (xy 401.32 135.89)
		)
	)
	(wire
		(pts
			(xy 270.51 224.79) (xy 270.51 223.52)
		)
	)
	(bus
		(pts
			(xy 401.32 162.56) (xy 401.32 160.02)
		)
	)
	(wire
		(pts
			(xy 213.36 133.35) (xy 234.95 133.35)
		)
	)
	(wire
		(pts
			(xy 257.81 71.12) (xy 279.4 71.12)
		)
	)
	(bus
		(pts
			(xy 401.32 203.2) (xy 401.32 205.74)
		)
	)
	(wire
		(pts
			(xy 120.65 223.52) (xy 142.24 223.52)
		)
	)
	(wire
		(pts
			(xy 332.74 200.66) (xy 351.79 200.66)
		)
	)
	(wire
		(pts
			(xy 189.23 231.14) (xy 208.28 231.14)
		)
	)
	(wire
		(pts
			(xy 83.82 31.75) (xy 83.82 30.48)
		)
	)
	(wire
		(pts
			(xy 269.24 167.64) (xy 276.86 167.64)
		)
	)
	(wire
		(pts
			(xy 382.27 157.48) (xy 398.78 157.48)
		)
	)
	(label "F_HWBYTE.H2_4"
		(at 166.37 242.57 0)
	)
	(label "I_HWBYTE2_RCLK"
		(at 260.35 201.93 0)
	)
	(label "F_HWBYTE.H1_2"
		(at 240.03 236.22 0)
	)
	(label "I_HWBYTE1_Q"
		(at 240.03 251.46 0)
	)
	(label "IOEXP_OE_N"
		(at 190.5 231.14 0)
	)
	(label "IOEXP_RST_N"
		(at 334.01 205.74 0)
	)
	(label "VMEF.SYSCLK_DIR"
		(at 93.98 247.65 0)
	)
	(label "IOEXP_OE_N"
		(at 116.84 232.41 0)
	)
	(label "RS485_DATA0_DE"
		(at 93.98 240.03 0)
	)
	(label "TTL_TURNCLK1"
		(at 196.85 157.48 0)
	)
	(label "TTC_DATA1_P"
		(at 259.08 76.2 0)
	)
	(label "LVDS_BUNCHCLK1_N"
		(at 198.12 190.5 0)
	)
	(label "P0_OE_N"
		(at 157.48 144.78 0)
	)
	(label "USERIO_A.DIR0"
		(at 308.61 142.24 0)
	)
	(label "TTL_TURNCLK1"
		(at 213.36 113.03 0)
	)
	(label "TTC_DATA0_N"
		(at 83.82 177.8 0)
	)
	(label "F_HWBYTE.L1_5"
		(at 383.54 210.82 0)
	)
	(label "P0_OE_N"
		(at 93.98 242.57 0)
	)
	(label "F_P0.TURNCLK2"
		(at 39.37 146.05 0)
	)
	(label "F_HWBYTE.H2_1"
		(at 166.37 234.95 0)
	)
	(label "LVDS_TURNCLK2_P"
		(at 82.55 143.51 0)
	)
	(label "F_HWBYTE.H1_3"
		(at 240.03 238.76 0)
	)
	(label "LVDS_BUNCHCLK1_N"
		(at 213.36 125.73 0)
	)
	(label "F_P0.BUNCHCLK2"
		(at 151.13 165.1 0)
	)
	(label "I_HWBYTE1_RCLK"
		(at 127 218.44 0)
	)
	(label "TTL_BUNCHCLK1"
		(at 196.85 162.56 0)
	)
	(label "TTL_TURNCLK2"
		(at 196.85 160.02 0)
	)
	(label "RS485_DATA1_N"
		(at 95.25 45.72 0)
	)
	(label "F_HWBYTE.H1_OE_N"
		(at 383.54 157.48 0)
	)
	(label "TTC_DATA1_P"
		(at 83.82 182.88 0)
	)
	(label "F_HWBYTE.H1_0"
		(at 240.03 231.14 0)
	)
	(label "RS485_DATA1_RE_N"
		(at 93.98 232.41 0)
	)
	(label "LVDS_TURNCLK2_P"
		(at 213.36 107.95 0)
	)
	(label "F_HWBYTE.L1_6"
		(at 383.54 213.36 0)
	)
	(label "LVDS_TURNCLK1_N"
		(at 213.36 105.41 0)
	)
	(label "F_P0.TURNCLK1"
		(at 151.13 157.48 0)
	)
	(label "I_IOEXP_RCLK"
		(at 46.99 234.95 0)
	)
	(label "I_IOEXP_SCLK"
		(at 46.99 242.57 0)
	)
	(label "F_HWBYTE.H2_OE_N"
		(at 383.54 162.56 0)
	)
	(label "TTC_DATA1_N"
		(at 259.08 78.74 0)
	)
	(label "F_HWBYTE.H1_7"
		(at 240.03 248.92 0)
	)
	(label "F_HWBYTE.H1_6"
		(at 240.03 246.38 0)
	)
	(label "I_IOEXP_RCLK"
		(at 334.01 147.32 0)
	)
	(label "RS485_DATA0_P"
		(at 259.08 87.63 0)
	)
	(label "I_IOEXP_SCLK"
		(at 259.08 152.4 0)
	)
	(label "IOEXP_OE_N"
		(at 334.01 144.78 0)
	)
	(label "I_HWBYTE2_Q"
		(at 166.37 252.73 0)
	)
	(label "{VMEPX_USERIO_A}"
		(at 243.84 44.45 0)
	)
	(label "F_HWBYTE.H1_5"
		(at 240.03 243.84 0)
	)
	(label "RS485_DATA0_RE_N"
		(at 93.98 237.49 0)
	)
	(label "I_HWBYTE1_D"
		(at 190.5 246.38 0)
	)
	(label "F_P0.BUNCHCLK1"
		(at 142.24 187.96 0)
	)
	(label "USERIO_A.OE_N1"
		(at 383.54 147.32 0)
	)
	(label "IOEXP_OE_N"
		(at 260.35 199.39 0)
	)
	(label "F_HWBYTE.L1_3"
		(at 383.54 205.74 0)
	)
	(label "F_HWBYTE.H2_3"
		(at 166.37 240.03 0)
	)
	(label "I_IOEXP_SCLK"
		(at 190.5 241.3 0)
	)
	(label "RS485_DATA0_N"
		(at 95.25 95.25 0)
	)
	(label "IOEXP_RST_N"
		(at 116.84 240.03 0)
	)
	(label "LVDS_TURNCLK1_P"
		(at 82.55 133.35 0)
	)
	(label "I_IOEXP_SCLK"
		(at 116.84 242.57 0)
	)
	(label "LVDS_BUNCHCLK2_P"
		(at 213.36 128.27 0)
	)
	(label "F_HWBYTE.L1_1"
		(at 383.54 200.66 0)
	)
	(label "F_HWBYTE.L2_4"
		(at 309.88 209.55 0)
	)
	(label "TTL_BUNCHCLK2"
		(at 196.85 165.1 0)
	)
	(label "F_HWBYTE.L2_0"
		(at 309.88 199.39 0)
	)
	(label "I_HWBYTE2_Q"
		(at 262.89 214.63 0)
	)
	(label "RS485_DATA0_P"
		(at 95.25 90.17 0)
	)
	(label "RS485_DATA1_DE"
		(at 93.98 234.95 0)
	)
	(label "F_HWBYTE.L1_7"
		(at 383.54 215.9 0)
	)
	(label "F_HWBYTE.H2_5"
		(at 166.37 245.11 0)
	)
	(label "LVDS_BUNCHCLK2_N"
		(at 213.36 130.81 0)
	)
	(label "F_HWBYTE.L2_OE_N"
		(at 383.54 160.02 0)
	)
	(label "TTC_DATA0_N"
		(at 259.08 73.66 0)
	)
	(label "IOEXP_OE_N"
		(at 259.08 142.24 0)
	)
	(label "{F_P0}"
		(at 120.65 92.71 0)
	)
	(label "I_HWBYTE1_RCLK"
		(at 190.5 233.68 0)
	)
	(label "{USERIO_A}"
		(at 342.9 135.89 0)
	)
	(label "LVDS_TURNCLK1_N"
		(at 82.55 138.43 0)
	)
	(label "IOEXP_OE_N"
		(at 334.01 198.12 0)
	)
	(label "I_IOEXP_SCLK"
		(at 260.35 209.55 0)
	)
	(label "F_P0.RS485_DATA1"
		(at 27.94 38.1 0)
	)
	(label "TTL_BUNCHCLK2"
		(at 213.36 135.89 0)
	)
	(label "I_HWBYTE2_RCLK"
		(at 127 223.52 0)
	)
	(label "I_IOEXP_RCLK"
		(at 259.08 144.78 0)
	)
	(label "F_HWBYTE.L2_6"
		(at 309.88 214.63 0)
	)
	(label "F_P0.TTC_DATA1"
		(at 43.18 185.42 0)
	)
	(label "F_HWBYTE.L1_OE_N"
		(at 383.54 154.94 0)
	)
	(label "{F_HWBYTE}"
		(at 186.69 226.06 0)
	)
	(label "VMEF.SYSRESET_N_DIR"
		(at 198.12 68.58 0)
	)
	(label "F_HWBYTE.L1_0"
		(at 383.54 198.12 0)
	)
	(label "TTC_DATA0_P"
		(at 259.08 71.12 0)
	)
	(label "USERIO_A.OE_N2"
		(at 383.54 149.86 0)
	)
	(label "LVDS_TURNCLK1_P"
		(at 213.36 102.87 0)
	)
	(label "RS485_DATA0_DE"
		(at 27.94 92.71 0)
	)
	(label "F_HWBYTE.H2_6"
		(at 166.37 247.65 0)
	)
	(label "VMEF.SYSRESET_N_DIR"
		(at 93.98 250.19 0)
	)
	(label "F_HWBYTE.L2_7"
		(at 309.88 217.17 0)
	)
	(label "F_P0.TURNCLK2"
		(at 151.13 160.02 0)
	)
	(label "F_HWBYTE.H2_2"
		(at 166.37 237.49 0)
	)
	(label "LVDS_BUNCHCLK1_P"
		(at 198.12 185.42 0)
	)
	(label "IOEXP_RST_N"
		(at 334.01 152.4 0)
	)
	(label "F_HWBYTE.H1_1"
		(at 240.03 233.68 0)
	)
	(label "F_P0.TURNCLK1"
		(at 39.37 135.89 0)
	)
	(label "F_P0.BUNCHCLK1"
		(at 151.13 162.56 0)
	)
	(label "F_HWBYTE.H2_0"
		(at 166.37 232.41 0)
	)
	(label "{USERIO_A}"
		(at 175.26 40.64 0)
	)
	(label "F_HWBYTE.L2_2"
		(at 309.88 204.47 0)
	)
	(label "F_HWBYTE.L1_4"
		(at 383.54 208.28 0)
	)
	(label "I_HWBYTE1_RCLK"
		(at 334.01 200.66 0)
	)
	(label "TTC_DATA0_P"
		(at 83.82 172.72 0)
	)
	(label "F_HWBYTE.L1_2"
		(at 383.54 203.2 0)
	)
	(label "LVDS_BUNCHCLK1_P"
		(at 213.36 123.19 0)
	)
	(label "F_HWBYTE.L2_3"
		(at 309.88 207.01 0)
	)
	(label "RS485_DATA1_RE_N"
		(at 27.94 33.02 0)
	)
	(label "IOEXP_RST_N"
		(at 190.5 238.76 0)
	)
	(label "I_HWBYTE2_RCLK"
		(at 116.84 234.95 0)
	)
	(label "LVDS_BUNCHCLK2_N"
		(at 198.12 200.66 0)
	)
	(label "I_HWBYTE2_D"
		(at 116.84 247.65 0)
	)
	(label "USERIO_A.OE_N3"
		(at 383.54 152.4 0)
	)
	(label "USERIO_A.DIR2"
		(at 308.61 147.32 0)
	)
	(label "LVDS_TURNCLK2_N"
		(at 213.36 110.49 0)
	)
	(label "LVDS_BUNCHCLK2_P"
		(at 198.12 195.58 0)
	)
	(label "TTL_BUNCHCLK1"
		(at 213.36 133.35 0)
	)
	(label "USERIO_A.DIR1"
		(at 308.61 144.78 0)
	)
	(label "USERIO_A.OE_N0"
		(at 383.54 144.78 0)
	)
	(label "F_HWBYTE.H2_7"
		(at 166.37 250.19 0)
	)
	(label "IOEXP_RST_N"
		(at 259.08 149.86 0)
	)
	(label "RS485_DATA1_N"
		(at 259.08 85.09 0)
	)
	(label "F_HWBYTE.L2_5"
		(at 309.88 212.09 0)
	)
	(label "F_HWBYTE.L2_1"
		(at 309.88 201.93 0)
	)
	(label "IOEXP_RST_N"
		(at 260.35 207.01 0)
	)
	(label "RS485_DATA1_DE"
		(at 27.94 43.18 0)
	)
	(label "RS485_DATA1_P"
		(at 259.08 82.55 0)
	)
	(label "RS485_DATA0_RE_N"
		(at 27.94 82.55 0)
	)
	(label "F_P0.BUNCHCLK2"
		(at 142.24 198.12 0)
	)
	(label "I_IOEXP_SCLK"
		(at 334.01 208.28 0)
	)
	(label "LVDS_TURNCLK2_N"
		(at 82.55 148.59 0)
	)
	(label "USERIO_A.DIR3"
		(at 308.61 149.86 0)
	)
	(label "TTC_DATA1_N"
		(at 83.82 187.96 0)
	)
	(label "{HWBYTE}"
		(at 205.74 100.33 0)
	)
	(label "F_HWBYTE.H1_4"
		(at 240.03 241.3 0)
	)
	(label "{VMEF}"
		(at 172.72 24.13 0)
	)
	(label "I_HWBYTE1_Q"
		(at 334.01 213.36 0)
	)
	(label "RS485_DATA0_N"
		(at 259.08 90.17 0)
	)
	(label "RS485_DATA1_P"
		(at 95.25 40.64 0)
	)
	(label "I_IOEXP_SCLK"
		(at 334.01 154.94 0)
	)
	(label "F_P0.RS485_DATA0"
		(at 27.94 87.63 0)
	)
	(label "F_P0.TTC_DATA0"
		(at 43.18 175.26 0)
	)
	(label "TTL_TURNCLK2"
		(at 213.36 115.57 0)
	)
	(label "{F_HWBYTE}"
		(at 121.92 118.11 0)
	)
	(hierarchical_label "IOEXP_HWBYTE1_RCLK"
		(shape input)
		(at 109.22 218.44 180)
	)
	(hierarchical_label "IOEXP_RCLK"
		(shape input)
		(at 30.48 234.95 180)
	)
	(hierarchical_label "IOEXP_HWBYTE2_RCLK"
		(shape input)
		(at 109.22 223.52 180)
	)
	(hierarchical_label "IOEXP_SCLK"
		(shape input)
		(at 30.48 242.57 180)
	)
	(hierarchical_label "IOEXP_HWBYTE1_D"
		(shape input)
		(at 172.72 278.13 180)
	)
	(hierarchical_label "IOEXP_OE_N"
		(shape input)
		(at 30.48 232.41 180)
	)
	(hierarchical_label "{F_P0}"
		(shape bidirectional)
		(at 129.54 92.71 0)
	)
	(hierarchical_label "{VMEF}"
		(shape bidirectional)
		(at 172.72 24.13 180)
	)
	(hierarchical_label "IOEXP_HWBYTE2_D"
		(shape input)
		(at 93.98 278.13 180)
	)
	(hierarchical_label "{USERIO_A}"
		(shape bidirectional)
		(at 172.72 40.64 180)
	)
	(hierarchical_label "IOEXP_D"
		(shape input)
		(at 30.48 247.65 180)
	)
	(hierarchical_label "IOEXP_RST_N"
		(shape input)
		(at 30.48 240.03 180)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 127 266.7 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C219"
			(at 130.81 261.6199 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 132.08 261.62 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 127 266.7 0)
		)
		(property "Datasheet" ""
			(at 127 266.7 0)
		)
		(property "Description" "100nF"
			(at 130.81 264.1599 90)
		)
		(property "SMD" "Yes"
			(at 126.492 268.986 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 138.938 266.7 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 140.843 266.7 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 142.748 266.7 0)
		)
		(property "Comment" "100nF"
			(at 144.653 266.7 0)
		)
		(property "Component Kind" "Standard"
			(at 146.558 266.7 0)
		)
		(property "Component Type" "Standard"
			(at 148.463 266.7 0)
		)
		(property "Pin Count" "2"
			(at 150.368 266.7 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 152.273 266.7 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 154.178 266.7 0)
		)
		(property "PackageDescription" " "
			(at 156.083 266.7 0)
		)
		(property "Status" "Not Recommended"
			(at 157.988 266.7 0)
		)
		(property "Status Comment" " "
			(at 159.893 266.7 0)
		)
		(property "Voltage" "16V"
			(at 161.798 266.7 0)
		)
		(property "Tolerance" "±10%"
			(at 165.608 266.7 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 167.513 266.7 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 169.418 266.7 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 171.323 266.7 0)
		)
		(property "Case" "0402"
			(at 173.228 266.7 0)
		)
		(property "Mounted" "Yes"
			(at 175.133 266.7 0)
		)
		(property "Socket" "No"
			(at 177.038 266.7 0)
		)
		(property "PressFit" " "
			(at 180.848 266.7 0)
		)
		(property "Sense" "No"
			(at 182.753 266.7 0)
		)
		(property "Sense Comment" " "
			(at 184.658 266.7 0)
		)
		(property "ComponentHeight" " "
			(at 186.563 266.7 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 188.468 266.7 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 190.373 266.7 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 192.278 266.7 0)
		)
		(property "HelpURL" ""
			(at 194.183 266.7 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 196.088 266.7 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 197.993 266.7 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 199.898 266.7 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 201.803 266.7 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 203.708 266.7 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 205.613 266.7 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 207.518 266.7 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C219")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 31.75 78.74 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R69"
			(at 34.29 73.6599 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 36.703 78.74 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 38.608 78.74 0)
		)
		(property "Datasheet" ""
			(at 40.513 78.74 0)
		)
		(property "Description" "±1%"
			(at 26.67 74.93 0)
		)
		(property "Val" "10k"
			(at 34.29 76.1999 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 42.418 78.74 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 44.323 78.74 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 46.228 78.74 0)
		)
		(property "Comment" "10k"
			(at 48.133 78.74 0)
		)
		(property "Component Kind" "Standard"
			(at 50.038 78.74 0)
		)
		(property "Component Type" "Standard"
			(at 51.943 78.74 0)
		)
		(property "PackageDescription" " "
			(at 53.848 78.74 0)
		)
		(property "Pin Count" "2"
			(at 55.753 78.74 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 57.658 78.74 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 59.563 78.74 0)
		)
		(property "Status" "Not Recommended"
			(at 61.468 78.74 0)
		)
		(property "Power" "0.0625W"
			(at 63.373 78.74 0)
		)
		(property "Voltage" " "
			(at 67.183 78.74 0)
		)
		(property "Tolerance" "±1%"
			(at 69.088 78.74 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 70.993 78.74 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 72.898 78.74 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 74.803 78.74 0)
		)
		(property "Case" "0402"
			(at 76.708 78.74 0)
		)
		(property "PressFit" "No"
			(at 78.613 78.74 0)
		)
		(property "Mounted" "Yes"
			(at 80.518 78.74 0)
		)
		(property "Sense Comment" " "
			(at 82.423 78.74 0)
		)
		(property "Sense" "No"
			(at 84.328 78.74 0)
		)
		(property "Status Comment" " "
			(at 86.233 78.74 0)
		)
		(property "Socket" "No"
			(at 88.138 78.74 0)
		)
		(property "SMD" "Yes"
			(at 90.043 78.74 0)
		)
		(property "ComponentHeight" " "
			(at 91.948 78.74 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 93.853 78.74 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 95.758 78.74 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 97.663 78.74 0)
		)
		(property "HelpURL" ""
			(at 99.568 78.74 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 101.473 78.74 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 103.378 78.74 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 105.283 78.74 0)
		)
		(property "Database Table Name" "Resistors"
			(at 107.188 78.74 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 109.093 78.74 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 110.998 78.74 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 112.903 78.74 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R69")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_33R_1%_0.0625W_100PPM")
		(at 34.29 247.65 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R456"
			(at 36.068 224.79 0)
		)
		(property "Value" "R0402_33R_1%_0.0625W_100PPM"
			(at 34.29 252.603 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 34.29 254.508 0)
		)
		(property "Datasheet" ""
			(at 34.29 256.413 0)
		)
		(property "Description" "±1%"
			(at 38.1 242.57 0)
		)
		(property "Val" "33"
			(at 40.894 224.79 0)
		)
		(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 34.29 258.318 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 34.29 260.223 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 34.29 262.128 0)
		)
		(property "Comment" "33"
			(at 34.29 264.033 0)
		)
		(property "Component Kind" "Standard"
			(at 34.29 265.938 0)
		)
		(property "Component Type" "Standard"
			(at 34.29 267.843 0)
		)
		(property "PackageDescription" " "
			(at 34.29 269.748 0)
		)
		(property "Pin Count" "2"
			(at 34.29 271.653 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 34.29 273.558 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 34.29 275.463 0)
		)
		(property "Status" "Not Recommended"
			(at 34.29 277.368 0)
		)
		(property "Power" "0.0625W"
			(at 34.29 279.273 0)
		)
		(property "Voltage" " "
			(at 34.29 283.083 0)
		)
		(property "Tolerance" "±1%"
			(at 34.29 284.988 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 34.29 286.893 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 34.29 288.798 0)
		)
		(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 34.29 290.703 0)
		)
		(property "Case" "0402"
			(at 34.29 292.608 0)
		)
		(property "PressFit" "No"
			(at 34.29 294.513 0)
		)
		(property "Mounted" "Yes"
			(at 34.29 296.418 0)
		)
		(property "Sense Comment" " "
			(at 34.29 298.323 0)
		)
		(property "Sense" "No"
			(at 34.29 300.228 0)
		)
		(property "Status Comment" " "
			(at 34.29 302.133 0)
		)
		(property "Socket" "No"
			(at 34.29 304.038 0)
		)
		(property "SMD" "Yes"
			(at 34.29 305.943 0)
		)
		(property "ComponentHeight" " "
			(at 34.29 307.848 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 34.29 309.753 0)
		)
		(property "Manufacturer1 Part Number" "232270673309L"
			(at 34.29 311.658 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 34.29 313.563 0)
		)
		(property "HelpURL" ""
			(at 34.29 315.468 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 34.29 317.373 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 34.29 319.278 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 34.29 321.183 0)
		)
		(property "Database Table Name" "Resistors"
			(at 34.29 323.088 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 34.29 324.993 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 34.29 326.898 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 34.29 328.803 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R456")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 242.57 266.7 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0722"
			(at 242.57 266.7 0)
		)
		(property "Value" "GND"
			(at 242.57 270.51 0)
		)
		(property "Footprint" ""
			(at 242.57 266.7 0)
		)
		(property "Datasheet" ""
			(at 242.57 266.7 0)
		)
		(property "Description" ""
			(at 242.57 266.7 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0722")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 154.94 144.78 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R260"
			(at 151.13 138.43 0)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 154.94 139.827 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 154.94 137.922 0)
		)
		(property "Datasheet" ""
			(at 154.94 136.017 0)
		)
		(property "Description" "±1%"
			(at 151.13 149.86 0)
		)
		(property "Val" "10k"
			(at 151.13 140.97 0)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 154.94 134.112 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 154.94 132.207 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 154.94 130.302 0)
		)
		(property "Comment" "10k"
			(at 154.94 128.397 0)
		)
		(property "Component Kind" "Standard"
			(at 154.94 126.492 0)
		)
		(property "Component Type" "Standard"
			(at 154.94 124.587 0)
		)
		(property "PackageDescription" " "
			(at 154.94 122.682 0)
		)
		(property "Pin Count" "2"
			(at 154.94 120.777 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 154.94 118.872 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 154.94 116.967 0)
		)
		(property "Status" "Not Recommended"
			(at 154.94 115.062 0)
		)
		(property "Power" "0.0625W"
			(at 154.94 113.157 0)
		)
		(property "Voltage" " "
			(at 154.94 109.347 0)
		)
		(property "Tolerance" "±1%"
			(at 154.94 107.442 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 154.94 105.537 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 154.94 103.632 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 154.94 101.727 0)
		)
		(property "Case" "0402"
			(at 154.94 99.822 0)
		)
		(property "PressFit" "No"
			(at 154.94 97.917 0)
		)
		(property "Mounted" "Yes"
			(at 154.94 96.012 0)
		)
		(property "Sense Comment" " "
			(at 154.94 94.107 0)
		)
		(property "Sense" "No"
			(at 154.94 92.202 0)
		)
		(property "Status Comment" " "
			(at 154.94 90.297 0)
		)
		(property "Socket" "No"
			(at 154.94 88.392 0)
		)
		(property "SMD" "Yes"
			(at 154.94 86.487 0)
		)
		(property "ComponentHeight" " "
			(at 154.94 84.582 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 154.94 82.677 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 154.94 80.772 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 154.94 78.867 0)
		)
		(property "HelpURL" ""
			(at 154.94 76.962 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 154.94 75.057 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 154.94 73.152 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 154.94 71.247 0)
		)
		(property "Database Table Name" "Resistors"
			(at 154.94 69.342 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 154.94 67.437 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 154.94 65.532 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 154.94 63.627 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R260")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 140.97 198.12 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R266"
			(at 137.16 191.77 0)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 140.97 193.167 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 140.97 191.262 0)
		)
		(property "Datasheet" ""
			(at 140.97 189.357 0)
		)
		(property "Description" "±1%"
			(at 137.16 203.2 0)
		)
		(property "Val" "10k"
			(at 137.16 194.31 0)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 140.97 187.452 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 140.97 185.547 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 140.97 183.642 0)
		)
		(property "Comment" "10k"
			(at 140.97 181.737 0)
		)
		(property "Component Kind" "Standard"
			(at 140.97 179.832 0)
		)
		(property "Component Type" "Standard"
			(at 140.97 177.927 0)
		)
		(property "PackageDescription" " "
			(at 140.97 176.022 0)
		)
		(property "Pin Count" "2"
			(at 140.97 174.117 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 140.97 172.212 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 140.97 170.307 0)
		)
		(property "Status" "Not Recommended"
			(at 140.97 168.402 0)
		)
		(property "Power" "0.0625W"
			(at 140.97 166.497 0)
		)
		(property "Voltage" " "
			(at 140.97 162.687 0)
		)
		(property "Tolerance" "±1%"
			(at 140.97 160.782 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 140.97 158.877 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 140.97 156.972 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 140.97 155.067 0)
		)
		(property "Case" "0402"
			(at 140.97 153.162 0)
		)
		(property "PressFit" "No"
			(at 140.97 151.257 0)
		)
		(property "Mounted" "Yes"
			(at 140.97 149.352 0)
		)
		(property "Sense Comment" " "
			(at 140.97 147.447 0)
		)
		(property "Sense" "No"
			(at 140.97 145.542 0)
		)
		(property "Status Comment" " "
			(at 140.97 143.637 0)
		)
		(property "Socket" "No"
			(at 140.97 141.732 0)
		)
		(property "SMD" "Yes"
			(at 140.97 139.827 0)
		)
		(property "ComponentHeight" " "
			(at 140.97 137.922 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 140.97 136.017 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 140.97 134.112 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 140.97 132.207 0)
		)
		(property "HelpURL" ""
			(at 140.97 130.302 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 140.97 128.397 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 140.97 126.492 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 140.97 124.587 0)
		)
		(property "Database Table Name" "Resistors"
			(at 140.97 122.682 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 140.97 120.777 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 140.97 118.872 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 140.97 116.967 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R266")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 38.1 156.21 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R124"
			(at 40.64 151.1299 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 43.053 156.21 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 44.958 156.21 0)
		)
		(property "Datasheet" ""
			(at 46.863 156.21 0)
		)
		(property "Description" "±1%"
			(at 33.02 152.4 0)
		)
		(property "Val" "10k"
			(at 40.64 153.6699 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 48.768 156.21 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 50.673 156.21 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 52.578 156.21 0)
		)
		(property "Comment" "10k"
			(at 54.483 156.21 0)
		)
		(property "Component Kind" "Standard"
			(at 56.388 156.21 0)
		)
		(property "Component Type" "Standard"
			(at 58.293 156.21 0)
		)
		(property "PackageDescription" " "
			(at 60.198 156.21 0)
		)
		(property "Pin Count" "2"
			(at 62.103 156.21 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 64.008 156.21 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 65.913 156.21 0)
		)
		(property "Status" "Not Recommended"
			(at 67.818 156.21 0)
		)
		(property "Power" "0.0625W"
			(at 69.723 156.21 0)
		)
		(property "Voltage" " "
			(at 73.533 156.21 0)
		)
		(property "Tolerance" "±1%"
			(at 75.438 156.21 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 77.343 156.21 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 79.248 156.21 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 81.153 156.21 0)
		)
		(property "Case" "0402"
			(at 83.058 156.21 0)
		)
		(property "PressFit" "No"
			(at 84.963 156.21 0)
		)
		(property "Mounted" "Yes"
			(at 86.868 156.21 0)
		)
		(property "Sense Comment" " "
			(at 88.773 156.21 0)
		)
		(property "Sense" "No"
			(at 90.678 156.21 0)
		)
		(property "Status Comment" " "
			(at 92.583 156.21 0)
		)
		(property "Socket" "No"
			(at 94.488 156.21 0)
		)
		(property "SMD" "Yes"
			(at 96.393 156.21 0)
		)
		(property "ComponentHeight" " "
			(at 98.298 156.21 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 100.203 156.21 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 102.108 156.21 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 104.013 156.21 0)
		)
		(property "HelpURL" ""
			(at 105.918 156.21 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 107.823 156.21 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 109.728 156.21 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 111.633 156.21 0)
		)
		(property "Database Table Name" "Resistors"
			(at 113.538 156.21 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 115.443 156.21 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 117.348 156.21 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 119.253 156.21 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R124")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Standard Logic:SN74LV595ARGYR")
		(at 283.21 196.85 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC64"
			(at 293.37 191.77 0)
		)
		(property "Value" "SN74LV595ARGYR"
			(at 293.37 194.31 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:TEXAS_RGY (R-PVQFN-N16)"
			(at 283.21 236.22 0)
		)
		(property "Datasheet" ""
			(at 283.21 238.125 0)
		)
		(property "Description" "SN74LV595ARGYR"
			(at 283.21 240.03 0)
		)
		(property "Library Ref" "74595_a"
			(at 283.21 241.935 0)
		)
		(property "Library Path" "SchLib\\Standard Logic.SchLib"
			(at 283.21 243.84 0)
		)
		(property "Comment" "SN74LV595ARGY"
			(at 283.21 245.745 0)
		)
		(property "Component Kind" "Standard"
			(at 283.21 247.65 0)
		)
		(property "Component Type" "Standard"
			(at 283.21 249.555 0)
		)
		(property "Device" "SN74LV595ARGY"
			(at 283.21 251.46 0)
		)
		(property "PackageDescription" "TEXAS Case Style RGY (R-PVQFN-N16), QFN, 0.50mm Pitch, Rect.; 16 Pin, 4.00mm L X 3.50mm W X 1mm H body (w/Thermal Tab 2.65 X 2.15mm)"
			(at 283.21 253.365 0)
		)
		(property "Status" " "
			(at 283.21 255.27 0)
		)
		(property "Part Description" "8-Bit Shift Register with 3-State Output Registers"
			(at 283.21 257.175 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 283.21 259.08 0)
		)
		(property "Manufacturer Part Number" "SN74LV595ARGY"
			(at 283.21 260.985 0)
		)
		(property "Pin Count" "17"
			(at 283.21 262.89 0)
		)
		(property "Case" "QFN16"
			(at 283.21 264.795 0)
		)
		(property "Mounted" "Yes"
			(at 283.21 266.7 0)
		)
		(property "Socket" "No"
			(at 283.21 268.605 0)
		)
		(property "SMD" "Yes"
			(at 283.21 270.51 0)
		)
		(property "PressFit" "No"
			(at 283.21 272.415 0)
		)
		(property "Sense" "No"
			(at 283.21 274.32 0)
		)
		(property "Sense Comment" " "
			(at 283.21 276.225 0)
		)
		(property "Bonding" "No"
			(at 283.21 278.13 0)
		)
		(property "Status Comment" " "
			(at 283.21 280.035 0)
		)
		(property "ComponentHeight" "1mm"
			(at 283.21 281.94 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 283.21 283.845 0)
		)
		(property "Footprint Ref" "TEXAS_RGY (R-PVQFN-N16)"
			(at 283.21 285.75 0)
		)
		(property "Author" "CERN DEM MR"
			(at 283.21 287.655 0)
		)
		(property "HelpURL" ""
			(at 283.21 289.56 0)
		)
		(property "ComponentLink1URL" " "
			(at 283.21 291.465 0)
		)
		(property "ComponentLink1Description" " "
			(at 283.21 293.37 0)
		)
		(property "ComponentLink2URL" " "
			(at 283.21 295.275 0)
		)
		(property "ComponentLink2Description" " "
			(at 283.21 297.18 0)
		)
		(property "CreateDate" "10/10/17 00:00:00"
			(at 283.21 299.085 0)
		)
		(property "LatestRevisionDate" "10/10/17 00:00:00"
			(at 283.21 300.99 0)
		)
		(property "SCEM" " "
			(at 283.21 302.895 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 283.21 304.8 0)
		)
		(property "Library Name" "Standard Logic"
			(at 283.21 306.705 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 283.21 308.61 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 283.21 310.515 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC64")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 76.2 53.34 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0328"
			(at 76.2 53.34 0)
		)
		(property "Value" "GND"
			(at 80.01 53.34 0)
		)
		(property "Footprint" ""
			(at 76.2 53.34 0)
		)
		(property "Datasheet" ""
			(at 76.2 53.34 0)
		)
		(property "Description" ""
			(at 76.2 53.34 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0328")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 344.17 220.98 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0727"
			(at 344.17 220.98 0)
		)
		(property "Value" "P3V3"
			(at 345.186 216.916 0)
		)
		(property "Footprint" ""
			(at 344.17 220.98 0)
		)
		(property "Datasheet" ""
			(at 344.17 220.98 0)
		)
		(property "Description" ""
			(at 344.17 220.98 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0727")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Standard Logic:SN74LVTH125RGY")
		(at 173.99 142.24 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC15"
			(at 181.61 175.26 0)
		)
		(property "Value" "SN74LVTH125RGY"
			(at 181.61 177.8 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:TEXAS_RGY (S-PVQFN-N14)"
			(at 173.99 179.07 0)
		)
		(property "Datasheet" ""
			(at 173.99 180.975 0)
		)
		(property "Description" ""
			(at 173.99 142.24 0)
		)
		(property "SMD" "Yes"
			(at 173.99 213.36 0)
		)
		(property "Part Number" "SN74LVTH125RGY"
			(at 173.99 182.88 0)
		)
		(property "Library Ref" "74125"
			(at 173.99 184.785 0)
		)
		(property "Library Path" "SchLib\\Standard Logic.SchLib"
			(at 173.99 186.69 0)
		)
		(property "Comment" "SN74LVTH125RGY"
			(at 173.99 188.595 0)
		)
		(property "Component Kind" "Standard"
			(at 173.99 190.5 0)
		)
		(property "Component Type" "Standard"
			(at 173.99 192.405 0)
		)
		(property "Device" "SN74LVTH125RGY"
			(at 173.99 194.31 0)
		)
		(property "PackageDescription" "TEXAS Case Style RGY (S-PVQFN-N14), QFN, 0.50mm Pitch, Rect.; 14 Pin, 3.50mm L X 3.50mm W X 1mm H body (w/Thermal Tab 2.15 X 2.15mm)"
			(at 173.99 196.215 0)
		)
		(property "Status" " "
			(at 173.99 198.12 0)
		)
		(property "Part Description" "3.3V ABT Quadruple Bus Buffer with 3-State Outputs"
			(at 173.99 200.025 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 173.99 201.93 0)
		)
		(property "Manufacturer Part Number" "SN74LVTH125RGY"
			(at 173.99 203.835 0)
		)
		(property "Pin Count" "15"
			(at 173.99 205.74 0)
		)
		(property "Case" "QFN14"
			(at 173.99 207.645 0)
		)
		(property "Mounted" "Yes"
			(at 173.99 209.55 0)
		)
		(property "Socket" "No"
			(at 173.99 211.455 0)
		)
		(property "PressFit" "No"
			(at 173.99 215.265 0)
		)
		(property "Sense" "No"
			(at 173.99 217.17 0)
		)
		(property "Sense Comment" " "
			(at 173.99 219.075 0)
		)
		(property "Bonding" "No"
			(at 173.99 220.98 0)
		)
		(property "Status Comment" " "
			(at 173.99 222.885 0)
		)
		(property "ComponentHeight" "1mm"
			(at 173.99 224.79 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 173.99 226.695 0)
		)
		(property "Footprint Ref" "TEXAS_RGY (S-PVQFN-N14)"
			(at 173.99 228.6 0)
		)
		(property "Author" "CERN DEM BC"
			(at 173.99 230.505 0)
		)
		(property "HelpURL" ""
			(at 173.99 232.41 0)
		)
		(property "ComponentLink1URL" " "
			(at 173.99 234.315 0)
		)
		(property "ComponentLink1Description" " "
			(at 173.99 236.22 0)
		)
		(property "ComponentLink2URL" " "
			(at 173.99 238.125 0)
		)
		(property "ComponentLink2Description" " "
			(at 173.99 240.03 0)
		)
		(property "CreateDate" "04/22/20 00:00:00"
			(at 173.99 241.935 0)
		)
		(property "LatestRevisionDate" "04/22/20 00:00:00"
			(at 173.99 243.84 0)
		)
		(property "SCEM" " "
			(at 173.99 245.745 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 173.99 247.65 0)
		)
		(property "Library Name" "Standard Logic"
			(at 173.99 249.555 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 173.99 251.46 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 173.99 253.365 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC15")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 114.3 38.1 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0105"
			(at 114.3 38.1 0)
		)
		(property "Value" "P3V3"
			(at 114.3 34.29 0)
		)
		(property "Footprint" ""
			(at 114.3 38.1 0)
		)
		(property "Datasheet" ""
			(at 114.3 38.1 0)
		)
		(property "Description" ""
			(at 114.3 38.1 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0105")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 226.06 157.48 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR084"
			(at 226.06 157.48 0)
		)
		(property "Value" "P3V3"
			(at 226.06 153.67 0)
		)
		(property "Footprint" ""
			(at 226.06 157.48 0)
		)
		(property "Datasheet" ""
			(at 226.06 157.48 0)
		)
		(property "Description" ""
			(at 226.06 157.48 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR084")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 54.61 266.7 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0338"
			(at 54.61 266.7 0)
		)
		(property "Value" "GND"
			(at 54.61 270.51 0)
		)
		(property "Footprint" ""
			(at 54.61 266.7 0)
		)
		(property "Datasheet" ""
			(at 54.61 266.7 0)
		)
		(property "Description" ""
			(at 54.61 266.7 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0338")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 93.98 66.04 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0329"
			(at 93.98 66.04 0)
		)
		(property "Value" "GND"
			(at 93.98 69.85 0)
		)
		(property "Footprint" ""
			(at 93.98 66.04 0)
		)
		(property "Datasheet" ""
			(at 93.98 66.04 0)
		)
		(property "Description" ""
			(at 93.98 66.04 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0329")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 196.85 172.72 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR077"
			(at 196.85 172.72 0)
		)
		(property "Value" "GND"
			(at 196.85 176.53 0)
		)
		(property "Footprint" ""
			(at 196.85 172.72 0)
		)
		(property "Datasheet" ""
			(at 196.85 172.72 0)
		)
		(property "Description" ""
			(at 196.85 172.72 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR077")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_33R_1%_0.0625W_100PPM")
		(at 34.29 234.95 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R455"
			(at 36.068 222.25 0)
		)
		(property "Value" "R0402_33R_1%_0.0625W_100PPM"
			(at 34.29 239.903 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 34.29 241.808 0)
		)
		(property "Datasheet" ""
			(at 34.29 243.713 0)
		)
		(property "Description" "±1%"
			(at 38.1 229.87 0)
		)
		(property "Val" "33"
			(at 40.894 222.25 0)
		)
		(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 34.29 245.618 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 34.29 247.523 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 34.29 249.428 0)
		)
		(property "Comment" "33"
			(at 34.29 251.333 0)
		)
		(property "Component Kind" "Standard"
			(at 34.29 253.238 0)
		)
		(property "Component Type" "Standard"
			(at 34.29 255.143 0)
		)
		(property "PackageDescription" " "
			(at 34.29 257.048 0)
		)
		(property "Pin Count" "2"
			(at 34.29 258.953 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 34.29 260.858 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 34.29 262.763 0)
		)
		(property "Status" "Not Recommended"
			(at 34.29 264.668 0)
		)
		(property "Power" "0.0625W"
			(at 34.29 266.573 0)
		)
		(property "Voltage" " "
			(at 34.29 270.383 0)
		)
		(property "Tolerance" "±1%"
			(at 34.29 272.288 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 34.29 274.193 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 34.29 276.098 0)
		)
		(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 34.29 278.003 0)
		)
		(property "Case" "0402"
			(at 34.29 279.908 0)
		)
		(property "PressFit" "No"
			(at 34.29 281.813 0)
		)
		(property "Mounted" "Yes"
			(at 34.29 283.718 0)
		)
		(property "Sense Comment" " "
			(at 34.29 285.623 0)
		)
		(property "Sense" "No"
			(at 34.29 287.528 0)
		)
		(property "Status Comment" " "
			(at 34.29 289.433 0)
		)
		(property "Socket" "No"
			(at 34.29 291.338 0)
		)
		(property "SMD" "Yes"
			(at 34.29 293.243 0)
		)
		(property "ComponentHeight" " "
			(at 34.29 295.148 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 34.29 297.053 0)
		)
		(property "Manufacturer1 Part Number" "232270673309L"
			(at 34.29 298.958 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 34.29 300.863 0)
		)
		(property "HelpURL" ""
			(at 34.29 302.768 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 34.29 304.673 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 34.29 306.578 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 34.29 308.483 0)
		)
		(property "Database Table Name" "Resistors"
			(at 34.29 310.388 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 34.29 312.293 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 34.29 314.198 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 34.29 316.103 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R455")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 31.75 200.66 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0353"
			(at 31.75 200.66 0)
		)
		(property "Value" "GND"
			(at 31.75 204.47 90)
		)
		(property "Footprint" ""
			(at 31.75 200.66 0)
		)
		(property "Datasheet" ""
			(at 31.75 200.66 0)
		)
		(property "Description" ""
			(at 31.75 200.66 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0353")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 312.42 234.95 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0725"
			(at 312.42 234.95 0)
		)
		(property "Value" "GND"
			(at 312.42 238.76 0)
		)
		(property "Footprint" ""
			(at 312.42 234.95 0)
		)
		(property "Datasheet" ""
			(at 312.42 234.95 0)
		)
		(property "Description" ""
			(at 312.42 234.95 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0725")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 161.29 205.74 270)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0734"
			(at 161.29 205.74 0)
		)
		(property "Value" "P3V3"
			(at 157.48 205.74 0)
		)
		(property "Footprint" ""
			(at 161.29 205.74 0)
		)
		(property "Datasheet" ""
			(at 161.29 205.74 0)
		)
		(property "Description" ""
			(at 161.29 205.74 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0734")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 344.17 232.41 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C390"
			(at 347.98 227.3299 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 349.25 227.33 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 344.17 232.41 0)
		)
		(property "Datasheet" ""
			(at 344.17 232.41 0)
		)
		(property "Description" "100nF"
			(at 347.98 229.8699 90)
		)
		(property "SMD" "Yes"
			(at 343.662 234.696 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 356.108 232.41 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 358.013 232.41 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 359.918 232.41 0)
		)
		(property "Comment" "100nF"
			(at 361.823 232.41 0)
		)
		(property "Component Kind" "Standard"
			(at 363.728 232.41 0)
		)
		(property "Component Type" "Standard"
			(at 365.633 232.41 0)
		)
		(property "Pin Count" "2"
			(at 367.538 232.41 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 369.443 232.41 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 371.348 232.41 0)
		)
		(property "PackageDescription" " "
			(at 373.253 232.41 0)
		)
		(property "Status" "Not Recommended"
			(at 375.158 232.41 0)
		)
		(property "Status Comment" " "
			(at 377.063 232.41 0)
		)
		(property "Voltage" "16V"
			(at 378.968 232.41 0)
		)
		(property "Tolerance" "±10%"
			(at 382.778 232.41 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 384.683 232.41 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 386.588 232.41 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 388.493 232.41 0)
		)
		(property "Case" "0402"
			(at 390.398 232.41 0)
		)
		(property "Mounted" "Yes"
			(at 392.303 232.41 0)
		)
		(property "Socket" "No"
			(at 394.208 232.41 0)
		)
		(property "PressFit" " "
			(at 398.018 232.41 0)
		)
		(property "Sense" "No"
			(at 399.923 232.41 0)
		)
		(property "Sense Comment" " "
			(at 401.828 232.41 0)
		)
		(property "ComponentHeight" " "
			(at 403.733 232.41 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 405.638 232.41 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 407.543 232.41 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 409.448 232.41 0)
		)
		(property "HelpURL" ""
			(at 411.353 232.41 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 413.258 232.41 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 415.163 232.41 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 417.068 232.41 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 418.973 232.41 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 420.878 232.41 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 422.783 232.41 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 424.688 232.41 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C390")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Standard Logic:SN74LV595ARGYR")
		(at 139.7 229.87 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC49"
			(at 149.86 224.79 0)
		)
		(property "Value" "SN74LV595ARGYR"
			(at 149.86 227.33 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:TEXAS_RGY (R-PVQFN-N16)"
			(at 139.7 269.24 0)
		)
		(property "Datasheet" ""
			(at 139.7 271.145 0)
		)
		(property "Description" "SN74LV595ARGYR"
			(at 139.7 273.05 0)
		)
		(property "Library Ref" "74595_a"
			(at 139.7 274.955 0)
		)
		(property "Library Path" "SchLib\\Standard Logic.SchLib"
			(at 139.7 276.86 0)
		)
		(property "Comment" "SN74LV595ARGY"
			(at 139.7 278.765 0)
		)
		(property "Component Kind" "Standard"
			(at 139.7 280.67 0)
		)
		(property "Component Type" "Standard"
			(at 139.7 282.575 0)
		)
		(property "Device" "SN74LV595ARGY"
			(at 139.7 284.48 0)
		)
		(property "PackageDescription" "TEXAS Case Style RGY (R-PVQFN-N16), QFN, 0.50mm Pitch, Rect.; 16 Pin, 4.00mm L X 3.50mm W X 1mm H body (w/Thermal Tab 2.65 X 2.15mm)"
			(at 139.7 286.385 0)
		)
		(property "Status" " "
			(at 139.7 288.29 0)
		)
		(property "Part Description" "8-Bit Shift Register with 3-State Output Registers"
			(at 139.7 290.195 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 139.7 292.1 0)
		)
		(property "Manufacturer Part Number" "SN74LV595ARGY"
			(at 139.7 294.005 0)
		)
		(property "Pin Count" "17"
			(at 139.7 295.91 0)
		)
		(property "Case" "QFN16"
			(at 139.7 297.815 0)
		)
		(property "Mounted" "Yes"
			(at 139.7 299.72 0)
		)
		(property "Socket" "No"
			(at 139.7 301.625 0)
		)
		(property "SMD" "Yes"
			(at 139.7 303.53 0)
		)
		(property "PressFit" "No"
			(at 139.7 305.435 0)
		)
		(property "Sense" "No"
			(at 139.7 307.34 0)
		)
		(property "Sense Comment" " "
			(at 139.7 309.245 0)
		)
		(property "Bonding" "No"
			(at 139.7 311.15 0)
		)
		(property "Status Comment" " "
			(at 139.7 313.055 0)
		)
		(property "ComponentHeight" "1mm"
			(at 139.7 314.96 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 139.7 316.865 0)
		)
		(property "Footprint Ref" "TEXAS_RGY (R-PVQFN-N16)"
			(at 139.7 318.77 0)
		)
		(property "Author" "CERN DEM MR"
			(at 139.7 320.675 0)
		)
		(property "HelpURL" ""
			(at 139.7 322.58 0)
		)
		(property "ComponentLink1URL" " "
			(at 139.7 324.485 0)
		)
		(property "ComponentLink1Description" " "
			(at 139.7 326.39 0)
		)
		(property "ComponentLink2URL" " "
			(at 139.7 328.295 0)
		)
		(property "ComponentLink2Description" " "
			(at 139.7 330.2 0)
		)
		(property "CreateDate" "10/10/17 00:00:00"
			(at 139.7 332.105 0)
		)
		(property "LatestRevisionDate" "10/10/17 00:00:00"
			(at 139.7 334.01 0)
		)
		(property "SCEM" " "
			(at 139.7 335.915 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 139.7 337.82 0)
		)
		(property "Library Name" "Standard Logic"
			(at 139.7 339.725 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 139.7 341.63 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 139.7 343.535 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC49")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 31.75 20.32 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0345"
			(at 31.75 20.32 0)
		)
		(property "Value" "P3V3"
			(at 31.75 16.51 0)
		)
		(property "Footprint" ""
			(at 31.75 20.32 0)
		)
		(property "Datasheet" ""
			(at 31.75 20.32 0)
		)
		(property "Description" ""
			(at 31.75 20.32 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0345")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 132.08 198.12 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0733"
			(at 132.08 198.12 0)
		)
		(property "Value" "GND"
			(at 128.27 198.12 90)
		)
		(property "Footprint" ""
			(at 132.08 198.12 0)
		)
		(property "Datasheet" ""
			(at 132.08 198.12 0)
		)
		(property "Description" ""
			(at 132.08 198.12 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0733")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0603_120R_1%_0.2W_200PPM")
		(at 82.55 88.9 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R87"
			(at 85.09 83.8199 90)
		)
		(property "Value" "R0603_120R_1%_0.2W_200PPM"
			(at 87.503 88.9 0)
		)
		(property "Footprint" "Resistors SMD:RESC1608X55N"
			(at 89.408 88.9 0)
		)
		(property "Datasheet" ""
			(at 91.313 88.9 0)
		)
		(property "Description" "±1%"
			(at 85.09 85.09 90)
		)
		(property "Val" "120"
			(at 85.09 86.3599 90)
		)
		(property "Part Number" "R0603_120R_1%_0.2W_200PPM"
			(at 93.218 88.9 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 95.123 88.9 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 97.028 88.9 0)
		)
		(property "Comment" "120"
			(at 98.933 88.9 0)
		)
		(property "Component Kind" "Standard"
			(at 100.838 88.9 0)
		)
		(property "Component Type" "Standard"
			(at 102.743 88.9 0)
		)
		(property "PackageDescription" " "
			(at 104.648 88.9 0)
		)
		(property "Pin Count" "2"
			(at 106.553 88.9 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 108.458 88.9 0)
		)
		(property "Footprint Ref" "RESC1608X55N"
			(at 110.363 88.9 0)
		)
		(property "Status" "Preferred"
			(at 112.268 88.9 0)
		)
		(property "Power" "0.2W"
			(at 114.173 88.9 0)
		)
		(property "Voltage" " "
			(at 117.983 88.9 0)
		)
		(property "Tolerance" "±1%"
			(at 119.888 88.9 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 121.793 88.9 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 123.698 88.9 0)
		)
		(property "Manufacturer Part Number" "R0603_120R_1%_0.2W_200PPM"
			(at 125.603 88.9 0)
		)
		(property "Case" "0603"
			(at 127.508 88.9 0)
		)
		(property "PressFit" "No"
			(at 129.413 88.9 0)
		)
		(property "Mounted" "Yes"
			(at 131.318 88.9 0)
		)
		(property "Sense Comment" " "
			(at 133.223 88.9 0)
		)
		(property "Sense" "No"
			(at 135.128 88.9 0)
		)
		(property "Status Comment" " "
			(at 137.033 88.9 0)
		)
		(property "Socket" "No"
			(at 138.938 88.9 0)
		)
		(property "SMD" "Yes"
			(at 140.843 88.9 0)
		)
		(property "ComponentHeight" " "
			(at 142.748 88.9 0)
		)
		(property "Manufacturer1 Example" "TE CONNECTIVITY"
			(at 144.653 88.9 0)
		)
		(property "Manufacturer1 Part Number" "CRGH0603F120R"
			(at 146.558 88.9 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 148.463 88.9 0)
		)
		(property "HelpURL" ""
			(at 150.368 88.9 0)
		)
		(property "Author" "CERN DEM HF"
			(at 152.273 88.9 0)
		)
		(property "CreateDate" "02/24/23 00:00:00"
			(at 154.178 88.9 0)
		)
		(property "LatestRevisionDate" "02/24/23 00:00:00"
			(at 156.083 88.9 0)
		)
		(property "Database Table Name" "Resistors"
			(at 157.988 88.9 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 159.893 88.9 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 161.798 88.9 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 163.703 88.9 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R87")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 200.66 265.43 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C388"
			(at 204.47 260.3499 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 205.74 260.35 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 200.66 265.43 0)
		)
		(property "Datasheet" ""
			(at 200.66 265.43 0)
		)
		(property "Description" "100nF"
			(at 204.47 262.8899 90)
		)
		(property "SMD" "Yes"
			(at 200.152 267.716 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 212.598 265.43 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 214.503 265.43 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 216.408 265.43 0)
		)
		(property "Comment" "100nF"
			(at 218.313 265.43 0)
		)
		(property "Component Kind" "Standard"
			(at 220.218 265.43 0)
		)
		(property "Component Type" "Standard"
			(at 222.123 265.43 0)
		)
		(property "Pin Count" "2"
			(at 224.028 265.43 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 225.933 265.43 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 227.838 265.43 0)
		)
		(property "PackageDescription" " "
			(at 229.743 265.43 0)
		)
		(property "Status" "Not Recommended"
			(at 231.648 265.43 0)
		)
		(property "Status Comment" " "
			(at 233.553 265.43 0)
		)
		(property "Voltage" "16V"
			(at 235.458 265.43 0)
		)
		(property "Tolerance" "±10%"
			(at 239.268 265.43 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 241.173 265.43 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 243.078 265.43 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 244.983 265.43 0)
		)
		(property "Case" "0402"
			(at 246.888 265.43 0)
		)
		(property "Mounted" "Yes"
			(at 248.793 265.43 0)
		)
		(property "Socket" "No"
			(at 250.698 265.43 0)
		)
		(property "PressFit" " "
			(at 254.508 265.43 0)
		)
		(property "Sense" "No"
			(at 256.413 265.43 0)
		)
		(property "Sense Comment" " "
			(at 258.318 265.43 0)
		)
		(property "ComponentHeight" " "
			(at 260.223 265.43 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 262.128 265.43 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 264.033 265.43 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 265.938 265.43 0)
		)
		(property "HelpURL" ""
			(at 267.843 265.43 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 269.748 265.43 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 271.653 265.43 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 273.558 265.43 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 275.463 265.43 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 277.368 265.43 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 279.273 265.43 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 281.178 265.43 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C388")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 30.48 156.21 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R122"
			(at 33.02 151.1299 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 35.433 156.21 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 37.338 156.21 0)
		)
		(property "Datasheet" ""
			(at 39.243 156.21 0)
		)
		(property "Description" "±1%"
			(at 25.4 152.4 0)
		)
		(property "Val" "10k"
			(at 33.02 153.6699 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 41.148 156.21 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 43.053 156.21 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 44.958 156.21 0)
		)
		(property "Comment" "10k"
			(at 46.863 156.21 0)
		)
		(property "Component Kind" "Standard"
			(at 48.768 156.21 0)
		)
		(property "Component Type" "Standard"
			(at 50.673 156.21 0)
		)
		(property "PackageDescription" " "
			(at 52.578 156.21 0)
		)
		(property "Pin Count" "2"
			(at 54.483 156.21 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 56.388 156.21 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 58.293 156.21 0)
		)
		(property "Status" "Not Recommended"
			(at 60.198 156.21 0)
		)
		(property "Power" "0.0625W"
			(at 62.103 156.21 0)
		)
		(property "Voltage" " "
			(at 65.913 156.21 0)
		)
		(property "Tolerance" "±1%"
			(at 67.818 156.21 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 69.723 156.21 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 71.628 156.21 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 73.533 156.21 0)
		)
		(property "Case" "0402"
			(at 75.438 156.21 0)
		)
		(property "PressFit" "No"
			(at 77.343 156.21 0)
		)
		(property "Mounted" "Yes"
			(at 79.248 156.21 0)
		)
		(property "Sense Comment" " "
			(at 81.153 156.21 0)
		)
		(property "Sense" "No"
			(at 83.058 156.21 0)
		)
		(property "Status Comment" " "
			(at 84.963 156.21 0)
		)
		(property "Socket" "No"
			(at 86.868 156.21 0)
		)
		(property "SMD" "Yes"
			(at 88.773 156.21 0)
		)
		(property "ComponentHeight" " "
			(at 90.678 156.21 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 92.583 156.21 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 94.488 156.21 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 96.393 156.21 0)
		)
		(property "HelpURL" ""
			(at 98.298 156.21 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 100.203 156.21 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 102.108 156.21 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 104.013 156.21 0)
		)
		(property "Database Table Name" "Resistors"
			(at 105.918 156.21 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 107.823 156.21 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 109.728 156.21 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 111.633 156.21 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R122")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 52.07 200.66 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0355"
			(at 52.07 200.66 0)
		)
		(property "Value" "GND"
			(at 52.07 204.47 0)
		)
		(property "Footprint" ""
			(at 52.07 200.66 0)
		)
		(property "Datasheet" ""
			(at 52.07 200.66 0)
		)
		(property "Description" ""
			(at 52.07 200.66 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0355")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 76.2 102.87 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0335"
			(at 76.2 102.87 0)
		)
		(property "Value" "GND"
			(at 80.01 102.87 0)
		)
		(property "Footprint" ""
			(at 76.2 102.87 0)
		)
		(property "Datasheet" ""
			(at 76.2 102.87 0)
		)
		(property "Description" ""
			(at 76.2 102.87 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0335")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 270.51 223.52 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0723"
			(at 270.51 223.52 0)
		)
		(property "Value" "P3V3"
			(at 270.51 219.71 0)
		)
		(property "Footprint" ""
			(at 270.51 223.52 0)
		)
		(property "Datasheet" ""
			(at 270.51 223.52 0)
		)
		(property "Description" ""
			(at 270.51 223.52 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0723")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 269.24 165.1 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR01081"
			(at 269.24 165.1 0)
		)
		(property "Value" "P3V3"
			(at 270.256 161.036 0)
		)
		(property "Footprint" ""
			(at 269.24 165.1 0)
		)
		(property "Datasheet" ""
			(at 269.24 165.1 0)
		)
		(property "Description" ""
			(at 269.24 165.1 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR01081")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Standard Logic:SN74LV595ARGYR")
		(at 67.31 229.87 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC48"
			(at 77.47 224.79 0)
		)
		(property "Value" "SN74LV595ARGYR"
			(at 77.47 227.33 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:TEXAS_RGY (R-PVQFN-N16)"
			(at 67.31 269.24 0)
		)
		(property "Datasheet" ""
			(at 67.31 271.145 0)
		)
		(property "Description" "SN74LV595ARGYR"
			(at 67.31 273.05 0)
		)
		(property "Library Ref" "74595_a"
			(at 67.31 274.955 0)
		)
		(property "Library Path" "SchLib\\Standard Logic.SchLib"
			(at 67.31 276.86 0)
		)
		(property "Comment" "SN74LV595ARGY"
			(at 67.31 278.765 0)
		)
		(property "Component Kind" "Standard"
			(at 67.31 280.67 0)
		)
		(property "Component Type" "Standard"
			(at 67.31 282.575 0)
		)
		(property "Device" "SN74LV595ARGY"
			(at 67.31 284.48 0)
		)
		(property "PackageDescription" "TEXAS Case Style RGY (R-PVQFN-N16), QFN, 0.50mm Pitch, Rect.; 16 Pin, 4.00mm L X 3.50mm W X 1mm H body (w/Thermal Tab 2.65 X 2.15mm)"
			(at 67.31 286.385 0)
		)
		(property "Status" " "
			(at 67.31 288.29 0)
		)
		(property "Part Description" "8-Bit Shift Register with 3-State Output Registers"
			(at 67.31 290.195 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 67.31 292.1 0)
		)
		(property "Manufacturer Part Number" "SN74LV595ARGY"
			(at 67.31 294.005 0)
		)
		(property "Pin Count" "17"
			(at 67.31 295.91 0)
		)
		(property "Case" "QFN16"
			(at 67.31 297.815 0)
		)
		(property "Mounted" "Yes"
			(at 67.31 299.72 0)
		)
		(property "Socket" "No"
			(at 67.31 301.625 0)
		)
		(property "SMD" "Yes"
			(at 67.31 303.53 0)
		)
		(property "PressFit" "No"
			(at 67.31 305.435 0)
		)
		(property "Sense" "No"
			(at 67.31 307.34 0)
		)
		(property "Sense Comment" " "
			(at 67.31 309.245 0)
		)
		(property "Bonding" "No"
			(at 67.31 311.15 0)
		)
		(property "Status Comment" " "
			(at 67.31 313.055 0)
		)
		(property "ComponentHeight" "1mm"
			(at 67.31 314.96 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 67.31 316.865 0)
		)
		(property "Footprint Ref" "TEXAS_RGY (R-PVQFN-N16)"
			(at 67.31 318.77 0)
		)
		(property "Author" "CERN DEM MR"
			(at 67.31 320.675 0)
		)
		(property "HelpURL" ""
			(at 67.31 322.58 0)
		)
		(property "ComponentLink1URL" " "
			(at 67.31 324.485 0)
		)
		(property "ComponentLink1Description" " "
			(at 67.31 326.39 0)
		)
		(property "ComponentLink2URL" " "
			(at 67.31 328.295 0)
		)
		(property "ComponentLink2Description" " "
			(at 67.31 330.2 0)
		)
		(property "CreateDate" "10/10/17 00:00:00"
			(at 67.31 332.105 0)
		)
		(property "LatestRevisionDate" "10/10/17 00:00:00"
			(at 67.31 334.01 0)
		)
		(property "SCEM" " "
			(at 67.31 335.915 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 67.31 337.82 0)
		)
		(property "Library Name" "Standard Logic"
			(at 67.31 339.725 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 67.31 341.63 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 67.31 343.535 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC48")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 270.51 233.68 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C389"
			(at 261.62 231.14 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 275.59 228.6 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 270.51 233.68 0)
		)
		(property "Datasheet" ""
			(at 270.51 233.68 0)
		)
		(property "Description" "100nF"
			(at 261.62 228.6 90)
		)
		(property "SMD" "Yes"
			(at 270.002 235.966 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 282.448 233.68 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 284.353 233.68 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 286.258 233.68 0)
		)
		(property "Comment" "100nF"
			(at 288.163 233.68 0)
		)
		(property "Component Kind" "Standard"
			(at 290.068 233.68 0)
		)
		(property "Component Type" "Standard"
			(at 291.973 233.68 0)
		)
		(property "Pin Count" "2"
			(at 293.878 233.68 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 295.783 233.68 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 297.688 233.68 0)
		)
		(property "PackageDescription" " "
			(at 299.593 233.68 0)
		)
		(property "Status" "Not Recommended"
			(at 301.498 233.68 0)
		)
		(property "Status Comment" " "
			(at 303.403 233.68 0)
		)
		(property "Voltage" "16V"
			(at 305.308 233.68 0)
		)
		(property "Tolerance" "±10%"
			(at 309.118 233.68 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 311.023 233.68 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 312.928 233.68 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 314.833 233.68 0)
		)
		(property "Case" "0402"
			(at 316.738 233.68 0)
		)
		(property "Mounted" "Yes"
			(at 318.643 233.68 0)
		)
		(property "Socket" "No"
			(at 320.548 233.68 0)
		)
		(property "PressFit" " "
			(at 324.358 233.68 0)
		)
		(property "Sense" "No"
			(at 326.263 233.68 0)
		)
		(property "Sense Comment" " "
			(at 328.168 233.68 0)
		)
		(property "ComponentHeight" " "
			(at 330.073 233.68 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 331.978 233.68 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 333.883 233.68 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 335.788 233.68 0)
		)
		(property "HelpURL" ""
			(at 337.693 233.68 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 339.598 233.68 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 341.503 233.68 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 343.408 233.68 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 345.313 233.68 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 347.218 233.68 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 349.123 233.68 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 351.028 233.68 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C389")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_33R_1%_0.0625W_100PPM")
		(at 113.03 223.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R387"
			(at 115.316 220.472 0)
		)
		(property "Value" "R0402_33R_1%_0.0625W_100PPM"
			(at 113.03 228.473 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 113.03 230.378 0)
		)
		(property "Datasheet" ""
			(at 113.03 232.283 0)
		)
		(property "Description" "±1%"
			(at 116.84 218.44 0)
		)
		(property "Val" "33"
			(at 120.142 220.472 0)
		)
		(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 113.03 234.188 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 113.03 236.093 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 113.03 237.998 0)
		)
		(property "Comment" "33"
			(at 113.03 239.903 0)
		)
		(property "Component Kind" "Standard"
			(at 113.03 241.808 0)
		)
		(property "Component Type" "Standard"
			(at 113.03 243.713 0)
		)
		(property "PackageDescription" " "
			(at 113.03 245.618 0)
		)
		(property "Pin Count" "2"
			(at 113.03 247.523 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 113.03 249.428 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 113.03 251.333 0)
		)
		(property "Status" "Not Recommended"
			(at 113.03 253.238 0)
		)
		(property "Power" "0.0625W"
			(at 113.03 255.143 0)
		)
		(property "Voltage" " "
			(at 113.03 258.953 0)
		)
		(property "Tolerance" "±1%"
			(at 113.03 260.858 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 113.03 262.763 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 113.03 264.668 0)
		)
		(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 113.03 266.573 0)
		)
		(property "Case" "0402"
			(at 113.03 268.478 0)
		)
		(property "PressFit" "No"
			(at 113.03 270.383 0)
		)
		(property "Mounted" "Yes"
			(at 113.03 272.288 0)
		)
		(property "Sense Comment" " "
			(at 113.03 274.193 0)
		)
		(property "Sense" "No"
			(at 113.03 276.098 0)
		)
		(property "Status Comment" " "
			(at 113.03 278.003 0)
		)
		(property "Socket" "No"
			(at 113.03 279.908 0)
		)
		(property "SMD" "Yes"
			(at 113.03 281.813 0)
		)
		(property "ComponentHeight" " "
			(at 113.03 283.718 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 113.03 285.623 0)
		)
		(property "Manufacturer1 Part Number" "232270673309L"
			(at 113.03 287.528 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 113.03 289.433 0)
		)
		(property "HelpURL" ""
			(at 113.03 291.338 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 113.03 293.243 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 113.03 295.148 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 113.03 297.053 0)
		)
		(property "Database Table Name" "Resistors"
			(at 113.03 298.958 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 113.03 300.863 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 113.03 302.768 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 113.03 304.673 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R387")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 269.24 176.53 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C512"
			(at 273.05 171.4499 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 274.32 171.45 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 269.24 176.53 0)
		)
		(property "Datasheet" ""
			(at 269.24 176.53 0)
		)
		(property "Description" "100nF"
			(at 273.05 173.9899 90)
		)
		(property "SMD" "Yes"
			(at 268.732 178.816 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 281.178 176.53 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 283.083 176.53 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 284.988 176.53 0)
		)
		(property "Comment" "100nF"
			(at 286.893 176.53 0)
		)
		(property "Component Kind" "Standard"
			(at 288.798 176.53 0)
		)
		(property "Component Type" "Standard"
			(at 290.703 176.53 0)
		)
		(property "Pin Count" "2"
			(at 292.608 176.53 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 294.513 176.53 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 296.418 176.53 0)
		)
		(property "PackageDescription" " "
			(at 298.323 176.53 0)
		)
		(property "Status" "Not Recommended"
			(at 300.228 176.53 0)
		)
		(property "Status Comment" " "
			(at 302.133 176.53 0)
		)
		(property "Voltage" "16V"
			(at 304.038 176.53 0)
		)
		(property "Tolerance" "±10%"
			(at 307.848 176.53 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 309.753 176.53 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 311.658 176.53 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 313.563 176.53 0)
		)
		(property "Case" "0402"
			(at 315.468 176.53 0)
		)
		(property "Mounted" "Yes"
			(at 317.373 176.53 0)
		)
		(property "Socket" "No"
			(at 319.278 176.53 0)
		)
		(property "PressFit" " "
			(at 323.088 176.53 0)
		)
		(property "Sense" "No"
			(at 324.993 176.53 0)
		)
		(property "Sense Comment" " "
			(at 326.898 176.53 0)
		)
		(property "ComponentHeight" " "
			(at 328.803 176.53 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 330.708 176.53 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 332.613 176.53 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 334.518 176.53 0)
		)
		(property "HelpURL" ""
			(at 336.423 176.53 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 338.328 176.53 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 340.233 176.53 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 342.138 176.53 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 344.043 176.53 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 345.948 176.53 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 347.853 176.53 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 349.758 176.53 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C512")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 344.17 179.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0730"
			(at 344.17 179.07 0)
		)
		(property "Value" "GND"
			(at 344.17 182.88 0)
		)
		(property "Footprint" ""
			(at 344.17 179.07 0)
		)
		(property "Datasheet" ""
			(at 344.17 179.07 0)
		)
		(property "Description" ""
			(at 344.17 179.07 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0730")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0603_120R_1%_0.2W_200PPM")
		(at 83.82 39.37 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R88"
			(at 86.36 34.2899 90)
		)
		(property "Value" "R0603_120R_1%_0.2W_200PPM"
			(at 88.773 39.37 0)
		)
		(property "Footprint" "Resistors SMD:RESC1608X55N"
			(at 90.678 39.37 0)
		)
		(property "Datasheet" ""
			(at 92.583 39.37 0)
		)
		(property "Description" "±1%"
			(at 86.36 35.56 90)
		)
		(property "Val" "120"
			(at 86.36 36.8299 90)
		)
		(property "Part Number" "R0603_120R_1%_0.2W_200PPM"
			(at 94.488 39.37 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 96.393 39.37 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 98.298 39.37 0)
		)
		(property "Comment" "120"
			(at 100.203 39.37 0)
		)
		(property "Component Kind" "Standard"
			(at 102.108 39.37 0)
		)
		(property "Component Type" "Standard"
			(at 104.013 39.37 0)
		)
		(property "PackageDescription" " "
			(at 105.918 39.37 0)
		)
		(property "Pin Count" "2"
			(at 107.823 39.37 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 109.728 39.37 0)
		)
		(property "Footprint Ref" "RESC1608X55N"
			(at 111.633 39.37 0)
		)
		(property "Status" "Preferred"
			(at 113.538 39.37 0)
		)
		(property "Power" "0.2W"
			(at 115.443 39.37 0)
		)
		(property "Voltage" " "
			(at 119.253 39.37 0)
		)
		(property "Tolerance" "±1%"
			(at 121.158 39.37 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 123.063 39.37 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 124.968 39.37 0)
		)
		(property "Manufacturer Part Number" "R0603_120R_1%_0.2W_200PPM"
			(at 126.873 39.37 0)
		)
		(property "Case" "0603"
			(at 128.778 39.37 0)
		)
		(property "PressFit" "No"
			(at 130.683 39.37 0)
		)
		(property "Mounted" "Yes"
			(at 132.588 39.37 0)
		)
		(property "Sense Comment" " "
			(at 134.493 39.37 0)
		)
		(property "Sense" "No"
			(at 136.398 39.37 0)
		)
		(property "Status Comment" " "
			(at 138.303 39.37 0)
		)
		(property "Socket" "No"
			(at 140.208 39.37 0)
		)
		(property "SMD" "Yes"
			(at 142.113 39.37 0)
		)
		(property "ComponentHeight" " "
			(at 144.018 39.37 0)
		)
		(property "Manufacturer1 Example" "TE CONNECTIVITY"
			(at 145.923 39.37 0)
		)
		(property "Manufacturer1 Part Number" "CRGH0603F120R"
			(at 147.828 39.37 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 149.733 39.37 0)
		)
		(property "HelpURL" ""
			(at 151.638 39.37 0)
		)
		(property "Author" "CERN DEM HF"
			(at 153.543 39.37 0)
		)
		(property "CreateDate" "02/24/23 00:00:00"
			(at 155.448 39.37 0)
		)
		(property "LatestRevisionDate" "02/24/23 00:00:00"
			(at 157.353 39.37 0)
		)
		(property "Database Table Name" "Resistors"
			(at 159.258 39.37 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 161.163 39.37 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 163.068 39.37 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 164.973 39.37 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R88")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Analog & Interface:MAX3430ESA")
		(at 53.34 30.48 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC26"
			(at 62.2935 25.4 0)
		)
		(property "Value" "MAX3430ESA"
			(at 62.2935 27.94 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOIC127P600X175-8N"
			(at 53.34 62.23 0)
		)
		(property "Datasheet" ""
			(at 53.34 64.135 0)
		)
		(property "Description" "MAX3430ESA"
			(at 53.34 66.04 0)
		)
		(property "Library Ref" "MAX3430"
			(at 53.34 67.945 0)
		)
		(property "Library Path" "SchLib\\Analog & Interface.SchLib"
			(at 53.34 69.85 0)
		)
		(property "Comment" "MAX3430ESA"
			(at 53.34 71.755 0)
		)
		(property "Component Kind" "Standard"
			(at 53.34 73.66 0)
		)
		(property "Component Type" "Standard"
			(at 53.34 75.565 0)
		)
		(property "Device" "MAX3430ESA"
			(at 53.34 77.47 0)
		)
		(property "PackageDescription" "SOIC, 1.27mm Pitch; 8 Pin, 3.90mm W X 4.90mm L X 1.75mm H body, IPC Medium Density"
			(at 53.34 79.375 0)
		)
		(property "Status" " "
			(at 53.34 81.28 0)
		)
		(property "Part Description" "±80V Fault-Protected, Fail-Safe, 1/4-Unit Load, +3.3V RS-485 Transceiver (-40°C to +85°C)"
			(at 53.34 83.185 0)
		)
		(property "Manufacturer" "MAXIM"
			(at 53.34 85.09 0)
		)
		(property "Manufacturer Part Number" "MAX3430ESA"
			(at 53.34 86.995 0)
		)
		(property "Pin Count" "8"
			(at 53.34 88.9 0)
		)
		(property "Case" "SOIC8"
			(at 53.34 90.805 0)
		)
		(property "Mounted" "Yes"
			(at 53.34 92.71 0)
		)
		(property "Socket" "No"
			(at 53.34 94.615 0)
		)
		(property "SMD" "Yes"
			(at 53.34 96.52 0)
		)
		(property "PressFit" "No"
			(at 53.34 98.425 0)
		)
		(property "Sense" "No"
			(at 53.34 100.33 0)
		)
		(property "Sense Comment" " "
			(at 53.34 102.235 0)
		)
		(property "Bonding" "No"
			(at 53.34 104.14 0)
		)
		(property "Status Comment" " "
			(at 53.34 106.045 0)
		)
		(property "ComponentHeight" "1.75mm"
			(at 53.34 107.95 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 53.34 109.855 0)
		)
		(property "Footprint Ref" "SOIC127P600X175-8N"
			(at 53.34 111.76 0)
		)
		(property "Author" "CERN DEM BC"
			(at 53.34 113.665 0)
		)
		(property "HelpURL" ""
			(at 53.34 115.57 0)
		)
		(property "ComponentLink1URL" " "
			(at 53.34 117.475 0)
		)
		(property "ComponentLink2URL" " "
			(at 53.34 119.38 0)
		)
		(property "ComponentLink2Description" " "
			(at 53.34 121.285 0)
		)
		(property "ComponentLink1Description" " "
			(at 53.34 123.19 0)
		)
		(property "CreateDate" "02/10/20 00:00:00"
			(at 53.34 125.095 0)
		)
		(property "LatestRevisionDate" "02/10/20 00:00:00"
			(at 53.34 127 0)
		)
		(property "SCEM" " "
			(at 53.34 128.905 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 53.34 130.81 0)
		)
		(property "Library Name" "Analog & Interface"
			(at 53.34 132.715 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 53.34 134.62 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 53.34 136.525 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(instances
			(project "vme-wren"
				(path
					(reference "IC26")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 269.24 176.53 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR01082"
			(at 269.24 176.53 0)
		)
		(property "Value" "GND"
			(at 269.24 180.34 0)
		)
		(property "Footprint" ""
			(at 269.24 176.53 0)
		)
		(property "Datasheet" ""
			(at 269.24 176.53 0)
		)
		(property "Description" ""
			(at 269.24 176.53 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR01082")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 31.75 104.14 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0331"
			(at 31.75 104.14 0)
		)
		(property "Value" "GND"
			(at 31.75 107.95 90)
		)
		(property "Footprint" ""
			(at 31.75 104.14 0)
		)
		(property "Datasheet" ""
			(at 31.75 104.14 0)
		)
		(property "Description" ""
			(at 31.75 104.14 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0331")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 60.96 229.87 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R104"
			(at 63.5 224.7899 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 65.913 229.87 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 67.818 229.87 0)
		)
		(property "Datasheet" ""
			(at 69.723 229.87 0)
		)
		(property "Description" "±1%"
			(at 55.88 226.06 0)
		)
		(property "Val" "10k"
			(at 63.5 227.3299 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 71.628 229.87 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 73.533 229.87 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 75.438 229.87 0)
		)
		(property "Comment" "10k"
			(at 77.343 229.87 0)
		)
		(property "Component Kind" "Standard"
			(at 79.248 229.87 0)
		)
		(property "Component Type" "Standard"
			(at 81.153 229.87 0)
		)
		(property "PackageDescription" " "
			(at 83.058 229.87 0)
		)
		(property "Pin Count" "2"
			(at 84.963 229.87 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 86.868 229.87 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 88.773 229.87 0)
		)
		(property "Status" "Not Recommended"
			(at 90.678 229.87 0)
		)
		(property "Power" "0.0625W"
			(at 92.583 229.87 0)
		)
		(property "Voltage" " "
			(at 96.393 229.87 0)
		)
		(property "Tolerance" "±1%"
			(at 98.298 229.87 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 100.203 229.87 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 102.108 229.87 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 104.013 229.87 0)
		)
		(property "Case" "0402"
			(at 105.918 229.87 0)
		)
		(property "PressFit" "No"
			(at 107.823 229.87 0)
		)
		(property "Mounted" "Yes"
			(at 109.728 229.87 0)
		)
		(property "Sense Comment" " "
			(at 111.633 229.87 0)
		)
		(property "Sense" "No"
			(at 113.538 229.87 0)
		)
		(property "Status Comment" " "
			(at 115.443 229.87 0)
		)
		(property "Socket" "No"
			(at 117.348 229.87 0)
		)
		(property "SMD" "Yes"
			(at 119.253 229.87 0)
		)
		(property "ComponentHeight" " "
			(at 121.158 229.87 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 123.063 229.87 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 124.968 229.87 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 126.873 229.87 0)
		)
		(property "HelpURL" ""
			(at 128.778 229.87 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 130.683 229.87 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 132.588 229.87 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 134.493 229.87 0)
		)
		(property "Database Table Name" "Resistors"
			(at 136.398 229.87 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 138.303 229.87 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 140.208 229.87 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 142.113 229.87 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R104")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 125.73 45.72 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0334"
			(at 125.73 45.72 0)
		)
		(property "Value" "GND"
			(at 125.73 49.53 0)
		)
		(property "Footprint" ""
			(at 125.73 45.72 0)
		)
		(property "Datasheet" ""
			(at 125.73 45.72 0)
		)
		(property "Description" ""
			(at 125.73 45.72 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0334")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 226.06 165.1 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C114"
			(at 229.87 160.0199 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 231.14 160.02 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 226.06 165.1 0)
		)
		(property "Datasheet" ""
			(at 226.06 165.1 0)
		)
		(property "Description" "100nF"
			(at 229.87 162.5599 90)
		)
		(property "SMD" "Yes"
			(at 225.552 167.386 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 237.998 165.1 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 239.903 165.1 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 241.808 165.1 0)
		)
		(property "Comment" "100nF"
			(at 243.713 165.1 0)
		)
		(property "Component Kind" "Standard"
			(at 245.618 165.1 0)
		)
		(property "Component Type" "Standard"
			(at 247.523 165.1 0)
		)
		(property "Pin Count" "2"
			(at 249.428 165.1 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 251.333 165.1 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 253.238 165.1 0)
		)
		(property "PackageDescription" " "
			(at 255.143 165.1 0)
		)
		(property "Status" "Not Recommended"
			(at 257.048 165.1 0)
		)
		(property "Status Comment" " "
			(at 258.953 165.1 0)
		)
		(property "Voltage" "16V"
			(at 260.858 165.1 0)
		)
		(property "Tolerance" "±10%"
			(at 264.668 165.1 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 266.573 165.1 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 268.478 165.1 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 270.383 165.1 0)
		)
		(property "Case" "0402"
			(at 272.288 165.1 0)
		)
		(property "Mounted" "Yes"
			(at 274.193 165.1 0)
		)
		(property "Socket" "No"
			(at 276.098 165.1 0)
		)
		(property "PressFit" " "
			(at 279.908 165.1 0)
		)
		(property "Sense" "No"
			(at 281.813 165.1 0)
		)
		(property "Sense Comment" " "
			(at 283.718 165.1 0)
		)
		(property "ComponentHeight" " "
			(at 285.623 165.1 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 287.528 165.1 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 289.433 165.1 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 291.338 165.1 0)
		)
		(property "HelpURL" ""
			(at 293.243 165.1 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 295.148 165.1 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 297.053 165.1 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 298.958 165.1 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 300.863 165.1 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 302.768 165.1 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 304.673 165.1 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 306.578 165.1 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C114")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 82.55 196.85 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0356"
			(at 82.55 196.85 0)
		)
		(property "Value" "GND"
			(at 82.55 200.66 0)
		)
		(property "Footprint" ""
			(at 82.55 196.85 0)
		)
		(property "Datasheet" ""
			(at 82.55 196.85 0)
		)
		(property "Description" ""
			(at 82.55 196.85 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0356")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 39.37 199.39 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R192"
			(at 41.91 194.3099 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 44.323 199.39 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 46.228 199.39 0)
		)
		(property "Datasheet" ""
			(at 48.133 199.39 0)
		)
		(property "Description" "±1%"
			(at 34.29 195.58 0)
		)
		(property "Val" "10k"
			(at 41.91 196.8499 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 50.038 199.39 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 51.943 199.39 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 53.848 199.39 0)
		)
		(property "Comment" "10k"
			(at 55.753 199.39 0)
		)
		(property "Component Kind" "Standard"
			(at 57.658 199.39 0)
		)
		(property "Component Type" "Standard"
			(at 59.563 199.39 0)
		)
		(property "PackageDescription" " "
			(at 61.468 199.39 0)
		)
		(property "Pin Count" "2"
			(at 63.373 199.39 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 65.278 199.39 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 67.183 199.39 0)
		)
		(property "Status" "Not Recommended"
			(at 69.088 199.39 0)
		)
		(property "Power" "0.0625W"
			(at 70.993 199.39 0)
		)
		(property "Voltage" " "
			(at 74.803 199.39 0)
		)
		(property "Tolerance" "±1%"
			(at 76.708 199.39 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 78.613 199.39 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 80.518 199.39 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 82.423 199.39 0)
		)
		(property "Case" "0402"
			(at 84.328 199.39 0)
		)
		(property "PressFit" "No"
			(at 86.233 199.39 0)
		)
		(property "Mounted" "Yes"
			(at 88.138 199.39 0)
		)
		(property "Sense Comment" " "
			(at 90.043 199.39 0)
		)
		(property "Sense" "No"
			(at 91.948 199.39 0)
		)
		(property "Status Comment" " "
			(at 93.853 199.39 0)
		)
		(property "Socket" "No"
			(at 95.758 199.39 0)
		)
		(property "SMD" "Yes"
			(at 97.663 199.39 0)
		)
		(property "ComponentHeight" " "
			(at 99.568 199.39 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 101.473 199.39 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 103.378 199.39 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 105.283 199.39 0)
		)
		(property "HelpURL" ""
			(at 107.188 199.39 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 109.093 199.39 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 110.998 199.39 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 112.903 199.39 0)
		)
		(property "Database Table Name" "Resistors"
			(at 114.808 199.39 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 116.713 199.39 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 118.618 199.39 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 120.523 199.39 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R192")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 31.75 69.85 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0346"
			(at 31.75 69.85 0)
		)
		(property "Value" "P3V3"
			(at 31.75 66.04 0)
		)
		(property "Footprint" ""
			(at 31.75 69.85 0)
		)
		(property "Datasheet" ""
			(at 31.75 69.85 0)
		)
		(property "Description" ""
			(at 31.75 69.85 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0346")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 52.07 161.29 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C222"
			(at 55.88 156.2099 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 57.15 156.21 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 52.07 161.29 0)
		)
		(property "Datasheet" ""
			(at 52.07 161.29 0)
		)
		(property "Description" "100nF"
			(at 55.88 158.7499 90)
		)
		(property "SMD" "Yes"
			(at 51.562 163.576 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 64.008 161.29 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 65.913 161.29 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 67.818 161.29 0)
		)
		(property "Comment" "100nF"
			(at 69.723 161.29 0)
		)
		(property "Component Kind" "Standard"
			(at 71.628 161.29 0)
		)
		(property "Component Type" "Standard"
			(at 73.533 161.29 0)
		)
		(property "Pin Count" "2"
			(at 75.438 161.29 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 77.343 161.29 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 79.248 161.29 0)
		)
		(property "PackageDescription" " "
			(at 81.153 161.29 0)
		)
		(property "Status" "Not Recommended"
			(at 83.058 161.29 0)
		)
		(property "Status Comment" " "
			(at 84.963 161.29 0)
		)
		(property "Voltage" "16V"
			(at 86.868 161.29 0)
		)
		(property "Tolerance" "±10%"
			(at 90.678 161.29 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 92.583 161.29 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 94.488 161.29 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 96.393 161.29 0)
		)
		(property "Case" "0402"
			(at 98.298 161.29 0)
		)
		(property "Mounted" "Yes"
			(at 100.203 161.29 0)
		)
		(property "Socket" "No"
			(at 102.108 161.29 0)
		)
		(property "PressFit" " "
			(at 105.918 161.29 0)
		)
		(property "Sense" "No"
			(at 107.823 161.29 0)
		)
		(property "Sense Comment" " "
			(at 109.728 161.29 0)
		)
		(property "ComponentHeight" " "
			(at 111.633 161.29 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 113.538 161.29 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 115.443 161.29 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 117.348 161.29 0)
		)
		(property "HelpURL" ""
			(at 119.253 161.29 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 121.158 161.29 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 123.063 161.29 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 124.968 161.29 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 126.873 161.29 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 128.778 161.29 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 130.683 161.29 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 132.588 161.29 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C222")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 60.96 220.98 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0341"
			(at 60.96 220.98 0)
		)
		(property "Value" "P3V3"
			(at 60.96 217.17 0)
		)
		(property "Footprint" ""
			(at 60.96 220.98 0)
		)
		(property "Datasheet" ""
			(at 60.96 220.98 0)
		)
		(property "Description" ""
			(at 60.96 220.98 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0341")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 114.3 45.72 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C215"
			(at 112.268 30.226 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 119.38 40.64 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 114.3 45.72 0)
		)
		(property "Datasheet" ""
			(at 114.3 45.72 0)
		)
		(property "Description" "100nF"
			(at 112.268 27.686 90)
		)
		(property "SMD" "Yes"
			(at 113.792 48.006 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 126.238 45.72 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 128.143 45.72 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 130.048 45.72 0)
		)
		(property "Comment" "100nF"
			(at 131.953 45.72 0)
		)
		(property "Component Kind" "Standard"
			(at 133.858 45.72 0)
		)
		(property "Component Type" "Standard"
			(at 135.763 45.72 0)
		)
		(property "Pin Count" "2"
			(at 137.668 45.72 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 139.573 45.72 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 141.478 45.72 0)
		)
		(property "PackageDescription" " "
			(at 143.383 45.72 0)
		)
		(property "Status" "Not Recommended"
			(at 145.288 45.72 0)
		)
		(property "Status Comment" " "
			(at 147.193 45.72 0)
		)
		(property "Voltage" "16V"
			(at 149.098 45.72 0)
		)
		(property "Tolerance" "±10%"
			(at 152.908 45.72 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 154.813 45.72 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 156.718 45.72 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 158.623 45.72 0)
		)
		(property "Case" "0402"
			(at 160.528 45.72 0)
		)
		(property "Mounted" "Yes"
			(at 162.433 45.72 0)
		)
		(property "Socket" "No"
			(at 164.338 45.72 0)
		)
		(property "PressFit" " "
			(at 168.148 45.72 0)
		)
		(property "Sense" "No"
			(at 170.053 45.72 0)
		)
		(property "Sense Comment" " "
			(at 171.958 45.72 0)
		)
		(property "ComponentHeight" " "
			(at 173.863 45.72 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 175.768 45.72 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 177.673 45.72 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 179.578 45.72 0)
		)
		(property "HelpURL" ""
			(at 181.483 45.72 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 183.388 45.72 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 185.293 45.72 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 187.198 45.72 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 189.103 45.72 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 191.008 45.72 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 192.913 45.72 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 194.818 45.72 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C215")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 127 266.7 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0343"
			(at 127 266.7 0)
		)
		(property "Value" "GND"
			(at 127 270.51 0)
		)
		(property "Footprint" ""
			(at 127 266.7 0)
		)
		(property "Datasheet" ""
			(at 127 266.7 0)
		)
		(property "Description" ""
			(at 127 266.7 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0343")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 386.08 180.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0731"
			(at 386.08 180.34 0)
		)
		(property "Value" "GND"
			(at 386.08 184.15 0)
		)
		(property "Footprint" ""
			(at 386.08 180.34 0)
		)
		(property "Datasheet" ""
			(at 386.08 180.34 0)
		)
		(property "Description" ""
			(at 386.08 180.34 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0731")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 54.61 266.7 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C217"
			(at 58.42 261.6199 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 59.69 261.62 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 54.61 266.7 0)
		)
		(property "Datasheet" ""
			(at 54.61 266.7 0)
		)
		(property "Description" "100nF"
			(at 58.42 264.1599 90)
		)
		(property "SMD" "Yes"
			(at 54.102 268.986 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 66.548 266.7 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 68.453 266.7 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 70.358 266.7 0)
		)
		(property "Comment" "100nF"
			(at 72.263 266.7 0)
		)
		(property "Component Kind" "Standard"
			(at 74.168 266.7 0)
		)
		(property "Component Type" "Standard"
			(at 76.073 266.7 0)
		)
		(property "Pin Count" "2"
			(at 77.978 266.7 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 79.883 266.7 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 81.788 266.7 0)
		)
		(property "PackageDescription" " "
			(at 83.693 266.7 0)
		)
		(property "Status" "Not Recommended"
			(at 85.598 266.7 0)
		)
		(property "Status Comment" " "
			(at 87.503 266.7 0)
		)
		(property "Voltage" "16V"
			(at 89.408 266.7 0)
		)
		(property "Tolerance" "±10%"
			(at 93.218 266.7 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 95.123 266.7 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 97.028 266.7 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 98.933 266.7 0)
		)
		(property "Case" "0402"
			(at 100.838 266.7 0)
		)
		(property "Mounted" "Yes"
			(at 102.743 266.7 0)
		)
		(property "Socket" "No"
			(at 104.648 266.7 0)
		)
		(property "PressFit" " "
			(at 108.458 266.7 0)
		)
		(property "Sense" "No"
			(at 110.363 266.7 0)
		)
		(property "Sense Comment" " "
			(at 112.268 266.7 0)
		)
		(property "ComponentHeight" " "
			(at 114.173 266.7 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 116.078 266.7 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 117.983 266.7 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 119.888 266.7 0)
		)
		(property "HelpURL" ""
			(at 121.793 266.7 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 123.698 266.7 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 125.603 266.7 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 127.508 266.7 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 129.413 266.7 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 131.318 266.7 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 133.223 266.7 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 135.128 266.7 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C217")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_33R_1%_0.0625W_100PPM")
		(at 176.53 278.13 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R399"
			(at 178.816 275.082 0)
		)
		(property "Value" "R0402_33R_1%_0.0625W_100PPM"
			(at 176.53 283.083 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 176.53 284.988 0)
		)
		(property "Datasheet" ""
			(at 176.53 286.893 0)
		)
		(property "Description" "±1%"
			(at 180.34 273.05 0)
		)
		(property "Val" "33"
			(at 183.642 275.082 0)
		)
		(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 176.53 288.798 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 176.53 290.703 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 176.53 292.608 0)
		)
		(property "Comment" "33"
			(at 176.53 294.513 0)
		)
		(property "Component Kind" "Standard"
			(at 176.53 296.418 0)
		)
		(property "Component Type" "Standard"
			(at 176.53 298.323 0)
		)
		(property "PackageDescription" " "
			(at 176.53 300.228 0)
		)
		(property "Pin Count" "2"
			(at 176.53 302.133 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 176.53 304.038 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 176.53 305.943 0)
		)
		(property "Status" "Not Recommended"
			(at 176.53 307.848 0)
		)
		(property "Power" "0.0625W"
			(at 176.53 309.753 0)
		)
		(property "Voltage" " "
			(at 176.53 313.563 0)
		)
		(property "Tolerance" "±1%"
			(at 176.53 315.468 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 176.53 317.373 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 176.53 319.278 0)
		)
		(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 176.53 321.183 0)
		)
		(property "Case" "0402"
			(at 176.53 323.088 0)
		)
		(property "PressFit" "No"
			(at 176.53 324.993 0)
		)
		(property "Mounted" "Yes"
			(at 176.53 326.898 0)
		)
		(property "Sense Comment" " "
			(at 176.53 328.803 0)
		)
		(property "Sense" "No"
			(at 176.53 330.708 0)
		)
		(property "Status Comment" " "
			(at 176.53 332.613 0)
		)
		(property "Socket" "No"
			(at 176.53 334.518 0)
		)
		(property "SMD" "Yes"
			(at 176.53 336.423 0)
		)
		(property "ComponentHeight" " "
			(at 176.53 338.328 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 176.53 340.233 0)
		)
		(property "Manufacturer1 Part Number" "232270673309L"
			(at 176.53 342.138 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 176.53 344.043 0)
		)
		(property "HelpURL" ""
			(at 176.53 345.948 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 176.53 347.853 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 176.53 349.758 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 176.53 351.663 0)
		)
		(property "Database Table Name" "Resistors"
			(at 176.53 353.568 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 176.53 355.473 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 176.53 357.378 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 176.53 359.283 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R399")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 344.17 232.41 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0726"
			(at 344.17 232.41 0)
		)
		(property "Value" "GND"
			(at 344.17 236.22 0)
		)
		(property "Footprint" ""
			(at 344.17 232.41 0)
		)
		(property "Datasheet" ""
			(at 344.17 232.41 0)
		)
		(property "Description" ""
			(at 344.17 232.41 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0726")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 165.1 213.36 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C392"
			(at 168.91 208.2799 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 170.18 208.28 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 165.1 213.36 0)
		)
		(property "Datasheet" ""
			(at 165.1 213.36 0)
		)
		(property "Description" "100nF"
			(at 168.91 210.8199 90)
		)
		(property "SMD" "Yes"
			(at 164.592 215.646 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 177.038 213.36 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 178.943 213.36 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 180.848 213.36 0)
		)
		(property "Comment" "100nF"
			(at 182.753 213.36 0)
		)
		(property "Component Kind" "Standard"
			(at 184.658 213.36 0)
		)
		(property "Component Type" "Standard"
			(at 186.563 213.36 0)
		)
		(property "Pin Count" "2"
			(at 188.468 213.36 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 190.373 213.36 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 192.278 213.36 0)
		)
		(property "PackageDescription" " "
			(at 194.183 213.36 0)
		)
		(property "Status" "Not Recommended"
			(at 196.088 213.36 0)
		)
		(property "Status Comment" " "
			(at 197.993 213.36 0)
		)
		(property "Voltage" "16V"
			(at 199.898 213.36 0)
		)
		(property "Tolerance" "±10%"
			(at 203.708 213.36 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 205.613 213.36 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 207.518 213.36 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 209.423 213.36 0)
		)
		(property "Case" "0402"
			(at 211.328 213.36 0)
		)
		(property "Mounted" "Yes"
			(at 213.233 213.36 0)
		)
		(property "Socket" "No"
			(at 215.138 213.36 0)
		)
		(property "PressFit" " "
			(at 218.948 213.36 0)
		)
		(property "Sense" "No"
			(at 220.853 213.36 0)
		)
		(property "Sense Comment" " "
			(at 222.758 213.36 0)
		)
		(property "ComponentHeight" " "
			(at 224.663 213.36 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 226.568 213.36 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 228.473 213.36 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 230.378 213.36 0)
		)
		(property "HelpURL" ""
			(at 232.283 213.36 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 234.188 213.36 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 236.093 213.36 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 237.998 213.36 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 239.903 213.36 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 241.808 213.36 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 243.713 213.36 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 245.618 213.36 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C392")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Analog & Interface:DS90LV027AQMA_NOPB")
		(at 173.99 182.88 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC67"
			(at 181.61 210.82 0)
		)
		(property "Value" "DS90LV027AQMA_NOPB"
			(at 181.61 213.36 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOIC127P600X175-8N"
			(at 173.99 214.63 0)
		)
		(property "Datasheet" ""
			(at 173.99 216.535 0)
		)
		(property "Description" "DS90LV027AQMA_NOPB"
			(at 173.99 218.44 0)
		)
		(property "Library Ref" "DS90LV027AQ"
			(at 173.99 220.345 0)
		)
		(property "Library Path" "SchLib\\Analog & Interface.SchLib"
			(at 173.99 222.25 0)
		)
		(property "Comment" "DS90LV027AQMA/NOPB"
			(at 173.99 224.155 0)
		)
		(property "Component Kind" "Standard"
			(at 173.99 226.06 0)
		)
		(property "Component Type" "Standard"
			(at 173.99 227.965 0)
		)
		(property "Device" "DS90LV027AQMA/NOPB"
			(at 173.99 229.87 0)
		)
		(property "PackageDescription" "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density"
			(at 173.99 231.775 0)
		)
		(property "Status" " "
			(at 173.99 233.68 0)
		)
		(property "Part Description" "Automotive LVDS Dual Differential Driver"
			(at 173.99 235.585 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 173.99 237.49 0)
		)
		(property "Manufacturer Part Number" "DS90LV027AQMA"
			(at 173.99 239.395 0)
		)
		(property "Pin Count" "8"
			(at 173.99 241.3 0)
		)
		(property "Case" "SOIC8"
			(at 173.99 243.205 0)
		)
		(property "Mounted" "Yes"
			(at 173.99 245.11 0)
		)
		(property "Socket" "No"
			(at 173.99 247.015 0)
		)
		(property "SMD" "Yes"
			(at 173.99 248.92 0)
		)
		(property "PressFit" "No"
			(at 173.99 250.825 0)
		)
		(property "Sense" "No"
			(at 173.99 252.73 0)
		)
		(property "Sense Comment" " "
			(at 173.99 254.635 0)
		)
		(property "Bonding" "No"
			(at 173.99 256.54 0)
		)
		(property "Status Comment" " "
			(at 173.99 258.445 0)
		)
		(property "ComponentHeight" "1.75mm"
			(at 173.99 260.35 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 173.99 262.255 0)
		)
		(property "Footprint Ref" "SOIC127P600X175-8N"
			(at 173.99 264.16 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 173.99 266.065 0)
		)
		(property "HelpURL" ""
			(at 173.99 267.97 0)
		)
		(property "ComponentLink1URL" " "
			(at 173.99 269.875 0)
		)
		(property "ComponentLink2URL" " "
			(at 173.99 271.78 0)
		)
		(property "ComponentLink2Description" " "
			(at 173.99 273.685 0)
		)
		(property "ComponentLink1Description" " "
			(at 173.99 275.59 0)
		)
		(property "CreateDate" "01/11/17 00:00:00"
			(at 173.99 277.495 0)
		)
		(property "LatestRevisionDate" "06/01/22 00:00:00"
			(at 173.99 279.4 0)
		)
		(property "SCEM" " "
			(at 173.99 281.305 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 173.99 283.21 0)
		)
		(property "Library Name" "Analog & Interface"
			(at 173.99 285.115 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 173.99 287.02 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 173.99 288.925 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(instances
			(project "vme-wren"
				(path
					(reference "IC67")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 39.37 200.66 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0352"
			(at 39.37 200.66 0)
		)
		(property "Value" "GND"
			(at 39.37 204.47 90)
		)
		(property "Footprint" ""
			(at 39.37 200.66 0)
		)
		(property "Datasheet" ""
			(at 39.37 200.66 0)
		)
		(property "Description" ""
			(at 39.37 200.66 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0352")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 54.61 256.54 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0337"
			(at 54.61 256.54 0)
		)
		(property "Value" "P3V3"
			(at 54.61 252.73 0)
		)
		(property "Footprint" ""
			(at 54.61 256.54 0)
		)
		(property "Datasheet" ""
			(at 54.61 256.54 0)
		)
		(property "Description" ""
			(at 54.61 256.54 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0337")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Standard Logic:SN74LV595ARGYR")
		(at 213.36 228.6 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC63"
			(at 223.52 264.16 0)
		)
		(property "Value" "SN74LV595ARGYR"
			(at 223.52 266.7 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:TEXAS_RGY (R-PVQFN-N16)"
			(at 213.36 267.97 0)
		)
		(property "Datasheet" ""
			(at 213.36 269.875 0)
		)
		(property "Description" "SN74LV595ARGYR"
			(at 213.36 271.78 0)
		)
		(property "Library Ref" "74595_a"
			(at 213.36 273.685 0)
		)
		(property "Library Path" "SchLib\\Standard Logic.SchLib"
			(at 213.36 275.59 0)
		)
		(property "Comment" "SN74LV595ARGY"
			(at 213.36 277.495 0)
		)
		(property "Component Kind" "Standard"
			(at 213.36 279.4 0)
		)
		(property "Component Type" "Standard"
			(at 213.36 281.305 0)
		)
		(property "Device" "SN74LV595ARGY"
			(at 213.36 283.21 0)
		)
		(property "PackageDescription" "TEXAS Case Style RGY (R-PVQFN-N16), QFN, 0.50mm Pitch, Rect.; 16 Pin, 4.00mm L X 3.50mm W X 1mm H body (w/Thermal Tab 2.65 X 2.15mm)"
			(at 213.36 285.115 0)
		)
		(property "Status" " "
			(at 213.36 287.02 0)
		)
		(property "Part Description" "8-Bit Shift Register with 3-State Output Registers"
			(at 213.36 288.925 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 213.36 290.83 0)
		)
		(property "Manufacturer Part Number" "SN74LV595ARGY"
			(at 213.36 292.735 0)
		)
		(property "Pin Count" "17"
			(at 213.36 294.64 0)
		)
		(property "Case" "QFN16"
			(at 213.36 296.545 0)
		)
		(property "Mounted" "Yes"
			(at 213.36 298.45 0)
		)
		(property "Socket" "No"
			(at 213.36 300.355 0)
		)
		(property "SMD" "Yes"
			(at 213.36 302.26 0)
		)
		(property "PressFit" "No"
			(at 213.36 304.165 0)
		)
		(property "Sense" "No"
			(at 213.36 306.07 0)
		)
		(property "Sense Comment" " "
			(at 213.36 307.975 0)
		)
		(property "Bonding" "No"
			(at 213.36 309.88 0)
		)
		(property "Status Comment" " "
			(at 213.36 311.785 0)
		)
		(property "ComponentHeight" "1mm"
			(at 213.36 313.69 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 213.36 315.595 0)
		)
		(property "Footprint Ref" "TEXAS_RGY (R-PVQFN-N16)"
			(at 213.36 317.5 0)
		)
		(property "Author" "CERN DEM MR"
			(at 213.36 319.405 0)
		)
		(property "HelpURL" ""
			(at 213.36 321.31 0)
		)
		(property "ComponentLink1URL" " "
			(at 213.36 323.215 0)
		)
		(property "ComponentLink1Description" " "
			(at 213.36 325.12 0)
		)
		(property "ComponentLink2URL" " "
			(at 213.36 327.025 0)
		)
		(property "ComponentLink2Description" " "
			(at 213.36 328.93 0)
		)
		(property "CreateDate" "10/10/17 00:00:00"
			(at 213.36 330.835 0)
		)
		(property "LatestRevisionDate" "10/10/17 00:00:00"
			(at 213.36 332.74 0)
		)
		(property "SCEM" " "
			(at 213.36 334.645 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 213.36 336.55 0)
		)
		(property "Library Name" "Standard Logic"
			(at 213.36 338.455 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 213.36 340.36 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 213.36 342.265 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC63")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 344.17 179.07 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C391"
			(at 347.98 173.9899 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 349.25 173.99 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 344.17 179.07 0)
		)
		(property "Datasheet" ""
			(at 344.17 179.07 0)
		)
		(property "Description" "100nF"
			(at 347.98 176.5299 90)
		)
		(property "SMD" "Yes"
			(at 343.662 181.356 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 356.108 179.07 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 358.013 179.07 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 359.918 179.07 0)
		)
		(property "Comment" "100nF"
			(at 361.823 179.07 0)
		)
		(property "Component Kind" "Standard"
			(at 363.728 179.07 0)
		)
		(property "Component Type" "Standard"
			(at 365.633 179.07 0)
		)
		(property "Pin Count" "2"
			(at 367.538 179.07 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 369.443 179.07 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 371.348 179.07 0)
		)
		(property "PackageDescription" " "
			(at 373.253 179.07 0)
		)
		(property "Status" "Not Recommended"
			(at 375.158 179.07 0)
		)
		(property "Status Comment" " "
			(at 377.063 179.07 0)
		)
		(property "Voltage" "16V"
			(at 378.968 179.07 0)
		)
		(property "Tolerance" "±10%"
			(at 382.778 179.07 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 384.683 179.07 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 386.588 179.07 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 388.493 179.07 0)
		)
		(property "Case" "0402"
			(at 390.398 179.07 0)
		)
		(property "Mounted" "Yes"
			(at 392.303 179.07 0)
		)
		(property "Socket" "No"
			(at 394.208 179.07 0)
		)
		(property "PressFit" " "
			(at 398.018 179.07 0)
		)
		(property "Sense" "No"
			(at 399.923 179.07 0)
		)
		(property "Sense Comment" " "
			(at 401.828 179.07 0)
		)
		(property "ComponentHeight" " "
			(at 403.733 179.07 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 405.638 179.07 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 407.543 179.07 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 409.448 179.07 0)
		)
		(property "HelpURL" ""
			(at 411.353 179.07 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 413.258 179.07 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 415.163 179.07 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 417.068 179.07 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 418.973 179.07 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 420.878 179.07 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 422.783 179.07 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 424.688 179.07 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C391")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 31.75 199.39 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R126"
			(at 34.29 194.3099 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 36.703 199.39 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 38.608 199.39 0)
		)
		(property "Datasheet" ""
			(at 40.513 199.39 0)
		)
		(property "Description" "±1%"
			(at 26.67 195.58 0)
		)
		(property "Val" "10k"
			(at 34.29 196.8499 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 42.418 199.39 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 44.323 199.39 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 46.228 199.39 0)
		)
		(property "Comment" "10k"
			(at 48.133 199.39 0)
		)
		(property "Component Kind" "Standard"
			(at 50.038 199.39 0)
		)
		(property "Component Type" "Standard"
			(at 51.943 199.39 0)
		)
		(property "PackageDescription" " "
			(at 53.848 199.39 0)
		)
		(property "Pin Count" "2"
			(at 55.753 199.39 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 57.658 199.39 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 59.563 199.39 0)
		)
		(property "Status" "Not Recommended"
			(at 61.468 199.39 0)
		)
		(property "Power" "0.0625W"
			(at 63.373 199.39 0)
		)
		(property "Voltage" " "
			(at 67.183 199.39 0)
		)
		(property "Tolerance" "±1%"
			(at 69.088 199.39 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 70.993 199.39 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 72.898 199.39 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 74.803 199.39 0)
		)
		(property "Case" "0402"
			(at 76.708 199.39 0)
		)
		(property "PressFit" "No"
			(at 78.613 199.39 0)
		)
		(property "Mounted" "Yes"
			(at 80.518 199.39 0)
		)
		(property "Sense Comment" " "
			(at 82.423 199.39 0)
		)
		(property "Sense" "No"
			(at 84.328 199.39 0)
		)
		(property "Status Comment" " "
			(at 86.233 199.39 0)
		)
		(property "Socket" "No"
			(at 88.138 199.39 0)
		)
		(property "SMD" "Yes"
			(at 90.043 199.39 0)
		)
		(property "ComponentHeight" " "
			(at 91.948 199.39 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 93.853 199.39 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 95.758 199.39 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 97.663 199.39 0)
		)
		(property "HelpURL" ""
			(at 99.568 199.39 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 101.473 199.39 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 103.378 199.39 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 105.283 199.39 0)
		)
		(property "Database Table Name" "Resistors"
			(at 107.188 199.39 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 109.093 199.39 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 110.998 199.39 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 112.903 199.39 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R126")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 270.51 233.68 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0724"
			(at 270.51 233.68 0)
		)
		(property "Value" "GND"
			(at 270.51 237.49 0)
		)
		(property "Footprint" ""
			(at 270.51 233.68 0)
		)
		(property "Datasheet" ""
			(at 270.51 233.68 0)
		)
		(property "Description" ""
			(at 270.51 233.68 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0724")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 140.97 187.96 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R265"
			(at 137.16 181.61 0)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 140.97 183.007 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 140.97 181.102 0)
		)
		(property "Datasheet" ""
			(at 140.97 179.197 0)
		)
		(property "Description" "±1%"
			(at 137.16 193.04 0)
		)
		(property "Val" "10k"
			(at 137.16 184.15 0)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 140.97 177.292 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 140.97 175.387 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 140.97 173.482 0)
		)
		(property "Comment" "10k"
			(at 140.97 171.577 0)
		)
		(property "Component Kind" "Standard"
			(at 140.97 169.672 0)
		)
		(property "Component Type" "Standard"
			(at 140.97 167.767 0)
		)
		(property "PackageDescription" " "
			(at 140.97 165.862 0)
		)
		(property "Pin Count" "2"
			(at 140.97 163.957 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 140.97 162.052 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 140.97 160.147 0)
		)
		(property "Status" "Not Recommended"
			(at 140.97 158.242 0)
		)
		(property "Power" "0.0625W"
			(at 140.97 156.337 0)
		)
		(property "Voltage" " "
			(at 140.97 152.527 0)
		)
		(property "Tolerance" "±1%"
			(at 140.97 150.622 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 140.97 148.717 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 140.97 146.812 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 140.97 144.907 0)
		)
		(property "Case" "0402"
			(at 140.97 143.002 0)
		)
		(property "PressFit" "No"
			(at 140.97 141.097 0)
		)
		(property "Mounted" "Yes"
			(at 140.97 139.192 0)
		)
		(property "Sense Comment" " "
			(at 140.97 137.287 0)
		)
		(property "Sense" "No"
			(at 140.97 135.382 0)
		)
		(property "Status Comment" " "
			(at 140.97 133.477 0)
		)
		(property "Socket" "No"
			(at 140.97 131.572 0)
		)
		(property "SMD" "Yes"
			(at 140.97 129.667 0)
		)
		(property "ComponentHeight" " "
			(at 140.97 127.762 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 140.97 125.857 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 140.97 123.952 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 140.97 122.047 0)
		)
		(property "HelpURL" ""
			(at 140.97 120.142 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 140.97 118.237 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 140.97 116.332 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 140.97 114.427 0)
		)
		(property "Database Table Name" "Resistors"
			(at 140.97 112.522 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 140.97 110.617 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 140.97 108.712 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 140.97 106.807 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R265")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Analog & Interface:DS90LV027AQMA_NOPB")
		(at 60.96 170.18 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC58"
			(at 68.58 165.1 0)
		)
		(property "Value" "DS90LV027AQMA_NOPB"
			(at 68.58 167.64 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOIC127P600X175-8N"
			(at 60.96 201.93 0)
		)
		(property "Datasheet" ""
			(at 60.96 203.835 0)
		)
		(property "Description" "DS90LV027AQMA_NOPB"
			(at 60.96 205.74 0)
		)
		(property "Library Ref" "DS90LV027AQ"
			(at 60.96 207.645 0)
		)
		(property "Library Path" "SchLib\\Analog & Interface.SchLib"
			(at 60.96 209.55 0)
		)
		(property "Comment" "DS90LV027AQMA/NOPB"
			(at 60.96 211.455 0)
		)
		(property "Component Kind" "Standard"
			(at 60.96 213.36 0)
		)
		(property "Component Type" "Standard"
			(at 60.96 215.265 0)
		)
		(property "Device" "DS90LV027AQMA/NOPB"
			(at 60.96 217.17 0)
		)
		(property "PackageDescription" "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density"
			(at 60.96 219.075 0)
		)
		(property "Status" " "
			(at 60.96 220.98 0)
		)
		(property "Part Description" "Automotive LVDS Dual Differential Driver"
			(at 60.96 222.885 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 60.96 224.79 0)
		)
		(property "Manufacturer Part Number" "DS90LV027AQMA"
			(at 60.96 226.695 0)
		)
		(property "Pin Count" "8"
			(at 60.96 228.6 0)
		)
		(property "Case" "SOIC8"
			(at 60.96 230.505 0)
		)
		(property "Mounted" "Yes"
			(at 60.96 232.41 0)
		)
		(property "Socket" "No"
			(at 60.96 234.315 0)
		)
		(property "SMD" "Yes"
			(at 60.96 236.22 0)
		)
		(property "PressFit" "No"
			(at 60.96 238.125 0)
		)
		(property "Sense" "No"
			(at 60.96 240.03 0)
		)
		(property "Sense Comment" " "
			(at 60.96 241.935 0)
		)
		(property "Bonding" "No"
			(at 60.96 243.84 0)
		)
		(property "Status Comment" " "
			(at 60.96 245.745 0)
		)
		(property "ComponentHeight" "1.75mm"
			(at 60.96 247.65 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 60.96 249.555 0)
		)
		(property "Footprint Ref" "SOIC127P600X175-8N"
			(at 60.96 251.46 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 60.96 253.365 0)
		)
		(property "HelpURL" ""
			(at 60.96 255.27 0)
		)
		(property "ComponentLink1URL" " "
			(at 60.96 257.175 0)
		)
		(property "ComponentLink2URL" " "
			(at 60.96 259.08 0)
		)
		(property "ComponentLink2Description" " "
			(at 60.96 260.985 0)
		)
		(property "ComponentLink1Description" " "
			(at 60.96 262.89 0)
		)
		(property "CreateDate" "01/11/17 00:00:00"
			(at 60.96 264.795 0)
		)
		(property "LatestRevisionDate" "06/01/22 00:00:00"
			(at 60.96 266.7 0)
		)
		(property "SCEM" " "
			(at 60.96 268.605 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 60.96 270.51 0)
		)
		(property "Library Name" "Analog & Interface"
			(at 60.96 272.415 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 60.96 274.32 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 60.96 276.225 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(instances
			(project "vme-wren"
				(path
					(reference "IC58")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 386.08 233.68 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0728"
			(at 386.08 233.68 0)
		)
		(property "Value" "GND"
			(at 386.08 237.49 0)
		)
		(property "Footprint" ""
			(at 386.08 233.68 0)
		)
		(property "Datasheet" ""
			(at 386.08 233.68 0)
		)
		(property "Description" ""
			(at 386.08 233.68 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0728")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_33R_1%_0.0625W_100PPM")
		(at 97.79 278.13 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R396"
			(at 100.076 275.082 0)
		)
		(property "Value" "R0402_33R_1%_0.0625W_100PPM"
			(at 97.79 283.083 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 97.79 284.988 0)
		)
		(property "Datasheet" ""
			(at 97.79 286.893 0)
		)
		(property "Description" "±1%"
			(at 101.6 273.05 0)
		)
		(property "Val" "33"
			(at 104.902 275.082 0)
		)
		(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 97.79 288.798 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 97.79 290.703 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 97.79 292.608 0)
		)
		(property "Comment" "33"
			(at 97.79 294.513 0)
		)
		(property "Component Kind" "Standard"
			(at 97.79 296.418 0)
		)
		(property "Component Type" "Standard"
			(at 97.79 298.323 0)
		)
		(property "PackageDescription" " "
			(at 97.79 300.228 0)
		)
		(property "Pin Count" "2"
			(at 97.79 302.133 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 97.79 304.038 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 97.79 305.943 0)
		)
		(property "Status" "Not Recommended"
			(at 97.79 307.848 0)
		)
		(property "Power" "0.0625W"
			(at 97.79 309.753 0)
		)
		(property "Voltage" " "
			(at 97.79 313.563 0)
		)
		(property "Tolerance" "±1%"
			(at 97.79 315.468 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 97.79 317.373 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 97.79 319.278 0)
		)
		(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 97.79 321.183 0)
		)
		(property "Case" "0402"
			(at 97.79 323.088 0)
		)
		(property "PressFit" "No"
			(at 97.79 324.993 0)
		)
		(property "Mounted" "Yes"
			(at 97.79 326.898 0)
		)
		(property "Sense Comment" " "
			(at 97.79 328.803 0)
		)
		(property "Sense" "No"
			(at 97.79 330.708 0)
		)
		(property "Status Comment" " "
			(at 97.79 332.613 0)
		)
		(property "Socket" "No"
			(at 97.79 334.518 0)
		)
		(property "SMD" "Yes"
			(at 97.79 336.423 0)
		)
		(property "ComponentHeight" " "
			(at 97.79 338.328 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 97.79 340.233 0)
		)
		(property "Manufacturer1 Part Number" "232270673309L"
			(at 97.79 342.138 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 97.79 344.043 0)
		)
		(property "HelpURL" ""
			(at 97.79 345.948 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 97.79 347.853 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 97.79 349.758 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 97.79 351.663 0)
		)
		(property "Database Table Name" "Resistors"
			(at 97.79 353.568 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 97.79 355.473 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 97.79 357.378 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 97.79 359.283 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R396")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 48.26 193.04 270)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0354"
			(at 48.26 193.04 0)
		)
		(property "Value" "P3V3"
			(at 48.768 191.77 90)
		)
		(property "Footprint" ""
			(at 48.26 193.04 0)
		)
		(property "Datasheet" ""
			(at 48.26 193.04 0)
		)
		(property "Description" ""
			(at 48.26 193.04 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0354")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 96.52 267.97 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0339"
			(at 96.52 267.97 0)
		)
		(property "Value" "GND"
			(at 96.52 271.78 0)
		)
		(property "Footprint" ""
			(at 96.52 267.97 0)
		)
		(property "Datasheet" ""
			(at 96.52 267.97 0)
		)
		(property "Description" ""
			(at 96.52 267.97 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0339")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Standard Logic:SN74LV595ARGYR")
		(at 356.87 142.24 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC66"
			(at 367.03 137.16 0)
		)
		(property "Value" "SN74LV595ARGYR"
			(at 367.03 139.7 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:TEXAS_RGY (R-PVQFN-N16)"
			(at 356.87 181.61 0)
		)
		(property "Datasheet" ""
			(at 356.87 183.515 0)
		)
		(property "Description" "SN74LV595ARGYR"
			(at 356.87 185.42 0)
		)
		(property "Library Ref" "74595_a"
			(at 356.87 187.325 0)
		)
		(property "Library Path" "SchLib\\Standard Logic.SchLib"
			(at 356.87 189.23 0)
		)
		(property "Comment" "SN74LV595ARGY"
			(at 356.87 191.135 0)
		)
		(property "Component Kind" "Standard"
			(at 356.87 193.04 0)
		)
		(property "Component Type" "Standard"
			(at 356.87 194.945 0)
		)
		(property "Device" "SN74LV595ARGY"
			(at 356.87 196.85 0)
		)
		(property "PackageDescription" "TEXAS Case Style RGY (R-PVQFN-N16), QFN, 0.50mm Pitch, Rect.; 16 Pin, 4.00mm L X 3.50mm W X 1mm H body (w/Thermal Tab 2.65 X 2.15mm)"
			(at 356.87 198.755 0)
		)
		(property "Status" " "
			(at 356.87 200.66 0)
		)
		(property "Part Description" "8-Bit Shift Register with 3-State Output Registers"
			(at 356.87 202.565 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 356.87 204.47 0)
		)
		(property "Manufacturer Part Number" "SN74LV595ARGY"
			(at 356.87 206.375 0)
		)
		(property "Pin Count" "17"
			(at 356.87 208.28 0)
		)
		(property "Case" "QFN16"
			(at 356.87 210.185 0)
		)
		(property "Mounted" "Yes"
			(at 356.87 212.09 0)
		)
		(property "Socket" "No"
			(at 356.87 213.995 0)
		)
		(property "SMD" "Yes"
			(at 356.87 215.9 0)
		)
		(property "PressFit" "No"
			(at 356.87 217.805 0)
		)
		(property "Sense" "No"
			(at 356.87 219.71 0)
		)
		(property "Sense Comment" " "
			(at 356.87 221.615 0)
		)
		(property "Bonding" "No"
			(at 356.87 223.52 0)
		)
		(property "Status Comment" " "
			(at 356.87 225.425 0)
		)
		(property "ComponentHeight" "1mm"
			(at 356.87 227.33 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 356.87 229.235 0)
		)
		(property "Footprint Ref" "TEXAS_RGY (R-PVQFN-N16)"
			(at 356.87 231.14 0)
		)
		(property "Author" "CERN DEM MR"
			(at 356.87 233.045 0)
		)
		(property "HelpURL" ""
			(at 356.87 234.95 0)
		)
		(property "ComponentLink1URL" " "
			(at 356.87 236.855 0)
		)
		(property "ComponentLink1Description" " "
			(at 356.87 238.76 0)
		)
		(property "ComponentLink2URL" " "
			(at 356.87 240.665 0)
		)
		(property "ComponentLink2Description" " "
			(at 356.87 242.57 0)
		)
		(property "CreateDate" "10/10/17 00:00:00"
			(at 356.87 244.475 0)
		)
		(property "LatestRevisionDate" "10/10/17 00:00:00"
			(at 356.87 246.38 0)
		)
		(property "SCEM" " "
			(at 356.87 248.285 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 356.87 250.19 0)
		)
		(property "Library Name" "Standard Logic"
			(at 356.87 252.095 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 356.87 254 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 356.87 255.905 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC66")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 48.26 102.87 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0332"
			(at 48.26 102.87 0)
		)
		(property "Value" "P3V3"
			(at 44.45 102.87 0)
		)
		(property "Footprint" ""
			(at 48.26 102.87 0)
		)
		(property "Datasheet" ""
			(at 48.26 102.87 0)
		)
		(property "Description" ""
			(at 48.26 102.87 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0332")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Analog & Interface:MAX3430ESA")
		(at 53.34 80.01 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC27"
			(at 62.2935 74.93 0)
		)
		(property "Value" "MAX3430ESA"
			(at 62.2935 77.47 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOIC127P600X175-8N"
			(at 53.34 111.76 0)
		)
		(property "Datasheet" ""
			(at 53.34 113.665 0)
		)
		(property "Description" "MAX3430ESA"
			(at 53.34 115.57 0)
		)
		(property "Library Ref" "MAX3430"
			(at 53.34 117.475 0)
		)
		(property "Library Path" "SchLib\\Analog & Interface.SchLib"
			(at 53.34 119.38 0)
		)
		(property "Comment" "MAX3430ESA"
			(at 53.34 121.285 0)
		)
		(property "Component Kind" "Standard"
			(at 53.34 123.19 0)
		)
		(property "Component Type" "Standard"
			(at 53.34 125.095 0)
		)
		(property "Device" "MAX3430ESA"
			(at 53.34 127 0)
		)
		(property "PackageDescription" "SOIC, 1.27mm Pitch; 8 Pin, 3.90mm W X 4.90mm L X 1.75mm H body, IPC Medium Density"
			(at 53.34 128.905 0)
		)
		(property "Status" " "
			(at 53.34 130.81 0)
		)
		(property "Part Description" "±80V Fault-Protected, Fail-Safe, 1/4-Unit Load, +3.3V RS-485 Transceiver (-40°C to +85°C)"
			(at 53.34 132.715 0)
		)
		(property "Manufacturer" "MAXIM"
			(at 53.34 134.62 0)
		)
		(property "Manufacturer Part Number" "MAX3430ESA"
			(at 53.34 136.525 0)
		)
		(property "Pin Count" "8"
			(at 53.34 138.43 0)
		)
		(property "Case" "SOIC8"
			(at 53.34 140.335 0)
		)
		(property "Mounted" "Yes"
			(at 53.34 142.24 0)
		)
		(property "Socket" "No"
			(at 53.34 144.145 0)
		)
		(property "SMD" "Yes"
			(at 53.34 146.05 0)
		)
		(property "PressFit" "No"
			(at 53.34 147.955 0)
		)
		(property "Sense" "No"
			(at 53.34 149.86 0)
		)
		(property "Sense Comment" " "
			(at 53.34 151.765 0)
		)
		(property "Bonding" "No"
			(at 53.34 153.67 0)
		)
		(property "Status Comment" " "
			(at 53.34 155.575 0)
		)
		(property "ComponentHeight" "1.75mm"
			(at 53.34 157.48 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 53.34 159.385 0)
		)
		(property "Footprint Ref" "SOIC127P600X175-8N"
			(at 53.34 161.29 0)
		)
		(property "Author" "CERN DEM BC"
			(at 53.34 163.195 0)
		)
		(property "HelpURL" ""
			(at 53.34 165.1 0)
		)
		(property "ComponentLink1URL" " "
			(at 53.34 167.005 0)
		)
		(property "ComponentLink2URL" " "
			(at 53.34 168.91 0)
		)
		(property "ComponentLink2Description" " "
			(at 53.34 170.815 0)
		)
		(property "ComponentLink1Description" " "
			(at 53.34 172.72 0)
		)
		(property "CreateDate" "02/10/20 00:00:00"
			(at 53.34 174.625 0)
		)
		(property "LatestRevisionDate" "02/10/20 00:00:00"
			(at 53.34 176.53 0)
		)
		(property "SCEM" " "
			(at 53.34 178.435 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 53.34 180.34 0)
		)
		(property "Library Name" "Analog & Interface"
			(at 53.34 182.245 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 53.34 184.15 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 53.34 186.055 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(instances
			(project "vme-wren"
				(path
					(reference "IC27")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 30.48 157.48 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0350"
			(at 30.48 157.48 0)
		)
		(property "Value" "GND"
			(at 30.48 161.29 90)
		)
		(property "Footprint" ""
			(at 30.48 157.48 0)
		)
		(property "Datasheet" ""
			(at 30.48 157.48 0)
		)
		(property "Description" ""
			(at 30.48 157.48 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0350")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 125.73 45.72 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C216"
			(at 123.698 30.226 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 130.81 40.64 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 125.73 45.72 0)
		)
		(property "Datasheet" ""
			(at 125.73 45.72 0)
		)
		(property "Description" "100nF"
			(at 123.698 27.686 90)
		)
		(property "SMD" "Yes"
			(at 125.222 48.006 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 137.668 45.72 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 139.573 45.72 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 141.478 45.72 0)
		)
		(property "Comment" "100nF"
			(at 143.383 45.72 0)
		)
		(property "Component Kind" "Standard"
			(at 145.288 45.72 0)
		)
		(property "Component Type" "Standard"
			(at 147.193 45.72 0)
		)
		(property "Pin Count" "2"
			(at 149.098 45.72 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 151.003 45.72 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 152.908 45.72 0)
		)
		(property "PackageDescription" " "
			(at 154.813 45.72 0)
		)
		(property "Status" "Not Recommended"
			(at 156.718 45.72 0)
		)
		(property "Status Comment" " "
			(at 158.623 45.72 0)
		)
		(property "Voltage" "16V"
			(at 160.528 45.72 0)
		)
		(property "Tolerance" "±10%"
			(at 164.338 45.72 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 166.243 45.72 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 168.148 45.72 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 170.053 45.72 0)
		)
		(property "Case" "0402"
			(at 171.958 45.72 0)
		)
		(property "Mounted" "Yes"
			(at 173.863 45.72 0)
		)
		(property "Socket" "No"
			(at 175.768 45.72 0)
		)
		(property "PressFit" " "
			(at 179.578 45.72 0)
		)
		(property "Sense" "No"
			(at 181.483 45.72 0)
		)
		(property "Sense Comment" " "
			(at 183.388 45.72 0)
		)
		(property "ComponentHeight" " "
			(at 185.293 45.72 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 187.198 45.72 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 189.103 45.72 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 191.008 45.72 0)
		)
		(property "HelpURL" ""
			(at 192.913 45.72 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 194.818 45.72 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 196.723 45.72 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 198.628 45.72 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 200.533 45.72 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 202.438 45.72 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 204.343 45.72 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 206.248 45.72 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C216")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diodes:SM712.TCT")
		(at 99.06 53.34 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D29"
			(at 100.33 55.8799 90)
		)
		(property "Value" "SM712.TCT"
			(at 100.33 58.4199 90)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOT95P237X112-3N"
			(at 82.55 53.34 0)
		)
		(property "Datasheet" ""
			(at 80.645 53.34 0)
		)
		(property "Description" "SM712.TCT"
			(at 78.74 53.34 0)
		)
		(property "Library Ref" "SM712"
			(at 76.835 53.34 0)
		)
		(property "Library Path" "SchLib\\Diodes.SchLib"
			(at 74.93 53.34 0)
		)
		(property "Comment" "SM712.TCT"
			(at 73.025 53.34 0)
		)
		(property "Component Kind" "Standard"
			(at 71.12 53.34 0)
		)
		(property "Component Type" "Standard"
			(at 69.215 53.34 0)
		)
		(property "Device" "SM712.TCT"
			(at 67.31 53.34 0)
		)
		(property "PackageDescription" "SOT, 0.95mm Pitch; 3 Pin, 1.30mm W X 2.92mm L X 1.12mm H body, IPC Medium Density"
			(at 65.405 53.34 0)
		)
		(property "Voltage" "12V/-7V"
			(at 63.5 53.34 0)
		)
		(property "Power" "400W"
			(at 61.595 53.34 0)
		)
		(property "Status" " "
			(at 59.69 53.34 0)
		)
		(property "Part Description" "Asymmetrical TVS Diode for Extended Common-Mode RS-485"
			(at 57.785 53.34 0)
		)
		(property "Manufacturer" "SEMTECH"
			(at 55.88 53.34 0)
		)
		(property "Manufacturer Part Number" "SM712.TCT"
			(at 53.975 53.34 0)
		)
		(property "Pin Count" "3"
			(at 52.07 53.34 0)
		)
		(property "Case" "SOT23-3"
			(at 50.165 53.34 0)
		)
		(property "Mounted" "Yes"
			(at 48.26 53.34 0)
		)
		(property "Socket" "No"
			(at 46.355 53.34 0)
		)
		(property "SMD" "Yes"
			(at 44.45 53.34 0)
		)
		(property "PressFit" "No"
			(at 42.545 53.34 0)
		)
		(property "Sense" "No"
			(at 40.64 53.34 0)
		)
		(property "Sense Comment" " "
			(at 38.735 53.34 0)
		)
		(property "Bonding" "No"
			(at 36.83 53.34 0)
		)
		(property "Status Comment" " "
			(at 34.925 53.34 0)
		)
		(property "ComponentHeight" "1.12mm"
			(at 33.02 53.34 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 31.115 53.34 0)
		)
		(property "Footprint Ref" "SOT95P237X112-3N"
			(at 29.21 53.34 0)
		)
		(property "HelpURL" ""
			(at 27.305 53.34 0)
		)
		(property "ComponentLink1URL" " "
			(at 25.4 53.34 0)
		)
		(property "ComponentLink1Description" " "
			(at 23.495 53.34 0)
		)
		(property "ComponentLink2URL" " "
			(at 21.59 53.34 0)
		)
		(property "ComponentLink2Description" " "
			(at 19.685 53.34 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 17.78 53.34 0)
		)
		(property "CreateDate" "09/03/14 00:00:00"
			(at 15.875 53.34 0)
		)
		(property "LatestRevisionDate" "01/13/15 00:00:00"
			(at 13.97 53.34 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 10.16 53.34 0)
		)
		(property "Library Name" "Diodes"
			(at 8.255 53.34 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 6.35 53.34 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 4.445 53.34 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "vme-wren"
				(path
					(reference "D29")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 311.15 177.8 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR03"
			(at 311.15 177.8 0)
		)
		(property "Value" "GND"
			(at 311.15 181.61 0)
		)
		(property "Footprint" ""
			(at 311.15 177.8 0)
		)
		(property "Datasheet" ""
			(at 311.15 177.8 0)
		)
		(property "Description" ""
			(at 311.15 177.8 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 93.98 115.57 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0336"
			(at 93.98 115.57 0)
		)
		(property "Value" "GND"
			(at 93.98 119.38 0)
		)
		(property "Footprint" ""
			(at 93.98 115.57 0)
		)
		(property "Datasheet" ""
			(at 93.98 115.57 0)
		)
		(property "Description" ""
			(at 93.98 115.57 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0336")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 31.75 54.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0330"
			(at 31.75 54.61 0)
		)
		(property "Value" "GND"
			(at 31.75 58.42 90)
		)
		(property "Footprint" ""
			(at 31.75 54.61 0)
		)
		(property "Datasheet" ""
			(at 31.75 54.61 0)
		)
		(property "Description" ""
			(at 31.75 54.61 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0330")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 31.75 29.21 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R117"
			(at 34.29 24.1299 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 36.703 29.21 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 38.608 29.21 0)
		)
		(property "Datasheet" ""
			(at 40.513 29.21 0)
		)
		(property "Description" "±1%"
			(at 26.67 25.4 0)
		)
		(property "Val" "10k"
			(at 34.29 26.6699 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 42.418 29.21 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 44.323 29.21 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 46.228 29.21 0)
		)
		(property "Comment" "10k"
			(at 48.133 29.21 0)
		)
		(property "Component Kind" "Standard"
			(at 50.038 29.21 0)
		)
		(property "Component Type" "Standard"
			(at 51.943 29.21 0)
		)
		(property "PackageDescription" " "
			(at 53.848 29.21 0)
		)
		(property "Pin Count" "2"
			(at 55.753 29.21 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 57.658 29.21 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 59.563 29.21 0)
		)
		(property "Status" "Not Recommended"
			(at 61.468 29.21 0)
		)
		(property "Power" "0.0625W"
			(at 63.373 29.21 0)
		)
		(property "Voltage" " "
			(at 67.183 29.21 0)
		)
		(property "Tolerance" "±1%"
			(at 69.088 29.21 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 70.993 29.21 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 72.898 29.21 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 74.803 29.21 0)
		)
		(property "Case" "0402"
			(at 76.708 29.21 0)
		)
		(property "PressFit" "No"
			(at 78.613 29.21 0)
		)
		(property "Mounted" "Yes"
			(at 80.518 29.21 0)
		)
		(property "Sense Comment" " "
			(at 82.423 29.21 0)
		)
		(property "Sense" "No"
			(at 84.328 29.21 0)
		)
		(property "Status Comment" " "
			(at 86.233 29.21 0)
		)
		(property "Socket" "No"
			(at 88.138 29.21 0)
		)
		(property "SMD" "Yes"
			(at 90.043 29.21 0)
		)
		(property "ComponentHeight" " "
			(at 91.948 29.21 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 93.853 29.21 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 95.758 29.21 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 97.663 29.21 0)
		)
		(property "HelpURL" ""
			(at 99.568 29.21 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 101.473 29.21 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 103.378 29.21 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 105.283 29.21 0)
		)
		(property "Database Table Name" "Resistors"
			(at 107.188 29.21 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 109.093 29.21 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 110.998 29.21 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 112.903 29.21 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R117")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 48.26 153.67 270)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0347"
			(at 48.26 153.67 0)
		)
		(property "Value" "P3V3"
			(at 44.45 153.67 0)
		)
		(property "Footprint" ""
			(at 48.26 153.67 0)
		)
		(property "Datasheet" ""
			(at 48.26 153.67 0)
		)
		(property "Description" ""
			(at 48.26 153.67 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0347")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 125.73 38.1 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0333"
			(at 125.73 38.1 0)
		)
		(property "Value" "P3V3"
			(at 125.73 34.29 0)
		)
		(property "Footprint" ""
			(at 125.73 38.1 0)
		)
		(property "Datasheet" ""
			(at 125.73 38.1 0)
		)
		(property "Description" ""
			(at 125.73 38.1 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0333")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 226.06 165.1 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR085"
			(at 226.06 165.1 0)
		)
		(property "Value" "GND"
			(at 226.06 168.91 0)
		)
		(property "Footprint" ""
			(at 226.06 165.1 0)
		)
		(property "Datasheet" ""
			(at 226.06 165.1 0)
		)
		(property "Description" ""
			(at 226.06 165.1 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR085")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 31.75 53.34 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R68"
			(at 34.29 48.2599 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 36.703 53.34 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 38.608 53.34 0)
		)
		(property "Datasheet" ""
			(at 40.513 53.34 0)
		)
		(property "Description" "±1%"
			(at 26.67 49.53 0)
		)
		(property "Val" "10k"
			(at 34.29 50.7999 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 42.418 53.34 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 44.323 53.34 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 46.228 53.34 0)
		)
		(property "Comment" "10k"
			(at 48.133 53.34 0)
		)
		(property "Component Kind" "Standard"
			(at 50.038 53.34 0)
		)
		(property "Component Type" "Standard"
			(at 51.943 53.34 0)
		)
		(property "PackageDescription" " "
			(at 53.848 53.34 0)
		)
		(property "Pin Count" "2"
			(at 55.753 53.34 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 57.658 53.34 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 59.563 53.34 0)
		)
		(property "Status" "Not Recommended"
			(at 61.468 53.34 0)
		)
		(property "Power" "0.0625W"
			(at 63.373 53.34 0)
		)
		(property "Voltage" " "
			(at 67.183 53.34 0)
		)
		(property "Tolerance" "±1%"
			(at 69.088 53.34 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 70.993 53.34 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 72.898 53.34 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 74.803 53.34 0)
		)
		(property "Case" "0402"
			(at 76.708 53.34 0)
		)
		(property "PressFit" "No"
			(at 78.613 53.34 0)
		)
		(property "Mounted" "Yes"
			(at 80.518 53.34 0)
		)
		(property "Sense Comment" " "
			(at 82.423 53.34 0)
		)
		(property "Sense" "No"
			(at 84.328 53.34 0)
		)
		(property "Status Comment" " "
			(at 86.233 53.34 0)
		)
		(property "Socket" "No"
			(at 88.138 53.34 0)
		)
		(property "SMD" "Yes"
			(at 90.043 53.34 0)
		)
		(property "ComponentHeight" " "
			(at 91.948 53.34 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 93.853 53.34 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 95.758 53.34 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 97.663 53.34 0)
		)
		(property "HelpURL" ""
			(at 99.568 53.34 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 101.473 53.34 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 103.378 53.34 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 105.283 53.34 0)
		)
		(property "Database Table Name" "Resistors"
			(at 107.188 53.34 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 109.093 53.34 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 110.998 53.34 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 112.903 53.34 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R68")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diodes:SM712.TCT")
		(at 99.06 102.87 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D30"
			(at 100.33 105.4099 90)
		)
		(property "Value" "SM712.TCT"
			(at 100.33 107.9499 90)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOT95P237X112-3N"
			(at 82.55 102.87 0)
		)
		(property "Datasheet" ""
			(at 80.645 102.87 0)
		)
		(property "Description" "SM712.TCT"
			(at 78.74 102.87 0)
		)
		(property "Library Ref" "SM712"
			(at 76.835 102.87 0)
		)
		(property "Library Path" "SchLib\\Diodes.SchLib"
			(at 74.93 102.87 0)
		)
		(property "Comment" "SM712.TCT"
			(at 73.025 102.87 0)
		)
		(property "Component Kind" "Standard"
			(at 71.12 102.87 0)
		)
		(property "Component Type" "Standard"
			(at 69.215 102.87 0)
		)
		(property "Device" "SM712.TCT"
			(at 67.31 102.87 0)
		)
		(property "PackageDescription" "SOT, 0.95mm Pitch; 3 Pin, 1.30mm W X 2.92mm L X 1.12mm H body, IPC Medium Density"
			(at 65.405 102.87 0)
		)
		(property "Voltage" "12V/-7V"
			(at 63.5 102.87 0)
		)
		(property "Power" "400W"
			(at 61.595 102.87 0)
		)
		(property "Status" " "
			(at 59.69 102.87 0)
		)
		(property "Part Description" "Asymmetrical TVS Diode for Extended Common-Mode RS-485"
			(at 57.785 102.87 0)
		)
		(property "Manufacturer" "SEMTECH"
			(at 55.88 102.87 0)
		)
		(property "Manufacturer Part Number" "SM712.TCT"
			(at 53.975 102.87 0)
		)
		(property "Pin Count" "3"
			(at 52.07 102.87 0)
		)
		(property "Case" "SOT23-3"
			(at 50.165 102.87 0)
		)
		(property "Mounted" "Yes"
			(at 48.26 102.87 0)
		)
		(property "Socket" "No"
			(at 46.355 102.87 0)
		)
		(property "SMD" "Yes"
			(at 44.45 102.87 0)
		)
		(property "PressFit" "No"
			(at 42.545 102.87 0)
		)
		(property "Sense" "No"
			(at 40.64 102.87 0)
		)
		(property "Sense Comment" " "
			(at 38.735 102.87 0)
		)
		(property "Bonding" "No"
			(at 36.83 102.87 0)
		)
		(property "Status Comment" " "
			(at 34.925 102.87 0)
		)
		(property "ComponentHeight" "1.12mm"
			(at 33.02 102.87 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 31.115 102.87 0)
		)
		(property "Footprint Ref" "SOT95P237X112-3N"
			(at 29.21 102.87 0)
		)
		(property "HelpURL" ""
			(at 27.305 102.87 0)
		)
		(property "ComponentLink1URL" " "
			(at 25.4 102.87 0)
		)
		(property "ComponentLink1Description" " "
			(at 23.495 102.87 0)
		)
		(property "ComponentLink2URL" " "
			(at 21.59 102.87 0)
		)
		(property "ComponentLink2Description" " "
			(at 19.685 102.87 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 17.78 102.87 0)
		)
		(property "CreateDate" "09/03/14 00:00:00"
			(at 15.875 102.87 0)
		)
		(property "LatestRevisionDate" "01/13/15 00:00:00"
			(at 13.97 102.87 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 10.16 102.87 0)
		)
		(property "Library Name" "Diodes"
			(at 8.255 102.87 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 6.35 102.87 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 4.445 102.87 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "vme-wren"
				(path
					(reference "D30")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 82.55 157.48 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0349"
			(at 82.55 157.48 0)
		)
		(property "Value" "GND"
			(at 82.55 161.29 0)
		)
		(property "Footprint" ""
			(at 82.55 157.48 0)
		)
		(property "Datasheet" ""
			(at 82.55 157.48 0)
		)
		(property "Description" ""
			(at 82.55 157.48 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0349")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 114.3 45.72 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0106"
			(at 114.3 45.72 0)
		)
		(property "Value" "GND"
			(at 114.3 49.53 0)
		)
		(property "Footprint" ""
			(at 114.3 45.72 0)
		)
		(property "Datasheet" ""
			(at 114.3 45.72 0)
		)
		(property "Description" ""
			(at 114.3 45.72 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0106")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 195.58 209.55 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0736"
			(at 195.58 209.55 0)
		)
		(property "Value" "GND"
			(at 195.58 213.36 0)
		)
		(property "Footprint" ""
			(at 195.58 209.55 0)
		)
		(property "Datasheet" ""
			(at 195.58 209.55 0)
		)
		(property "Description" ""
			(at 195.58 209.55 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0736")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Standard Logic:SN74LV595ARGYR")
		(at 281.94 139.7 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC1"
			(at 292.1 134.62 0)
		)
		(property "Value" "SN74LV595ARGYR"
			(at 292.1 137.16 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:TEXAS_RGY (R-PVQFN-N16)"
			(at 281.94 179.07 0)
		)
		(property "Datasheet" ""
			(at 281.94 180.975 0)
		)
		(property "Description" "SN74LV595ARGYR"
			(at 281.94 182.88 0)
		)
		(property "Library Ref" "74595_a"
			(at 281.94 184.785 0)
		)
		(property "Library Path" "SchLib\\Standard Logic.SchLib"
			(at 281.94 186.69 0)
		)
		(property "Comment" "SN74LV595ARGY"
			(at 281.94 188.595 0)
		)
		(property "Component Kind" "Standard"
			(at 281.94 190.5 0)
		)
		(property "Component Type" "Standard"
			(at 281.94 192.405 0)
		)
		(property "Device" "SN74LV595ARGY"
			(at 281.94 194.31 0)
		)
		(property "PackageDescription" "TEXAS Case Style RGY (R-PVQFN-N16), QFN, 0.50mm Pitch, Rect.; 16 Pin, 4.00mm L X 3.50mm W X 1mm H body (w/Thermal Tab 2.65 X 2.15mm)"
			(at 281.94 196.215 0)
		)
		(property "Status" " "
			(at 281.94 198.12 0)
		)
		(property "Part Description" "8-Bit Shift Register with 3-State Output Registers"
			(at 281.94 200.025 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 281.94 201.93 0)
		)
		(property "Manufacturer Part Number" "SN74LV595ARGY"
			(at 281.94 203.835 0)
		)
		(property "Pin Count" "17"
			(at 281.94 205.74 0)
		)
		(property "Case" "QFN16"
			(at 281.94 207.645 0)
		)
		(property "Mounted" "Yes"
			(at 281.94 209.55 0)
		)
		(property "Socket" "No"
			(at 281.94 211.455 0)
		)
		(property "SMD" "Yes"
			(at 281.94 213.36 0)
		)
		(property "PressFit" "No"
			(at 281.94 215.265 0)
		)
		(property "Sense" "No"
			(at 281.94 217.17 0)
		)
		(property "Sense Comment" " "
			(at 281.94 219.075 0)
		)
		(property "Bonding" "No"
			(at 281.94 220.98 0)
		)
		(property "Status Comment" " "
			(at 281.94 222.885 0)
		)
		(property "ComponentHeight" "1mm"
			(at 281.94 224.79 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 281.94 226.695 0)
		)
		(property "Footprint Ref" "TEXAS_RGY (R-PVQFN-N16)"
			(at 281.94 228.6 0)
		)
		(property "Author" "CERN DEM MR"
			(at 281.94 230.505 0)
		)
		(property "HelpURL" ""
			(at 281.94 232.41 0)
		)
		(property "ComponentLink1URL" " "
			(at 281.94 234.315 0)
		)
		(property "ComponentLink1Description" " "
			(at 281.94 236.22 0)
		)
		(property "ComponentLink2URL" " "
			(at 281.94 238.125 0)
		)
		(property "ComponentLink2Description" " "
			(at 281.94 240.03 0)
		)
		(property "CreateDate" "10/10/17 00:00:00"
			(at 281.94 241.935 0)
		)
		(property "LatestRevisionDate" "10/10/17 00:00:00"
			(at 281.94 243.84 0)
		)
		(property "SCEM" " "
			(at 281.94 245.745 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 281.94 247.65 0)
		)
		(property "Library Name" "Standard Logic"
			(at 281.94 249.555 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 281.94 251.46 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 281.94 253.365 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Capacitors SMD:CC0402_100NF_16V_10%_X7R")
		(at 52.07 200.66 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C223"
			(at 56.388 200.66 90)
		)
		(property "Value" "CC0402_100NF_16V_10%_X7R"
			(at 57.15 195.58 0)
		)
		(property "Footprint" "Capacitors SMD:CAPC1005X55N"
			(at 52.07 200.66 0)
		)
		(property "Datasheet" ""
			(at 52.07 200.66 0)
		)
		(property "Description" "100nF"
			(at 56.388 198.12 90)
		)
		(property "SMD" "Yes"
			(at 51.562 202.946 0)
		)
		(property "Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 64.008 200.66 0)
		)
		(property "Library Ref" "Capacitor - non polarized"
			(at 65.913 200.66 0)
		)
		(property "Library Path" "SchLib\\Capacitors.SchLib"
			(at 67.818 200.66 0)
		)
		(property "Comment" "100nF"
			(at 69.723 200.66 0)
		)
		(property "Component Kind" "Standard"
			(at 71.628 200.66 0)
		)
		(property "Component Type" "Standard"
			(at 73.533 200.66 0)
		)
		(property "Pin Count" "2"
			(at 75.438 200.66 0)
		)
		(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
			(at 77.343 200.66 0)
		)
		(property "Footprint Ref" "CAPC1005X55N"
			(at 79.248 200.66 0)
		)
		(property "PackageDescription" " "
			(at 81.153 200.66 0)
		)
		(property "Status" "Not Recommended"
			(at 83.058 200.66 0)
		)
		(property "Status Comment" " "
			(at 84.963 200.66 0)
		)
		(property "Voltage" "16V"
			(at 86.868 200.66 0)
		)
		(property "Tolerance" "±10%"
			(at 90.678 200.66 0)
		)
		(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
			(at 92.583 200.66 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 94.488 200.66 0)
		)
		(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
			(at 96.393 200.66 0)
		)
		(property "Case" "0402"
			(at 98.298 200.66 0)
		)
		(property "Mounted" "Yes"
			(at 100.203 200.66 0)
		)
		(property "Socket" "No"
			(at 102.108 200.66 0)
		)
		(property "PressFit" " "
			(at 105.918 200.66 0)
		)
		(property "Sense" "No"
			(at 107.823 200.66 0)
		)
		(property "Sense Comment" " "
			(at 109.728 200.66 0)
		)
		(property "ComponentHeight" " "
			(at 111.633 200.66 0)
		)
		(property "Manufacturer1 Example" "MURATA"
			(at 113.538 200.66 0)
		)
		(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
			(at 115.443 200.66 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.55mm"
			(at 117.348 200.66 0)
		)
		(property "HelpURL" ""
			(at 119.253 200.66 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 121.158 200.66 0)
		)
		(property "CreateDate" "12/05/13 00:00:00"
			(at 123.063 200.66 0)
		)
		(property "LatestRevisionDate" "12/03/07 00:00:00"
			(at 124.968 200.66 0)
		)
		(property "Database Table Name" "Capacitors"
			(at 126.873 200.66 0)
		)
		(property "Library Name" "Capacitors SMD"
			(at 128.778 200.66 0)
		)
		(property "Footprint Library" "Capacitors SMD"
			(at 130.683 200.66 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 132.588 200.66 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "C223")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 165.1 213.36 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0735"
			(at 165.1 213.36 0)
		)
		(property "Value" "GND"
			(at 165.1 217.17 0)
		)
		(property "Footprint" ""
			(at 165.1 213.36 0)
		)
		(property "Datasheet" ""
			(at 165.1 213.36 0)
		)
		(property "Description" ""
			(at 165.1 213.36 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0735")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 168.91 267.97 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0344"
			(at 168.91 267.97 0)
		)
		(property "Value" "GND"
			(at 168.91 271.78 0)
		)
		(property "Footprint" ""
			(at 168.91 267.97 0)
		)
		(property "Datasheet" ""
			(at 168.91 267.97 0)
		)
		(property "Description" ""
			(at 168.91 267.97 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0344")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 344.17 167.64 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0729"
			(at 344.17 167.64 0)
		)
		(property "Value" "P3V3"
			(at 345.186 163.576 0)
		)
		(property "Footprint" ""
			(at 344.17 167.64 0)
		)
		(property "Datasheet" ""
			(at 344.17 167.64 0)
		)
		(property "Description" ""
			(at 344.17 167.64 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0729")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Standard Logic:SN74LV595ARGYR")
		(at 356.87 195.58 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC65"
			(at 367.03 190.5 0)
		)
		(property "Value" "SN74LV595ARGYR"
			(at 367.03 193.04 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:TEXAS_RGY (R-PVQFN-N16)"
			(at 356.87 234.95 0)
		)
		(property "Datasheet" ""
			(at 356.87 236.855 0)
		)
		(property "Description" "SN74LV595ARGYR"
			(at 356.87 238.76 0)
		)
		(property "Library Ref" "74595_a"
			(at 356.87 240.665 0)
		)
		(property "Library Path" "SchLib\\Standard Logic.SchLib"
			(at 356.87 242.57 0)
		)
		(property "Comment" "SN74LV595ARGY"
			(at 356.87 244.475 0)
		)
		(property "Component Kind" "Standard"
			(at 356.87 246.38 0)
		)
		(property "Component Type" "Standard"
			(at 356.87 248.285 0)
		)
		(property "Device" "SN74LV595ARGY"
			(at 356.87 250.19 0)
		)
		(property "PackageDescription" "TEXAS Case Style RGY (R-PVQFN-N16), QFN, 0.50mm Pitch, Rect.; 16 Pin, 4.00mm L X 3.50mm W X 1mm H body (w/Thermal Tab 2.65 X 2.15mm)"
			(at 356.87 252.095 0)
		)
		(property "Status" " "
			(at 356.87 254 0)
		)
		(property "Part Description" "8-Bit Shift Register with 3-State Output Registers"
			(at 356.87 255.905 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 356.87 257.81 0)
		)
		(property "Manufacturer Part Number" "SN74LV595ARGY"
			(at 356.87 259.715 0)
		)
		(property "Pin Count" "17"
			(at 356.87 261.62 0)
		)
		(property "Case" "QFN16"
			(at 356.87 263.525 0)
		)
		(property "Mounted" "Yes"
			(at 356.87 265.43 0)
		)
		(property "Socket" "No"
			(at 356.87 267.335 0)
		)
		(property "SMD" "Yes"
			(at 356.87 269.24 0)
		)
		(property "PressFit" "No"
			(at 356.87 271.145 0)
		)
		(property "Sense" "No"
			(at 356.87 273.05 0)
		)
		(property "Sense Comment" " "
			(at 356.87 274.955 0)
		)
		(property "Bonding" "No"
			(at 356.87 276.86 0)
		)
		(property "Status Comment" " "
			(at 356.87 278.765 0)
		)
		(property "ComponentHeight" "1mm"
			(at 356.87 280.67 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 356.87 282.575 0)
		)
		(property "Footprint Ref" "TEXAS_RGY (R-PVQFN-N16)"
			(at 356.87 284.48 0)
		)
		(property "Author" "CERN DEM MR"
			(at 356.87 286.385 0)
		)
		(property "HelpURL" ""
			(at 356.87 288.29 0)
		)
		(property "ComponentLink1URL" " "
			(at 356.87 290.195 0)
		)
		(property "ComponentLink1Description" " "
			(at 356.87 292.1 0)
		)
		(property "ComponentLink2URL" " "
			(at 356.87 294.005 0)
		)
		(property "ComponentLink2Description" " "
			(at 356.87 295.91 0)
		)
		(property "CreateDate" "10/10/17 00:00:00"
			(at 356.87 297.815 0)
		)
		(property "LatestRevisionDate" "10/10/17 00:00:00"
			(at 356.87 299.72 0)
		)
		(property "SCEM" " "
			(at 356.87 301.625 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 356.87 303.53 0)
		)
		(property "Library Name" "Standard Logic"
			(at 356.87 305.435 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 356.87 307.34 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 356.87 309.245 0)
		)
		(pin "1")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(instances
			(project "vme-wren"
				(path
					(reference "IC65")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_33R_1%_0.0625W_100PPM")
		(at 34.29 242.57 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R458"
			(at 36.068 229.87 0)
		)
		(property "Value" "R0402_33R_1%_0.0625W_100PPM"
			(at 34.29 247.523 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 34.29 249.428 0)
		)
		(property "Datasheet" ""
			(at 34.29 251.333 0)
		)
		(property "Description" "±1%"
			(at 38.1 237.49 0)
		)
		(property "Val" "33"
			(at 40.894 229.87 0)
		)
		(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 34.29 253.238 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 34.29 255.143 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 34.29 257.048 0)
		)
		(property "Comment" "33"
			(at 34.29 258.953 0)
		)
		(property "Component Kind" "Standard"
			(at 34.29 260.858 0)
		)
		(property "Component Type" "Standard"
			(at 34.29 262.763 0)
		)
		(property "PackageDescription" " "
			(at 34.29 264.668 0)
		)
		(property "Pin Count" "2"
			(at 34.29 266.573 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 34.29 268.478 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 34.29 270.383 0)
		)
		(property "Status" "Not Recommended"
			(at 34.29 272.288 0)
		)
		(property "Power" "0.0625W"
			(at 34.29 274.193 0)
		)
		(property "Voltage" " "
			(at 34.29 278.003 0)
		)
		(property "Tolerance" "±1%"
			(at 34.29 279.908 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 34.29 281.813 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 34.29 283.718 0)
		)
		(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 34.29 285.623 0)
		)
		(property "Case" "0402"
			(at 34.29 287.528 0)
		)
		(property "PressFit" "No"
			(at 34.29 289.433 0)
		)
		(property "Mounted" "Yes"
			(at 34.29 291.338 0)
		)
		(property "Sense Comment" " "
			(at 34.29 293.243 0)
		)
		(property "Sense" "No"
			(at 34.29 295.148 0)
		)
		(property "Status Comment" " "
			(at 34.29 297.053 0)
		)
		(property "Socket" "No"
			(at 34.29 298.958 0)
		)
		(property "SMD" "Yes"
			(at 34.29 300.863 0)
		)
		(property "ComponentHeight" " "
			(at 34.29 302.768 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 34.29 304.673 0)
		)
		(property "Manufacturer1 Part Number" "232270673309L"
			(at 34.29 306.578 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 34.29 308.483 0)
		)
		(property "HelpURL" ""
			(at 34.29 310.388 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 34.29 312.293 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 34.29 314.198 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 34.29 316.103 0)
		)
		(property "Database Table Name" "Resistors"
			(at 34.29 318.008 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 34.29 319.913 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 34.29 321.818 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 34.29 323.723 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R458")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 146.05 144.78 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR01029"
			(at 146.05 144.78 0)
		)
		(property "Value" "P3V3"
			(at 142.24 144.78 0)
		)
		(property "Footprint" ""
			(at 146.05 144.78 0)
		)
		(property "Datasheet" ""
			(at 146.05 144.78 0)
		)
		(property "Description" ""
			(at 146.05 144.78 0)
		)
		(pin "")
		(instances
			(project "vme-wren"
				(path
					(reference "#PWR01029")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 54.61 229.87 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R103"
			(at 52.07 224.7899 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 59.563 229.87 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 61.468 229.87 0)
		)
		(property "Datasheet" ""
			(at 63.373 229.87 0)
		)
		(property "Description" "±1%"
			(at 49.53 226.06 0)
		)
		(property "Val" "10k"
			(at 52.07 227.3299 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 65.278 229.87 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 67.183 229.87 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 69.088 229.87 0)
		)
		(property "Comment" "10k"
			(at 70.993 229.87 0)
		)
		(property "Component Kind" "Standard"
			(at 72.898 229.87 0)
		)
		(property "Component Type" "Standard"
			(at 74.803 229.87 0)
		)
		(property "PackageDescription" " "
			(at 76.708 229.87 0)
		)
		(property "Pin Count" "2"
			(at 78.613 229.87 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 80.518 229.87 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 82.423 229.87 0)
		)
		(property "Status" "Not Recommended"
			(at 84.328 229.87 0)
		)
		(property "Power" "0.0625W"
			(at 86.233 229.87 0)
		)
		(property "Voltage" " "
			(at 90.043 229.87 0)
		)
		(property "Tolerance" "±1%"
			(at 91.948 229.87 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 93.853 229.87 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 95.758 229.87 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 97.663 229.87 0)
		)
		(property "Case" "0402"
			(at 99.568 229.87 0)
		)
		(property "PressFit" "No"
			(at 101.473 229.87 0)
		)
		(property "Mounted" "Yes"
			(at 103.378 229.87 0)
		)
		(property "Sense Comment" " "
			(at 105.283 229.87 0)
		)
		(property "Sense" "No"
			(at 107.188 229.87 0)
		)
		(property "Status Comment" " "
			(at 109.093 229.87 0)
		)
		(property "Socket" "No"
			(at 110.998 229.87 0)
		)
		(property "SMD" "Yes"
			(at 112.903 229.87 0)
		)
		(property "ComponentHeight" " "
			(at 114.808 229.87 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 116.713 229.87 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 118.618 229.87 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 120.523 229.87 0)
		)
		(property "HelpURL" ""
			(at 122.428 229.87 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 124.333 229.87 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 126.238 229.87 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 128.143 229.87 0)
		)
		(property "Database Table Name" "Resistors"
			(at 130.048 229.87 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 131.953 229.87 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 133.858 229.87 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 135.763 229.87 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R103")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 48.26 53.34 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0327"
			(at 48.26 53.34 0)
		)
		(property "Value" "P3V3"
			(at 44.45 53.34 0)
		)
		(property "Footprint" ""
			(at 48.26 53.34 0)
		)
		(property "Datasheet" ""
			(at 48.26 53.34 0)
		)
		(property "Description" ""
			(at 48.26 53.34 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0327")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 132.08 187.96 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0732"
			(at 132.08 187.96 0)
		)
		(property "Value" "GND"
			(at 128.27 187.96 90)
		)
		(property "Footprint" ""
			(at 132.08 187.96 0)
		)
		(property "Datasheet" ""
			(at 132.08 187.96 0)
		)
		(property "Description" ""
			(at 132.08 187.96 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0732")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 54.61 220.98 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0340"
			(at 54.61 220.98 0)
		)
		(property "Value" "GND"
			(at 54.61 217.17 90)
		)
		(property "Footprint" ""
			(at 54.61 220.98 0)
		)
		(property "Datasheet" ""
			(at 54.61 220.98 0)
		)
		(property "Description" ""
			(at 54.61 220.98 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0340")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 167.64 170.18 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR086"
			(at 167.64 170.18 0)
		)
		(property "Value" "P3V3"
			(at 163.83 170.18 0)
		)
		(property "Footprint" ""
			(at 167.64 170.18 0)
		)
		(property "Datasheet" ""
			(at 167.64 170.18 0)
		)
		(property "Description" ""
			(at 167.64 170.18 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR086")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_10K_1%_0.0625W_100PPM")
		(at 31.75 102.87 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R121"
			(at 34.29 97.7899 90)
		)
		(property "Value" "R0402_10K_1%_0.0625W_100PPM"
			(at 36.703 102.87 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 38.608 102.87 0)
		)
		(property "Datasheet" ""
			(at 40.513 102.87 0)
		)
		(property "Description" "±1%"
			(at 26.67 99.06 0)
		)
		(property "Val" "10k"
			(at 34.29 100.3299 90)
		)
		(property "Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 42.418 102.87 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 44.323 102.87 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 46.228 102.87 0)
		)
		(property "Comment" "10k"
			(at 48.133 102.87 0)
		)
		(property "Component Kind" "Standard"
			(at 50.038 102.87 0)
		)
		(property "Component Type" "Standard"
			(at 51.943 102.87 0)
		)
		(property "PackageDescription" " "
			(at 53.848 102.87 0)
		)
		(property "Pin Count" "2"
			(at 55.753 102.87 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 57.658 102.87 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 59.563 102.87 0)
		)
		(property "Status" "Not Recommended"
			(at 61.468 102.87 0)
		)
		(property "Power" "0.0625W"
			(at 63.373 102.87 0)
		)
		(property "Voltage" " "
			(at 67.183 102.87 0)
		)
		(property "Tolerance" "±1%"
			(at 69.088 102.87 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 70.993 102.87 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 72.898 102.87 0)
		)
		(property "Manufacturer Part Number" "R0402_10K_1%_0.0625W_100PPM"
			(at 74.803 102.87 0)
		)
		(property "Case" "0402"
			(at 76.708 102.87 0)
		)
		(property "PressFit" "No"
			(at 78.613 102.87 0)
		)
		(property "Mounted" "Yes"
			(at 80.518 102.87 0)
		)
		(property "Sense Comment" " "
			(at 82.423 102.87 0)
		)
		(property "Sense" "No"
			(at 84.328 102.87 0)
		)
		(property "Status Comment" " "
			(at 86.233 102.87 0)
		)
		(property "Socket" "No"
			(at 88.138 102.87 0)
		)
		(property "SMD" "Yes"
			(at 90.043 102.87 0)
		)
		(property "ComponentHeight" " "
			(at 91.948 102.87 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 93.853 102.87 0)
		)
		(property "Manufacturer1 Part Number" "232270671003L"
			(at 95.758 102.87 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 97.663 102.87 0)
		)
		(property "HelpURL" ""
			(at 99.568 102.87 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 101.473 102.87 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 103.378 102.87 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 105.283 102.87 0)
		)
		(property "Database Table Name" "Resistors"
			(at 107.188 102.87 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 109.093 102.87 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 110.998 102.87 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 112.903 102.87 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "vme-wren"
				(path
					(reference "R121")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 52.07 161.29 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0348"
			(at 52.07 161.29 0)
		)
		(property "Value" "GND"
			(at 52.07 165.1 0)
		)
		(property "Footprint" ""
			(at 52.07 161.29 0)
		)
		(property "Datasheet" ""
			(at 52.07 161.29 0)
		)
		(property "Description" ""
			(at 52.07 161.29 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0348")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 124.46 257.81 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0342"
			(at 124.46 257.81 0)
		)
		(property "Value" "P3V3"
			(at 120.65 257.81 0)
		)
		(property "Footprint" ""
			(at 124.46 257.81 0)
		)
		(property "Datasheet" ""
			(at 124.46 257.81 0)
		)
		(property "Description" ""
			(at 124.46 257.81 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0342")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "vme-wren:P3V3")
		(at 200.66 255.27 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0720"
			(at 200.66 255.27 0)
		)
		(property "Value" "P3V3"
			(at 200.66 251.46 0)
		)
		(property "Footprint" ""
			(at 200.66 255.27 0)
		)
		(property "Datasheet" ""
			(at 200.66 255.27 0)
		)
		(property "Description" ""
			(at 200.66 255.27 0)
		)
		(pin "")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0720")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Analog & Interface:DS90LV027AQMA_NOPB")
		(at 60.96 130.81 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "IC57"
			(at 68.58 125.73 0)
		)
		(property "Value" "DS90LV027AQMA_NOPB"
			(at 68.58 128.27 0)
		)
		(property "Footprint" "ICs And Semiconductors SMD:SOIC127P600X175-8N"
			(at 60.96 162.56 0)
		)
		(property "Datasheet" ""
			(at 60.96 164.465 0)
		)
		(property "Description" "DS90LV027AQMA_NOPB"
			(at 60.96 166.37 0)
		)
		(property "Library Ref" "DS90LV027AQ"
			(at 60.96 168.275 0)
		)
		(property "Library Path" "SchLib\\Analog & Interface.SchLib"
			(at 60.96 170.18 0)
		)
		(property "Comment" "DS90LV027AQMA/NOPB"
			(at 60.96 172.085 0)
		)
		(property "Component Kind" "Standard"
			(at 60.96 173.99 0)
		)
		(property "Component Type" "Standard"
			(at 60.96 175.895 0)
		)
		(property "Device" "DS90LV027AQMA/NOPB"
			(at 60.96 177.8 0)
		)
		(property "PackageDescription" "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density"
			(at 60.96 179.705 0)
		)
		(property "Status" " "
			(at 60.96 181.61 0)
		)
		(property "Part Description" "Automotive LVDS Dual Differential Driver"
			(at 60.96 183.515 0)
		)
		(property "Manufacturer" "TEXAS INSTRUMENTS"
			(at 60.96 185.42 0)
		)
		(property "Manufacturer Part Number" "DS90LV027AQMA"
			(at 60.96 187.325 0)
		)
		(property "Pin Count" "8"
			(at 60.96 189.23 0)
		)
		(property "Case" "SOIC8"
			(at 60.96 191.135 0)
		)
		(property "Mounted" "Yes"
			(at 60.96 193.04 0)
		)
		(property "Socket" "No"
			(at 60.96 194.945 0)
		)
		(property "SMD" "Yes"
			(at 60.96 196.85 0)
		)
		(property "PressFit" "No"
			(at 60.96 198.755 0)
		)
		(property "Sense" "No"
			(at 60.96 200.66 0)
		)
		(property "Sense Comment" " "
			(at 60.96 202.565 0)
		)
		(property "Bonding" "No"
			(at 60.96 204.47 0)
		)
		(property "Status Comment" " "
			(at 60.96 206.375 0)
		)
		(property "ComponentHeight" "1.75mm"
			(at 60.96 208.28 0)
		)
		(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
			(at 60.96 210.185 0)
		)
		(property "Footprint Ref" "SOIC127P600X175-8N"
			(at 60.96 212.09 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 60.96 213.995 0)
		)
		(property "HelpURL" ""
			(at 60.96 215.9 0)
		)
		(property "ComponentLink1URL" " "
			(at 60.96 217.805 0)
		)
		(property "ComponentLink2URL" " "
			(at 60.96 219.71 0)
		)
		(property "ComponentLink2Description" " "
			(at 60.96 221.615 0)
		)
		(property "ComponentLink1Description" " "
			(at 60.96 223.52 0)
		)
		(property "CreateDate" "01/11/17 00:00:00"
			(at 60.96 225.425 0)
		)
		(property "LatestRevisionDate" "06/01/22 00:00:00"
			(at 60.96 227.33 0)
		)
		(property "SCEM" " "
			(at 60.96 229.235 0)
		)
		(property "Database Table Name" "ICs And Semiconductors"
			(at 60.96 231.14 0)
		)
		(property "Library Name" "Analog & Interface"
			(at 60.96 233.045 0)
		)
		(property "Footprint Library" "ICs And Semiconductors SMD"
			(at 60.96 234.95 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 60.96 236.855 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(instances
			(project "vme-wren"
				(path
					(reference "IC57")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 38.1 157.48 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR0351"
			(at 38.1 157.48 0)
		)
		(property "Value" "GND"
			(at 38.1 161.29 90)
		)
		(property "Footprint" ""
			(at 38.1 157.48 0)
		)
		(property "Datasheet" ""
			(at 38.1 157.48 0)
		)
		(property "Description" ""
			(at 38.1 157.48 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0351")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Resistors SMD:R0402_33R_1%_0.0625W_100PPM")
		(at 113.03 218.44 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R386"
			(at 115.316 215.392 0)
		)
		(property "Value" "R0402_33R_1%_0.0625W_100PPM"
			(at 113.03 223.393 0)
		)
		(property "Footprint" "Resistors SMD:RESC1005X40N"
			(at 113.03 225.298 0)
		)
		(property "Datasheet" ""
			(at 113.03 227.203 0)
		)
		(property "Description" "±1%"
			(at 116.84 213.36 0)
		)
		(property "Val" "33"
			(at 120.142 215.392 0)
		)
		(property "Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 113.03 229.108 0)
		)
		(property "Library Ref" "Resistor - 1%"
			(at 113.03 231.013 0)
		)
		(property "Library Path" "SchLib\\Resistors.SchLib"
			(at 113.03 232.918 0)
		)
		(property "Comment" "33"
			(at 113.03 234.823 0)
		)
		(property "Component Kind" "Standard"
			(at 113.03 236.728 0)
		)
		(property "Component Type" "Standard"
			(at 113.03 238.633 0)
		)
		(property "PackageDescription" " "
			(at 113.03 240.538 0)
		)
		(property "Pin Count" "2"
			(at 113.03 242.443 0)
		)
		(property "Footprint Path" "PcbLib\\Resistors SMD.PcbLib"
			(at 113.03 244.348 0)
		)
		(property "Footprint Ref" "RESC1005X40N"
			(at 113.03 246.253 0)
		)
		(property "Status" "Not Recommended"
			(at 113.03 248.158 0)
		)
		(property "Power" "0.0625W"
			(at 113.03 250.063 0)
		)
		(property "Voltage" " "
			(at 113.03 253.873 0)
		)
		(property "Tolerance" "±1%"
			(at 113.03 255.778 0)
		)
		(property "Part Description" "General Purpose Thick Film Chip Resistor"
			(at 113.03 257.683 0)
		)
		(property "Manufacturer" "GENERIC"
			(at 113.03 259.588 0)
		)
		(property "Manufacturer Part Number" "R0402_33R_1%_0.0625W_100PPM"
			(at 113.03 261.493 0)
		)
		(property "Case" "0402"
			(at 113.03 263.398 0)
		)
		(property "PressFit" "No"
			(at 113.03 265.303 0)
		)
		(property "Mounted" "Yes"
			(at 113.03 267.208 0)
		)
		(property "Sense Comment" " "
			(at 113.03 269.113 0)
		)
		(property "Sense" "No"
			(at 113.03 271.018 0)
		)
		(property "Status Comment" " "
			(at 113.03 272.923 0)
		)
		(property "Socket" "No"
			(at 113.03 274.828 0)
		)
		(property "SMD" "Yes"
			(at 113.03 276.733 0)
		)
		(property "ComponentHeight" " "
			(at 113.03 278.638 0)
		)
		(property "Manufacturer1 Example" "YAGEO PHYCOMP"
			(at 113.03 280.543 0)
		)
		(property "Manufacturer1 Part Number" "232270673309L"
			(at 113.03 282.448 0)
		)
		(property "Manufacturer1 ComponentHeight" "0.4mm"
			(at 113.03 284.353 0)
		)
		(property "HelpURL" ""
			(at 113.03 286.258 0)
		)
		(property "Author" "CERN DEM JLC"
			(at 113.03 288.163 0)
		)
		(property "CreateDate" "12/03/07 00:00:00"
			(at 113.03 290.068 0)
		)
		(property "LatestRevisionDate" "10/17/12 00:00:00"
			(at 113.03 291.973 0)
		)
		(property "Database Table Name" "Resistors"
			(at 113.03 293.878 0)
		)
		(property "Library Name" "Resistors SMD"
			(at 113.03 295.783 0)
		)
		(property "Footprint Library" "Resistors SMD"
			(at 113.03 297.688 0)
		)
		(property "License" "CC-BY-SA 4.0"
			(at 113.03 299.593 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "vme-wren"
				(path
					(reference "R386")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 200.66 265.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0721"
			(at 200.66 265.43 0)
		)
		(property "Value" "GND"
			(at 200.66 269.24 0)
		)
		(property "Footprint" ""
			(at 200.66 265.43 0)
		)
		(property "Datasheet" ""
			(at 200.66 265.43 0)
		)
		(property "Description" ""
			(at 200.66 265.43 0)
		)
		(pin "1")
		(instances
			(project "dupa"
				(path
					(reference "#PWR?")
					(unit 1)
				)
			)
			(project "vme-wren"
				(path
					(reference "#PWR0721")
					(unit 1)
				)
			)
		)
	)
	(sheet
		(at 234.95 97.79)
		(size 38.1 40.64)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "vme_p0"
			(at 234.95 97.0784 0)
		)
		(property "Sheetfile" "vme_p0.kicad_sch"
			(at 234.95 139.0146 0)
		)
		(pin "LVDS_TURNCLK2_N" input
			(at 234.95 110.49 180)
		)
		(pin "TTL_TURNCLK2" input
			(at 234.95 115.57 180)
		)
		(pin "LVDS_TURNCLK2_P" input
			(at 234.95 107.95 180)
		)
		(pin "LVDS_TURNCLK1_P" input
			(at 234.95 102.87 180)
		)
		(pin "LVDS_TURNCLK1_N" input
			(at 234.95 105.41 180)
		)
		(pin "TTL_TURNCLK1" input
			(at 234.95 113.03 180)
		)
		(pin "{HWBYTE}" bidirectional
			(at 234.95 100.33 180)
		)
		(pin "LVDS_BUNCHCLK1_N" input
			(at 234.95 125.73 180)
		)
		(pin "LVDS_BUNCHCLK1_P" input
			(at 234.95 123.19 180)
		)
		(pin "TTL_BUNCHCLK1" input
			(at 234.95 133.35 180)
		)
		(pin "LVDS_BUNCHCLK2_P" input
			(at 234.95 128.27 180)
		)
		(pin "LVDS_BUNCHCLK2_N" input
			(at 234.95 130.81 180)
		)
		(pin "TTL_BUNCHCLK2" input
			(at 234.95 135.89 180)
		)
		(instances
			(project "vme-wren"
				(path
					(page "18")
				)
			)
		)
	)
	(sheet
		(at 341.63 41.91)
		(size 34.29 15.24)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "vme_buffers_addr"
			(at 341.63 41.1984 0)
		)
		(property "Sheetfile" "vme_buffers_addr.kicad_sch"
			(at 341.63 57.7346 0)
		)
		(pin "{VMEPX}" bidirectional
			(at 341.63 44.45 180)
		)
		(pin "{VMEF}" bidirectional
			(at 375.92 44.45 0)
		)
		(instances
			(project "vme-wren"
				(path
					(page "15")
				)
			)
		)
	)
	(sheet
		(at 198.12 38.1)
		(size 43.18 19.05)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "vme_buffers_userio_p2"
			(at 198.12 37.3884 0)
		)
		(property "Sheetfile" "vme_buffers_userio_p2.kicad_sch"
			(at 198.12 57.7346 0)
		)
		(pin "{USERIO_A}" bidirectional
			(at 198.12 40.64 180)
		)
		(pin "{VMEPX_USERIO_A}" bidirectional
			(at 241.3 44.45 0)
		)
		(instances
			(project "vme-wren"
				(path
					(page "28")
				)
			)
		)
	)
	(sheet
		(at 143.51 97.79)
		(size 53.34 36.83)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "vme_buffers_p0_hwbyte"
			(at 143.51 97.0784 0)
		)
		(property "Sheetfile" "vme_buffers_p0_hwbyte.kicad_sch"
			(at 143.51 135.2046 0)
		)
		(pin "{HWBYTE}" bidirectional
			(at 196.85 100.33 0)
		)
		(pin "{F_HWBYTE}" bidirectional
			(at 143.51 118.11 180)
		)
		(instances
			(project "vme-wren"
				(path
					(page "29")
				)
			)
		)
	)
	(sheet
		(at 279.4 41.91)
		(size 38.1 53.34)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "vme_p1_p2"
			(at 279.4 41.1984 0)
		)
		(property "Sheetfile" "vme_p1_p2.kicad_sch"
			(at 279.4 95.8346 0)
		)
		(pin "TTC_DATA1_N" input
			(at 279.4 76.2 180)
		)
		(pin "TTC_DATA0_N" input
			(at 279.4 71.12 180)
		)
		(pin "TTC_DATA1_P" input
			(at 279.4 78.74 180)
		)
		(pin "TTC_DATA0_P" input
			(at 279.4 73.66 180)
		)
		(pin "{VMEPX}" bidirectional
			(at 317.5 44.45 0)
		)
		(pin "{VMEPX_USERIO_A}" bidirectional
			(at 279.4 44.45 180)
		)
		(pin "RS485_DATA1_P" input
			(at 279.4 82.55 180)
		)
		(pin "RS485_DATA0_P" input
			(at 279.4 87.63 180)
		)
		(pin "RS485_DATA1_N" input
			(at 279.4 85.09 180)
		)
		(pin "RS485_DATA0_N" input
			(at 279.4 90.17 180)
		)
		(instances
			(project "vme-wren"
				(path
					(page "17")
				)
			)
		)
	)
	(sheet
		(at 341.63 63.5)
		(size 34.29 15.24)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "vme_buffers_data"
			(at 341.63 62.7884 0)
		)
		(property "Sheetfile" "vme_buffers_data.kicad_sch"
			(at 341.63 79.3246 0)
		)
		(pin "{VMEPX}" bidirectional
			(at 341.63 66.04 180)
		)
		(pin "{VMEF}" bidirectional
			(at 375.92 66.04 0)
		)
		(instances
			(project "vme-wren"
				(path
					(page "16")
				)
			)
		)
	)
	(sheet
		(at 341.63 86.36)
		(size 34.29 16.51)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fill
			(color 0 0 0 0.0000)
		)
		(property "Sheetname" "vme_buffers_aux"
			(at 341.9344 85.598 0)
		)
		(property "Sheetfile" "vme_buffers_aux.kicad_sch"
			(at 340.9446 103.886 0)
		)
		(pin "{VMEF}" bidirectional
			(at 375.92 88.9 0)
		)
		(pin "{VMEPX}" bidirectional
			(at 341.63 88.9 180)
		)
		(instances
			(project "vme-wren"
				(path
					(page "27")
				)
			)
		)
	)
)
