(footprint "JACK_ALIM"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "module 1 pin (ou trou mecanique de percage)")
	(tags "CONN JACK")
	(property "Reference" "REF**"
		(at 0.254 -5.588 180)
		(layer "F.SilkS")
	)
	(property "Value" "JACK_2P"
		(at -5.5 0 90)
		(layer "F.SilkS")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(pad "1" thru_hole rect
		(at 7.9 0.1)
		(size 4.8006 5.5)
		(drill oval 1.2 4.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 0 0)
		(size 4.8006 5)
		(drill oval 1.016 4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 3.1 6.2)
		(size 4.8006 3.5)
		(drill oval 4 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/prj.3dshapes/Jack.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
