(footprint "SW_SPDT"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Switch inverseur")
	(tags "SWITCH DEV")
	(property "Reference" "REF**"
		(at 9.017 2.413 180)
		(layer "F.SilkS")
	)
	(property "Value" "SWITCH_INV"
		(at 8.89 -2.286 180)
		(layer "F.SilkS")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(pad "1" thru_hole rect
		(at 0 -5.08)
		(size 3.81 2.54)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole rect
		(at 0 0)
		(size 3.81 2.54)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole rect
		(at 0 5.08)
		(size 3.81 2.54)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/prj.3dshapes/Device.switch_toggle_horizontal_right_angle_PC_terminal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
