(footprint "SOIC127P600X175-8N"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density")
	(property "Reference" "REF**"
		(at 0 -4.006 0)
		(layer "F.SilkS")
	)
	(property "Value" "TL072CD"
		(at 0 3.776 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" "TL072CD"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "Operational Amplifier x2 Type1"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Operational Amplifiers.SchLib"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "TL072CD"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Device" "TL072CD"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" "SOIC 8, Pitch 1.27mm - Body 4x5mm, IPC Medium Density"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "Dual Low-Noise JFET-Input Operational Amplifier"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "TEXAS INSTRUMENTS"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "TL072CD"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "8"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" "SOIC8"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" "No"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Bonding" "No"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "1.75mm"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "SOIC127P600X175-8N"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM JMW"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" "\\\\cern.ch\\dfs\\Applications\\Altium\\Datasheets\\TL072CD.pdf"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1URL" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2URL" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2Description" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1Description" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "05/07/08 00:00:00"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "05/07/08 00:00:00"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SCEM" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate1" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Field1" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "ICs And Semiconductors"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Operational Amplifiers"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "ICs And Semiconductors SMD"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "This work is licensed under the Creative Commons CC-BY-SA 4.0 License. To the extent that circuit schematics that use Licensed Material can be considered to be ‘Adapted Material’, then the copyright holder waives article 3.b of the license with respect to these schematics."
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at -2.7 -1.905 270)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.7 -0.635 270)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.7 0.635 270)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.7 1.905 270)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 2.7 1.905 270)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 2.7 0.635 270)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 2.7 -0.635 270)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 2.7 -1.905 270)
		(size 0.6 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
