(kicad_symbol_lib
	(version 20231120)
	(generator "kicad_symbol_editor")
	(generator_version "7.99")
	(symbol "VCA810"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 6.35 0)
		)
		(property "Value" "VCA810"
			(at 1.27 3.81 0)
		)
		(property "Footprint" ""
			(at 1.27 1.27 0)
		)
		(property "Datasheet" ""
			(at 1.27 3.81 0)
		)
		(property "Description" "High Gain Adjust Range, Wideband and Variable Gain Amplifier"
			(at 0 0 0)
		)
		(property "ki_keywords" "single opamp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm* TO*99*"
			(at 0 0 0)
		)
		(symbol "VCA810_0_1")
		(symbol "VCA810_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 6.35)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 5.08)
				(name "Gain")
				(number "3")
			)
			(pin no_connect line
				(at 0 2.54 270)
				(length 2.54) hide
				(name "NC")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "7")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "8")
			)
		)
	)
)