(kicad_symbol_lib (version 20230620) (generator kicad_symbol_editor)
  (symbol "PWM" (pin_names (offset 1.016) hide) (exclude_from_sim no) (in_bom yes) (on_board yes)
    (property "Reference" "A1" (at -3.81 1.7146 0))
    (property "Value" "PWM" (at -3.81 -0.8254 0))
    (property "Footprint" "" (at 0 0 0))
    (property "Datasheet" "https://ngspice.sourceforge.io/docs.html" (at 0 16.51 0))
    (property "Description" "Voltage-dependent Voltage source symbol for simulation only" (at 0 0 0))
    (property "Sim.Library" "pwm2_model.lib" (at 0 0 0))
    (property "Sim.Name" "pwm" (at 0 0 0))
    (property "Sim.Device" "SUBCKT" (at 0 0 0))
    (property "Sim.Pins" "1=out+ 2=out- 3=in+ 4=in-" (at -27.94 -6.35 0))
    (property "Sim.Params" "freq=100k vlo=0.7 vhi=3.5" (at -16.51 -3.81 0))
    (property "ki_keywords" "simulation" (at 0 0 0))
    (symbol "PWM_0_1")
    (symbol "PWM_1_1"
      (text "V" (at 5.08 -0.254 0))
      (pin input line (at 0 5.08 270) (length 2.54)
        (name "N+")
        (number "1")
      )
      (pin input line (at 0 -5.08 90) (length 2.54)
        (name "N-")
        (number "2")
      )
      (pin passive line (at 5.08 5.08 270) (length 2.54)
        (name "C+")
        (number "3")
      )
      (pin passive line (at 5.08 -5.08 90) (length 2.54)
        (name "C-")
        (number "4")
      )
    )
  )
)
