(footprint "1005_C"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(tags "0402 1005")
	(property "Reference" "REF**"
		(at 0.15 -0.762742 180)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "0.1uF"
		(at 1.25 0.4 180)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "MPN" "0402WGF1003TCE"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "USD_per_1" "0,08"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "USD_per_1000" "0,024"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Dielectric" "X7R"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint_Density" "C"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Package" "1608"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Tolerance" "10%"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Voltage" "16V"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sim.Device" "C"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sim.Params" "c=\"\""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sim.Pins" "1=+ 2=-"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin 0.03)
	(solder_paste_margin -0.02)
	(attr smd)
	(pad "1" smd roundrect
		(at -0.45 0 180)
		(size 0.4 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "2" smd roundrect
		(at 0.45 0 180)
		(size 0.4 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(embedded_fonts no)
	(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
