(footprint "1P-1.5x1.5"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 4 -0.3 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "EXTGND"
		(at 0.025 -10.225 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "Description" "Not Populated"
		(at 157.25 -100.25 0)
		(layer "B.Fab")
		(hide yes)
	)
	(attr through_hole)
	(pad "1" connect roundrect
		(at 0 0 180)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.067)
		(zone_connect 1)
		(thermal_bridge_width 0.5)
		(thermal_gap 0.25)
	)
	(embedded_fonts no)
)
