(footprint "Crystal_4-SMD_2.5x2mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 2.135711 -0.830583 90)
		(layer "F.SilkS")
	)
	(property "Value" "12MHz 50ppm 16-20pF"
		(at 0 0.75 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "MPN" "CM4012M00020T8188026"
		(at 0 0 45)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin 0.001)
	(solder_paste_margin -0.025)
	(attr smd)
	(pad "" smd roundrect
		(at -0.85 -0.7 180)
		(size 1 1)
		(layers "F.Paste")
		(roundrect_rratio 0.33)
	)
	(pad "" smd roundrect
		(at -0.85 0.7 180)
		(size 1 1)
		(layers "F.Paste")
		(roundrect_rratio 0.33)
	)
	(pad "" smd roundrect
		(at 0.85 -0.7 180)
		(size 1 1)
		(layers "F.Paste")
		(roundrect_rratio 0.33)
	)
	(pad "" smd roundrect
		(at 0.85 0.7 180)
		(size 1 1)
		(layers "F.Paste")
		(roundrect_rratio 0.33)
	)
	(pad "1" smd roundrect
		(at -0.85 0.7 180)
		(size 1.2 1.1)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "2" smd roundrect
		(at 0.85 0.7 180)
		(size 1.2 1.1)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "3" smd roundrect
		(at 0.85 -0.7 180)
		(size 1.2 1.1)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(pad "4" smd roundrect
		(at -0.85 -0.7 180)
		(size 1.2 1.1)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.1)
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/3dmodels/Crystal_SMD_4P_2520.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
