(footprint "D_0402"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(tags "SMD 0402")
	(property "Reference" "REF**"
		(at 1.35 0 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "TVS"
		(at 1.25 0.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" "0.5pF 3.3V"
		(at 150.4 103.75 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "MPN" "AR0521P1"
		(at -0.1 -0.75 0)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_paste_margin -0.02)
	(attr smd)
	(pad "1" smd roundrect
		(at -0.45 0 180)
		(size 0.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "2" smd roundrect
		(at 0.45 0 180)
		(size 0.4 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(embedded_fonts no)
	(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-923.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
