(footprint "JP-2_1.5x1.5"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -1.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "EXTPWR"
		(at 0 1.1 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "Description" "Not Populated"
		(at 157.25 -105.9 90)
		(layer "B.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files allow_soldermask_bridges)
	(fp_text user "${REFERENCE}"
		(at 0 1.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" connect custom
		(at -0.975 -0.05 270)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.000001 1.05) (xy -0.249999 0.55) (xy 0.25 0.55)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.5 1.049999) (xy -0.75 0.55) (xy -0.249999 0.55)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.5 1.05) (xy 0.25 0.55) (xy 0.75 0.550001)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" connect custom
		(at 0.975 -0.05 270)
		(size 1.5 1.5)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.249994 -1.05) (xy -0.000007 -0.55) (xy -0.5 -0.55)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 0.250006 -1.049999) (xy 0.499994 -0.55) (xy -0.000001 -0.55)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
)
