(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "7seg-single" (pin_names (offset 0.635)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -2.54 13.97 0))
    (property "Value" "7seg-single" (id 1) (at -3.81 -13.97 0))
    (property "Footprint" "" (id 2) (at 0 -15.24 0))
    (property "Datasheet" "" (id 3) (at -12.7 12.065 0))
    (property "ki_keywords" "display LED 7-segment" (id 4) (at 0 0 0))
    (property "ki_description" "One digit 7 segment blue LED, common cathode" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "KCSC02?136*" (id 6) (at 0 0 0))
    (symbol "7seg-single_0_0"
      (text "A" (at 0.254 5.588 0))
      (text "B" (at 2.54 4.826 0))
      (text "C" (at 2.286 1.778 0))
      (text "D" (at -0.254 1.016 0))
      (text "DP" (at 3.556 0.254 0))
      (text "E" (at -2.54 1.778 0))
      (text "F" (at -2.286 4.826 0))
      (text "G" (at 0 4.064 0))
    )
    (symbol "7seg-single_0_1")
    (symbol "7seg-single_1_1"
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "E")
        (number "1")
      )
      (pin input line (at -7.62 -7.62 0) (length 2.54)
        (name "G")
        (number "10")
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "D")
        (number "2")
      )
      (pin input line (at 7.62 -7.62 180) (length 2.54)
        (name "CC")
        (number "3")
      )
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "C")
        (number "4")
      )
      (pin input line (at -7.62 -10.16 0) (length 2.54)
        (name "DP")
        (number "5")
      )
      (pin input line (at -7.62 5.08 0) (length 2.54)
        (name "B")
        (number "6")
      )
      (pin input line (at -7.62 7.62 0) (length 2.54)
        (name "A")
        (number "7")
      )
      (pin input line (at 7.62 -10.16 180) (length 2.54)
        (name "CC")
        (number "8")
      )
      (pin input line (at -7.62 -5.08 0) (length 2.54)
        (name "F")
        (number "9")
      )
    )
  )
  (symbol "MCP1319" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -2.54 6.35 0))
    (property "Value" "MCP1319" (id 1) (at 1.27 -6.35 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5" (id 2) (at 0 -8.89 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (symbol "MCP1319_0_1")
    (symbol "MCP1319_1_1"
      (pin input line (at -6.35 2.54 0) (length 2.54)
        (name "~{RST}")
        (number "1")
      )
      (pin input line (at -6.35 0 0) (length 2.54)
        (name "GND")
        (number "2")
      )
      (pin input line (at -6.35 -2.54 0) (length 2.54)
        (name "RST")
        (number "3")
      )
      (pin input line (at 8.89 -2.54 180) (length 2.54)
        (name "~{MR}")
        (number "4")
      )
      (pin input line (at 8.89 2.54 180) (length 2.54)
        (name "VDD")
        (number "5")
      )
    )
  )
  (symbol "MIC5318" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -3.81 5.08 0))
    (property "Value" "MIC5318" (id 1) (at -1.27 -5.08 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5" (id 2) (at -2.54 6.35 0))
    (property "Datasheet" "" (id 3) (at -2.54 6.35 0))
    (symbol "MIC5318_0_1")
    (symbol "MIC5318_1_1"
      (pin input line (at -7.62 2.54 0) (length 2.54)
        (name "VIN")
        (number "1")
      )
      (pin input line (at -7.62 0 0) (length 2.54)
        (name "GND")
        (number "2")
      )
      (pin input line (at -7.62 -2.54 0) (length 2.54)
        (name "EN")
        (number "3")
      )
      (pin input line (at 7.62 -2.54 180) (length 2.54)
        (name "ADJ")
        (number "4")
      )
      (pin input line (at 7.62 2.54 180) (length 2.54)
        (name "VOUT")
        (number "5")
      )
    )
  )
)
