(footprint "LRTDK"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 1.548684 -12.766603 90)
		(layer "F.SilkS")
	)
	(property "Value" "470ns"
		(at 7.009684 -13.020603 0)
		(layer "F.SilkS")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(pad "1" thru_hole circle
		(at -12.7 0)
		(size 1.524 1.524)
		(drill 0.8128)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 12.7 0)
		(size 1.524 1.524)
		(drill 0.8128)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at -10.16 0)
		(size 1.524 1.524)
		(drill 0.8128)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 7.62 0)
		(size 1.524 1.524)
		(drill 0.8128)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
