(footprint "subclick"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(locked yes)
	(layer "F.Cu")
	(descr "Connecteur Subclick")
	(tags "CONN DEV")
	(property "Reference" "REF**"
		(at 0 6.35 0)
		(layer "F.SilkS")
	)
	(property "Value" "BNC"
		(at -4.191 6.477 0)
		(layer "F.SilkS")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.778 1.778)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -2.54 -2.54)
		(size 3.048 3.048)
		(drill 1.524)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -2.54 2.54)
		(size 3.048 3.048)
		(drill 1.524)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.54 -2.54)
		(size 3.048 3.048)
		(drill 1.524)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.54 2.54)
		(size 3.048 3.048)
		(drill 1.524)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/libs/fp.3dshapes/subclick_horiz.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
