(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "+12V"
		(power)
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -1.27 0)
		)
		(property "Value" "+12V"
			(at 0 2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "+12V_0_0"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "+12V")
				(number "1")
			)
		)
		(symbol "+12V_0_1")
		(embedded_fonts no)
	)
	(symbol "+3.3V"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -1.016 0)
		)
		(property "Value" "+3.3V"
			(at 0 2.794 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "+3.3V_0_0"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "+3.3V")
				(number "1")
			)
		)
		(symbol "+3.3V_0_1")
		(embedded_fonts no)
	)
	(symbol "+5F"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 -1.27 0)
		)
		(property "Value" "+5F"
			(at 0 2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "+5F_0_0"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "+5F")
				(number "1")
			)
		)
		(symbol "+5F_0_1")
		(embedded_fonts no)
	)
	(symbol "+5V"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 2.286 0)
		)
		(property "Value" "+5V"
			(at 0 2.286 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "+5V_0_0"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "+5V")
				(number "1")
			)
		)
		(symbol "+5V_0_1")
		(embedded_fonts no)
	)
	(symbol "24C16"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "24C16"
			(at 5.08 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "24C16_0_0"
			(pin power_in line
				(at 0 12.7 270)
				(length 5.08)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
		)
		(symbol "24C16_1_1"
			(pin input line
				(at -17.78 5.08 0)
				(length 7.62)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 7.62)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -17.78 0 0)
				(length 7.62)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 7.62)
				(name "WP")
				(number "7")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 7.62)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 7.62)
				(name "SDA")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4C4001"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 0 0)
		)
		(property "Value" "4C4001"
			(at 1.27 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "4C4001_0_1")
		(symbol "4C4001_1_1"
			(pin input line
				(at -16.51 17.78 0)
				(length 7.62)
				(name "A0")
				(number "6")
			)
			(pin input line
				(at -16.51 15.24 0)
				(length 7.62)
				(name "A1")
				(number "7")
			)
			(pin input line
				(at -16.51 12.7 0)
				(length 7.62)
				(name "A2")
				(number "8")
			)
			(pin input line
				(at -16.51 10.16 0)
				(length 7.62)
				(name "A3")
				(number "9")
			)
			(pin input line
				(at -16.51 7.62 0)
				(length 7.62)
				(name "A4")
				(number "11")
			)
			(pin input line
				(at -16.51 5.08 0)
				(length 7.62)
				(name "A5")
				(number "12")
			)
			(pin input line
				(at -16.51 2.54 0)
				(length 7.62)
				(name "A6")
				(number "13")
			)
			(pin input line
				(at -16.51 0 0)
				(length 7.62)
				(name "A7")
				(number "14")
			)
			(pin input line
				(at -16.51 -2.54 0)
				(length 7.62)
				(name "A8")
				(number "15")
			)
			(pin input line
				(at -16.51 -5.08 0)
				(length 7.62)
				(name "A9")
				(number "5")
			)
			(pin input inverted
				(at -16.51 -10.16 0)
				(length 7.62)
				(name "RAS")
				(number "4")
			)
			(pin input inverted
				(at -16.51 -12.7 0)
				(length 7.62)
				(name "CAS")
				(number "17")
			)
			(pin input inverted
				(at -16.51 -15.24 0)
				(length 7.62)
				(name "WR")
				(number "3")
			)
			(pin input inverted
				(at -16.51 -17.78 0)
				(length 7.62)
				(name "OE")
				(number "16")
			)
			(pin power_in line
				(at -6.35 19.05 90)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at -6.35 -19.05 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin tri_state line
				(at 16.51 17.78 180)
				(length 7.62)
				(name "D0")
				(number "1")
			)
			(pin tri_state line
				(at 16.51 15.24 180)
				(length 7.62)
				(name "D1")
				(number "2")
			)
			(pin tri_state line
				(at 16.51 12.7 180)
				(length 7.62)
				(name "D2")
				(number "18")
			)
			(pin tri_state line
				(at 16.51 10.16 180)
				(length 7.62)
				(name "D3")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LS245"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 14.605 0)
		)
		(property "Value" "74LS245"
			(at 1.27 -14.605 0)
		)
		(property "Footprint" ""
			(at 1.27 -16.51 0)
		)
		(property "Datasheet" ""
			(at 2.54 14.605 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "74LS245_0_0"
			(pin power_in line
				(at 0 13.97 270)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -13.97 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "10")
			)
		)
		(symbol "74LS245_0_1")
		(symbol "74LS245_1_1"
			(pin tri_state line
				(at -17.78 12.7 0)
				(length 7.62)
				(name "A0")
				(number "2")
			)
			(pin tri_state line
				(at -17.78 10.16 0)
				(length 7.62)
				(name "A1")
				(number "3")
			)
			(pin tri_state line
				(at -17.78 7.62 0)
				(length 7.62)
				(name "A2")
				(number "4")
			)
			(pin tri_state line
				(at -17.78 5.08 0)
				(length 7.62)
				(name "A3")
				(number "5")
			)
			(pin tri_state line
				(at -17.78 2.54 0)
				(length 7.62)
				(name "A4")
				(number "6")
			)
			(pin tri_state line
				(at -17.78 0 0)
				(length 7.62)
				(name "A5")
				(number "7")
			)
			(pin tri_state line
				(at -17.78 -2.54 0)
				(length 7.62)
				(name "A6")
				(number "8")
			)
			(pin tri_state line
				(at -17.78 -5.08 0)
				(length 7.62)
				(name "A7")
				(number "9")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 7.62)
				(name "A->B")
				(number "1")
			)
			(pin input inverted
				(at -17.78 -12.7 0)
				(length 7.62)
				(name "CE")
				(number "19")
			)
			(pin tri_state line
				(at 17.78 12.7 180)
				(length 7.62)
				(name "B0")
				(number "18")
			)
			(pin tri_state line
				(at 17.78 10.16 180)
				(length 7.62)
				(name "B1")
				(number "17")
			)
			(pin tri_state line
				(at 17.78 7.62 180)
				(length 7.62)
				(name "B2")
				(number "16")
			)
			(pin tri_state line
				(at 17.78 5.08 180)
				(length 7.62)
				(name "B3")
				(number "15")
			)
			(pin tri_state line
				(at 17.78 2.54 180)
				(length 7.62)
				(name "B4")
				(number "14")
			)
			(pin tri_state line
				(at 17.78 0 180)
				(length 7.62)
				(name "B5")
				(number "13")
			)
			(pin tri_state line
				(at 17.78 -2.54 180)
				(length 7.62)
				(name "B6")
				(number "12")
			)
			(pin tri_state line
				(at 17.78 -5.08 180)
				(length 7.62)
				(name "B7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AV9173"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 4.318 11.43 0)
		)
		(property "Value" "AV9173"
			(at 6.604 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "AV9173_0_1")
		(symbol "AV9173_1_1"
			(pin input line
				(at -24.13 7.62 0)
				(length 7.62)
				(name "FREFIN")
				(number "2")
			)
			(pin input line
				(at -24.13 2.54 0)
				(length 7.62)
				(name "FSIGIN")
				(number "1")
			)
			(pin input line
				(at -24.13 -2.54 0)
				(length 7.62)
				(name "FS0")
				(number "4")
			)
			(pin input line
				(at -24.13 -7.62 0)
				(length 7.62)
				(name "OE")
				(number "5")
			)
			(pin input line
				(at -1.27 12.7 270)
				(length 3.81)
				(name "VCC")
				(number "7")
			)
			(pin input line
				(at -1.27 -12.7 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin tri_state line
				(at 24.13 2.54 180)
				(length 7.62)
				(name "CKKOUT")
				(number "6")
			)
			(pin tri_state line
				(at 24.13 -2.54 180)
				(length 7.62)
				(name "CLK/2")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BNC"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at 0.254 3.048 0)
		)
		(property "Value" "BNC"
			(at 2.794 -1.524 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "BNC_0_1")
		(symbol "BNC_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 3.302)
				(name "In")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 3.302)
				(name "Ext")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BT253"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "BT253"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "BT253_0_1")
		(symbol "BT253_1_1"
			(pin input line
				(at -26.67 63.5 0)
				(length 7.62)
				(name "CEXT2")
				(number "7")
			)
			(pin output line
				(at -26.67 60.96 0)
				(length 7.62)
				(name "CEXT1")
				(number "6")
			)
			(pin input line
				(at -26.67 58.42 0)
				(length 7.62)
				(name "RSET")
				(number "69")
			)
			(pin passive line
				(at -26.67 53.34 0)
				(length 7.62)
				(name "IOUT0")
				(number "82")
			)
			(pin passive line
				(at -26.67 50.8 0)
				(length 7.62)
				(name "IOUT1")
				(number "80")
			)
			(pin passive line
				(at -26.67 48.26 0)
				(length 7.62)
				(name "IOUT2")
				(number "78")
			)
			(pin passive line
				(at -26.67 45.72 0)
				(length 7.62)
				(name "IOUT3")
				(number "76")
			)
			(pin passive line
				(at -26.67 43.18 0)
				(length 7.62)
				(name "IOUT4")
				(number "73")
			)
			(pin passive line
				(at -26.67 40.64 0)
				(length 7.62)
				(name "IOUT5")
				(number "71")
			)
			(pin input line
				(at -26.67 35.56 0)
				(length 7.62)
				(name "RREF+")
				(number "66")
			)
			(pin input line
				(at -26.67 33.02 0)
				(length 7.62)
				(name "GREF+")
				(number "65")
			)
			(pin input line
				(at -26.67 30.48 0)
				(length 7.62)
				(name "BREF+")
				(number "64")
			)
			(pin input line
				(at -26.67 25.4 0)
				(length 7.62)
				(name "RREF-")
				(number "21")
			)
			(pin input line
				(at -26.67 22.86 0)
				(length 7.62)
				(name "GREF-")
				(number "22")
			)
			(pin input line
				(at -26.67 20.32 0)
				(length 7.62)
				(name "BREF-")
				(number "23")
			)
			(pin input line
				(at -26.67 15.24 0)
				(length 7.62)
				(name "RVID0")
				(number "83")
			)
			(pin input line
				(at -26.67 12.7 0)
				(length 7.62)
				(name "GVID0")
				(number "79")
			)
			(pin input line
				(at -26.67 10.16 0)
				(length 7.62)
				(name "BVID0")
				(number "75")
			)
			(pin input inverted
				(at -26.67 7.62 0)
				(length 7.62)
				(name "SYNC0")
				(number "4")
			)
			(pin input line
				(at -26.67 2.54 0)
				(length 7.62)
				(name "RVID1")
				(number "81")
			)
			(pin input line
				(at -26.67 0 0)
				(length 7.62)
				(name "GVID1")
				(number "77")
			)
			(pin input line
				(at -26.67 -2.54 0)
				(length 7.62)
				(name "BVID1")
				(number "74")
			)
			(pin input inverted
				(at -26.67 -5.08 0)
				(length 7.62)
				(name "SYNC1")
				(number "5")
			)
			(pin tri_state line
				(at -26.67 -15.24 0)
				(length 7.62)
				(name "D0")
				(number "16")
			)
			(pin tri_state line
				(at -26.67 -17.78 0)
				(length 7.62)
				(name "D1")
				(number "15")
			)
			(pin tri_state line
				(at -26.67 -20.32 0)
				(length 7.62)
				(name "D2")
				(number "14")
			)
			(pin tri_state line
				(at -26.67 -22.86 0)
				(length 7.62)
				(name "D3")
				(number "13")
			)
			(pin tri_state line
				(at -26.67 -25.4 0)
				(length 7.62)
				(name "D4")
				(number "12")
			)
			(pin tri_state line
				(at -26.67 -27.94 0)
				(length 7.62)
				(name "D5")
				(number "11")
			)
			(pin tri_state line
				(at -26.67 -30.48 0)
				(length 7.62)
				(name "D6")
				(number "10")
			)
			(pin tri_state line
				(at -26.67 -33.02 0)
				(length 7.62)
				(name "D7")
				(number "9")
			)
			(pin input inverted
				(at -26.67 -38.1 0)
				(length 7.62)
				(name "RD")
				(number "20")
			)
			(pin input inverted
				(at -26.67 -40.64 0)
				(length 7.62)
				(name "WR")
				(number "24")
			)
			(pin input line
				(at -26.67 -45.72 0)
				(length 7.62)
				(name "A0")
				(number "17")
			)
			(pin input line
				(at -26.67 -48.26 0)
				(length 7.62)
				(name "A1")
				(number "18")
			)
			(pin input line
				(at -26.67 -50.8 0)
				(length 7.62)
				(name "A2")
				(number "19")
			)
			(pin input line
				(at -3.81 73.66 270)
				(length 7.62)
				(name "VAA")
				(number "84")
			)
			(pin input line
				(at -3.81 -73.66 90)
				(length 7.62)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at -1.27 73.66 270)
				(length 7.62)
				(name "VAA")
				(number "1")
			)
			(pin input line
				(at -1.27 -73.66 90)
				(length 7.62)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at 1.27 73.66 270)
				(length 7.62)
				(name "VAA")
				(number "43")
			)
			(pin input line
				(at 1.27 -73.66 90)
				(length 7.62)
				(name "GND")
				(number "41")
			)
			(pin input line
				(at 3.81 73.66 270)
				(length 7.62)
				(name "VAA")
				(number "44")
			)
			(pin input line
				(at 3.81 -73.66 90)
				(length 7.62)
				(name "GND")
				(number "42")
			)
			(pin output inverted
				(at 26.67 63.5 180)
				(length 7.62)
				(name "CSYNC")
				(number "8")
			)
			(pin output line
				(at 26.67 53.34 180)
				(length 7.62)
				(name "ROUT")
				(number "72")
			)
			(pin input line
				(at 26.67 50.8 180)
				(length 7.62)
				(name "RIN")
				(number "62")
			)
			(pin output line
				(at 26.67 45.72 180)
				(length 7.62)
				(name "GOUT")
				(number "70")
			)
			(pin input line
				(at 26.67 43.18 180)
				(length 7.62)
				(name "GIN")
				(number "60")
			)
			(pin output line
				(at 26.67 38.1 180)
				(length 7.62)
				(name "BOUT")
				(number "68")
			)
			(pin input line
				(at 26.67 35.56 180)
				(length 7.62)
				(name "BIN")
				(number "58")
			)
			(pin input line
				(at 26.67 30.48 180)
				(length 7.62)
				(name "CLAMP")
				(number "59")
			)
			(pin input line
				(at 26.67 27.94 180)
				(length 7.62)
				(name "ZERO")
				(number "37")
			)
			(pin input line
				(at 26.67 25.4 180)
				(length 7.62)
				(name "RLEVEL")
				(number "67")
			)
			(pin input line
				(at 26.67 22.86 180)
				(length 7.62)
				(name "GLEVEL")
				(number "63")
			)
			(pin input line
				(at 26.67 20.32 180)
				(length 7.62)
				(name "BLEVEL")
				(number "61")
			)
			(pin input clock
				(at 26.67 15.24 180)
				(length 7.62)
				(name "RCLOCK")
				(number "40")
			)
			(pin input clock
				(at 26.67 12.7 180)
				(length 7.62)
				(name "GCLOCK")
				(number "39")
			)
			(pin input clock
				(at 26.67 10.16 180)
				(length 7.62)
				(name "BCLOCK")
				(number "38")
			)
			(pin tri_state line
				(at 26.67 5.08 180)
				(length 7.62)
				(name "R0")
				(number "56")
			)
			(pin tri_state line
				(at 26.67 2.54 180)
				(length 7.62)
				(name "R1")
				(number "55")
			)
			(pin tri_state line
				(at 26.67 0 180)
				(length 7.62)
				(name "R2")
				(number "54")
			)
			(pin tri_state line
				(at 26.67 -2.54 180)
				(length 7.62)
				(name "R3")
				(number "53")
			)
			(pin tri_state line
				(at 26.67 -5.08 180)
				(length 7.62)
				(name "R4")
				(number "52")
			)
			(pin tri_state line
				(at 26.67 -7.62 180)
				(length 7.62)
				(name "R5")
				(number "51")
			)
			(pin tri_state line
				(at 26.67 -10.16 180)
				(length 7.62)
				(name "R6")
				(number "50")
			)
			(pin tri_state line
				(at 26.67 -12.7 180)
				(length 7.62)
				(name "R7")
				(number "49")
			)
			(pin tri_state line
				(at 26.67 -17.78 180)
				(length 7.62)
				(name "G0")
				(number "48")
			)
			(pin tri_state line
				(at 26.67 -20.32 180)
				(length 7.62)
				(name "G1")
				(number "47")
			)
			(pin tri_state line
				(at 26.67 -22.86 180)
				(length 7.62)
				(name "G2")
				(number "46")
			)
			(pin tri_state line
				(at 26.67 -25.4 180)
				(length 7.62)
				(name "G3")
				(number "45")
			)
			(pin tri_state line
				(at 26.67 -27.94 180)
				(length 7.62)
				(name "G4")
				(number "36")
			)
			(pin tri_state line
				(at 26.67 -30.48 180)
				(length 7.62)
				(name "G5")
				(number "35")
			)
			(pin tri_state line
				(at 26.67 -33.02 180)
				(length 7.62)
				(name "G6")
				(number "34")
			)
			(pin tri_state line
				(at 26.67 -35.56 180)
				(length 7.62)
				(name "G7")
				(number "33")
			)
			(pin tri_state line
				(at 26.67 -40.64 180)
				(length 7.62)
				(name "B0")
				(number "32")
			)
			(pin tri_state line
				(at 26.67 -43.18 180)
				(length 7.62)
				(name "B1")
				(number "31")
			)
			(pin tri_state line
				(at 26.67 -45.72 180)
				(length 7.62)
				(name "B2")
				(number "30")
			)
			(pin tri_state line
				(at 26.67 -48.26 180)
				(length 7.62)
				(name "B3")
				(number "29")
			)
			(pin tri_state line
				(at 26.67 -50.8 180)
				(length 7.62)
				(name "B4")
				(number "28")
			)
			(pin tri_state line
				(at 26.67 -53.34 180)
				(length 7.62)
				(name "B5")
				(number "27")
			)
			(pin tri_state line
				(at 26.67 -55.88 180)
				(length 7.62)
				(name "B6")
				(number "26")
			)
			(pin tri_state line
				(at 26.67 -58.42 180)
				(length 7.62)
				(name "B7")
				(number "25")
			)
			(pin input inverted
				(at 26.67 -63.5 180)
				(length 7.62)
				(name "OE")
				(number "57")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BT473"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "BT473"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "BT473_0_1")
		(symbol "BT473_1_1"
			(pin input line
				(at -25.4 58.42 0)
				(length 7.62)
				(name "R0")
				(number "45")
			)
			(pin input line
				(at -25.4 55.88 0)
				(length 7.62)
				(name "R1")
				(number "46")
			)
			(pin input line
				(at -25.4 53.34 0)
				(length 7.62)
				(name "R2")
				(number "47")
			)
			(pin input line
				(at -25.4 50.8 0)
				(length 7.62)
				(name "R3")
				(number "48")
			)
			(pin input line
				(at -25.4 48.26 0)
				(length 7.62)
				(name "R4")
				(number "49")
			)
			(pin input line
				(at -25.4 45.72 0)
				(length 7.62)
				(name "R5")
				(number "50")
			)
			(pin input line
				(at -25.4 43.18 0)
				(length 7.62)
				(name "R6")
				(number "51")
			)
			(pin input line
				(at -25.4 40.64 0)
				(length 7.62)
				(name "R7")
				(number "52")
			)
			(pin input line
				(at -25.4 35.56 0)
				(length 7.62)
				(name "G0")
				(number "53")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 7.62)
				(name "G1")
				(number "54")
			)
			(pin input line
				(at -25.4 30.48 0)
				(length 7.62)
				(name "G2")
				(number "55")
			)
			(pin input line
				(at -25.4 27.94 0)
				(length 7.62)
				(name "G3")
				(number "56")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 7.62)
				(name "G4")
				(number "57")
			)
			(pin input line
				(at -25.4 22.86 0)
				(length 7.62)
				(name "G5")
				(number "58")
			)
			(pin input line
				(at -25.4 20.32 0)
				(length 7.62)
				(name "G6")
				(number "59")
			)
			(pin input line
				(at -25.4 17.78 0)
				(length 7.62)
				(name "G7")
				(number "60")
			)
			(pin input line
				(at -25.4 12.7 0)
				(length 7.62)
				(name "B0")
				(number "61")
			)
			(pin input line
				(at -25.4 10.16 0)
				(length 7.62)
				(name "B1")
				(number "62")
			)
			(pin input line
				(at -25.4 7.62 0)
				(length 7.62)
				(name "B2")
				(number "63")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 7.62)
				(name "B3")
				(number "64")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 7.62)
				(name "B4")
				(number "65")
			)
			(pin input line
				(at -25.4 0 0)
				(length 7.62)
				(name "B5")
				(number "66")
			)
			(pin input line
				(at -25.4 -2.54 0)
				(length 7.62)
				(name "B6")
				(number "67")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 7.62)
				(name "B7")
				(number "68")
			)
			(pin input line
				(at -25.4 -10.16 0)
				(length 7.62)
				(name "D0")
				(number "14")
			)
			(pin input line
				(at -25.4 -12.7 0)
				(length 7.62)
				(name "D1")
				(number "15")
			)
			(pin input line
				(at -25.4 -15.24 0)
				(length 7.62)
				(name "D2")
				(number "16")
			)
			(pin input line
				(at -25.4 -17.78 0)
				(length 7.62)
				(name "D3")
				(number "17")
			)
			(pin input line
				(at -25.4 -20.32 0)
				(length 7.62)
				(name "D4")
				(number "18")
			)
			(pin input line
				(at -25.4 -22.86 0)
				(length 7.62)
				(name "D5")
				(number "19")
			)
			(pin input line
				(at -25.4 -25.4 0)
				(length 7.62)
				(name "D6")
				(number "20")
			)
			(pin input line
				(at -25.4 -27.94 0)
				(length 7.62)
				(name "D7")
				(number "21")
			)
			(pin input line
				(at -25.4 -33.02 0)
				(length 7.62)
				(name "RS0")
				(number "24")
			)
			(pin input line
				(at -25.4 -35.56 0)
				(length 7.62)
				(name "RS1")
				(number "25")
			)
			(pin input line
				(at -25.4 -38.1 0)
				(length 7.62)
				(name "RS2")
				(number "26")
			)
			(pin input inverted
				(at -25.4 -43.18 0)
				(length 7.62)
				(name "WR")
				(number "22")
			)
			(pin input inverted
				(at -25.4 -45.72 0)
				(length 7.62)
				(name "RD")
				(number "23")
			)
			(pin input line
				(at -25.4 -50.8 0)
				(length 7.62)
				(name "OL0")
				(number "10")
			)
			(pin input line
				(at -25.4 -53.34 0)
				(length 7.62)
				(name "OL1")
				(number "11")
			)
			(pin input line
				(at -25.4 -55.88 0)
				(length 7.62)
				(name "OL2")
				(number "12")
			)
			(pin input line
				(at -25.4 -58.42 0)
				(length 7.62)
				(name "OL3")
				(number "13")
			)
			(pin input line
				(at -7.62 68.58 270)
				(length 7.62)
				(name "VAA")
				(number "1")
			)
			(pin input line
				(at -5.08 68.58 270)
				(length 7.62)
				(name "VAA")
				(number "2")
			)
			(pin input line
				(at -5.08 -68.58 90)
				(length 7.62)
				(name "GND")
				(number "3")
			)
			(pin input line
				(at -2.54 68.58 270)
				(length 7.62)
				(name "VAA")
				(number "33")
			)
			(pin input line
				(at -2.54 -68.58 90)
				(length 7.62)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 0 68.58 270)
				(length 7.62)
				(name "VAA")
				(number "34")
			)
			(pin input line
				(at 0 -68.58 90)
				(length 7.62)
				(name "GND")
				(number "31")
			)
			(pin input line
				(at 2.54 68.58 270)
				(length 7.62)
				(name "VAA")
				(number "35")
			)
			(pin input line
				(at 2.54 -68.58 90)
				(length 7.62)
				(name "GND")
				(number "32")
			)
			(pin input line
				(at 5.08 68.58 270)
				(length 7.62)
				(name "VAA")
				(number "36")
			)
			(pin output line
				(at 25.4 50.8 180)
				(length 7.62)
				(name "RED")
				(number "37")
			)
			(pin output line
				(at 25.4 45.72 180)
				(length 7.62)
				(name "GRE")
				(number "38")
			)
			(pin output line
				(at 25.4 40.64 180)
				(length 7.62)
				(name "BLU")
				(number "39")
			)
			(pin input line
				(at 25.4 30.48 180)
				(length 7.62)
				(name "IREF")
				(number "40")
			)
			(pin input line
				(at 25.4 25.4 180)
				(length 7.62)
				(name "VREF")
				(number "43")
			)
			(pin input line
				(at 25.4 20.32 180)
				(length 7.62)
				(name "COMP")
				(number "41")
			)
			(pin output line
				(at 25.4 15.24 180)
				(length 7.62)
				(name "OPA")
				(number "42")
			)
			(pin output line
				(at 25.4 10.16 180)
				(length 7.62)
				(name "VREFOUT")
				(number "44")
			)
			(pin input inverted
				(at 25.4 0 180)
				(length 7.62)
				(name "SYNC")
				(number "8")
			)
			(pin input inverted
				(at 25.4 -5.08 180)
				(length 7.62)
				(name "BLANK")
				(number "7")
			)
			(pin input clock
				(at 25.4 -10.16 180)
				(length 7.62)
				(name "CLOCK")
				(number "9")
			)
			(pin output line
				(at 25.4 -20.32 180)
				(length 7.62)
				(name "CR0")
				(number "27")
			)
			(pin output line
				(at 25.4 -22.86 180)
				(length 7.62)
				(name "CR1")
				(number "28")
			)
			(pin output line
				(at 25.4 -25.4 180)
				(length 7.62)
				(name "CR2")
				(number "29")
			)
			(pin output line
				(at 25.4 -27.94 180)
				(length 7.62)
				(name "CR3")
				(number "30")
			)
			(pin input line
				(at 25.4 -38.1 180)
				(length 7.62)
				(name "S0")
				(number "5")
			)
			(pin input line
				(at 25.4 -40.64 180)
				(length 7.62)
				(name "S1")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BT812"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 47.498 85.09 0)
		)
		(property "Value" "BT812"
			(at 31.242 -85.09 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "BT812_0_1")
		(symbol "BT812_1_1"
			(pin input line
				(at -52.07 73.66 0)
				(length 7.62)
				(name "XTAL1_IN")
				(number "108")
			)
			(pin output line
				(at -52.07 71.12 0)
				(length 7.62)
				(name "XTAL1_OUT")
				(number "109")
			)
			(pin input line
				(at -52.07 66.04 0)
				(length 7.62)
				(name "XTAL2_IN")
				(number "106")
			)
			(pin output line
				(at -52.07 63.5 0)
				(length 7.62)
				(name "XTAL2_OUT")
				(number "107")
			)
			(pin input inverted
				(at -52.07 58.42 0)
				(length 7.62)
				(name "VTU_EN")
				(number "46")
			)
			(pin input inverted
				(at -52.07 55.88 0)
				(length 7.62)
				(name "PIXEL_EN")
				(number "47")
			)
			(pin input line
				(at -52.07 50.8 0)
				(length 7.62)
				(name "TCLK")
				(number "90")
			)
			(pin input line
				(at -52.07 48.26 0)
				(length 7.62)
				(name "TMS")
				(number "89")
			)
			(pin input line
				(at -52.07 45.72 0)
				(length 7.62)
				(name "TDI")
				(number "88")
			)
			(pin output line
				(at -52.07 43.18 0)
				(length 7.62)
				(name "TDO")
				(number "101")
			)
			(pin input line
				(at -52.07 38.1 0)
				(length 7.62)
				(name "VID0_Y")
				(number "156")
			)
			(pin input line
				(at -52.07 35.56 0)
				(length 7.62)
				(name "VID0_C")
				(number "125")
			)
			(pin input line
				(at -52.07 30.48 0)
				(length 7.62)
				(name "VID1_Y")
				(number "154")
			)
			(pin input line
				(at -52.07 27.94 0)
				(length 7.62)
				(name "VID1_C")
				(number "127")
			)
			(pin input line
				(at -52.07 22.86 0)
				(length 7.62)
				(name "VID2_Y")
				(number "152")
			)
			(pin input line
				(at -52.07 20.32 0)
				(length 7.62)
				(name "VID2_C")
				(number "129")
			)
			(pin input line
				(at -52.07 15.24 0)
				(length 7.62)
				(name "VID3_Y")
				(number "150")
			)
			(pin input line
				(at -52.07 12.7 0)
				(length 7.62)
				(name "VID3_C")
				(number "131")
			)
			(pin input line
				(at -52.07 7.62 0)
				(length 7.62)
				(name "SYNC_DET")
				(number "140")
			)
			(pin input line
				(at -52.07 2.54 0)
				(length 7.62)
				(name "YLEVEL")
				(number "7")
			)
			(pin input line
				(at -52.07 0 0)
				(length 7.62)
				(name "YREF+")
				(number "144")
			)
			(pin input line
				(at -52.07 -2.54 0)
				(length 7.62)
				(name "YREF-")
				(number "3")
			)
			(pin input line
				(at -52.07 -7.62 0)
				(length 7.62)
				(name "CLEVEL")
				(number "114")
			)
			(pin input line
				(at -52.07 -10.16 0)
				(length 7.62)
				(name "CREF+")
				(number "137")
			)
			(pin input line
				(at -52.07 -12.7 0)
				(length 7.62)
				(name "CREF-")
				(number "118")
			)
			(pin input line
				(at -52.07 -17.78 0)
				(length 7.62)
				(name "R/2")
				(number "135")
			)
			(pin output line
				(at -52.07 -20.32 0)
				(length 7.62)
				(name "REFOUT")
				(number "113")
			)
			(pin tri_state line
				(at -52.07 -30.48 0)
				(length 7.62)
				(name "D0")
				(number "92")
			)
			(pin tri_state line
				(at -52.07 -33.02 0)
				(length 7.62)
				(name "D1")
				(number "93")
			)
			(pin tri_state line
				(at -52.07 -35.56 0)
				(length 7.62)
				(name "D2")
				(number "94")
			)
			(pin tri_state line
				(at -52.07 -38.1 0)
				(length 7.62)
				(name "D3")
				(number "95")
			)
			(pin tri_state line
				(at -52.07 -40.64 0)
				(length 7.62)
				(name "D4")
				(number "96")
			)
			(pin tri_state line
				(at -52.07 -43.18 0)
				(length 7.62)
				(name "D5")
				(number "97")
			)
			(pin tri_state line
				(at -52.07 -45.72 0)
				(length 7.62)
				(name "D6")
				(number "99")
			)
			(pin tri_state line
				(at -52.07 -48.26 0)
				(length 7.62)
				(name "D7")
				(number "100")
			)
			(pin input line
				(at -52.07 -53.34 0)
				(length 7.62)
				(name "RS0")
				(number "84")
			)
			(pin input line
				(at -52.07 -55.88 0)
				(length 7.62)
				(name "RS1")
				(number "85")
			)
			(pin input inverted
				(at -52.07 -60.96 0)
				(length 7.62)
				(name "RD")
				(number "86")
			)
			(pin input inverted
				(at -52.07 -63.5 0)
				(length 7.62)
				(name "WR")
				(number "83")
			)
			(pin input inverted
				(at -52.07 -68.58 0)
				(length 7.62)
				(name "RESET")
				(number "87")
			)
			(pin input line
				(at -41.91 91.44 270)
				(length 7.62)
				(name "VCC")
				(number "31")
			)
			(pin input line
				(at -41.91 -91.44 90)
				(length 7.62)
				(name "GND")
				(number "16")
			)
			(pin input line
				(at -39.37 91.44 270)
				(length 7.62)
				(name "VCC")
				(number "45")
			)
			(pin input line
				(at -39.37 -91.44 90)
				(length 7.62)
				(name "GND")
				(number "30")
			)
			(pin input line
				(at -36.83 91.44 270)
				(length 7.62)
				(name "VCC")
				(number "57")
			)
			(pin input line
				(at -36.83 -91.44 90)
				(length 7.62)
				(name "GND")
				(number "44")
			)
			(pin input line
				(at -34.29 91.44 270)
				(length 7.62)
				(name "VCC")
				(number "76")
			)
			(pin input line
				(at -34.29 -91.44 90)
				(length 7.62)
				(name "GND")
				(number "56")
			)
			(pin passive line
				(at -31.75 91.44 270)
				(length 7.62)
				(name "VCC")
				(number "91")
			)
			(pin input line
				(at -31.75 -91.44 90)
				(length 7.62)
				(name "GND")
				(number "66")
			)
			(pin input line
				(at -29.21 91.44 270)
				(length 7.62)
				(name "VCC")
				(number "102")
			)
			(pin input line
				(at -29.21 -91.44 90)
				(length 7.62)
				(name "GND")
				(number "75")
			)
			(pin input line
				(at -26.67 91.44 270)
				(length 7.62)
				(name "VCC")
				(number "112")
			)
			(pin input line
				(at -26.67 -91.44 90)
				(length 7.62)
				(name "GND")
				(number "98")
			)
			(pin input line
				(at -24.13 -91.44 90)
				(length 7.62)
				(name "GND")
				(number "103")
			)
			(pin input line
				(at -21.59 -91.44 90)
				(length 7.62)
				(name "GND")
				(number "111")
			)
			(pin input line
				(at -16.51 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "1")
			)
			(pin input line
				(at -16.51 -91.44 90)
				(length 7.62)
				(name "GNDA")
				(number "5")
			)
			(pin input line
				(at -13.97 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "2")
			)
			(pin input line
				(at -13.97 -91.44 90)
				(length 7.62)
				(name "GNDA")
				(number "116")
			)
			(pin input line
				(at -11.43 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "39")
			)
			(pin input line
				(at -11.43 -91.44 90)
				(length 7.62)
				(name "GNDA")
				(number "124")
			)
			(pin input line
				(at -8.89 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "40")
			)
			(pin input line
				(at -8.89 -91.44 90)
				(length 7.62)
				(name "GNDA")
				(number "126")
			)
			(pin input line
				(at -6.35 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "41")
			)
			(pin input line
				(at -6.35 -91.44 90)
				(length 7.62)
				(name "GNDA")
				(number "128")
			)
			(pin input line
				(at -3.81 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "42")
			)
			(pin input line
				(at -3.81 -91.44 90)
				(length 7.62)
				(name "GNDA")
				(number "130")
			)
			(pin input line
				(at -1.27 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "43")
			)
			(pin input line
				(at -1.27 -91.44 90)
				(length 7.62)
				(name "GNDA")
				(number "134")
			)
			(pin input line
				(at 1.27 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "78")
			)
			(pin input line
				(at 1.27 -91.44 90)
				(length 7.62)
				(name "GNDA")
				(number "136")
			)
			(pin input line
				(at 3.81 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "79")
			)
			(pin input line
				(at 3.81 -91.44 90)
				(length 7.62)
				(name "GNDA")
				(number "138")
			)
			(pin input line
				(at 6.35 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "80")
			)
			(pin input line
				(at 6.35 -91.44 90)
				(length 7.62)
				(name "GNDA")
				(number "139")
			)
			(pin input line
				(at 8.89 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "81")
			)
			(pin input line
				(at 8.89 -91.44 90)
				(length 7.62)
				(name "GNDA")
				(number "143")
			)
			(pin input line
				(at 11.43 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "82")
			)
			(pin input line
				(at 11.43 -91.44 90)
				(length 7.62)
				(name "GNDA")
				(number "145")
			)
			(pin input line
				(at 13.97 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "119")
			)
			(pin input line
				(at 13.97 -91.44 90)
				(length 7.62)
				(name "GNDA")
				(number "147")
			)
			(pin input line
				(at 16.51 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "120")
			)
			(pin input line
				(at 16.51 -91.44 90)
				(length 7.62)
				(name "GNDA")
				(number "151")
			)
			(pin input line
				(at 19.05 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "121")
			)
			(pin input line
				(at 19.05 -91.44 90)
				(length 7.62)
				(name "GNDA")
				(number "153")
			)
			(pin input line
				(at 21.59 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "122")
			)
			(pin input line
				(at 21.59 -91.44 90)
				(length 7.62)
				(name "GNDA")
				(number "155")
			)
			(pin passive line
				(at 24.13 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "123")
			)
			(pin input line
				(at 24.13 -91.44 90)
				(length 7.62)
				(name "GNDA")
				(number "157")
			)
			(pin input line
				(at 26.67 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "132")
			)
			(pin input line
				(at 29.21 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "141")
			)
			(pin input line
				(at 31.75 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "142")
			)
			(pin input line
				(at 34.29 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "149")
			)
			(pin input line
				(at 36.83 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "158")
			)
			(pin input line
				(at 39.37 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "159")
			)
			(pin input line
				(at 41.91 91.44 270)
				(length 7.62)
				(name "VAA")
				(number "160")
			)
			(pin tri_state line
				(at 52.07 73.66 180)
				(length 7.62)
				(name "R0")
				(number "65")
			)
			(pin tri_state line
				(at 52.07 71.12 180)
				(length 7.62)
				(name "R1")
				(number "64")
			)
			(pin tri_state line
				(at 52.07 68.58 180)
				(length 7.62)
				(name "R2")
				(number "63")
			)
			(pin tri_state line
				(at 52.07 66.04 180)
				(length 7.62)
				(name "R3")
				(number "62")
			)
			(pin tri_state line
				(at 52.07 63.5 180)
				(length 7.62)
				(name "R4")
				(number "61")
			)
			(pin tri_state line
				(at 52.07 60.96 180)
				(length 7.62)
				(name "R5")
				(number "60")
			)
			(pin tri_state line
				(at 52.07 58.42 180)
				(length 7.62)
				(name "R6")
				(number "59")
			)
			(pin tri_state line
				(at 52.07 55.88 180)
				(length 7.62)
				(name "R7")
				(number "58")
			)
			(pin tri_state line
				(at 52.07 50.8 180)
				(length 7.62)
				(name "G0")
				(number "74")
			)
			(pin tri_state line
				(at 52.07 48.26 180)
				(length 7.62)
				(name "G1")
				(number "73")
			)
			(pin tri_state line
				(at 52.07 45.72 180)
				(length 7.62)
				(name "G2")
				(number "72")
			)
			(pin tri_state line
				(at 52.07 43.18 180)
				(length 7.62)
				(name "G3")
				(number "71")
			)
			(pin tri_state line
				(at 52.07 40.64 180)
				(length 7.62)
				(name "G4")
				(number "70")
			)
			(pin tri_state line
				(at 52.07 38.1 180)
				(length 7.62)
				(name "G5")
				(number "69")
			)
			(pin tri_state line
				(at 52.07 35.56 180)
				(length 7.62)
				(name "G6")
				(number "68")
			)
			(pin tri_state line
				(at 52.07 33.02 180)
				(length 7.62)
				(name "G7")
				(number "67")
			)
			(pin tri_state line
				(at 52.07 27.94 180)
				(length 7.62)
				(name "B0")
				(number "55")
			)
			(pin tri_state line
				(at 52.07 25.4 180)
				(length 7.62)
				(name "B1")
				(number "54")
			)
			(pin tri_state line
				(at 52.07 22.86 180)
				(length 7.62)
				(name "B2")
				(number "53")
			)
			(pin tri_state line
				(at 52.07 20.32 180)
				(length 7.62)
				(name "B3")
				(number "52")
			)
			(pin tri_state line
				(at 52.07 17.78 180)
				(length 7.62)
				(name "B4")
				(number "51")
			)
			(pin tri_state line
				(at 52.07 15.24 180)
				(length 7.62)
				(name "B5")
				(number "50")
			)
			(pin tri_state line
				(at 52.07 12.7 180)
				(length 7.62)
				(name "B6")
				(number "49")
			)
			(pin tri_state line
				(at 52.07 10.16 180)
				(length 7.62)
				(name "B7")
				(number "48")
			)
			(pin output line
				(at 52.07 0 180)
				(length 7.62)
				(name "OUT_Y")
				(number "6")
			)
			(pin output line
				(at 52.07 -2.54 180)
				(length 7.62)
				(name "OUT_C")
				(number "115")
			)
			(pin input line
				(at 52.07 -7.62 180)
				(length 7.62)
				(name "VIN_Y/COMP.")
				(number "4")
			)
			(pin input line
				(at 52.07 -10.16 180)
				(length 7.62)
				(name "VIN_C")
				(number "117")
			)
			(pin output line
				(at 52.07 -20.32 180)
				(length 7.62)
				(name "CAPTURE")
				(number "38")
			)
			(pin output line
				(at 52.07 -22.86 180)
				(length 7.62)
				(name "VALID")
				(number "29")
			)
			(pin output line
				(at 52.07 -25.4 180)
				(length 7.62)
				(name "CBFLAG")
				(number "28")
			)
			(pin output line
				(at 52.07 -27.94 180)
				(length 7.62)
				(name "SERROR")
				(number "37")
			)
			(pin output inverted
				(at 52.07 -35.56 180)
				(length 7.62)
				(name "HRESET")
				(number "36")
			)
			(pin output inverted
				(at 52.07 -38.1 180)
				(length 7.62)
				(name "VRESET")
				(number "34")
			)
			(pin output inverted
				(at 52.07 -40.64 180)
				(length 7.62)
				(name "HACTIVE")
				(number "35")
			)
			(pin output inverted
				(at 52.07 -43.18 180)
				(length 7.62)
				(name "VACTIVE")
				(number "33")
			)
			(pin output line
				(at 52.07 -45.72 180)
				(length 7.62)
				(name "ACTIVE")
				(number "32")
			)
			(pin bidirectional line
				(at 52.07 -50.8 180)
				(length 7.62)
				(name "FIELD_0")
				(number "26")
			)
			(pin bidirectional line
				(at 52.07 -53.34 180)
				(length 7.62)
				(name "FIELD_1")
				(number "25")
			)
			(pin output line
				(at 52.07 -55.88 180)
				(length 7.62)
				(name "FIELD_2")
				(number "27")
			)
			(pin output line
				(at 52.07 -60.96 180)
				(length 7.62)
				(name "CLKX1")
				(number "104")
			)
			(pin output line
				(at 52.07 -63.5 180)
				(length 7.62)
				(name "CLKX2")
				(number "105")
			)
			(pin input line
				(at 52.07 -73.66 180)
				(length 7.62)
				(name "N/C")
				(number "110")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 0 2.54 0)
		)
		(property "Value" "C"
			(at 0.1524 -2.159 0)
		)
		(property "Footprint" ""
			(at 0.9652 -3.81 0)
		)
		(property "Datasheet" ""
			(at 0 2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SM* C? C1-1"
			(at 0 0 0)
		)
		(symbol "C_0_1")
		(symbol "C_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 4.318)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CONN_1"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at 2.032 0 0)
		)
		(property "Value" "CONN_1"
			(at 0 1.397 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_1_0_1")
		(symbol "CONN_1_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CONN_2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at -1.27 0 90)
		)
		(property "Value" "CONN_2"
			(at 1.27 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_2_0_1")
		(symbol "CONN_2_1_1"
			(pin passive inverted
				(at -8.89 2.54 0)
				(length 6.35)
				(name "P1")
				(number "1")
			)
			(pin passive inverted
				(at -8.89 -2.54 0)
				(length 6.35)
				(name "PM")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CONN_5"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "P"
			(at -1.27 0 90)
		)
		(property "Value" "CONN_5"
			(at 1.27 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CONN_5_0_1")
		(symbol "CONN_5_1_1"
			(pin passive inverted
				(at -10.16 5.08 0)
				(length 7.62)
				(name "~")
				(number "1")
			)
			(pin passive inverted
				(at -10.16 2.54 0)
				(length 7.62)
				(name "~")
				(number "2")
			)
			(pin passive inverted
				(at -10.16 0 0)
				(length 7.62)
				(name "~")
				(number "3")
			)
			(pin passive inverted
				(at -10.16 -2.54 0)
				(length 7.62)
				(name "~")
				(number "4")
			)
			(pin passive inverted
				(at -10.16 -5.08 0)
				(length 7.62)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CP"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 1.27 2.54 0)
		)
		(property "Value" "CP"
			(at 1.27 -2.54 0)
		)
		(property "Footprint" ""
			(at 2.54 -3.81 0)
		)
		(property "Datasheet" ""
			(at 1.27 2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CP* SM*"
			(at 0 0 0)
		)
		(symbol "CP_0_1")
		(symbol "CP_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 3.81)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 3.81)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CRYSTAL"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "X"
			(at 0 3.81 0)
		)
		(property "Value" "CRYSTAL"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CRYSTAL_0_1")
		(symbol "CRYSTAL_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CTRIM"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "C"
			(at 3.302 -2.032 0)
		)
		(property "Value" "CTRIM"
			(at 3.81 -4.064 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CTRIM_0_1")
		(symbol "CTRIM_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 4.318)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 4.318)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DB9"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 13.97 0)
		)
		(property "Value" "DB9"
			(at 0 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DB9*"
			(at 0 0 0)
		)
		(symbol "DB9_0_1")
		(symbol "DB9_1_1"
			(pin passive line
				(at -11.43 10.16 0)
				(length 7.62)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at -11.43 7.62 0)
				(length 7.62)
				(name "P9")
				(number "9")
			)
			(pin passive line
				(at -11.43 5.08 0)
				(length 7.62)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at -11.43 2.54 0)
				(length 7.62)
				(name "P8")
				(number "8")
			)
			(pin passive line
				(at -11.43 0 0)
				(length 7.62)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -11.43 -2.54 0)
				(length 7.62)
				(name "P7")
				(number "7")
			)
			(pin passive line
				(at -11.43 -5.08 0)
				(length 7.62)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at -11.43 -7.62 0)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin passive line
				(at -11.43 -10.16 0)
				(length 7.62)
				(name "1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DIODESCH"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "DIODESCH"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "D? S*"
			(at 0 0 0)
		)
		(symbol "DIODESCH_0_1")
		(symbol "DIODESCH_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "K")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GND"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 0 0)
		)
		(property "Value" "GND"
			(at 0 -1.778 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "GND_0_1")
		(symbol "GND_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "INDUCTOR"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "L"
			(at -1.27 0 90)
		)
		(property "Value" "INDUCTOR"
			(at 2.54 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "INDUCTOR_0_1")
		(symbol "INDUCTOR_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LED"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "LED"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV"
			(at 0 0 0)
		)
		(symbol "LED_0_1")
		(symbol "LED_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 3.81)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 3.81)
				(name "K")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LIGNE_A_RETARD"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "L"
			(at 0 2.54 0)
		)
		(property "Value" "LIGNE_A_RETARD"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LIGNE_A_RETARD_0_1")
		(symbol "LIGNE_A_RETARD_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "COMMUN")
				(number "3")
			)
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NPN"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 0 -3.81 0)
		)
		(property "Value" "NPN"
			(at 0 3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "NPN_0_1")
		(symbol "NPN_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 5.08)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCI_CONUNIV"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at 0 81.28 0)
		)
		(property "Value" "PCI_CONUNIV"
			(at 0 -81.28 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "PCI_CONUNIV_0_1")
		(symbol "PCI_CONUNIV_1_1"
			(pin power_in line
				(at -27.94 77.47 0)
				(length 8.89)
				(name "-12V")
				(number "B1")
			)
			(pin output line
				(at -27.94 74.93 0)
				(length 8.89)
				(name "TCK")
				(number "B2")
			)
			(pin input line
				(at -27.94 72.39 0)
				(length 8.89)
				(name "GND")
				(number "B3")
			)
			(pin input line
				(at -27.94 69.85 0)
				(length 8.89)
				(name "TDO")
				(number "B4")
			)
			(pin power_in line
				(at -27.94 67.31 0)
				(length 8.89)
				(name "+5V")
				(number "B5")
			)
			(pin power_in line
				(at -27.94 64.77 0)
				(length 8.89)
				(name "+5V")
				(number "B6")
			)
			(pin input inverted
				(at -27.94 62.23 0)
				(length 8.89)
				(name "INTB#")
				(number "B7")
			)
			(pin input inverted
				(at -27.94 59.69 0)
				(length 8.89)
				(name "INTD#")
				(number "B8")
			)
			(pin input inverted
				(at -27.94 57.15 0)
				(length 8.89)
				(name "PRSNT1#")
				(number "B9")
			)
			(pin passive line
				(at -27.94 54.61 0)
				(length 8.89)
				(name "RESERVED")
				(number "B10")
			)
			(pin input inverted
				(at -27.94 52.07 0)
				(length 8.89)
				(name "PRSNT2#")
				(number "B11")
			)
			(pin passive line
				(at -27.94 49.53 0)
				(length 8.89)
				(name "RESERVED")
				(number "B12")
			)
			(pin passive line
				(at -27.94 46.99 0)
				(length 8.89)
				(name "RESERVED")
				(number "B13")
			)
			(pin passive line
				(at -27.94 44.45 0)
				(length 8.89)
				(name "RESERVED")
				(number "B14")
			)
			(pin power_in line
				(at -27.94 41.91 0)
				(length 8.89)
				(name "GND")
				(number "B15")
			)
			(pin output line
				(at -27.94 39.37 0)
				(length 8.89)
				(name "CLK")
				(number "B16")
			)
			(pin power_in line
				(at -27.94 36.83 0)
				(length 8.89)
				(name "GND")
				(number "B17")
			)
			(pin bidirectional inverted
				(at -27.94 34.29 0)
				(length 8.89)
				(name "REQ#")
				(number "B18")
			)
			(pin power_in line
				(at -27.94 31.75 0)
				(length 8.89)
				(name "VIO")
				(number "B19")
			)
			(pin bidirectional line
				(at -27.94 29.21 0)
				(length 8.89)
				(name "AD[31]")
				(number "B20")
			)
			(pin bidirectional line
				(at -27.94 26.67 0)
				(length 8.89)
				(name "AD[29]")
				(number "B21")
			)
			(pin power_in line
				(at -27.94 24.13 0)
				(length 8.89)
				(name "GND")
				(number "B22")
			)
			(pin bidirectional line
				(at -27.94 21.59 0)
				(length 8.89)
				(name "AD[27]")
				(number "B23")
			)
			(pin bidirectional line
				(at -27.94 19.05 0)
				(length 8.89)
				(name "AD[25]")
				(number "B24")
			)
			(pin power_in line
				(at -27.94 16.51 0)
				(length 8.89)
				(name "+3.3V")
				(number "B25")
			)
			(pin bidirectional line
				(at -27.94 13.97 0)
				(length 8.89)
				(name "C/BE#[3]")
				(number "B26")
			)
			(pin bidirectional line
				(at -27.94 11.43 0)
				(length 8.89)
				(name "AD[23]")
				(number "B27")
			)
			(pin power_in line
				(at -27.94 8.89 0)
				(length 8.89)
				(name "GND")
				(number "B28")
			)
			(pin bidirectional line
				(at -27.94 6.35 0)
				(length 8.89)
				(name "AD[21]")
				(number "B29")
			)
			(pin bidirectional line
				(at -27.94 3.81 0)
				(length 8.89)
				(name "AD[19]")
				(number "B30")
			)
			(pin power_in line
				(at -27.94 1.27 0)
				(length 8.89)
				(name "+3.3V")
				(number "B31")
			)
			(pin bidirectional line
				(at -27.94 -1.27 0)
				(length 8.89)
				(name "AD[17]")
				(number "B32")
			)
			(pin bidirectional inverted
				(at -27.94 -3.81 0)
				(length 8.89)
				(name "C/BE#[2]")
				(number "B33")
			)
			(pin power_in line
				(at -27.94 -6.35 0)
				(length 8.89)
				(name "GND")
				(number "B34")
			)
			(pin bidirectional inverted
				(at -27.94 -8.89 0)
				(length 8.89)
				(name "IRDY#")
				(number "B35")
			)
			(pin power_in line
				(at -27.94 -11.43 0)
				(length 8.89)
				(name "+3.3V")
				(number "B36")
			)
			(pin bidirectional inverted
				(at -27.94 -13.97 0)
				(length 8.89)
				(name "DEVSEL#")
				(number "B37")
			)
			(pin power_in line
				(at -27.94 -16.51 0)
				(length 8.89)
				(name "GND")
				(number "B38")
			)
			(pin bidirectional inverted
				(at -27.94 -19.05 0)
				(length 8.89)
				(name "LOCK#")
				(number "B39")
			)
			(pin bidirectional inverted
				(at -27.94 -21.59 0)
				(length 8.89)
				(name "PERR#")
				(number "B40")
			)
			(pin power_in line
				(at -27.94 -24.13 0)
				(length 8.89)
				(name "+3.3V")
				(number "B41")
			)
			(pin input inverted
				(at -27.94 -26.67 0)
				(length 8.89)
				(name "SERR#")
				(number "B42")
			)
			(pin power_in line
				(at -27.94 -29.21 0)
				(length 8.89)
				(name "+3.3V")
				(number "B43")
			)
			(pin bidirectional inverted
				(at -27.94 -31.75 0)
				(length 8.89)
				(name "C/BE#[1]")
				(number "B44")
			)
			(pin bidirectional line
				(at -27.94 -34.29 0)
				(length 8.89)
				(name "AD[14]")
				(number "B45")
			)
			(pin power_in line
				(at -27.94 -36.83 0)
				(length 8.89)
				(name "GND")
				(number "B46")
			)
			(pin bidirectional line
				(at -27.94 -39.37 0)
				(length 8.89)
				(name "AD[12]")
				(number "B47")
			)
			(pin bidirectional line
				(at -27.94 -41.91 0)
				(length 8.89)
				(name "AD[10]")
				(number "B48")
			)
			(pin power_in line
				(at -27.94 -44.45 0)
				(length 8.89)
				(name "M66EN")
				(number "B49")
			)
			(pin bidirectional line
				(at -27.94 -52.07 0)
				(length 8.89)
				(name "AD[08]")
				(number "B52")
			)
			(pin bidirectional line
				(at -27.94 -54.61 0)
				(length 8.89)
				(name "AD[07]")
				(number "B53")
			)
			(pin input line
				(at -27.94 -57.15 0)
				(length 8.89)
				(name "+3.3V")
				(number "B54")
			)
			(pin bidirectional line
				(at -27.94 -59.69 0)
				(length 8.89)
				(name "AD[05]")
				(number "B55")
			)
			(pin bidirectional line
				(at -27.94 -62.23 0)
				(length 8.89)
				(name "AD[03]")
				(number "B56")
			)
			(pin power_in line
				(at -27.94 -64.77 0)
				(length 8.89)
				(name "GND")
				(number "B57")
			)
			(pin bidirectional line
				(at -27.94 -67.31 0)
				(length 8.89)
				(name "AD[01]")
				(number "B58")
			)
			(pin power_in line
				(at -27.94 -69.85 0)
				(length 8.89)
				(name "VIO")
				(number "B59")
			)
			(pin bidirectional inverted
				(at -27.94 -72.39 0)
				(length 8.89)
				(name "ACK64#")
				(number "B60")
			)
			(pin power_in line
				(at -27.94 -74.93 0)
				(length 8.89)
				(name "+5V")
				(number "B61")
			)
			(pin power_in line
				(at -27.94 -77.47 0)
				(length 8.89)
				(name "+5V")
				(number "B62")
			)
			(pin output inverted
				(at 27.94 77.47 180)
				(length 8.89)
				(name "TRST#")
				(number "A1")
			)
			(pin power_in line
				(at 27.94 74.93 180)
				(length 8.89)
				(name "+12V")
				(number "A2")
			)
			(pin output line
				(at 27.94 72.39 180)
				(length 8.89)
				(name "TMS")
				(number "A3")
			)
			(pin output line
				(at 27.94 69.85 180)
				(length 8.89)
				(name "TDI")
				(number "A4")
			)
			(pin power_in line
				(at 27.94 67.31 180)
				(length 8.89)
				(name "+5V")
				(number "A5")
			)
			(pin input inverted
				(at 27.94 64.77 180)
				(length 8.89)
				(name "INTA#")
				(number "A6")
			)
			(pin input inverted
				(at 27.94 62.23 180)
				(length 8.89)
				(name "INTC#")
				(number "A7")
			)
			(pin power_in line
				(at 27.94 59.69 180)
				(length 8.89)
				(name "+5V")
				(number "A8")
			)
			(pin passive line
				(at 27.94 57.15 180)
				(length 8.89)
				(name "RESERVED")
				(number "A9")
			)
			(pin power_in line
				(at 27.94 54.61 180)
				(length 8.89)
				(name "VIO")
				(number "A10")
			)
			(pin passive line
				(at 27.94 52.07 180)
				(length 8.89)
				(name "RESERVED")
				(number "A11")
			)
			(pin passive line
				(at 27.94 49.53 180)
				(length 8.89)
				(name "RESERVED")
				(number "A12")
			)
			(pin passive line
				(at 27.94 46.99 180)
				(length 8.89)
				(name "RESERVED")
				(number "A13")
			)
			(pin passive line
				(at 27.94 44.45 180)
				(length 8.89)
				(name "3.3VAUX")
				(number "A14")
			)
			(pin output inverted
				(at 27.94 41.91 180)
				(length 8.89)
				(name "RST#")
				(number "A15")
			)
			(pin power_in line
				(at 27.94 39.37 180)
				(length 8.89)
				(name "VIO")
				(number "A16")
			)
			(pin bidirectional inverted
				(at 27.94 36.83 180)
				(length 8.89)
				(name "GNT#")
				(number "A17")
			)
			(pin power_in line
				(at 27.94 34.29 180)
				(length 8.89)
				(name "GND")
				(number "A18")
			)
			(pin passive line
				(at 27.94 31.75 180)
				(length 8.89)
				(name "PME#")
				(number "A19")
			)
			(pin bidirectional line
				(at 27.94 29.21 180)
				(length 8.89)
				(name "AD[30]")
				(number "A20")
			)
			(pin power_in line
				(at 27.94 26.67 180)
				(length 8.89)
				(name "+3.3V")
				(number "A21")
			)
			(pin bidirectional line
				(at 27.94 24.13 180)
				(length 8.89)
				(name "AD[28]")
				(number "A22")
			)
			(pin bidirectional line
				(at 27.94 21.59 180)
				(length 8.89)
				(name "AD[26]")
				(number "A23")
			)
			(pin power_in line
				(at 27.94 19.05 180)
				(length 8.89)
				(name "GND")
				(number "A24")
			)
			(pin bidirectional line
				(at 27.94 16.51 180)
				(length 8.89)
				(name "AD[24]")
				(number "A25")
			)
			(pin output line
				(at 27.94 13.97 180)
				(length 8.89)
				(name "IDSEL")
				(number "A26")
			)
			(pin power_in line
				(at 27.94 11.43 180)
				(length 8.89)
				(name "+3.3V")
				(number "A27")
			)
			(pin bidirectional line
				(at 27.94 8.89 180)
				(length 8.89)
				(name "AD[22]")
				(number "A28")
			)
			(pin bidirectional line
				(at 27.94 6.35 180)
				(length 8.89)
				(name "AD[20]")
				(number "A29")
			)
			(pin power_in line
				(at 27.94 3.81 180)
				(length 8.89)
				(name "GND")
				(number "A30")
			)
			(pin bidirectional line
				(at 27.94 1.27 180)
				(length 8.89)
				(name "AD[18]")
				(number "A31")
			)
			(pin bidirectional line
				(at 27.94 -1.27 180)
				(length 8.89)
				(name "AD[16]")
				(number "A32")
			)
			(pin power_in line
				(at 27.94 -3.81 180)
				(length 8.89)
				(name "+3.3V")
				(number "A33")
			)
			(pin bidirectional inverted
				(at 27.94 -6.35 180)
				(length 8.89)
				(name "FRAME#")
				(number "A34")
			)
			(pin power_in line
				(at 27.94 -8.89 180)
				(length 8.89)
				(name "GND")
				(number "A35")
			)
			(pin bidirectional inverted
				(at 27.94 -11.43 180)
				(length 8.89)
				(name "TRDY#")
				(number "A36")
			)
			(pin power_in line
				(at 27.94 -13.97 180)
				(length 8.89)
				(name "GND")
				(number "A37")
			)
			(pin bidirectional inverted
				(at 27.94 -16.51 180)
				(length 8.89)
				(name "STOP#")
				(number "A38")
			)
			(pin power_in line
				(at 27.94 -19.05 180)
				(length 8.89)
				(name "+3.3V")
				(number "A39")
			)
			(pin bidirectional line
				(at 27.94 -21.59 180)
				(length 8.89)
				(name "RESERVED")
				(number "A40")
			)
			(pin bidirectional line
				(at 27.94 -24.13 180)
				(length 8.89)
				(name "RESERVED")
				(number "A41")
			)
			(pin power_in line
				(at 27.94 -26.67 180)
				(length 8.89)
				(name "GND")
				(number "A42")
			)
			(pin bidirectional line
				(at 27.94 -29.21 180)
				(length 8.89)
				(name "PAR")
				(number "A43")
			)
			(pin bidirectional line
				(at 27.94 -31.75 180)
				(length 8.89)
				(name "AD[15]")
				(number "A44")
			)
			(pin power_in line
				(at 27.94 -34.29 180)
				(length 8.89)
				(name "+3.3V")
				(number "A45")
			)
			(pin bidirectional line
				(at 27.94 -36.83 180)
				(length 8.89)
				(name "AD[13]")
				(number "A46")
			)
			(pin bidirectional line
				(at 27.94 -39.37 180)
				(length 8.89)
				(name "AD[11]")
				(number "A47")
			)
			(pin power_in line
				(at 27.94 -41.91 180)
				(length 8.89)
				(name "GND")
				(number "A48")
			)
			(pin bidirectional line
				(at 27.94 -44.45 180)
				(length 8.89)
				(name "AD[09]")
				(number "A49")
			)
			(pin bidirectional inverted
				(at 27.94 -52.07 180)
				(length 8.89)
				(name "C/BE#[0]")
				(number "A52")
			)
			(pin power_in line
				(at 27.94 -54.61 180)
				(length 8.89)
				(name "+3.3V")
				(number "A53")
			)
			(pin bidirectional line
				(at 27.94 -57.15 180)
				(length 8.89)
				(name "AD[06]")
				(number "A54")
			)
			(pin bidirectional line
				(at 27.94 -59.69 180)
				(length 8.89)
				(name "AD[04]")
				(number "A55")
			)
			(pin power_in line
				(at 27.94 -62.23 180)
				(length 8.89)
				(name "GND")
				(number "A56")
			)
			(pin bidirectional line
				(at 27.94 -64.77 180)
				(length 8.89)
				(name "AD[02]")
				(number "A57")
			)
			(pin bidirectional line
				(at 27.94 -67.31 180)
				(length 8.89)
				(name "AD[00]")
				(number "A58")
			)
			(pin power_in line
				(at 27.94 -69.85 180)
				(length 8.89)
				(name "VIO")
				(number "A59")
			)
			(pin bidirectional inverted
				(at 27.94 -72.39 180)
				(length 8.89)
				(name "REQ64#")
				(number "A60")
			)
			(pin power_in line
				(at 27.94 -74.93 180)
				(length 8.89)
				(name "+5V")
				(number "A61")
			)
			(pin power_in line
				(at 27.94 -77.47 180)
				(length 8.89)
				(name "+5V")
				(number "A62")
			)
		)
		(embedded_fonts no)
	)
	(symbol "POT"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "RV"
			(at 0 -2.54 0)
		)
		(property "Value" "POT"
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "POT_0_1")
		(symbol "POT_1_1"
			(pin passive line
				(at -6.35 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 0 3.81 270)
				(length 2.032)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 6.35 0 180)
				(length 2.54)
				(name "3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PWR_FLAG"
		(power)
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#FLG"
			(at 0 2.413 0)
		)
		(property "Value" "PWR_FLAG"
			(at 0 4.572 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "PWR_FLAG_0_0"
			(pin power_out line
				(at 0 0 90)
				(length 0)
				(name "pwr")
				(number "1")
			)
		)
		(symbol "PWR_FLAG_0_1")
		(embedded_fonts no)
	)
	(symbol "R"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at 2.032 0 90)
		)
		(property "Value" "R"
			(at 0.1778 0.0254 90)
		)
		(property "Footprint" ""
			(at -1.778 0 90)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R? SM0603 SM0805 R?-* SM1206"
			(at 0 0 0)
		)
		(symbol "R_0_1")
		(symbol "R_1_1"
			(pin passive line
				(at 0 6.35 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -6.35 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RR8"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "RR"
			(at 1.27 13.97 0)
		)
		(property "Value" "RR8"
			(at 0.762 0 90)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "RR8_0_1")
		(symbol "RR8_1_1"
			(pin passive inverted
				(at -8.89 11.43 0)
				(length 7.62)
				(name "COM")
				(number "1")
			)
			(pin passive inverted
				(at -8.89 8.89 0)
				(length 7.62)
				(name "2")
				(number "2")
			)
			(pin passive inverted
				(at -8.89 6.35 0)
				(length 7.62)
				(name "3")
				(number "3")
			)
			(pin passive inverted
				(at -8.89 3.81 0)
				(length 7.62)
				(name "4")
				(number "4")
			)
			(pin passive inverted
				(at -8.89 1.27 0)
				(length 7.62)
				(name "5")
				(number "5")
			)
			(pin passive inverted
				(at -8.89 -1.27 0)
				(length 7.62)
				(name "6")
				(number "6")
			)
			(pin passive inverted
				(at -8.89 -3.81 0)
				(length 7.62)
				(name "7")
				(number "7")
			)
			(pin passive inverted
				(at -8.89 -6.35 0)
				(length 7.62)
				(name "8")
				(number "8")
			)
			(pin passive inverted
				(at -8.89 -8.89 0)
				(length 7.62)
				(name "9")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "S5933_PQ160"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 57.15 0)
		)
		(property "Value" "S5933_PQ160"
			(at 25.4 -110.49 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "S5933_PQ160_0_0"
			(pin power_in line
				(at -7.62 107.95 270)
				(length 3.81)
				(name "VCC")
				(number "11")
			)
			(pin power_in line
				(at -6.35 -107.95 90)
				(length 3.81)
				(name "VSS")
				(number "150")
			)
			(pin power_in line
				(at -5.08 107.95 270)
				(length 3.81)
				(name "VCC")
				(number "31")
			)
			(pin power_in line
				(at -3.81 -107.95 90)
				(length 3.81)
				(name "VSS")
				(number "10")
			)
			(pin power_in line
				(at -2.54 107.95 270)
				(length 3.81)
				(name "VCC")
				(number "51")
			)
			(pin power_in line
				(at -1.27 -107.95 90)
				(length 3.81)
				(name "VSS")
				(number "30")
			)
			(pin power_in line
				(at 0 107.95 270)
				(length 3.81)
				(name "VCC")
				(number "71")
			)
			(pin power_in line
				(at 1.27 -107.95 90)
				(length 3.81)
				(name "VSS")
				(number "70")
			)
			(pin power_in line
				(at 2.54 107.95 270)
				(length 3.81)
				(name "VCC")
				(number "91")
			)
			(pin power_in line
				(at 3.81 -107.95 90)
				(length 3.81)
				(name "VSS")
				(number "50")
			)
			(pin power_in line
				(at 5.08 107.95 270)
				(length 3.81)
				(name "VCC")
				(number "111")
			)
			(pin power_in line
				(at 6.35 -107.95 90)
				(length 3.81)
				(name "VSS")
				(number "90")
			)
			(pin power_in line
				(at 7.62 107.95 270)
				(length 3.81)
				(name "VCC")
				(number "131")
			)
			(pin power_in line
				(at 8.89 -107.95 90)
				(length 3.81)
				(name "VSS")
				(number "110")
			)
			(pin power_in line
				(at 10.16 107.95 270)
				(length 3.81)
				(name "VCC")
				(number "151")
			)
			(pin power_in line
				(at 11.43 -107.95 90)
				(length 3.81)
				(name "VSS")
				(number "130")
			)
		)
		(symbol "S5933_PQ160_0_1")
		(symbol "S5933_PQ160_1_1"
			(pin bidirectional line
				(at -29.21 102.87 0)
				(length 7.62)
				(name "AD0")
				(number "56")
			)
			(pin bidirectional line
				(at -29.21 100.33 0)
				(length 7.62)
				(name "AD1")
				(number "55")
			)
			(pin bidirectional line
				(at -29.21 97.79 0)
				(length 7.62)
				(name "AD2")
				(number "54")
			)
			(pin bidirectional line
				(at -29.21 95.25 0)
				(length 7.62)
				(name "AD3")
				(number "52")
			)
			(pin bidirectional line
				(at -29.21 92.71 0)
				(length 7.62)
				(name "AD4")
				(number "48")
			)
			(pin bidirectional line
				(at -29.21 90.17 0)
				(length 7.62)
				(name "AD5")
				(number "47")
			)
			(pin bidirectional line
				(at -29.21 87.63 0)
				(length 7.62)
				(name "AD6")
				(number "46")
			)
			(pin bidirectional line
				(at -29.21 85.09 0)
				(length 7.62)
				(name "AD7")
				(number "44")
			)
			(pin bidirectional line
				(at -29.21 82.55 0)
				(length 7.62)
				(name "AD8")
				(number "42")
			)
			(pin bidirectional line
				(at -29.21 80.01 0)
				(length 7.62)
				(name "AD9")
				(number "40")
			)
			(pin bidirectional line
				(at -29.21 77.47 0)
				(length 7.62)
				(name "AD10")
				(number "39")
			)
			(pin bidirectional line
				(at -29.21 74.93 0)
				(length 7.62)
				(name "AD11")
				(number "38")
			)
			(pin bidirectional line
				(at -29.21 72.39 0)
				(length 7.62)
				(name "AD12")
				(number "36")
			)
			(pin bidirectional line
				(at -29.21 69.85 0)
				(length 7.62)
				(name "AD13")
				(number "35")
			)
			(pin bidirectional line
				(at -29.21 67.31 0)
				(length 7.62)
				(name "AD14")
				(number "34")
			)
			(pin bidirectional line
				(at -29.21 64.77 0)
				(length 7.62)
				(name "AD15")
				(number "32")
			)
			(pin bidirectional line
				(at -29.21 62.23 0)
				(length 7.62)
				(name "AD16")
				(number "14")
			)
			(pin bidirectional line
				(at -29.21 59.69 0)
				(length 7.62)
				(name "AD17")
				(number "12")
			)
			(pin bidirectional line
				(at -29.21 57.15 0)
				(length 7.62)
				(name "AD18")
				(number "8")
			)
			(pin bidirectional line
				(at -29.21 54.61 0)
				(length 7.62)
				(name "AD19")
				(number "7")
			)
			(pin bidirectional line
				(at -29.21 52.07 0)
				(length 7.62)
				(name "AD20")
				(number "6")
			)
			(pin bidirectional line
				(at -29.21 49.53 0)
				(length 7.62)
				(name "AD21")
				(number "4")
			)
			(pin bidirectional line
				(at -29.21 46.99 0)
				(length 7.62)
				(name "AD22")
				(number "3")
			)
			(pin bidirectional line
				(at -29.21 44.45 0)
				(length 7.62)
				(name "AD23")
				(number "2")
			)
			(pin bidirectional line
				(at -29.21 41.91 0)
				(length 7.62)
				(name "AD24")
				(number "158")
			)
			(pin bidirectional line
				(at -29.21 39.37 0)
				(length 7.62)
				(name "AD25")
				(number "156")
			)
			(pin bidirectional line
				(at -29.21 36.83 0)
				(length 7.62)
				(name "AD26")
				(number "155")
			)
			(pin bidirectional line
				(at -29.21 34.29 0)
				(length 7.62)
				(name "AD27")
				(number "154")
			)
			(pin bidirectional line
				(at -29.21 31.75 0)
				(length 7.62)
				(name "AD28")
				(number "152")
			)
			(pin bidirectional line
				(at -29.21 29.21 0)
				(length 7.62)
				(name "AD29")
				(number "148")
			)
			(pin bidirectional line
				(at -29.21 26.67 0)
				(length 7.62)
				(name "AD30")
				(number "147")
			)
			(pin bidirectional line
				(at -29.21 24.13 0)
				(length 7.62)
				(name "AD31")
				(number "146")
			)
			(pin bidirectional line
				(at -29.21 21.59 0)
				(length 7.62)
				(name "C/BE0#")
				(number "43")
			)
			(pin bidirectional line
				(at -29.21 19.05 0)
				(length 7.62)
				(name "C/BE1#")
				(number "28")
			)
			(pin bidirectional line
				(at -29.21 16.51 0)
				(length 7.62)
				(name "C/BE2#")
				(number "15")
			)
			(pin bidirectional line
				(at -29.21 13.97 0)
				(length 7.62)
				(name "C/BE3#")
				(number "159")
			)
			(pin bidirectional line
				(at -29.21 11.43 0)
				(length 7.62)
				(name "PAR")
				(number "27")
			)
			(pin input line
				(at -29.21 8.89 0)
				(length 7.62)
				(name "CLK")
				(number "142")
			)
			(pin input line
				(at -29.21 6.35 0)
				(length 7.62)
				(name "RST#")
				(number "139")
			)
			(pin bidirectional line
				(at -29.21 1.27 0)
				(length 7.62)
				(name "FRAME#")
				(number "16")
			)
			(pin bidirectional line
				(at -29.21 -1.27 0)
				(length 7.62)
				(name "IRDY#")
				(number "18")
			)
			(pin bidirectional line
				(at -29.21 -3.81 0)
				(length 7.62)
				(name "TRDY#")
				(number "19")
			)
			(pin bidirectional line
				(at -29.21 -6.35 0)
				(length 7.62)
				(name "STOP#")
				(number "22")
			)
			(pin input line
				(at -29.21 -8.89 0)
				(length 7.62)
				(name "LOCK#")
				(number "23")
			)
			(pin input line
				(at -29.21 -13.97 0)
				(length 7.62)
				(name "IDSEL")
				(number "160")
			)
			(pin bidirectional line
				(at -29.21 -16.51 0)
				(length 7.62)
				(name "DEVSEL#")
				(number "20")
			)
			(pin output line
				(at -29.21 -19.05 0)
				(length 7.62)
				(name "REQ#")
				(number "144")
			)
			(pin input line
				(at -29.21 -21.59 0)
				(length 7.62)
				(name "GNT#")
				(number "143")
			)
			(pin bidirectional line
				(at -29.21 -24.13 0)
				(length 7.62)
				(name "PERR#")
				(number "24")
			)
			(pin output line
				(at -29.21 -26.67 0)
				(length 7.62)
				(name "SERR#")
				(number "26")
			)
			(pin output line
				(at -29.21 -31.75 0)
				(length 7.62)
				(name "INTA#")
				(number "58")
			)
			(pin bidirectional line
				(at -29.21 -39.37 0)
				(length 7.62)
				(name "EA0")
				(number "57")
			)
			(pin bidirectional line
				(at -29.21 -41.91 0)
				(length 7.62)
				(name "EA1")
				(number "61")
			)
			(pin bidirectional line
				(at -29.21 -44.45 0)
				(length 7.62)
				(name "EA2")
				(number "69")
			)
			(pin bidirectional line
				(at -29.21 -46.99 0)
				(length 7.62)
				(name "EA3")
				(number "73")
			)
			(pin bidirectional line
				(at -29.21 -49.53 0)
				(length 7.62)
				(name "EA4")
				(number "81")
			)
			(pin bidirectional line
				(at -29.21 -52.07 0)
				(length 7.62)
				(name "EA5")
				(number "89")
			)
			(pin bidirectional line
				(at -29.21 -54.61 0)
				(length 7.62)
				(name "EA6")
				(number "97")
			)
			(pin bidirectional line
				(at -29.21 -57.15 0)
				(length 7.62)
				(name "EA7")
				(number "101")
			)
			(pin bidirectional line
				(at -29.21 -59.69 0)
				(length 7.62)
				(name "EA8")
				(number "109")
			)
			(pin output line
				(at -29.21 -62.23 0)
				(length 7.62)
				(name "EA9")
				(number "113")
			)
			(pin output line
				(at -29.21 -64.77 0)
				(length 7.62)
				(name "EA10")
				(number "121")
			)
			(pin output line
				(at -29.21 -67.31 0)
				(length 7.62)
				(name "EA11")
				(number "129")
			)
			(pin output line
				(at -29.21 -69.85 0)
				(length 7.62)
				(name "EA12")
				(number "137")
			)
			(pin output line
				(at -29.21 -72.39 0)
				(length 7.62)
				(name "EA13")
				(number "141")
			)
			(pin bidirectional line
				(at -29.21 -74.93 0)
				(length 7.62)
				(name "EA14/FWE")
				(number "149")
			)
			(pin bidirectional line
				(at -29.21 -77.47 0)
				(length 7.62)
				(name "EA15/FRF")
				(number "153")
			)
			(pin bidirectional line
				(at -29.21 -80.01 0)
				(length 7.62)
				(name "EQ0")
				(number "1")
			)
			(pin bidirectional line
				(at -29.21 -82.55 0)
				(length 7.62)
				(name "EQ1")
				(number "9")
			)
			(pin bidirectional line
				(at -29.21 -85.09 0)
				(length 7.62)
				(name "EQ2")
				(number "17")
			)
			(pin bidirectional line
				(at -29.21 -87.63 0)
				(length 7.62)
				(name "EQ3")
				(number "21")
			)
			(pin bidirectional line
				(at -29.21 -90.17 0)
				(length 7.62)
				(name "EQ4/FWC#")
				(number "29")
			)
			(pin bidirectional line
				(at -29.21 -92.71 0)
				(length 7.62)
				(name "EQ5/FRC#")
				(number "33")
			)
			(pin bidirectional line
				(at -29.21 -95.25 0)
				(length 7.62)
				(name "EQ6/AMREN")
				(number "41")
			)
			(pin bidirectional line
				(at -29.21 -97.79 0)
				(length 7.62)
				(name "EQ7/AMWEN")
				(number "49")
			)
			(pin output line
				(at -29.21 -100.33 0)
				(length 7.62)
				(name "ERD#/SCL")
				(number "128")
			)
			(pin bidirectional line
				(at -29.21 -102.87 0)
				(length 7.62)
				(name "EWR#/SDA")
				(number "127")
			)
			(pin no_connect line
				(at 24.13 -95.25 180)
				(length 2.54)
				(name "NC")
				(number "134")
			)
			(pin no_connect line
				(at 24.13 -96.52 180)
				(length 2.54)
				(name "NC")
				(number "136")
			)
			(pin bidirectional line
				(at 29.21 102.87 180)
				(length 7.62)
				(name "DQ0")
				(number "100")
			)
			(pin bidirectional line
				(at 29.21 100.33 180)
				(length 7.62)
				(name "DQ1")
				(number "99")
			)
			(pin bidirectional line
				(at 29.21 97.79 180)
				(length 7.62)
				(name "DQ2")
				(number "98")
			)
			(pin bidirectional line
				(at 29.21 95.25 180)
				(length 7.62)
				(name "DQ3")
				(number "96")
			)
			(pin bidirectional line
				(at 29.21 92.71 180)
				(length 7.62)
				(name "DQ4")
				(number "95")
			)
			(pin bidirectional line
				(at 29.21 90.17 180)
				(length 7.62)
				(name "DQ5")
				(number "94")
			)
			(pin bidirectional line
				(at 29.21 87.63 180)
				(length 7.62)
				(name "DQ6")
				(number "92")
			)
			(pin bidirectional line
				(at 29.21 85.09 180)
				(length 7.62)
				(name "DQ7")
				(number "88")
			)
			(pin bidirectional line
				(at 29.21 82.55 180)
				(length 7.62)
				(name "DQ8")
				(number "86")
			)
			(pin bidirectional line
				(at 29.21 80.01 180)
				(length 7.62)
				(name "DQ9")
				(number "84")
			)
			(pin bidirectional line
				(at 29.21 77.47 180)
				(length 7.62)
				(name "DQ10")
				(number "83")
			)
			(pin bidirectional line
				(at 29.21 74.93 180)
				(length 7.62)
				(name "DQ11")
				(number "82")
			)
			(pin bidirectional line
				(at 29.21 72.39 180)
				(length 7.62)
				(name "DQ12")
				(number "80")
			)
			(pin bidirectional line
				(at 29.21 69.85 180)
				(length 7.62)
				(name "DQ13")
				(number "79")
			)
			(pin bidirectional line
				(at 29.21 67.31 180)
				(length 7.62)
				(name "DQ14")
				(number "78")
			)
			(pin bidirectional line
				(at 29.21 64.77 180)
				(length 7.62)
				(name "DQ15")
				(number "76")
			)
			(pin bidirectional line
				(at 29.21 62.23 180)
				(length 7.62)
				(name "DQ16")
				(number "157")
			)
			(pin bidirectional line
				(at 29.21 59.69 180)
				(length 7.62)
				(name "DQ17")
				(number "145")
			)
			(pin bidirectional line
				(at 29.21 57.15 180)
				(length 7.62)
				(name "DQ18")
				(number "133")
			)
			(pin bidirectional line
				(at 29.21 54.61 180)
				(length 7.62)
				(name "DQ19")
				(number "125")
			)
			(pin bidirectional line
				(at 29.21 52.07 180)
				(length 7.62)
				(name "DQ20")
				(number "117")
			)
			(pin bidirectional line
				(at 29.21 49.53 180)
				(length 7.62)
				(name "DQ21")
				(number "105")
			)
			(pin bidirectional line
				(at 29.21 46.99 180)
				(length 7.62)
				(name "DQ22")
				(number "93")
			)
			(pin bidirectional line
				(at 29.21 44.45 180)
				(length 7.62)
				(name "DQ23")
				(number "85")
			)
			(pin bidirectional line
				(at 29.21 41.91 180)
				(length 7.62)
				(name "DQ24")
				(number "77")
			)
			(pin bidirectional line
				(at 29.21 39.37 180)
				(length 7.62)
				(name "DQ25")
				(number "65")
			)
			(pin bidirectional line
				(at 29.21 36.83 180)
				(length 7.62)
				(name "DQ26")
				(number "53")
			)
			(pin bidirectional line
				(at 29.21 34.29 180)
				(length 7.62)
				(name "DQ27")
				(number "45")
			)
			(pin bidirectional line
				(at 29.21 31.75 180)
				(length 7.62)
				(name "DQ28")
				(number "37")
			)
			(pin bidirectional line
				(at 29.21 29.21 180)
				(length 7.62)
				(name "DQ29")
				(number "25")
			)
			(pin bidirectional line
				(at 29.21 26.67 180)
				(length 7.62)
				(name "DQ30")
				(number "13")
			)
			(pin bidirectional line
				(at 29.21 24.13 180)
				(length 7.62)
				(name "DQ31")
				(number "5")
			)
			(pin output line
				(at 29.21 21.59 180)
				(length 7.62)
				(name "PTATN#")
				(number "114")
			)
			(pin input line
				(at 29.21 19.05 180)
				(length 7.62)
				(name "PTRDY#")
				(number "115")
			)
			(pin output line
				(at 29.21 16.51 180)
				(length 7.62)
				(name "PTNUM0")
				(number "123")
			)
			(pin output line
				(at 29.21 13.97 180)
				(length 7.62)
				(name "PTNUM1")
				(number "122")
			)
			(pin output line
				(at 29.21 11.43 180)
				(length 7.62)
				(name "PTBE0#")
				(number "116")
			)
			(pin output line
				(at 29.21 8.89 180)
				(length 7.62)
				(name "PTBE1#")
				(number "118")
			)
			(pin output line
				(at 29.21 6.35 180)
				(length 7.62)
				(name "PTBE2#")
				(number "119")
			)
			(pin output line
				(at 29.21 3.81 180)
				(length 7.62)
				(name "PTBE3#")
				(number "120")
			)
			(pin input line
				(at 29.21 1.27 180)
				(length 7.62)
				(name "PTADR#")
				(number "107")
			)
			(pin output line
				(at 29.21 -1.27 180)
				(length 7.62)
				(name "PTWR")
				(number "108")
			)
			(pin output line
				(at 29.21 -3.81 180)
				(length 7.62)
				(name "PTBURST#")
				(number "112")
			)
			(pin input line
				(at 29.21 -8.89 180)
				(length 7.62)
				(name "ADR2")
				(number "68")
			)
			(pin input line
				(at 29.21 -11.43 180)
				(length 7.62)
				(name "ADR3")
				(number "67")
			)
			(pin input line
				(at 29.21 -13.97 180)
				(length 7.62)
				(name "ADR4")
				(number "66")
			)
			(pin input line
				(at 29.21 -16.51 180)
				(length 7.62)
				(name "ADR5")
				(number "64")
			)
			(pin input line
				(at 29.21 -19.05 180)
				(length 7.62)
				(name "ADR6")
				(number "132")
			)
			(pin input line
				(at 29.21 -21.59 180)
				(length 7.62)
				(name "BE0#")
				(number "87")
			)
			(pin input line
				(at 29.21 -24.13 180)
				(length 7.62)
				(name "BE1#")
				(number "63")
			)
			(pin input line
				(at 29.21 -26.67 180)
				(length 7.62)
				(name "BE2#")
				(number "62")
			)
			(pin input line
				(at 29.21 -29.21 180)
				(length 7.62)
				(name "BE3#")
				(number "60")
			)
			(pin input line
				(at 29.21 -31.75 180)
				(length 7.62)
				(name "MODE_16/32")
				(number "59")
			)
			(pin input line
				(at 29.21 -34.29 180)
				(length 7.62)
				(name "SELECT#")
				(number "75")
			)
			(pin input line
				(at 29.21 -36.83 180)
				(length 7.62)
				(name "WR#")
				(number "74")
			)
			(pin input line
				(at 29.21 -39.37 180)
				(length 7.62)
				(name "RD#")
				(number "72")
			)
			(pin input line
				(at 29.21 -44.45 180)
				(length 7.62)
				(name "WRFIFO#")
				(number "102")
			)
			(pin input line
				(at 29.21 -46.99 180)
				(length 7.62)
				(name "RDFIFO#")
				(number "104")
			)
			(pin output line
				(at 29.21 -52.07 180)
				(length 7.62)
				(name "WRFULL")
				(number "103")
			)
			(pin output line
				(at 29.21 -54.61 180)
				(length 7.62)
				(name "RDEMPTY")
				(number "106")
			)
			(pin input line
				(at 29.21 -57.15 180)
				(length 7.62)
				(name "FLT#")
				(number "138")
			)
			(pin input line
				(at 29.21 -59.69 180)
				(length 7.62)
				(name "SNV")
				(number "135")
			)
			(pin output line
				(at 29.21 -62.23 180)
				(length 7.62)
				(name "IRQ#")
				(number "124")
			)
			(pin output line
				(at 29.21 -64.77 180)
				(length 7.62)
				(name "BPCLK")
				(number "140")
			)
			(pin output line
				(at 29.21 -67.31 180)
				(length 7.62)
				(name "SYSRST#")
				(number "126")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SIM4X32"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "SIM4X32"
			(at 11.43 -50.8 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "SIM4X32_0_1")
		(symbol "SIM4X32_1_1"
			(pin input line
				(at -20.32 45.72 0)
				(length 7.62)
				(name "A0")
				(number "12")
			)
			(pin input line
				(at -20.32 43.18 0)
				(length 7.62)
				(name "A1")
				(number "13")
			)
			(pin input line
				(at -20.32 40.64 0)
				(length 7.62)
				(name "A2")
				(number "14")
			)
			(pin input line
				(at -20.32 38.1 0)
				(length 7.62)
				(name "A3")
				(number "15")
			)
			(pin input line
				(at -20.32 35.56 0)
				(length 7.62)
				(name "A4")
				(number "16")
			)
			(pin input line
				(at -20.32 33.02 0)
				(length 7.62)
				(name "A5")
				(number "17")
			)
			(pin input line
				(at -20.32 30.48 0)
				(length 7.62)
				(name "A6")
				(number "18")
			)
			(pin input line
				(at -20.32 27.94 0)
				(length 7.62)
				(name "A7")
				(number "28")
			)
			(pin input line
				(at -20.32 25.4 0)
				(length 7.62)
				(name "A8")
				(number "31")
			)
			(pin input line
				(at -20.32 22.86 0)
				(length 7.62)
				(name "A9")
				(number "32")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 7.62)
				(name "A10")
				(number "19")
			)
			(pin input inverted
				(at -20.32 7.62 0)
				(length 7.62)
				(name "RAS0")
				(number "44")
			)
			(pin input inverted
				(at -20.32 2.54 0)
				(length 7.62)
				(name "RAS2")
				(number "34")
			)
			(pin input inverted
				(at -20.32 -5.08 0)
				(length 7.62)
				(name "CAS0")
				(number "40")
			)
			(pin input inverted
				(at -20.32 -7.62 0)
				(length 7.62)
				(name "CAS1")
				(number "41")
			)
			(pin input inverted
				(at -20.32 -10.16 0)
				(length 7.62)
				(name "CAS2")
				(number "42")
			)
			(pin input inverted
				(at -20.32 -12.7 0)
				(length 7.62)
				(name "CAS3")
				(number "43")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 7.62)
				(name "R/W")
				(number "47")
			)
			(pin input line
				(at -20.32 -22.86 0)
				(length 7.62)
				(name "PRD0")
				(number "67")
			)
			(pin input line
				(at -20.32 -25.4 0)
				(length 7.62)
				(name "PRD1")
				(number "68")
			)
			(pin input line
				(at -20.32 -27.94 0)
				(length 7.62)
				(name "PRD2")
				(number "69")
			)
			(pin input line
				(at -20.32 -30.48 0)
				(length 7.62)
				(name "PRD3")
				(number "70")
			)
			(pin no_connect line
				(at -13.97 -33.02 0)
				(length 1.27)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at -13.97 -34.29 0)
				(length 1.27)
				(name "NC")
				(number "29")
			)
			(pin no_connect line
				(at -13.97 -35.56 0)
				(length 1.27)
				(name "NC")
				(number "33")
			)
			(pin no_connect line
				(at -13.97 -36.83 0)
				(length 1.27)
				(name "NC")
				(number "35")
			)
			(pin no_connect line
				(at -13.97 -38.1 0)
				(length 1.27)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at -13.97 -39.37 0)
				(length 1.27)
				(name "NC")
				(number "37")
			)
			(pin no_connect line
				(at -13.97 -40.64 0)
				(length 1.27)
				(name "NC")
				(number "38")
			)
			(pin no_connect line
				(at -13.97 -41.91 0)
				(length 1.27)
				(name "NC")
				(number "45")
			)
			(pin no_connect line
				(at -13.97 -43.18 0)
				(length 1.27)
				(name "NC")
				(number "46")
			)
			(pin no_connect line
				(at -13.97 -44.45 0)
				(length 1.27)
				(name "NC")
				(number "48")
			)
			(pin no_connect line
				(at -13.97 -45.72 0)
				(length 1.27)
				(name "NC")
				(number "66")
			)
			(pin no_connect line
				(at -13.97 -46.99 0)
				(length 1.27)
				(name "NC")
				(number "71")
			)
			(pin power_in line
				(at -2.54 52.07 270)
				(length 3.81)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -52.07 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 0 52.07 270)
				(length 3.81)
				(name "VCC")
				(number "30")
			)
			(pin power_in line
				(at 0 -52.07 90)
				(length 3.81)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 2.54 52.07 270)
				(length 3.81)
				(name "VCC")
				(number "59")
			)
			(pin power_in line
				(at 2.54 -52.07 90)
				(length 3.81)
				(name "GND")
				(number "72")
			)
			(pin tri_state line
				(at 20.32 45.72 180)
				(length 7.62)
				(name "DQ0")
				(number "2")
			)
			(pin tri_state line
				(at 20.32 43.18 180)
				(length 7.62)
				(name "DQ1")
				(number "4")
			)
			(pin tri_state line
				(at 20.32 40.64 180)
				(length 7.62)
				(name "DQ2")
				(number "6")
			)
			(pin tri_state line
				(at 20.32 38.1 180)
				(length 7.62)
				(name "DQ3")
				(number "8")
			)
			(pin tri_state line
				(at 20.32 35.56 180)
				(length 7.62)
				(name "DQ4")
				(number "20")
			)
			(pin tri_state line
				(at 20.32 33.02 180)
				(length 7.62)
				(name "DQ5")
				(number "22")
			)
			(pin tri_state line
				(at 20.32 30.48 180)
				(length 7.62)
				(name "DQ6")
				(number "24")
			)
			(pin tri_state line
				(at 20.32 27.94 180)
				(length 7.62)
				(name "DQ7")
				(number "26")
			)
			(pin tri_state line
				(at 20.32 22.86 180)
				(length 7.62)
				(name "DQ8")
				(number "49")
			)
			(pin tri_state line
				(at 20.32 20.32 180)
				(length 7.62)
				(name "DQ9")
				(number "51")
			)
			(pin tri_state line
				(at 20.32 17.78 180)
				(length 7.62)
				(name "DQ10")
				(number "53")
			)
			(pin tri_state line
				(at 20.32 15.24 180)
				(length 7.62)
				(name "DQ11")
				(number "55")
			)
			(pin tri_state line
				(at 20.32 12.7 180)
				(length 7.62)
				(name "DQ12")
				(number "57")
			)
			(pin tri_state line
				(at 20.32 10.16 180)
				(length 7.62)
				(name "DQ13")
				(number "61")
			)
			(pin tri_state line
				(at 20.32 7.62 180)
				(length 7.62)
				(name "DQ14")
				(number "63")
			)
			(pin tri_state line
				(at 20.32 5.08 180)
				(length 7.62)
				(name "DQ15")
				(number "65")
			)
			(pin tri_state line
				(at 20.32 0 180)
				(length 7.62)
				(name "DQ16")
				(number "3")
			)
			(pin tri_state line
				(at 20.32 -2.54 180)
				(length 7.62)
				(name "DQ17")
				(number "5")
			)
			(pin tri_state line
				(at 20.32 -5.08 180)
				(length 7.62)
				(name "DQ18")
				(number "7")
			)
			(pin tri_state line
				(at 20.32 -7.62 180)
				(length 7.62)
				(name "DQ19")
				(number "9")
			)
			(pin tri_state line
				(at 20.32 -10.16 180)
				(length 7.62)
				(name "DQ20")
				(number "21")
			)
			(pin tri_state line
				(at 20.32 -12.7 180)
				(length 7.62)
				(name "DQ21")
				(number "23")
			)
			(pin tri_state line
				(at 20.32 -15.24 180)
				(length 7.62)
				(name "DQ22")
				(number "25")
			)
			(pin tri_state line
				(at 20.32 -17.78 180)
				(length 7.62)
				(name "DQ23")
				(number "27")
			)
			(pin tri_state line
				(at 20.32 -22.86 180)
				(length 7.62)
				(name "DQ24")
				(number "50")
			)
			(pin tri_state line
				(at 20.32 -25.4 180)
				(length 7.62)
				(name "DQ25")
				(number "52")
			)
			(pin tri_state line
				(at 20.32 -27.94 180)
				(length 7.62)
				(name "DQ26")
				(number "54")
			)
			(pin tri_state line
				(at 20.32 -30.48 180)
				(length 7.62)
				(name "DQ27")
				(number "56")
			)
			(pin tri_state line
				(at 20.32 -33.02 180)
				(length 7.62)
				(name "DQ28")
				(number "58")
			)
			(pin tri_state line
				(at 20.32 -35.56 180)
				(length 7.62)
				(name "DQ29")
				(number "60")
			)
			(pin tri_state line
				(at 20.32 -38.1 180)
				(length 7.62)
				(name "DQ30")
				(number "62")
			)
			(pin tri_state line
				(at 20.32 -40.64 180)
				(length 7.62)
				(name "DQ31")
				(number "64")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA8501"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 24.13 0)
		)
		(property "Value" "TDA8501"
			(at 8.89 -21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TDA8501_0_1")
		(symbol "TDA8501_1_1"
			(pin input line
				(at -22.86 20.32 0)
				(length 7.62)
				(name "CS")
				(number "24")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 7.62)
				(name "-R.Y")
				(number "1")
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 7.62)
				(name "-B.Y")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 7.62)
				(name "H/2")
				(number "4")
			)
			(pin input line
				(at -22.86 7.62 0)
				(length 7.62)
				(name "Y")
				(number "5")
			)
			(pin output line
				(at -22.86 5.08 0)
				(length 7.62)
				(name "UOFF")
				(number "6")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 7.62)
				(name "MCTR")
				(number "2")
			)
			(pin input line
				(at -22.86 -2.54 0)
				(length 7.62)
				(name "R")
				(number "7")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 7.62)
				(name "G")
				(number "9")
			)
			(pin input line
				(at -22.86 -7.62 0)
				(length 7.62)
				(name "B")
				(number "11")
			)
			(pin output line
				(at -22.86 -12.7 0)
				(length 7.62)
				(name "VOFF")
				(number "12")
			)
			(pin output line
				(at -22.86 -17.78 0)
				(length 7.62)
				(name "OSC")
				(number "23")
			)
			(pin input line
				(at 0 29.21 270)
				(length 7.62)
				(name "VCC")
				(number "8")
			)
			(pin input line
				(at 0 -26.67 90)
				(length 7.62)
				(name "VSS")
				(number "10")
			)
			(pin output line
				(at 22.86 20.32 180)
				(length 7.62)
				(name "Y+SOUT")
				(number "22")
			)
			(pin input line
				(at 22.86 17.78 180)
				(length 7.62)
				(name "Y+SIN")
				(number "20")
			)
			(pin output line
				(at 22.86 10.16 180)
				(length 7.62)
				(name "VREF")
				(number "13")
			)
			(pin output line
				(at 22.86 5.08 180)
				(length 7.62)
				(name "Y/OUT")
				(number "19")
			)
			(pin output line
				(at 22.86 2.54 180)
				(length 7.62)
				(name "CVBS")
				(number "16")
			)
			(pin output line
				(at 22.86 0 180)
				(length 7.62)
				(name "C/OUT")
				(number "14")
			)
			(pin passive line
				(at 22.86 -5.08 180)
				(length 7.62)
				(name "B/ADJ")
				(number "21")
			)
			(pin input line
				(at 22.86 -7.62 180)
				(length 7.62)
				(name "NOTCH")
				(number "18")
			)
			(pin input line
				(at 22.86 -10.16 180)
				(length 7.62)
				(name "NTSC/PAL")
				(number "17")
			)
			(pin passive line
				(at 22.86 -12.7 180)
				(length 7.62)
				(name "FLT")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEST"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "W"
			(at 0 1.524 0)
		)
		(property "Value" "TEST"
			(at 0 -1.778 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TEST_0_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VCC"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 2.54 0)
		)
		(property "Value" "VCC"
			(at 0 2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "VCC_0_0"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "VCC")
				(number "1")
			)
		)
		(symbol "VCC_0_1")
		(embedded_fonts no)
	)
	(symbol "VSS"
		(power)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#PWR"
			(at 0 0 0)
		)
		(property "Value" "VSS"
			(at 0 -1.778 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "VSS_0_1")
		(symbol "VSS_1_1"
			(pin power_in line
				(at 0 0 90)
				(length 0)
				(hide yes)
				(name "VSS")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC1736APD8"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 13.97 0)
		)
		(property "Value" "XC1736APD8"
			(at 10.16 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC1736APD8_0_1")
		(symbol "XC1736APD8_1_1"
			(pin input line
				(at -19.05 8.89 0)
				(length 7.62)
				(name "VPP")
				(number "7")
			)
			(pin input clock
				(at -19.05 3.81 0)
				(length 7.62)
				(name "CLK")
				(number "2")
			)
			(pin input inverted
				(at -19.05 -1.27 0)
				(length 7.62)
				(name "RAZ/OE")
				(number "3")
			)
			(pin input inverted
				(at -19.05 -6.35 0)
				(length 7.62)
				(name "CE")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin tri_state line
				(at 19.05 3.81 180)
				(length 7.62)
				(name "DATA")
				(number "1")
			)
			(pin output inverted
				(at 19.05 -3.81 180)
				(length 7.62)
				(name "CEO")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC4003-VQ100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC4003-VQ100"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC4003-VQ100_0_1")
		(symbol "XC4003-VQ100_1_1"
			(pin input line
				(at -24.13 57.15 0)
				(length 7.62)
				(name "M0/RT")
				(number "24")
			)
			(pin input line
				(at -24.13 54.61 0)
				(length 7.62)
				(name "M1/RD")
				(number "22")
			)
			(pin passive line
				(at -24.13 52.07 0)
				(length 7.62)
				(name "M2")
				(number "26")
			)
			(pin input inverted
				(at -24.13 46.99 0)
				(length 7.62)
				(name "PROG")
				(number "52")
			)
			(pin open_collector line
				(at -24.13 44.45 0)
				(length 7.62)
				(name "DONE")
				(number "50")
			)
			(pin passive line
				(at -24.13 41.91 0)
				(length 7.62)
				(name "DIN")
				(number "72")
			)
			(pin passive line
				(at -24.13 39.37 0)
				(length 7.62)
				(name "DOUT/SGCK4")
				(number "73")
			)
			(pin input clock
				(at -24.13 36.83 0)
				(length 7.62)
				(name "CCLK")
				(number "74")
			)
			(pin passive line
				(at -24.13 34.29 0)
				(length 7.62)
				(name "P/HDC")
				(number "28")
			)
			(pin passive line
				(at -24.13 31.75 0)
				(length 7.62)
				(name "P/LDC")
				(number "30")
			)
			(pin passive line
				(at -24.13 29.21 0)
				(length 7.62)
				(name "PGCK1")
				(number "2")
			)
			(pin passive line
				(at -24.13 26.67 0)
				(length 7.62)
				(name "P/A17")
				(number "3")
			)
			(pin passive line
				(at -24.13 24.13 0)
				(length 7.62)
				(name "P/TDI")
				(number "4")
			)
			(pin passive line
				(at -24.13 21.59 0)
				(length 7.62)
				(name "P/TCK")
				(number "5")
			)
			(pin passive line
				(at -24.13 19.05 0)
				(length 7.62)
				(name "P/A3")
				(number "6")
			)
			(pin passive line
				(at -24.13 16.51 0)
				(length 7.62)
				(name "P7")
				(number "7")
			)
			(pin passive line
				(at -24.13 13.97 0)
				(length 7.62)
				(name "P8")
				(number "8")
			)
			(pin passive line
				(at -24.13 11.43 0)
				(length 7.62)
				(name "P/A15")
				(number "9")
			)
			(pin passive line
				(at -24.13 8.89 0)
				(length 7.62)
				(name "P/A4")
				(number "10")
			)
			(pin bidirectional line
				(at -24.13 3.81 0)
				(length 7.62)
				(name "P13")
				(number "13")
			)
			(pin passive line
				(at -24.13 1.27 0)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -24.13 -1.27 0)
				(length 7.62)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -24.13 -3.81 0)
				(length 7.62)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -24.13 -6.35 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -24.13 -8.89 0)
				(length 7.62)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at -24.13 -11.43 0)
				(length 7.62)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -24.13 -13.97 0)
				(length 7.62)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at -24.13 -16.51 0)
				(length 7.62)
				(name "SGCK2")
				(number "21")
			)
			(pin passive line
				(at -24.13 -24.13 0)
				(length 7.62)
				(name "PGCK2")
				(number "27")
			)
			(pin passive line
				(at -24.13 -29.21 0)
				(length 7.62)
				(name "P29")
				(number "29")
			)
			(pin passive line
				(at -24.13 -34.29 0)
				(length 7.62)
				(name "P31")
				(number "31")
			)
			(pin passive line
				(at -24.13 -36.83 0)
				(length 7.62)
				(name "P32")
				(number "32")
			)
			(pin passive line
				(at -24.13 -39.37 0)
				(length 7.62)
				(name "P33")
				(number "33")
			)
			(pin passive line
				(at -24.13 -41.91 0)
				(length 7.62)
				(name "P34")
				(number "34")
			)
			(pin passive line
				(at -24.13 -44.45 0)
				(length 7.62)
				(name "P35")
				(number "35")
			)
			(pin passive line
				(at -24.13 -46.99 0)
				(length 7.62)
				(name "P36/INIT")
				(number "36")
			)
			(pin passive line
				(at -24.13 -52.07 0)
				(length 7.62)
				(name "P39")
				(number "39")
			)
			(pin passive line
				(at -24.13 -54.61 0)
				(length 7.62)
				(name "P40")
				(number "40")
			)
			(pin power_in line
				(at -10.16 63.5 270)
				(length 3.81)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at -10.16 -63.5 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -7.62 63.5 270)
				(length 3.81)
				(name "VCC")
				(number "25")
			)
			(pin power_in line
				(at -7.62 -63.5 90)
				(length 3.81)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at -5.08 63.5 270)
				(length 3.81)
				(name "VCC")
				(number "37")
			)
			(pin power_in line
				(at -5.08 -63.5 90)
				(length 3.81)
				(name "GND")
				(number "23")
			)
			(pin power_in line
				(at -2.54 63.5 270)
				(length 3.81)
				(name "VCC")
				(number "51")
			)
			(pin power_in line
				(at -2.54 -63.5 90)
				(length 3.81)
				(name "GND")
				(number "38")
			)
			(pin power_in line
				(at 0 63.5 270)
				(length 3.81)
				(name "VCC")
				(number "63")
			)
			(pin power_in line
				(at 0 -63.5 90)
				(length 3.81)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at 2.54 63.5 270)
				(length 3.81)
				(name "VCC")
				(number "75")
			)
			(pin power_in line
				(at 2.54 -63.5 90)
				(length 3.81)
				(name "GND")
				(number "64")
			)
			(pin power_in line
				(at 5.08 63.5 270)
				(length 3.81)
				(name "VCC")
				(number "89")
			)
			(pin power_in line
				(at 5.08 -63.5 90)
				(length 3.81)
				(name "GND")
				(number "77")
			)
			(pin power_in line
				(at 7.62 63.5 270)
				(length 3.81)
				(name "VCC")
				(number "100")
			)
			(pin power_in line
				(at 7.62 -63.5 90)
				(length 3.81)
				(name "GND")
				(number "88")
			)
			(pin bidirectional line
				(at 24.13 57.15 180)
				(length 7.62)
				(name "SGCK1")
				(number "99")
			)
			(pin bidirectional line
				(at 24.13 54.61 180)
				(length 7.62)
				(name "P98")
				(number "98")
			)
			(pin passive line
				(at 24.13 52.07 180)
				(length 7.62)
				(name "P97")
				(number "97")
			)
			(pin passive line
				(at 24.13 49.53 180)
				(length 7.62)
				(name "P96")
				(number "96")
			)
			(pin passive line
				(at 24.13 46.99 180)
				(length 7.62)
				(name "P91")
				(number "95")
			)
			(pin passive line
				(at 24.13 44.45 180)
				(length 7.62)
				(name "P94")
				(number "94")
			)
			(pin passive line
				(at 24.13 41.91 180)
				(length 7.62)
				(name "P93")
				(number "93")
			)
			(pin passive line
				(at 24.13 39.37 180)
				(length 7.62)
				(name "P92")
				(number "92")
			)
			(pin passive line
				(at 24.13 36.83 180)
				(length 7.62)
				(name "P91")
				(number "91")
			)
			(pin bidirectional line
				(at 24.13 34.29 180)
				(length 7.62)
				(name "P90")
				(number "90")
			)
			(pin passive line
				(at 24.13 31.75 180)
				(length 7.62)
				(name "P87")
				(number "87")
			)
			(pin passive line
				(at 24.13 29.21 180)
				(length 7.62)
				(name "P86")
				(number "86")
			)
			(pin passive line
				(at 24.13 26.67 180)
				(length 7.62)
				(name "P85")
				(number "85")
			)
			(pin passive line
				(at 24.13 24.13 180)
				(length 7.62)
				(name "P84")
				(number "84")
			)
			(pin passive line
				(at 24.13 21.59 180)
				(length 7.62)
				(name "P83")
				(number "83")
			)
			(pin passive line
				(at 24.13 19.05 180)
				(length 7.62)
				(name "P82")
				(number "82")
			)
			(pin passive line
				(at 24.13 16.51 180)
				(length 7.62)
				(name "P81")
				(number "81")
			)
			(pin passive line
				(at 24.13 13.97 180)
				(length 7.62)
				(name "P80")
				(number "80")
			)
			(pin passive line
				(at 24.13 11.43 180)
				(length 7.62)
				(name "PGCK4")
				(number "79")
			)
			(pin passive line
				(at 24.13 8.89 180)
				(length 7.62)
				(name "P78")
				(number "78")
			)
			(pin output line
				(at 24.13 6.35 180)
				(length 7.62)
				(name "TDO")
				(number "76")
			)
			(pin passive line
				(at 24.13 3.81 180)
				(length 7.62)
				(name "P71/RDY")
				(number "71")
			)
			(pin passive line
				(at 24.13 1.27 180)
				(length 7.62)
				(name "P70")
				(number "70")
			)
			(pin passive line
				(at 24.13 -1.27 180)
				(length 7.62)
				(name "P69")
				(number "69")
			)
			(pin passive line
				(at 24.13 -3.81 180)
				(length 7.62)
				(name "P68")
				(number "68")
			)
			(pin passive line
				(at 24.13 -6.35 180)
				(length 7.62)
				(name "P67")
				(number "67")
			)
			(pin passive line
				(at 24.13 -8.89 180)
				(length 7.62)
				(name "P66")
				(number "66")
			)
			(pin passive line
				(at 24.13 -11.43 180)
				(length 7.62)
				(name "P65")
				(number "65")
			)
			(pin passive line
				(at 24.13 -13.97 180)
				(length 7.62)
				(name "P62")
				(number "62")
			)
			(pin passive line
				(at 24.13 -16.51 180)
				(length 7.62)
				(name "P61")
				(number "61")
			)
			(pin passive line
				(at 24.13 -19.05 180)
				(length 7.62)
				(name "P60")
				(number "60")
			)
			(pin passive line
				(at 24.13 -21.59 180)
				(length 7.62)
				(name "P59")
				(number "59")
			)
			(pin passive line
				(at 24.13 -24.13 180)
				(length 7.62)
				(name "P58")
				(number "58")
			)
			(pin passive line
				(at 24.13 -26.67 180)
				(length 7.62)
				(name "P57")
				(number "57")
			)
			(pin bidirectional line
				(at 24.13 -29.21 180)
				(length 7.62)
				(name "P56")
				(number "56")
			)
			(pin passive line
				(at 24.13 -31.75 180)
				(length 7.62)
				(name "P55")
				(number "55")
			)
			(pin bidirectional line
				(at 24.13 -34.29 180)
				(length 7.62)
				(name "PGCK3")
				(number "54")
			)
			(pin bidirectional line
				(at 24.13 -36.83 180)
				(length 7.62)
				(name "P53")
				(number "53")
			)
			(pin passive line
				(at 24.13 -39.37 180)
				(length 7.62)
				(name "SGCK3")
				(number "48")
			)
			(pin passive line
				(at 24.13 -41.91 180)
				(length 7.62)
				(name "P47")
				(number "47")
			)
			(pin passive line
				(at 24.13 -44.45 180)
				(length 7.62)
				(name "P46")
				(number "46")
			)
			(pin passive line
				(at 24.13 -46.99 180)
				(length 7.62)
				(name "P45")
				(number "45")
			)
			(pin passive line
				(at 24.13 -49.53 180)
				(length 7.62)
				(name "P44")
				(number "44")
			)
			(pin passive line
				(at 24.13 -52.07 180)
				(length 7.62)
				(name "P43")
				(number "43")
			)
			(pin passive line
				(at 24.13 -54.61 180)
				(length 7.62)
				(name "P42")
				(number "42")
			)
			(pin passive line
				(at 24.13 -57.15 180)
				(length 7.62)
				(name "P41")
				(number "41")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC4005-PQ100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC4005-PQ100"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC4005-PQ100_0_1")
		(symbol "XC4005-PQ100_1_1"
			(pin input line
				(at -26.67 55.88 0)
				(length 7.62)
				(name "M0")
				(number "27")
			)
			(pin passive line
				(at -26.67 53.34 0)
				(length 7.62)
				(name "M1")
				(number "25")
			)
			(pin input line
				(at -26.67 50.8 0)
				(length 7.62)
				(name "M2")
				(number "29")
			)
			(pin input inverted
				(at -26.67 48.26 0)
				(length 7.62)
				(name "PROG")
				(number "55")
			)
			(pin open_collector line
				(at -26.67 45.72 0)
				(length 7.62)
				(name "DONE")
				(number "53")
			)
			(pin passive line
				(at -26.67 43.18 0)
				(length 7.62)
				(name "DIN/D0")
				(number "75")
			)
			(pin passive line
				(at -26.67 40.64 0)
				(length 7.62)
				(name "DOUT/SGCK4")
				(number "76")
			)
			(pin input clock
				(at -26.67 38.1 0)
				(length 7.62)
				(name "CCLK")
				(number "77")
			)
			(pin passive line
				(at -26.67 33.02 0)
				(length 7.62)
				(name "P31/HDC")
				(number "31")
			)
			(pin passive line
				(at -26.67 30.48 0)
				(length 7.62)
				(name "P33/LDC")
				(number "33")
			)
			(pin passive line
				(at -26.67 25.4 0)
				(length 7.62)
				(name "PGCK1")
				(number "5")
			)
			(pin passive line
				(at -26.67 22.86 0)
				(length 7.62)
				(name "P6")
				(number "6")
			)
			(pin passive line
				(at -26.67 20.32 0)
				(length 7.62)
				(name "P7/TDI")
				(number "7")
			)
			(pin passive line
				(at -26.67 17.78 0)
				(length 7.62)
				(name "P8/TCK")
				(number "8")
			)
			(pin passive line
				(at -26.67 15.24 0)
				(length 7.62)
				(name "P9/TMS")
				(number "9")
			)
			(pin passive line
				(at -26.67 12.7 0)
				(length 7.62)
				(name "P11")
				(number "11")
			)
			(pin passive line
				(at -26.67 10.16 0)
				(length 7.62)
				(name "P12")
				(number "12")
			)
			(pin passive line
				(at -26.67 7.62 0)
				(length 7.62)
				(name "P13")
				(number "13")
			)
			(pin passive line
				(at -26.67 5.08 0)
				(length 7.62)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -26.67 2.54 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -26.67 0 0)
				(length 7.62)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at -26.67 -2.54 0)
				(length 7.62)
				(name "P19")
				(number "19")
			)
			(pin passive line
				(at -26.67 -5.08 0)
				(length 7.62)
				(name "P20")
				(number "20")
			)
			(pin passive line
				(at -26.67 -7.62 0)
				(length 7.62)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at -26.67 -10.16 0)
				(length 7.62)
				(name "P22")
				(number "22")
			)
			(pin passive line
				(at -26.67 -12.7 0)
				(length 7.62)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at -26.67 -17.78 0)
				(length 7.62)
				(name "SGCK2")
				(number "24")
			)
			(pin passive line
				(at -26.67 -20.32 0)
				(length 7.62)
				(name "PGCK2")
				(number "30")
			)
			(pin passive line
				(at -26.67 -25.4 0)
				(length 7.62)
				(name "P32")
				(number "32")
			)
			(pin passive line
				(at -26.67 -27.94 0)
				(length 7.62)
				(name "P34")
				(number "34")
			)
			(pin passive line
				(at -26.67 -30.48 0)
				(length 7.62)
				(name "P35")
				(number "35")
			)
			(pin passive line
				(at -26.67 -33.02 0)
				(length 7.62)
				(name "P36")
				(number "36")
			)
			(pin passive line
				(at -26.67 -35.56 0)
				(length 7.62)
				(name "P37")
				(number "37")
			)
			(pin passive line
				(at -26.67 -38.1 0)
				(length 7.62)
				(name "P38")
				(number "38")
			)
			(pin passive line
				(at -26.67 -40.64 0)
				(length 7.62)
				(name "P39/INIT")
				(number "39")
			)
			(pin passive line
				(at -26.67 -43.18 0)
				(length 7.62)
				(name "P42")
				(number "42")
			)
			(pin passive line
				(at -26.67 -45.72 0)
				(length 7.62)
				(name "P43")
				(number "43")
			)
			(pin passive line
				(at -26.67 -48.26 0)
				(length 7.62)
				(name "P44")
				(number "44")
			)
			(pin passive line
				(at -26.67 -50.8 0)
				(length 7.62)
				(name "P45")
				(number "45")
			)
			(pin passive line
				(at -26.67 -53.34 0)
				(length 7.62)
				(name "P46")
				(number "46")
			)
			(pin passive line
				(at -26.67 -55.88 0)
				(length 7.62)
				(name "P47")
				(number "47")
			)
			(pin power_in line
				(at -10.16 62.23 270)
				(length 3.81)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at -10.16 -62.23 90)
				(length 3.81)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at -7.62 62.23 270)
				(length 3.81)
				(name "VCC")
				(number "15")
			)
			(pin power_in line
				(at -7.62 -62.23 90)
				(length 3.81)
				(name "GND")
				(number "14")
			)
			(pin power_in line
				(at -5.08 62.23 270)
				(length 3.81)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at -5.08 -62.23 90)
				(length 3.81)
				(name "GND")
				(number "26")
			)
			(pin power_in line
				(at -2.54 62.23 270)
				(length 3.81)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at -2.54 -62.23 90)
				(length 3.81)
				(name "GND")
				(number "41")
			)
			(pin power_in line
				(at 0 62.23 270)
				(length 3.81)
				(name "VCC")
				(number "54")
			)
			(pin power_in line
				(at 0 -62.23 90)
				(length 3.81)
				(name "GND")
				(number "52")
			)
			(pin power_in line
				(at 2.54 62.23 270)
				(length 3.81)
				(name "VCC")
				(number "66")
			)
			(pin power_in line
				(at 2.54 -62.23 90)
				(length 3.81)
				(name "GND")
				(number "67")
			)
			(pin power_in line
				(at 5.08 62.23 270)
				(length 3.81)
				(name "VCC")
				(number "78")
			)
			(pin power_in line
				(at 5.08 -62.23 90)
				(length 3.81)
				(name "GND")
				(number "80")
			)
			(pin power_in line
				(at 7.62 62.23 270)
				(length 3.81)
				(name "VCC")
				(number "92")
			)
			(pin power_in line
				(at 7.62 -62.23 90)
				(length 3.81)
				(name "GND")
				(number "91")
			)
			(pin passive line
				(at 26.67 55.88 180)
				(length 7.62)
				(name "SGCK1")
				(number "2")
			)
			(pin passive line
				(at 26.67 53.34 180)
				(length 7.62)
				(name "P1")
				(number "1")
			)
			(pin passive line
				(at 26.67 50.8 180)
				(length 7.62)
				(name "P100")
				(number "100")
			)
			(pin passive line
				(at 26.67 48.26 180)
				(length 7.62)
				(name "P99")
				(number "99")
			)
			(pin passive line
				(at 26.67 45.72 180)
				(length 7.62)
				(name "P98")
				(number "98")
			)
			(pin passive line
				(at 26.67 43.18 180)
				(length 7.62)
				(name "P97")
				(number "97")
			)
			(pin passive line
				(at 26.67 40.64 180)
				(length 7.62)
				(name "P96")
				(number "96")
			)
			(pin passive line
				(at 26.67 38.1 180)
				(length 7.62)
				(name "P95")
				(number "95")
			)
			(pin passive line
				(at 26.67 35.56 180)
				(length 7.62)
				(name "P94")
				(number "94")
			)
			(pin passive line
				(at 26.67 33.02 180)
				(length 7.62)
				(name "P93")
				(number "93")
			)
			(pin passive line
				(at 26.67 30.48 180)
				(length 7.62)
				(name "P90")
				(number "90")
			)
			(pin passive line
				(at 26.67 27.94 180)
				(length 7.62)
				(name "P89")
				(number "89")
			)
			(pin passive line
				(at 26.67 25.4 180)
				(length 7.62)
				(name "P88")
				(number "88")
			)
			(pin passive line
				(at 26.67 22.86 180)
				(length 7.62)
				(name "P87")
				(number "87")
			)
			(pin passive line
				(at 26.67 20.32 180)
				(length 7.62)
				(name "P86")
				(number "86")
			)
			(pin passive line
				(at 26.67 17.78 180)
				(length 7.62)
				(name "P85")
				(number "85")
			)
			(pin passive line
				(at 26.67 15.24 180)
				(length 7.62)
				(name "P84")
				(number "84")
			)
			(pin passive line
				(at 26.67 12.7 180)
				(length 7.62)
				(name "P83")
				(number "83")
			)
			(pin passive line
				(at 26.67 7.62 180)
				(length 7.62)
				(name "PGCK4")
				(number "82")
			)
			(pin passive line
				(at 26.67 5.08 180)
				(length 7.62)
				(name "P81")
				(number "81")
			)
			(pin output line
				(at 26.67 2.54 180)
				(length 7.62)
				(name "TDO")
				(number "79")
			)
			(pin passive line
				(at 26.67 0 180)
				(length 7.62)
				(name "P74/BUSY")
				(number "74")
			)
			(pin passive line
				(at 26.67 -2.54 180)
				(length 7.62)
				(name "P73")
				(number "73")
			)
			(pin passive line
				(at 26.67 -5.08 180)
				(length 7.62)
				(name "P72")
				(number "72")
			)
			(pin passive line
				(at 26.67 -7.62 180)
				(length 7.62)
				(name "P71")
				(number "71")
			)
			(pin passive line
				(at 26.67 -10.16 180)
				(length 7.62)
				(name "P70")
				(number "70")
			)
			(pin passive line
				(at 26.67 -12.7 180)
				(length 7.62)
				(name "P69")
				(number "69")
			)
			(pin passive line
				(at 26.67 -15.24 180)
				(length 7.62)
				(name "P68")
				(number "68")
			)
			(pin passive line
				(at 26.67 -17.78 180)
				(length 7.62)
				(name "P65")
				(number "65")
			)
			(pin passive line
				(at 26.67 -20.32 180)
				(length 7.62)
				(name "P64")
				(number "64")
			)
			(pin passive line
				(at 26.67 -22.86 180)
				(length 7.62)
				(name "P63")
				(number "63")
			)
			(pin passive line
				(at 26.67 -25.4 180)
				(length 7.62)
				(name "P62")
				(number "62")
			)
			(pin passive line
				(at 26.67 -27.94 180)
				(length 7.62)
				(name "P61")
				(number "61")
			)
			(pin passive line
				(at 26.67 -30.48 180)
				(length 7.62)
				(name "P60")
				(number "60")
			)
			(pin passive line
				(at 26.67 -33.02 180)
				(length 7.62)
				(name "P59")
				(number "59")
			)
			(pin passive line
				(at 26.67 -35.56 180)
				(length 7.62)
				(name "P58")
				(number "58")
			)
			(pin passive line
				(at 26.67 -40.64 180)
				(length 7.62)
				(name "PGCK3")
				(number "57")
			)
			(pin passive line
				(at 26.67 -43.18 180)
				(length 7.62)
				(name "P56")
				(number "56")
			)
			(pin passive line
				(at 26.67 -45.72 180)
				(length 7.62)
				(name "SGCK3")
				(number "51")
			)
			(pin passive line
				(at 26.67 -50.8 180)
				(length 7.62)
				(name "P50")
				(number "50")
			)
			(pin passive line
				(at 26.67 -53.34 180)
				(length 7.62)
				(name "P49")
				(number "49")
			)
			(pin passive line
				(at 26.67 -55.88 180)
				(length 7.62)
				(name "P48")
				(number "48")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC4005-PQ160"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "XC4005-PQ160"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XC4005-PQ160_0_1")
		(symbol "XC4005-PQ160_1_1"
			(pin input line
				(at -27.94 76.2 0)
				(length 7.62)
				(name "M0")
				(number "40")
			)
			(pin input line
				(at -27.94 73.66 0)
				(length 7.62)
				(name "M1")
				(number "38")
			)
			(pin input line
				(at -27.94 71.12 0)
				(length 7.62)
				(name "M2")
				(number "42")
			)
			(pin input inverted
				(at -27.94 66.04 0)
				(length 7.62)
				(name "PROG")
				(number "82")
			)
			(pin bidirectional line
				(at -27.94 63.5 0)
				(length 7.62)
				(name "DONE")
				(number "80")
			)
			(pin input line
				(at -27.94 60.96 0)
				(length 7.62)
				(name "DIN")
				(number "117")
			)
			(pin passive line
				(at -27.94 58.42 0)
				(length 7.62)
				(name "DOUT-SGI4")
				(number "118")
			)
			(pin passive clock
				(at -27.94 55.88 0)
				(length 7.62)
				(name "CCLK")
				(number "119")
			)
			(pin passive line
				(at -27.94 50.8 0)
				(length 7.62)
				(name "HDC")
				(number "44")
			)
			(pin passive line
				(at -27.94 48.26 0)
				(length 7.62)
				(name "LDC")
				(number "48")
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 7.62)
				(name "PGCK1")
				(number "2")
			)
			(pin passive line
				(at -27.94 40.64 0)
				(length 7.62)
				(name "P3")
				(number "3")
			)
			(pin passive line
				(at -27.94 38.1 0)
				(length 7.62)
				(name "P4")
				(number "4")
			)
			(pin passive line
				(at -27.94 35.56 0)
				(length 7.62)
				(name "P5")
				(number "5")
			)
			(pin passive line
				(at -27.94 33.02 0)
				(length 7.62)
				(name "TDI")
				(number "6")
			)
			(pin passive line
				(at -27.94 30.48 0)
				(length 7.62)
				(name "TCK")
				(number "7")
			)
			(pin passive line
				(at -27.94 27.94 0)
				(length 7.62)
				(name "P11")
				(number "11")
			)
			(pin passive line
				(at -27.94 25.4 0)
				(length 7.62)
				(name "P12")
				(number "12")
			)
			(pin passive line
				(at -27.94 22.86 0)
				(length 7.62)
				(name "TMS")
				(number "13")
			)
			(pin passive line
				(at -27.94 20.32 0)
				(length 7.62)
				(name "P14")
				(number "14")
			)
			(pin passive line
				(at -27.94 17.78 0)
				(length 7.62)
				(name "P15")
				(number "15")
			)
			(pin passive line
				(at -27.94 15.24 0)
				(length 7.62)
				(name "P16")
				(number "16")
			)
			(pin passive line
				(at -27.94 12.7 0)
				(length 7.62)
				(name "P17")
				(number "17")
			)
			(pin passive line
				(at -27.94 10.16 0)
				(length 7.62)
				(name "P18")
				(number "18")
			)
			(pin passive line
				(at -27.94 7.62 0)
				(length 7.62)
				(name "P21")
				(number "21")
			)
			(pin passive line
				(at -27.94 5.08 0)
				(length 7.62)
				(name "P22")
				(number "22")
			)
			(pin passive line
				(at -27.94 2.54 0)
				(length 7.62)
				(name "P23")
				(number "23")
			)
			(pin passive line
				(at -27.94 0 0)
				(length 7.62)
				(name "P24")
				(number "24")
			)
			(pin passive line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "P25")
				(number "25")
			)
			(pin passive line
				(at -27.94 -5.08 0)
				(length 7.62)
				(name "P26")
				(number "26")
			)
			(pin passive line
				(at -27.94 -7.62 0)
				(length 7.62)
				(name "P27")
				(number "27")
			)
			(pin passive line
				(at -27.94 -10.16 0)
				(length 7.62)
				(name "P28")
				(number "28")
			)
			(pin passive line
				(at -27.94 -12.7 0)
				(length 7.62)
				(name "P32")
				(number "32")
			)
			(pin passive line
				(at -27.94 -15.24 0)
				(length 7.62)
				(name "P33")
				(number "33")
			)
			(pin passive line
				(at -27.94 -17.78 0)
				(length 7.62)
				(name "P34")
				(number "34")
			)
			(pin passive line
				(at -27.94 -20.32 0)
				(length 7.62)
				(name "P35")
				(number "35")
			)
			(pin passive line
				(at -27.94 -22.86 0)
				(length 7.62)
				(name "P36")
				(number "36")
			)
			(pin passive line
				(at -27.94 -25.4 0)
				(length 7.62)
				(name "SGCK2")
				(number "37")
			)
			(pin passive line
				(at -27.94 -27.94 0)
				(length 7.62)
				(name "PGCK2")
				(number "43")
			)
			(pin passive line
				(at -27.94 -30.48 0)
				(length 7.62)
				(name "P45")
				(number "45")
			)
			(pin passive line
				(at -27.94 -33.02 0)
				(length 7.62)
				(name "P46")
				(number "46")
			)
			(pin passive line
				(at -27.94 -35.56 0)
				(length 7.62)
				(name "P47")
				(number "47")
			)
			(pin passive line
				(at -27.94 -38.1 0)
				(length 7.62)
				(name "P52")
				(number "52")
			)
			(pin passive line
				(at -27.94 -40.64 0)
				(length 7.62)
				(name "P53")
				(number "53")
			)
			(pin passive line
				(at -27.94 -43.18 0)
				(length 7.62)
				(name "P54")
				(number "54")
			)
			(pin passive line
				(at -27.94 -45.72 0)
				(length 7.62)
				(name "P55")
				(number "55")
			)
			(pin passive line
				(at -27.94 -48.26 0)
				(length 7.62)
				(name "P56")
				(number "56")
			)
			(pin passive line
				(at -27.94 -50.8 0)
				(length 7.62)
				(name "P57")
				(number "57")
			)
			(pin passive line
				(at -27.94 -53.34 0)
				(length 7.62)
				(name "P58")
				(number "58")
			)
			(pin passive line
				(at -27.94 -55.88 0)
				(length 7.62)
				(name "P59-INIT")
				(number "59")
			)
			(pin passive line
				(at -27.94 -58.42 0)
				(length 7.62)
				(name "P62")
				(number "62")
			)
			(pin passive line
				(at -27.94 -60.96 0)
				(length 7.62)
				(name "P63")
				(number "63")
			)
			(pin passive line
				(at -27.94 -63.5 0)
				(length 7.62)
				(name "P64")
				(number "64")
			)
			(pin passive line
				(at -27.94 -66.04 0)
				(length 7.62)
				(name "P65")
				(number "65")
			)
			(pin passive line
				(at -27.94 -68.58 0)
				(length 7.62)
				(name "P66")
				(number "66")
			)
			(pin passive line
				(at -27.94 -71.12 0)
				(length 7.62)
				(name "P67")
				(number "67")
			)
			(pin bidirectional line
				(at -27.94 -73.66 0)
				(length 7.62)
				(name "P68")
				(number "68")
			)
			(pin passive line
				(at -27.94 -76.2 0)
				(length 7.62)
				(name "P69")
				(number "69")
			)
			(pin power_in line
				(at -20.32 -85.09 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -17.78 -85.09 90)
				(length 3.81)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at -15.24 -85.09 90)
				(length 3.81)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at -12.7 -85.09 90)
				(length 3.81)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at -10.16 82.55 270)
				(length 3.81)
				(name "VCC")
				(number "41")
			)
			(pin power_in line
				(at -10.16 -85.09 90)
				(length 3.81)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at -7.62 82.55 270)
				(length 3.81)
				(name "VCC")
				(number "60")
			)
			(pin power_in line
				(at -7.62 -85.09 90)
				(length 3.81)
				(name "GND")
				(number "51")
			)
			(pin power_in line
				(at -5.08 82.55 270)
				(length 3.81)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at -5.08 -85.09 90)
				(length 3.81)
				(name "GND")
				(number "61")
			)
			(pin power_in line
				(at -2.54 82.55 270)
				(length 3.81)
				(name "VCC")
				(number "81")
			)
			(pin power_in line
				(at -2.54 -85.09 90)
				(length 3.81)
				(name "GND")
				(number "70")
			)
			(pin power_in line
				(at 0 82.55 270)
				(length 3.81)
				(name "VCC")
				(number "100")
			)
			(pin power_in line
				(at 0 -85.09 90)
				(length 3.81)
				(name "GND")
				(number "79")
			)
			(pin power_in line
				(at 2.54 82.55 270)
				(length 3.81)
				(name "VCC")
				(number "120")
			)
			(pin power_in line
				(at 2.54 -85.09 90)
				(length 3.81)
				(name "GND")
				(number "91")
			)
			(pin power_in line
				(at 5.08 82.55 270)
				(length 3.81)
				(name "VCC")
				(number "142")
			)
			(pin power_in line
				(at 5.08 -85.09 90)
				(length 3.81)
				(name "GND")
				(number "101")
			)
			(pin power_in line
				(at 7.62 82.55 270)
				(length 3.81)
				(name "VCC")
				(number "160")
			)
			(pin power_in line
				(at 7.62 -85.09 90)
				(length 3.81)
				(name "GND")
				(number "110")
			)
			(pin power_in line
				(at 10.16 -85.09 90)
				(length 3.81)
				(name "GND")
				(number "122")
			)
			(pin power_in line
				(at 12.7 -85.09 90)
				(length 3.81)
				(name "GND")
				(number "131")
			)
			(pin power_in line
				(at 15.24 -85.09 90)
				(length 3.81)
				(name "GND")
				(number "141")
			)
			(pin power_in line
				(at 17.78 -85.09 90)
				(length 3.81)
				(name "GND")
				(number "151")
			)
			(pin passive line
				(at 27.94 76.2 180)
				(length 7.62)
				(name "SGCK1")
				(number "159")
			)
			(pin passive line
				(at 27.94 73.66 180)
				(length 7.62)
				(name "P158")
				(number "158")
			)
			(pin passive line
				(at 27.94 71.12 180)
				(length 7.62)
				(name "P157")
				(number "157")
			)
			(pin passive line
				(at 27.94 68.58 180)
				(length 7.62)
				(name "P156")
				(number "156")
			)
			(pin passive line
				(at 27.94 66.04 180)
				(length 7.62)
				(name "P155")
				(number "155")
			)
			(pin passive line
				(at 27.94 63.5 180)
				(length 7.62)
				(name "P154")
				(number "154")
			)
			(pin passive line
				(at 27.94 60.96 180)
				(length 7.62)
				(name "P150")
				(number "150")
			)
			(pin passive line
				(at 27.94 58.42 180)
				(length 7.62)
				(name "P149")
				(number "149")
			)
			(pin passive line
				(at 27.94 55.88 180)
				(length 7.62)
				(name "P148")
				(number "148")
			)
			(pin passive line
				(at 27.94 53.34 180)
				(length 7.62)
				(name "P147")
				(number "147")
			)
			(pin passive line
				(at 27.94 50.8 180)
				(length 7.62)
				(name "P146")
				(number "146")
			)
			(pin passive line
				(at 27.94 48.26 180)
				(length 7.62)
				(name "P145")
				(number "145")
			)
			(pin passive line
				(at 27.94 45.72 180)
				(length 7.62)
				(name "P144")
				(number "144")
			)
			(pin passive line
				(at 27.94 43.18 180)
				(length 7.62)
				(name "P143")
				(number "143")
			)
			(pin passive line
				(at 27.94 40.64 180)
				(length 7.62)
				(name "P140")
				(number "140")
			)
			(pin passive line
				(at 27.94 38.1 180)
				(length 7.62)
				(name "P139")
				(number "139")
			)
			(pin passive line
				(at 27.94 35.56 180)
				(length 7.62)
				(name "P138")
				(number "138")
			)
			(pin passive line
				(at 27.94 33.02 180)
				(length 7.62)
				(name "P137")
				(number "137")
			)
			(pin passive line
				(at 27.94 30.48 180)
				(length 7.62)
				(name "P135")
				(number "135")
			)
			(pin passive line
				(at 27.94 27.94 180)
				(length 7.62)
				(name "P134")
				(number "134")
			)
			(pin passive line
				(at 27.94 25.4 180)
				(length 7.62)
				(name "P133")
				(number "133")
			)
			(pin passive line
				(at 27.94 22.86 180)
				(length 7.62)
				(name "P132")
				(number "132")
			)
			(pin passive line
				(at 27.94 20.32 180)
				(length 7.62)
				(name "P128")
				(number "128")
			)
			(pin passive line
				(at 27.94 17.78 180)
				(length 7.62)
				(name "P127")
				(number "127")
			)
			(pin passive line
				(at 27.94 15.24 180)
				(length 7.62)
				(name "P126")
				(number "126")
			)
			(pin passive line
				(at 27.94 12.7 180)
				(length 7.62)
				(name "P125")
				(number "125")
			)
			(pin passive line
				(at 27.94 10.16 180)
				(length 7.62)
				(name "P124")
				(number "124")
			)
			(pin passive line
				(at 27.94 7.62 180)
				(length 7.62)
				(name "P123")
				(number "123")
			)
			(pin output line
				(at 27.94 5.08 180)
				(length 7.62)
				(name "TDO")
				(number "121")
			)
			(pin passive line
				(at 27.94 2.54 180)
				(length 7.62)
				(name "P116")
				(number "116")
			)
			(pin passive line
				(at 27.94 0 180)
				(length 7.62)
				(name "P115")
				(number "115")
			)
			(pin passive line
				(at 27.94 -2.54 180)
				(length 7.62)
				(name "P114-RDY")
				(number "114")
			)
			(pin passive line
				(at 27.94 -5.08 180)
				(length 7.62)
				(name "P113")
				(number "113")
			)
			(pin passive line
				(at 27.94 -7.62 180)
				(length 7.62)
				(name "P109")
				(number "109")
			)
			(pin passive line
				(at 27.94 -10.16 180)
				(length 7.62)
				(name "P108")
				(number "108")
			)
			(pin passive line
				(at 27.94 -12.7 180)
				(length 7.62)
				(name "P107")
				(number "107")
			)
			(pin passive line
				(at 27.94 -15.24 180)
				(length 7.62)
				(name "P106")
				(number "106")
			)
			(pin passive line
				(at 27.94 -17.78 180)
				(length 7.62)
				(name "P105")
				(number "105")
			)
			(pin passive line
				(at 27.94 -20.32 180)
				(length 7.62)
				(name "P104")
				(number "104")
			)
			(pin passive line
				(at 27.94 -22.86 180)
				(length 7.62)
				(name "P103")
				(number "103")
			)
			(pin passive line
				(at 27.94 -25.4 180)
				(length 7.62)
				(name "P102")
				(number "102")
			)
			(pin passive line
				(at 27.94 -27.94 180)
				(length 7.62)
				(name "P90")
				(number "99")
			)
			(pin passive line
				(at 27.94 -30.48 180)
				(length 7.62)
				(name "P98")
				(number "98")
			)
			(pin passive line
				(at 27.94 -33.02 180)
				(length 7.62)
				(name "P97")
				(number "97")
			)
			(pin passive line
				(at 27.94 -35.56 180)
				(length 7.62)
				(name "P96")
				(number "96")
			)
			(pin passive line
				(at 27.94 -38.1 180)
				(length 7.62)
				(name "P95")
				(number "95")
			)
			(pin passive line
				(at 27.94 -40.64 180)
				(length 7.62)
				(name "P93")
				(number "94")
			)
			(pin passive line
				(at 27.94 -43.18 180)
				(length 7.62)
				(name "P93")
				(number "93")
			)
			(pin passive line
				(at 27.94 -45.72 180)
				(length 7.62)
				(name "P92")
				(number "92")
			)
			(pin passive line
				(at 27.94 -48.26 180)
				(length 7.62)
				(name "P88")
				(number "88")
			)
			(pin passive line
				(at 27.94 -50.8 180)
				(length 7.62)
				(name "P87")
				(number "87")
			)
			(pin passive line
				(at 27.94 -53.34 180)
				(length 7.62)
				(name "P86")
				(number "86")
			)
			(pin passive line
				(at 27.94 -55.88 180)
				(length 7.62)
				(name "P85")
				(number "85")
			)
			(pin passive line
				(at 27.94 -58.42 180)
				(length 7.62)
				(name "PGCK3")
				(number "84")
			)
			(pin passive line
				(at 27.94 -60.96 180)
				(length 7.62)
				(name "P83")
				(number "83")
			)
			(pin passive line
				(at 27.94 -63.5 180)
				(length 7.62)
				(name "SGCK3")
				(number "78")
			)
			(pin passive line
				(at 27.94 -66.04 180)
				(length 7.62)
				(name "P77")
				(number "77")
			)
			(pin passive line
				(at 27.94 -68.58 180)
				(length 7.62)
				(name "P76")
				(number "76")
			)
			(pin passive line
				(at 27.94 -71.12 180)
				(length 7.62)
				(name "P75")
				(number "75")
			)
			(pin passive line
				(at 27.94 -73.66 180)
				(length 7.62)
				(name "P74")
				(number "74")
			)
			(pin passive line
				(at 27.94 -76.2 180)
				(length 7.62)
				(name "P73")
				(number "73")
			)
		)
		(embedded_fonts no)
	)
	(symbol "+3,3V"
		(extends "+3.3V")
		(property "Reference" "#PWR"
			(at 0 -1.016 0)
		)
		(property "Value" "+3,3V"
			(at 0 2.794 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "24C512"
		(extends "24C16")
		(property "Reference" "U"
			(at 3.81 8.89 0)
		)
		(property "Value" "24C512"
			(at 5.08 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "74HC245"
		(extends "74LS245")
		(property "Reference" "U"
			(at 2.54 14.605 0)
		)
		(property "Value" "74HC245"
			(at 1.27 -14.605 0)
		)
		(property "Footprint" ""
			(at 1.27 -16.51 0)
		)
		(property "Datasheet" ""
			(at 2.54 14.605 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "BT254"
		(extends "BT253")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "BT254"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "BUSPCI-5V"
		(extends "PCI_CONUNIV")
		(property "Reference" "J"
			(at 0 81.28 0)
		)
		(property "Value" "BUSPCI-5V"
			(at 0 -81.28 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "CAPAPOL"
		(extends "CP")
		(property "Reference" "C"
			(at 1.27 2.54 0)
		)
		(property "Value" "CAPAPOL"
			(at 1.27 -2.54 0)
		)
		(property "Footprint" ""
			(at 2.54 -3.81 0)
		)
		(property "Datasheet" ""
			(at 1.27 2.54 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CP* SM*"
			(at 0 0 0)
		)
	)
)
