(footprint "BIVAR_VLP-350-F"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.05 9.75 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "BIVAR_VLP-350-F"
		(at 0.05 11.25 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0.05 10.25 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0.05 10.25 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0.05 10.25 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.05 12.75 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2.05 2.05)
		(size 0.6096 0.6096)
		(drill 0.6096)
		(layers "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.05 -2.05)
		(size 0.6096 0.6096)
		(drill 0.6096)
		(layers "*.Mask")
	)
)