(footprint "HARWIN_M22-6541042R"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "7.99")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -0.9 -6.9 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "HARWIN_M22-6541042R"
		(at -1.5 -4.9 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at -1.1 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at -1.1 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at -1.1 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -5.545 9 90)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -1.5 -3.4 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at 0 0)
		(size 2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "2" smd rect
		(at 0 2)
		(size 2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "3" smd rect
		(at 0 4)
		(size 2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "4" smd rect
		(at 0 6)
		(size 2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "5" smd rect
		(at 0 8)
		(size 2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "6" smd rect
		(at 0 10)
		(size 2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "7" smd rect
		(at 0 12)
		(size 2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "8" smd rect
		(at 0 14)
		(size 2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "9" smd rect
		(at 0 16)
		(size 2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "10" smd rect
		(at 0 18)
		(size 2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
)