(footprint "BGA784C80P28X28_2300X2300X332"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "BGA,0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, 23.00mm X 23.00mm X 3.32mm H")
	(property "Reference" "REF**"
		(at 12.87722 -9.986695 270)
		(layer "F.SilkS")
	)
	(property "Value" "XCZU4CG-1SFVC784E"
		(at 0 13.526 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" "kicad-embed://ds891-zynq-ultrascale-plus-overview.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM HF"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Bonding" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" "BGA784"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "XCZU4CG-1SFVC784E"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "3.32mm"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1Description" "Package/Pinout"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1URL" ""
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2Description" "Pinout"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2URL" ""
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "09/20/22 00:00:00"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "ICs And Semiconductors"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Device" "XCZU4CG-1SFVC784E"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "BGA784C80P28X28_2300X2300X332"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "09/20/22 00:00:00"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Logic"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Logic.SchLib"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "XCZU4CG-1SFVC784E"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "XILINX"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "XCZU4CG-1SFVC784E"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" "BGA, 0.80mm Pitch, Square; 784 Pin, 28 Columns X 28 Rows, Body 23.0mm X 23.0mm X 3.32mm H, IPC Medium Density"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "Zynq UltraScale+ MPSoC, Quad-Core ARM® Cortex™-A53 MPCore™ up to 1.5GHz, 214 PS I/O, 156 HP I/O, 96 HD I/O, 784-Pin BGA"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "XCZU4CG-1SFVC784E"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "784"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SCEM" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "4"
		(at -8.35 -12 270)
		(layer "F.Fab")
	)
	(fp_text user "19"
		(at 3.65 -12.25 270)
		(layer "F.Fab")
	)
	(fp_text user "M"
		(at -12 -1.9 180)
		(layer "F.Fab")
	)
	(fp_text user "T"
		(at -12 1.3 180)
		(layer "F.Fab")
	)
	(fp_text user "A"
		(at -12 -10.7 180)
		(layer "F.Fab")
	)
	(fp_text user "W"
		(at -12 3.7 180)
		(layer "F.Fab")
	)
	(fp_text user "9"
		(at -4.35 -12 270)
		(layer "F.Fab")
	)
	(fp_text user "AD"
		(at -12.335 7.7 180)
		(layer "F.Fab")
	)
	(fp_text user "26"
		(at 9.25 -12.3 270)
		(layer "F.Fab")
	)
	(fp_text user "27"
		(at 10.05 -12.3 270)
		(layer "F.Fab")
	)
	(fp_text user "22"
		(at 6.05 -12.3 270)
		(layer "F.Fab")
	)
	(fp_text user "10"
		(at -3.55 -12.25 270)
		(layer "F.Fab")
	)
	(fp_text user "16"
		(at 1.25 -12.25 270)
		(layer "F.Fab")
	)
	(fp_text user "18"
		(at 2.85 -12.25 270)
		(layer "F.Fab")
	)
	(fp_text user "8"
		(at -5.15 -12 270)
		(layer "F.Fab")
	)
	(fp_text user "D"
		(at -12 -8.3 180)
		(layer "F.Fab")
	)
	(fp_text user "17"
		(at 2.05 -12.25 270)
		(layer "F.Fab")
	)
	(fp_text user "15"
		(at 0.45 -12.25 270)
		(layer "F.Fab")
	)
	(fp_text user "U"
		(at -12 2.1 180)
		(layer "F.Fab")
	)
	(fp_text user "7"
		(at -5.95 -12 270)
		(layer "F.Fab")
	)
	(fp_text user "E"
		(at -12 -7.5 180)
		(layer "F.Fab")
	)
	(fp_text user "AG"
		(at -12.335 10.1 180)
		(layer "F.Fab")
	)
	(fp_text user "F"
		(at -12 -6.7 180)
		(layer "F.Fab")
	)
	(fp_text user "11"
		(at -2.75 -12.15 270)
		(layer "F.Fab")
	)
	(fp_text user "AC"
		(at -12.335 6.9 180)
		(layer "F.Fab")
	)
	(fp_text user "N"
		(at -12 -1.1 180)
		(layer "F.Fab")
	)
	(fp_text user "C"
		(at -12 -9.1 180)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at -10.75 -11.9 270)
		(layer "F.Fab")
	)
	(fp_text user "R"
		(at -12 0.5 180)
		(layer "F.Fab")
	)
	(fp_text user "13"
		(at -1.15 -12.25 270)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at -9.15 -12 270)
		(layer "F.Fab")
	)
	(fp_text user "21"
		(at 5.25 -12.2 270)
		(layer "F.Fab")
	)
	(fp_text user "23"
		(at 6.85 -12.3 270)
		(layer "F.Fab")
	)
	(fp_text user "14"
		(at -0.35 -12.25 270)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at -6.75 -12 270)
		(layer "F.Fab")
	)
	(fp_text user "L"
		(at -12 -2.7 180)
		(layer "F.Fab")
	)
	(fp_text user "12"
		(at -1.95 -12.25 270)
		(layer "F.Fab")
	)
	(fp_text user "AE"
		(at -12.335 8.5 180)
		(layer "F.Fab")
	)
	(fp_text user "AA"
		(at -12.335 5.3 180)
		(layer "F.Fab")
	)
	(fp_text user "V"
		(at -12 2.9 180)
		(layer "F.Fab")
	)
	(fp_text user "20"
		(at 4.45 -12.3 270)
		(layer "F.Fab")
	)
	(fp_text user "B"
		(at -12 -9.9 180)
		(layer "F.Fab")
	)
	(fp_text user "24"
		(at 7.65 -12.3 270)
		(layer "F.Fab")
	)
	(fp_text user "P"
		(at -12 -0.3 180)
		(layer "F.Fab")
	)
	(fp_text user "25"
		(at 8.45 -12.3 270)
		(layer "F.Fab")
	)
	(fp_text user "AF"
		(at -12.335 9.3 180)
		(layer "F.Fab")
	)
	(fp_text user "Y"
		(at -12 4.5 180)
		(layer "F.Fab")
	)
	(fp_text user "28"
		(at 10.85 -12.3 270)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at -7.55 -12 270)
		(layer "F.Fab")
	)
	(fp_text user "AH"
		(at -12.335 10.9 180)
		(layer "F.Fab")
	)
	(fp_text user "J"
		(at -12 -4.3 180)
		(layer "F.Fab")
	)
	(fp_text user "H"
		(at -12 -5.1 180)
		(layer "F.Fab")
	)
	(fp_text user "K"
		(at -12 -3.5 180)
		(layer "F.Fab")
	)
	(fp_text user "AB"
		(at -12.335 6.1 180)
		(layer "F.Fab")
	)
	(fp_text user "2"
		(at -9.95 -12 270)
		(layer "F.Fab")
	)
	(fp_text user "G"
		(at -12 -5.9 180)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -10.8 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -10 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at -9.2 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at -8.4 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at -7.6 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd circle
		(at -6.8 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd circle
		(at -6 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd circle
		(at -5.2 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd circle
		(at -4.4 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd circle
		(at -3.6 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd circle
		(at -2.8 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd circle
		(at -2 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A13" smd circle
		(at -1.2 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A14" smd circle
		(at -0.4 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A15" smd circle
		(at 0.4 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A16" smd circle
		(at 1.2 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A17" smd circle
		(at 2 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A18" smd circle
		(at 2.8 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A19" smd circle
		(at 3.6 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A20" smd circle
		(at 4.4 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A21" smd circle
		(at 5.2 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A22" smd circle
		(at 6 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A23" smd circle
		(at 6.8 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A24" smd circle
		(at 7.6 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A25" smd circle
		(at 8.4 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A26" smd circle
		(at 9.2 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A27" smd circle
		(at 10 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A28" smd circle
		(at 10.8 -10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA1" smd circle
		(at -10.8 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA2" smd circle
		(at -10 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA3" smd circle
		(at -9.2 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA4" smd circle
		(at -8.4 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA5" smd circle
		(at -7.6 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA6" smd circle
		(at -6.8 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA7" smd circle
		(at -6 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA8" smd circle
		(at -5.2 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA9" smd circle
		(at -4.4 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA10" smd circle
		(at -3.6 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA11" smd circle
		(at -2.8 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA12" smd circle
		(at -2 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA13" smd circle
		(at -1.2 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA14" smd circle
		(at -0.4 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA15" smd circle
		(at 0.4 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA16" smd circle
		(at 1.2 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA17" smd circle
		(at 2 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA18" smd circle
		(at 2.8 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA19" smd circle
		(at 3.6 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA20" smd circle
		(at 4.4 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA21" smd circle
		(at 5.2 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA22" smd circle
		(at 6 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA23" smd circle
		(at 6.8 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA24" smd circle
		(at 7.6 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA25" smd circle
		(at 8.4 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA26" smd circle
		(at 9.2 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA27" smd circle
		(at 10 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA28" smd circle
		(at 10.8 5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB1" smd circle
		(at -10.8 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB2" smd circle
		(at -10 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB3" smd circle
		(at -9.2 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB4" smd circle
		(at -8.4 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB5" smd circle
		(at -7.6 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB6" smd circle
		(at -6.8 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB7" smd circle
		(at -6 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB8" smd circle
		(at -5.2 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB9" smd circle
		(at -4.4 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB10" smd circle
		(at -3.6 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB11" smd circle
		(at -2.8 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB12" smd circle
		(at -2 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB13" smd circle
		(at -1.2 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB14" smd circle
		(at -0.4 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB15" smd circle
		(at 0.4 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB16" smd circle
		(at 1.2 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB17" smd circle
		(at 2 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB18" smd circle
		(at 2.8 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB19" smd circle
		(at 3.6 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB20" smd circle
		(at 4.4 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB21" smd circle
		(at 5.2 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB22" smd circle
		(at 6 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB23" smd circle
		(at 6.8 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB24" smd circle
		(at 7.6 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB25" smd circle
		(at 8.4 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB26" smd circle
		(at 9.2 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB27" smd circle
		(at 10 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB28" smd circle
		(at 10.8 6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC1" smd circle
		(at -10.8 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC2" smd circle
		(at -10 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC3" smd circle
		(at -9.2 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC4" smd circle
		(at -8.4 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC5" smd circle
		(at -7.6 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC6" smd circle
		(at -6.8 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC7" smd circle
		(at -6 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC8" smd circle
		(at -5.2 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC9" smd circle
		(at -4.4 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC10" smd circle
		(at -3.6 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC11" smd circle
		(at -2.8 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC12" smd circle
		(at -2 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC13" smd circle
		(at -1.2 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC14" smd circle
		(at -0.4 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC15" smd circle
		(at 0.4 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC16" smd circle
		(at 1.2 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC17" smd circle
		(at 2 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC18" smd circle
		(at 2.8 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC19" smd circle
		(at 3.6 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC20" smd circle
		(at 4.4 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC21" smd circle
		(at 5.2 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC22" smd circle
		(at 6 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC23" smd circle
		(at 6.8 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC24" smd circle
		(at 7.6 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC25" smd circle
		(at 8.4 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC26" smd circle
		(at 9.2 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC27" smd circle
		(at 10 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC28" smd circle
		(at 10.8 6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD1" smd circle
		(at -10.8 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD2" smd circle
		(at -10 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD3" smd circle
		(at -9.2 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD4" smd circle
		(at -8.4 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD5" smd circle
		(at -7.6 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD6" smd circle
		(at -6.8 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD7" smd circle
		(at -6 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD8" smd circle
		(at -5.2 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD9" smd circle
		(at -4.4 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD10" smd circle
		(at -3.6 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD11" smd circle
		(at -2.8 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD12" smd circle
		(at -2 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD13" smd circle
		(at -1.2 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD14" smd circle
		(at -0.4 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD15" smd circle
		(at 0.4 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD16" smd circle
		(at 1.2 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD17" smd circle
		(at 2 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD18" smd circle
		(at 2.8 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD19" smd circle
		(at 3.6 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD20" smd circle
		(at 4.4 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD21" smd circle
		(at 5.2 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD22" smd circle
		(at 6 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD23" smd circle
		(at 6.8 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD24" smd circle
		(at 7.6 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD25" smd circle
		(at 8.4 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD26" smd circle
		(at 9.2 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD27" smd circle
		(at 10 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AD28" smd circle
		(at 10.8 7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE1" smd circle
		(at -10.8 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE2" smd circle
		(at -10 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE3" smd circle
		(at -9.2 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE4" smd circle
		(at -8.4 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE5" smd circle
		(at -7.6 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE6" smd circle
		(at -6.8 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE7" smd circle
		(at -6 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE8" smd circle
		(at -5.2 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE9" smd circle
		(at -4.4 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE10" smd circle
		(at -3.6 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE11" smd circle
		(at -2.8 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE12" smd circle
		(at -2 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE13" smd circle
		(at -1.2 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE14" smd circle
		(at -0.4 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE15" smd circle
		(at 0.4 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE16" smd circle
		(at 1.2 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE17" smd circle
		(at 2 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE18" smd circle
		(at 2.8 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE19" smd circle
		(at 3.6 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE20" smd circle
		(at 4.4 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE21" smd circle
		(at 5.2 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE22" smd circle
		(at 6 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE23" smd circle
		(at 6.8 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE24" smd circle
		(at 7.6 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE25" smd circle
		(at 8.4 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE26" smd circle
		(at 9.2 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE27" smd circle
		(at 10 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AE28" smd circle
		(at 10.8 8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF1" smd circle
		(at -10.8 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF2" smd circle
		(at -10 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF3" smd circle
		(at -9.2 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF4" smd circle
		(at -8.4 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF5" smd circle
		(at -7.6 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF6" smd circle
		(at -6.8 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF7" smd circle
		(at -6 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF8" smd circle
		(at -5.2 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF9" smd circle
		(at -4.4 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF10" smd circle
		(at -3.6 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF11" smd circle
		(at -2.8 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF12" smd circle
		(at -2 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF13" smd circle
		(at -1.2 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF14" smd circle
		(at -0.4 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF15" smd circle
		(at 0.4 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF16" smd circle
		(at 1.2 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF17" smd circle
		(at 2 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF18" smd circle
		(at 2.8 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF19" smd circle
		(at 3.6 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF20" smd circle
		(at 4.4 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF21" smd circle
		(at 5.2 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF22" smd circle
		(at 6 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF23" smd circle
		(at 6.8 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF24" smd circle
		(at 7.6 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF25" smd circle
		(at 8.4 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF26" smd circle
		(at 9.2 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF27" smd circle
		(at 10 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AF28" smd circle
		(at 10.8 9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG1" smd circle
		(at -10.8 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG2" smd circle
		(at -10 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG3" smd circle
		(at -9.2 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG4" smd circle
		(at -8.4 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG5" smd circle
		(at -7.6 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG6" smd circle
		(at -6.8 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG7" smd circle
		(at -6 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG8" smd circle
		(at -5.2 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG9" smd circle
		(at -4.4 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG10" smd circle
		(at -3.6 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG11" smd circle
		(at -2.8 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG12" smd circle
		(at -2 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG13" smd circle
		(at -1.2 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG14" smd circle
		(at -0.4 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG15" smd circle
		(at 0.4 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG16" smd circle
		(at 1.2 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG17" smd circle
		(at 2 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG18" smd circle
		(at 2.8 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG19" smd circle
		(at 3.6 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG20" smd circle
		(at 4.4 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG21" smd circle
		(at 5.2 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG22" smd circle
		(at 6 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG23" smd circle
		(at 6.8 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG24" smd circle
		(at 7.6 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG25" smd circle
		(at 8.4 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG26" smd circle
		(at 9.2 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG27" smd circle
		(at 10 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AG28" smd circle
		(at 10.8 10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH1" smd circle
		(at -10.8 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH2" smd circle
		(at -10 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH3" smd circle
		(at -9.2 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH4" smd circle
		(at -8.4 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH5" smd circle
		(at -7.6 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH6" smd circle
		(at -6.8 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH7" smd circle
		(at -6 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH8" smd circle
		(at -5.2 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH9" smd circle
		(at -4.4 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH10" smd circle
		(at -3.6 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH11" smd circle
		(at -2.8 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH12" smd circle
		(at -2 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH13" smd circle
		(at -1.2 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH14" smd circle
		(at -0.4 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH15" smd circle
		(at 0.4 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH16" smd circle
		(at 1.2 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH17" smd circle
		(at 2 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH18" smd circle
		(at 2.8 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH19" smd circle
		(at 3.6 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH20" smd circle
		(at 4.4 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH21" smd circle
		(at 5.2 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH22" smd circle
		(at 6 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH23" smd circle
		(at 6.8 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH24" smd circle
		(at 7.6 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH25" smd circle
		(at 8.4 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH26" smd circle
		(at 9.2 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH27" smd circle
		(at 10 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AH28" smd circle
		(at 10.8 10.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -10.8 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -10 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -9.2 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at -8.4 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at -7.6 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd circle
		(at -6.8 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd circle
		(at -6 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd circle
		(at -5.2 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd circle
		(at -4.4 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd circle
		(at -3.6 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B11" smd circle
		(at -2.8 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B12" smd circle
		(at -2 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B13" smd circle
		(at -1.2 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B14" smd circle
		(at -0.4 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B15" smd circle
		(at 0.4 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B16" smd circle
		(at 1.2 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B17" smd circle
		(at 2 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B18" smd circle
		(at 2.8 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B19" smd circle
		(at 3.6 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B20" smd circle
		(at 4.4 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B21" smd circle
		(at 5.2 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B22" smd circle
		(at 6 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B23" smd circle
		(at 6.8 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B24" smd circle
		(at 7.6 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B25" smd circle
		(at 8.4 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B26" smd circle
		(at 9.2 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B27" smd circle
		(at 10 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B28" smd circle
		(at 10.8 -10)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -10.8 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -10 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at -9.2 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at -8.4 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd circle
		(at -7.6 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C6" smd circle
		(at -6.8 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C7" smd circle
		(at -6 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C8" smd circle
		(at -5.2 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C9" smd circle
		(at -4.4 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C10" smd circle
		(at -3.6 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C11" smd circle
		(at -2.8 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C12" smd circle
		(at -2 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C13" smd circle
		(at -1.2 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C14" smd circle
		(at -0.4 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C15" smd circle
		(at 0.4 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C16" smd circle
		(at 1.2 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C17" smd circle
		(at 2 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C18" smd circle
		(at 2.8 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C19" smd circle
		(at 3.6 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C20" smd circle
		(at 4.4 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C21" smd circle
		(at 5.2 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C22" smd circle
		(at 6 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C23" smd circle
		(at 6.8 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C24" smd circle
		(at 7.6 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C25" smd circle
		(at 8.4 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C26" smd circle
		(at 9.2 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C27" smd circle
		(at 10 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C28" smd circle
		(at 10.8 -9.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -10.8 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -10 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at -9.2 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at -8.4 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd circle
		(at -7.6 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D6" smd circle
		(at -6.8 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D7" smd circle
		(at -6 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D8" smd circle
		(at -5.2 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D9" smd circle
		(at -4.4 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D10" smd circle
		(at -3.6 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D11" smd circle
		(at -2.8 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D12" smd circle
		(at -2 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D13" smd circle
		(at -1.2 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D14" smd circle
		(at -0.4 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D15" smd circle
		(at 0.4 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D16" smd circle
		(at 1.2 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D17" smd circle
		(at 2 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D18" smd circle
		(at 2.8 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D19" smd circle
		(at 3.6 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D20" smd circle
		(at 4.4 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D21" smd circle
		(at 5.2 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D22" smd circle
		(at 6 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D23" smd circle
		(at 6.8 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D24" smd circle
		(at 7.6 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D25" smd circle
		(at 8.4 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D26" smd circle
		(at 9.2 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D27" smd circle
		(at 10 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D28" smd circle
		(at 10.8 -8.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -10.8 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -10 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at -9.2 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at -8.4 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E5" smd circle
		(at -7.6 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E6" smd circle
		(at -6.8 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E7" smd circle
		(at -6 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E8" smd circle
		(at -5.2 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E9" smd circle
		(at -4.4 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E10" smd circle
		(at -3.6 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E11" smd circle
		(at -2.8 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E12" smd circle
		(at -2 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E13" smd circle
		(at -1.2 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E14" smd circle
		(at -0.4 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E15" smd circle
		(at 0.4 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E16" smd circle
		(at 1.2 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E17" smd circle
		(at 2 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E18" smd circle
		(at 2.8 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E19" smd circle
		(at 3.6 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E20" smd circle
		(at 4.4 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E21" smd circle
		(at 5.2 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E22" smd circle
		(at 6 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E23" smd circle
		(at 6.8 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E24" smd circle
		(at 7.6 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E25" smd circle
		(at 8.4 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E26" smd circle
		(at 9.2 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E27" smd circle
		(at 10 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E28" smd circle
		(at 10.8 -7.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at -10.8 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -10 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at -9.2 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at -8.4 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F5" smd circle
		(at -7.6 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F6" smd circle
		(at -6.8 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F7" smd circle
		(at -6 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F8" smd circle
		(at -5.2 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F9" smd circle
		(at -4.4 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F10" smd circle
		(at -3.6 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F11" smd circle
		(at -2.8 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F12" smd circle
		(at -2 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F13" smd circle
		(at -1.2 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F14" smd circle
		(at -0.4 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F15" smd circle
		(at 0.4 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F16" smd circle
		(at 1.2 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F17" smd circle
		(at 2 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F18" smd circle
		(at 2.8 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F19" smd circle
		(at 3.6 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F20" smd circle
		(at 4.4 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F21" smd circle
		(at 5.2 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F22" smd circle
		(at 6 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F23" smd circle
		(at 6.8 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F24" smd circle
		(at 7.6 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F25" smd circle
		(at 8.4 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F26" smd circle
		(at 9.2 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F27" smd circle
		(at 10 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F28" smd circle
		(at 10.8 -6.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at -10.8 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -10 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G3" smd circle
		(at -9.2 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G4" smd circle
		(at -8.4 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G5" smd circle
		(at -7.6 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G6" smd circle
		(at -6.8 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G7" smd circle
		(at -6 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G8" smd circle
		(at -5.2 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G9" smd circle
		(at -4.4 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G10" smd circle
		(at -3.6 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G11" smd circle
		(at -2.8 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G12" smd circle
		(at -2 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G13" smd circle
		(at -1.2 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G14" smd circle
		(at -0.4 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G15" smd circle
		(at 0.4 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G16" smd circle
		(at 1.2 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G17" smd circle
		(at 2 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G18" smd circle
		(at 2.8 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G19" smd circle
		(at 3.6 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G20" smd circle
		(at 4.4 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G21" smd circle
		(at 5.2 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G22" smd circle
		(at 6 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G23" smd circle
		(at 6.8 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G24" smd circle
		(at 7.6 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G25" smd circle
		(at 8.4 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G26" smd circle
		(at 9.2 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G27" smd circle
		(at 10 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G28" smd circle
		(at 10.8 -6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H1" smd circle
		(at -10.8 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -10 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H3" smd circle
		(at -9.2 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H4" smd circle
		(at -8.4 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H5" smd circle
		(at -7.6 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H6" smd circle
		(at -6.8 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H7" smd circle
		(at -6 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H8" smd circle
		(at -5.2 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H9" smd circle
		(at -4.4 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H10" smd circle
		(at -3.6 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H11" smd circle
		(at -2.8 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H12" smd circle
		(at -2 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H13" smd circle
		(at -1.2 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H14" smd circle
		(at -0.4 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H15" smd circle
		(at 0.4 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H16" smd circle
		(at 1.2 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H17" smd circle
		(at 2 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H18" smd circle
		(at 2.8 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H19" smd circle
		(at 3.6 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H20" smd circle
		(at 4.4 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H21" smd circle
		(at 5.2 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H22" smd circle
		(at 6 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H23" smd circle
		(at 6.8 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H24" smd circle
		(at 7.6 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H25" smd circle
		(at 8.4 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H26" smd circle
		(at 9.2 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H27" smd circle
		(at 10 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H28" smd circle
		(at 10.8 -5.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J1" smd circle
		(at -10.8 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J2" smd circle
		(at -10 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J3" smd circle
		(at -9.2 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J4" smd circle
		(at -8.4 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J5" smd circle
		(at -7.6 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J6" smd circle
		(at -6.8 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J7" smd circle
		(at -6 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J8" smd circle
		(at -5.2 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J9" smd circle
		(at -4.4 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J10" smd circle
		(at -3.6 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J11" smd circle
		(at -2.8 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J12" smd circle
		(at -2 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J13" smd circle
		(at -1.2 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J14" smd circle
		(at -0.4 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J15" smd circle
		(at 0.4 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J16" smd circle
		(at 1.2 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J17" smd circle
		(at 2 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J18" smd circle
		(at 2.8 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J19" smd circle
		(at 3.6 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J20" smd circle
		(at 4.4 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J21" smd circle
		(at 5.2 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J22" smd circle
		(at 6 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J23" smd circle
		(at 6.8 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J24" smd circle
		(at 7.6 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J25" smd circle
		(at 8.4 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J26" smd circle
		(at 9.2 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J27" smd circle
		(at 10 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J28" smd circle
		(at 10.8 -4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K1" smd circle
		(at -10.8 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K2" smd circle
		(at -10 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K3" smd circle
		(at -9.2 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K4" smd circle
		(at -8.4 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K5" smd circle
		(at -7.6 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K6" smd circle
		(at -6.8 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K7" smd circle
		(at -6 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K8" smd circle
		(at -5.2 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K9" smd circle
		(at -4.4 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K10" smd circle
		(at -3.6 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K11" smd circle
		(at -2.8 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K12" smd circle
		(at -2 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K13" smd circle
		(at -1.2 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K14" smd circle
		(at -0.4 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K15" smd circle
		(at 0.4 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K16" smd circle
		(at 1.2 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K17" smd circle
		(at 2 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K18" smd circle
		(at 2.8 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K19" smd circle
		(at 3.6 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K20" smd circle
		(at 4.4 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K21" smd circle
		(at 5.2 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K22" smd circle
		(at 6 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K23" smd circle
		(at 6.8 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K24" smd circle
		(at 7.6 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K25" smd circle
		(at 8.4 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K26" smd circle
		(at 9.2 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K27" smd circle
		(at 10 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K28" smd circle
		(at 10.8 -3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L1" smd circle
		(at -10.8 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L2" smd circle
		(at -10 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L3" smd circle
		(at -9.2 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L4" smd circle
		(at -8.4 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L5" smd circle
		(at -7.6 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L6" smd circle
		(at -6.8 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L7" smd circle
		(at -6 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L8" smd circle
		(at -5.2 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L9" smd circle
		(at -4.4 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L10" smd circle
		(at -3.6 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L11" smd circle
		(at -2.8 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L12" smd circle
		(at -2 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L13" smd circle
		(at -1.2 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L14" smd circle
		(at -0.4 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L15" smd circle
		(at 0.4 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L16" smd circle
		(at 1.2 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L17" smd circle
		(at 2 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L18" smd circle
		(at 2.8 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L19" smd circle
		(at 3.6 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L20" smd circle
		(at 4.4 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L21" smd circle
		(at 5.2 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L22" smd circle
		(at 6 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L23" smd circle
		(at 6.8 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L24" smd circle
		(at 7.6 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L25" smd circle
		(at 8.4 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L26" smd circle
		(at 9.2 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L27" smd circle
		(at 10 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L28" smd circle
		(at 10.8 -2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M1" smd circle
		(at -10.8 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M2" smd circle
		(at -10 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M3" smd circle
		(at -9.2 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M4" smd circle
		(at -8.4 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M5" smd circle
		(at -7.6 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M6" smd circle
		(at -6.8 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M7" smd circle
		(at -6 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M8" smd circle
		(at -5.2 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M9" smd circle
		(at -4.4 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M10" smd circle
		(at -3.6 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M11" smd circle
		(at -2.8 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M12" smd circle
		(at -2 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M13" smd circle
		(at -1.2 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M14" smd circle
		(at -0.4 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M15" smd circle
		(at 0.4 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M16" smd circle
		(at 1.2 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M17" smd circle
		(at 2 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M18" smd circle
		(at 2.8 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M19" smd circle
		(at 3.6 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M20" smd circle
		(at 4.4 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M21" smd circle
		(at 5.2 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M22" smd circle
		(at 6 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M23" smd circle
		(at 6.8 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M24" smd circle
		(at 7.6 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M25" smd circle
		(at 8.4 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M26" smd circle
		(at 9.2 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M27" smd circle
		(at 10 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M28" smd circle
		(at 10.8 -2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N1" smd circle
		(at -10.8 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N2" smd circle
		(at -10 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N3" smd circle
		(at -9.2 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N4" smd circle
		(at -8.4 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N5" smd circle
		(at -7.6 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N6" smd circle
		(at -6.8 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N7" smd circle
		(at -6 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N8" smd circle
		(at -5.2 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N9" smd circle
		(at -4.4 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N10" smd circle
		(at -3.6 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N11" smd circle
		(at -2.8 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N12" smd circle
		(at -2 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N13" smd circle
		(at -1.2 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N14" smd circle
		(at -0.4 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N15" smd circle
		(at 0.4 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N16" smd circle
		(at 1.2 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N17" smd circle
		(at 2 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N18" smd circle
		(at 2.8 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N19" smd circle
		(at 3.6 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N20" smd circle
		(at 4.4 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N21" smd circle
		(at 5.2 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N22" smd circle
		(at 6 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N23" smd circle
		(at 6.8 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N24" smd circle
		(at 7.6 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N25" smd circle
		(at 8.4 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N26" smd circle
		(at 9.2 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N27" smd circle
		(at 10 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N28" smd circle
		(at 10.8 -1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P1" smd circle
		(at -10.8 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P2" smd circle
		(at -10 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P3" smd circle
		(at -9.2 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P4" smd circle
		(at -8.4 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P5" smd circle
		(at -7.6 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P6" smd circle
		(at -6.8 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P7" smd circle
		(at -6 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P8" smd circle
		(at -5.2 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P9" smd circle
		(at -4.4 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P10" smd circle
		(at -3.6 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P11" smd circle
		(at -2.8 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P12" smd circle
		(at -2 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P13" smd circle
		(at -1.2 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P14" smd circle
		(at -0.4 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P15" smd circle
		(at 0.4 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P16" smd circle
		(at 1.2 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P17" smd circle
		(at 2 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P18" smd circle
		(at 2.8 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P19" smd circle
		(at 3.6 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P20" smd circle
		(at 4.4 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P21" smd circle
		(at 5.2 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P22" smd circle
		(at 6 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P23" smd circle
		(at 6.8 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P24" smd circle
		(at 7.6 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P25" smd circle
		(at 8.4 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P26" smd circle
		(at 9.2 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P27" smd circle
		(at 10 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P28" smd circle
		(at 10.8 -0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R1" smd circle
		(at -10.8 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R2" smd circle
		(at -10 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R3" smd circle
		(at -9.2 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R4" smd circle
		(at -8.4 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R5" smd circle
		(at -7.6 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R6" smd circle
		(at -6.8 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R7" smd circle
		(at -6 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R8" smd circle
		(at -5.2 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R9" smd circle
		(at -4.4 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R10" smd circle
		(at -3.6 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R11" smd circle
		(at -2.8 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R12" smd circle
		(at -2 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R13" smd circle
		(at -1.2 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R14" smd circle
		(at -0.4 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R15" smd circle
		(at 0.4 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R16" smd circle
		(at 1.2 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R17" smd circle
		(at 2 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R18" smd circle
		(at 2.8 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R19" smd circle
		(at 3.6 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R20" smd circle
		(at 4.4 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R21" smd circle
		(at 5.2 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R22" smd circle
		(at 6 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R23" smd circle
		(at 6.8 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R24" smd circle
		(at 7.6 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R25" smd circle
		(at 8.4 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R26" smd circle
		(at 9.2 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R27" smd circle
		(at 10 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R28" smd circle
		(at 10.8 0.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T1" smd circle
		(at -10.8 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T2" smd circle
		(at -10 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T3" smd circle
		(at -9.2 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T4" smd circle
		(at -8.4 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T5" smd circle
		(at -7.6 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T6" smd circle
		(at -6.8 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T7" smd circle
		(at -6 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T8" smd circle
		(at -5.2 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T9" smd circle
		(at -4.4 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T10" smd circle
		(at -3.6 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T11" smd circle
		(at -2.8 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T12" smd circle
		(at -2 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T13" smd circle
		(at -1.2 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T14" smd circle
		(at -0.4 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T15" smd circle
		(at 0.4 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T16" smd circle
		(at 1.2 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T17" smd circle
		(at 2 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T18" smd circle
		(at 2.8 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T19" smd circle
		(at 3.6 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T20" smd circle
		(at 4.4 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T21" smd circle
		(at 5.2 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T22" smd circle
		(at 6 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T23" smd circle
		(at 6.8 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T24" smd circle
		(at 7.6 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T25" smd circle
		(at 8.4 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T26" smd circle
		(at 9.2 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T27" smd circle
		(at 10 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T28" smd circle
		(at 10.8 1.2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U1" smd circle
		(at -10.8 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U2" smd circle
		(at -10 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U3" smd circle
		(at -9.2 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U4" smd circle
		(at -8.4 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U5" smd circle
		(at -7.6 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U6" smd circle
		(at -6.8 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U7" smd circle
		(at -6 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U8" smd circle
		(at -5.2 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U9" smd circle
		(at -4.4 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U10" smd circle
		(at -3.6 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U11" smd circle
		(at -2.8 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U12" smd circle
		(at -2 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U13" smd circle
		(at -1.2 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U14" smd circle
		(at -0.4 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U15" smd circle
		(at 0.4 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U16" smd circle
		(at 1.2 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U17" smd circle
		(at 2 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U18" smd circle
		(at 2.8 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U19" smd circle
		(at 3.6 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U20" smd circle
		(at 4.4 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U21" smd circle
		(at 5.2 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U22" smd circle
		(at 6 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U23" smd circle
		(at 6.8 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U24" smd circle
		(at 7.6 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U25" smd circle
		(at 8.4 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U26" smd circle
		(at 9.2 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U27" smd circle
		(at 10 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U28" smd circle
		(at 10.8 2)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V1" smd circle
		(at -10.8 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V2" smd circle
		(at -10 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V3" smd circle
		(at -9.2 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V4" smd circle
		(at -8.4 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V5" smd circle
		(at -7.6 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V6" smd circle
		(at -6.8 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V7" smd circle
		(at -6 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V8" smd circle
		(at -5.2 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V9" smd circle
		(at -4.4 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V10" smd circle
		(at -3.6 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V11" smd circle
		(at -2.8 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V12" smd circle
		(at -2 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V13" smd circle
		(at -1.2 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V14" smd circle
		(at -0.4 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V15" smd circle
		(at 0.4 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V16" smd circle
		(at 1.2 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V17" smd circle
		(at 2 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V18" smd circle
		(at 2.8 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V19" smd circle
		(at 3.6 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V20" smd circle
		(at 4.4 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V21" smd circle
		(at 5.2 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V22" smd circle
		(at 6 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V23" smd circle
		(at 6.8 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V24" smd circle
		(at 7.6 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V25" smd circle
		(at 8.4 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V26" smd circle
		(at 9.2 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V27" smd circle
		(at 10 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V28" smd circle
		(at 10.8 2.8)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W1" smd circle
		(at -10.8 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W2" smd circle
		(at -10 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W3" smd circle
		(at -9.2 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W4" smd circle
		(at -8.4 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W5" smd circle
		(at -7.6 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W6" smd circle
		(at -6.8 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W7" smd circle
		(at -6 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W8" smd circle
		(at -5.2 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W9" smd circle
		(at -4.4 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W10" smd circle
		(at -3.6 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W11" smd circle
		(at -2.8 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W12" smd circle
		(at -2 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W13" smd circle
		(at -1.2 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W14" smd circle
		(at -0.4 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W15" smd circle
		(at 0.4 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W16" smd circle
		(at 1.2 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W17" smd circle
		(at 2 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W18" smd circle
		(at 2.8 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W19" smd circle
		(at 3.6 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W20" smd circle
		(at 4.4 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W21" smd circle
		(at 5.2 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W22" smd circle
		(at 6 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W23" smd circle
		(at 6.8 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W24" smd circle
		(at 7.6 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W25" smd circle
		(at 8.4 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W26" smd circle
		(at 9.2 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W27" smd circle
		(at 10 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W28" smd circle
		(at 10.8 3.6)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y1" smd circle
		(at -10.8 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y2" smd circle
		(at -10 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y3" smd circle
		(at -9.2 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y4" smd circle
		(at -8.4 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y5" smd circle
		(at -7.6 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y6" smd circle
		(at -6.8 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y7" smd circle
		(at -6 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y8" smd circle
		(at -5.2 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y9" smd circle
		(at -4.4 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y10" smd circle
		(at -3.6 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y11" smd circle
		(at -2.8 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y12" smd circle
		(at -2 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y13" smd circle
		(at -1.2 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y14" smd circle
		(at -0.4 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y15" smd circle
		(at 0.4 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y16" smd circle
		(at 1.2 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y17" smd circle
		(at 2 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y18" smd circle
		(at 2.8 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y19" smd circle
		(at 3.6 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y20" smd circle
		(at 4.4 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y21" smd circle
		(at 5.2 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y22" smd circle
		(at 6 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y23" smd circle
		(at 6.8 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y24" smd circle
		(at 7.6 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y25" smd circle
		(at 8.4 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y26" smd circle
		(at 9.2 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y27" smd circle
		(at 10 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y28" smd circle
		(at 10.8 4.4)
		(size 0.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "BGA784C80P28X28_2300X2300X332.step")
			(type model)
		)
		(file
			(name "ds891-zynq-ultrascale-plus-overview.pdf")
			(type datasheet)
		)
	)
	(model "kicad-embed://BGA784C80P28X28_2300X2300X332.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
