(footprint "BGA96C80P9X16_750X1350X120"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "BGA, 0.80mm Pitch, Rect.; 96 Pin, 9 Columns X 16 Rows, 7.50mm X 13.50mm X 1.20mm H")
	(property "Reference" "REF**"
		(at 0 -8.826 0)
		(layer "F.SilkS")
	)
	(property "Value" "MT40A512M16LY-075-E"
		(at 0 8.826 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" "kicad-embed://MT40A512M16LY-075-E.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" "MT40A512M16LY-075-E"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SCEM" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "MT40A512M16LY"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Logic.SchLib"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "MT40A512M16LY-075-E"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Device" "MT40A512M16LY-075-E"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" "BGA, 0.80mm Pitch, Rect.; 96 Pin, 9 Columns X 16 Rows, Body 13.50mm X 7.50mm X 1.20mm H"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "+1.2V, 8Gb (512 Meg x 16) Automotive DDR4 SDRAM"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "MICRON TECHNOLOGY"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "MT40A512M16LY-075-E"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "96"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" "BGA96"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" "No"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Bonding" "No"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "1.2mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD_BGA.PcbLib"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "BGA96C80P9X16_750X1350X120"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" "kicad-embed://MT40A512M16LY-075-E.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1URL" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1Description" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2URL" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2Description" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM WB"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "07/26/19 00:00:00"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "07/26/19 00:00:00"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "ICs And Semiconductors"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Logic"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "ICs And Semiconductors SMD_BGA"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "P"
		(at -4.217 4.4 0)
		(layer "F.Fab")
	)
	(fp_text user "L"
		(at -4.217 2 0)
		(layer "F.Fab")
	)
	(fp_text user "R"
		(at -4.217 5.2 0)
		(layer "F.Fab")
	)
	(fp_text user "9"
		(at 3.208 -7.225 0)
		(layer "F.Fab")
	)
	(fp_text user "E"
		(at -4.217 -2.8 0)
		(layer "F.Fab")
	)
	(fp_text user "B"
		(at -4.217 -5.2 0)
		(layer "F.Fab")
	)
	(fp_text user "M"
		(at -4.217 2.8 0)
		(layer "F.Fab")
	)
	(fp_text user "H"
		(at -4.217 -0.4 0)
		(layer "F.Fab")
	)
	(fp_text user "D"
		(at -4.217 -3.6 0)
		(layer "F.Fab")
	)
	(fp_text user "C"
		(at -4.217 -4.4 0)
		(layer "F.Fab")
	)
	(fp_text user "7"
		(at 1.608 -7.225 0)
		(layer "F.Fab")
	)
	(fp_text user "8"
		(at 2.408 -7.225 0)
		(layer "F.Fab")
	)
	(fp_text user "T"
		(at -4.217 6 0)
		(layer "F.Fab")
	)
	(fp_text user "J"
		(at -4.217 0.4 0)
		(layer "F.Fab")
	)
	(fp_text user "F"
		(at -4.217 -2 0)
		(layer "F.Fab")
	)
	(fp_text user "K"
		(at -4.217 1.2 0)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at -3.258 -7.225 0)
		(layer "F.Fab")
	)
	(fp_text user "N"
		(at -4.217 3.6 0)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at -1.592 -7.225 0)
		(layer "F.Fab")
	)
	(fp_text user "2"
		(at -2.392 -7.225 0)
		(layer "F.Fab")
	)
	(fp_text user "G"
		(at -4.217 -1.2 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -3.2 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -2.4 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at -1.6 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd circle
		(at 1.6 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd circle
		(at 2.4 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd circle
		(at 3.2 -6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -3.2 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -2.4 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -1.6 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd circle
		(at 1.6 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd circle
		(at 2.4 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd circle
		(at 3.2 -5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -3.2 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -2.4 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at -1.6 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C7" smd circle
		(at 1.6 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C8" smd circle
		(at 2.4 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C9" smd circle
		(at 3.2 -4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -3.2 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -2.4 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at -1.6 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D7" smd circle
		(at 1.6 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D8" smd circle
		(at 2.4 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D9" smd circle
		(at 3.2 -3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -3.2 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -2.4 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at -1.6 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E7" smd circle
		(at 1.6 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E8" smd circle
		(at 2.4 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E9" smd circle
		(at 3.2 -2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at -3.2 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -2.4 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at -1.6 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F7" smd circle
		(at 1.6 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F8" smd circle
		(at 2.4 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F9" smd circle
		(at 3.2 -2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at -3.2 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -2.4 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G3" smd circle
		(at -1.6 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G7" smd circle
		(at 1.6 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G8" smd circle
		(at 2.4 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G9" smd circle
		(at 3.2 -1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H1" smd circle
		(at -3.2 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -2.4 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H3" smd circle
		(at -1.6 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H7" smd circle
		(at 1.6 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H8" smd circle
		(at 2.4 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H9" smd circle
		(at 3.2 -0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J1" smd circle
		(at -3.2 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J2" smd circle
		(at -2.4 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J3" smd circle
		(at -1.6 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J7" smd circle
		(at 1.6 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J8" smd circle
		(at 2.4 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J9" smd circle
		(at 3.2 0.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K1" smd circle
		(at -3.2 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K2" smd circle
		(at -2.4 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K3" smd circle
		(at -1.6 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K7" smd circle
		(at 1.6 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K8" smd circle
		(at 2.4 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K9" smd circle
		(at 3.2 1.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L1" smd circle
		(at -3.2 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L2" smd circle
		(at -2.4 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L3" smd circle
		(at -1.6 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L7" smd circle
		(at 1.6 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L8" smd circle
		(at 2.4 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L9" smd circle
		(at 3.2 2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M1" smd circle
		(at -3.2 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M2" smd circle
		(at -2.4 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M3" smd circle
		(at -1.6 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M7" smd circle
		(at 1.6 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M8" smd circle
		(at 2.4 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M9" smd circle
		(at 3.2 2.8)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N1" smd circle
		(at -3.2 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N2" smd circle
		(at -2.4 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N3" smd circle
		(at -1.6 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N7" smd circle
		(at 1.6 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N8" smd circle
		(at 2.4 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N9" smd circle
		(at 3.2 3.6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P1" smd circle
		(at -3.2 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P2" smd circle
		(at -2.4 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P3" smd circle
		(at -1.6 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P7" smd circle
		(at 1.6 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P8" smd circle
		(at 2.4 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P9" smd circle
		(at 3.2 4.4)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R1" smd circle
		(at -3.2 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R2" smd circle
		(at -2.4 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R3" smd circle
		(at -1.6 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R7" smd circle
		(at 1.6 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R8" smd circle
		(at 2.4 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R9" smd circle
		(at 3.2 5.2)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T1" smd circle
		(at -3.2 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T2" smd circle
		(at -2.4 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T3" smd circle
		(at -1.6 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T7" smd circle
		(at 1.6 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T8" smd circle
		(at 2.4 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T9" smd circle
		(at 3.2 6)
		(size 0.4 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "BGA96C80P9X16_750X1350X120.step")
			(type model)
		)
		(file
			(name "MT40A512M16LY-075-E.pdf")
			(type datasheet)
		)
	)
	(model "kicad-embed://BGA96C80P9X16_750X1350X120.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
