(footprint "CAPC1005X55N"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Capacitor, Non-Polarized, Chip; 1.00mm L X 0.50mm W X 0.70mm H, IPC Medium Density")
	(property "Reference" "REF**"
		(at 0 -1.526 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "CC0402_100NF_16V_10%_X7R"
		(at 0 1.526 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" "100nF"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "TC" "X7R"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "CC0402_100NF_16V_10%_X7R"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "Capacitor - non polarized"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Capacitors.SchLib"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "100nF"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "2"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "CAPC1005X55N"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" "Not Recommended"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Voltage" "16V"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Tolerance" "±10%"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "SMD Multilayer Chip Ceramic Capacitor"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "GENERIC"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "CC0402_100NF_16V_10%_X7R"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" "0402"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" " "
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer1 Example" "MURATA"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer1 Part Number" "GRM155R71C104KA88D"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer1 ComponentHeight" "0.55mm"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM JLC"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "12/05/13 00:00:00"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "12/03/07 00:00:00"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "Capacitors"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Capacitors SMD"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "Capacitors SMD"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 180)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at -0.45 0 180)
		(size 0.62 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0.45 0 180)
		(size 0.62 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
