(footprint "CAPC2013X145N"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Capacitor, Non-Polarized, Chip; 2.00mm L X 1.25mm W X 1.45mm H, IPC Medium Density")
	(property "Reference" "REF**"
		(at 0 -2.026 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
		(at 0 2.026 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM BC"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" "0805"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "100uF"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "1.45mm"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "09/02/20 00:00:00"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "Capacitors"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "Capacitors SMD"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\Capacitors SMD.PcbLib"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "CAPC2013X145N"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "09/02/20 00:00:00"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Capacitors SMD"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Capacitors.SchLib"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "Capacitor - non polarized"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "MURATA"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "GRM21BC80G107ME15"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer1 ComponentHeight" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer1 Example" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer1 Part Number" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "Chip Multilayer Ceramic Capacitor for General Purpose"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "CC0805_100UF_4V_20%_X6S_MURATA_GRM21BC80G107ME15"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "2"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" "Not Recommended"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "TC" "X6S"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Tolerance" "±20%"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Val" "100uF"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Voltage" "4V"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at -0.9 0 270)
		(size 1.45 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0.9 0 270)
		(size 1.45 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
