(footprint "EATON_0402ESDA-MLP"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "0402, 2-Leads, Body 1.1mm L X 0.53mm W X 0.44mm H body, IPC Medium Density")
	(property "Reference" "REF**"
		(at 0 -1.626 180)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "0402ESDA-MLP"
		(at 0 1.626 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" "https://www.eaton.com/content/dam/eaton/products/electronic-components/resources/data-sheet/eaton-0402esda-mlp-esd-suppressor-data-sheet.pdf"
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 180)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM MR"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Bonding" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" "0402"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "0402ESDA-MLP"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "0.44mm"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1Description" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1URL" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2Description" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2URL" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "11/22/19 00:00:00"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "ICs And Semiconductors"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Device" "0402ESDA-MLP"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "ICs And Semiconductors SMD"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "EATON_0402ESDA-MLP"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "11/22/19 00:00:00"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Diodes"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Diodes.SchLib"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "Diode TVS Bi-Directional"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "EATON"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "0402ESDA-MLP"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" "0402, 2-Leads, Body 1.1mm L X 0.53mm W X 0.44mm H body, IPC Medium Density"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "0.05pF 8kV Bidirectional ESD Voltage Suppressor"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "0402ESDA-MLP"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "2"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Power" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Voltage" "8kV"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at -0.65 0)
		(size 0.9 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0.65 0)
		(size 0.9 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0402_1005Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
