(footprint "HARTING_17 25 095 2102"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Type B19, 95 Contacts (abcde) Female Connector, Angled, HAR-BUS HM with Pre-installed Upper Shield (f)")
	(property "Reference" "REF**"
		(at -9.06 -2.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "HARTING_17_25_095_2102"
		(at 0 38.101 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" "HAR-BUS HM Type B19"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "HARTING_17_25_095_2102"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "Connector HAR-BUS 95 Female (abcdef) + Shield (f)"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Connectors.SchLib"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "105"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\HARTING THD.PcbLib"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "HARTING_17 25 095 2102"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Family" "HAR-BUS HM Type B19"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "No"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" "Yes"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" "None"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SCEM" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Device" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "Har-bus HM Type B19, 95 Contacts (abcde), Pitch 2mm, 3.4mm Press-in Terminations, Female Angled Connector, with Pre-installed Upper Shield (f)"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "HARTING"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "17 25 095 2102"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "7.57mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1URL" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1Description" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2URL" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2Description" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM JMW"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "05/28/08 00:00:00"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "06/18/14 00:00:00"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "Connectors"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "HARTING"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "HARTING THD"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "a"
		(at 0.009 -2.067 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(fp_text user "19"
		(at -12.1 41.419175 90)
		(layer "F.SilkS")
		(hide yes)
	)
	(fp_text user "e"
		(at -7.99 -2.067 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(fp_text user "f"
		(at -10.134 -2.1 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(fp_text user "1"
		(at -12.1 0.107 90)
		(layer "F.SilkS")
		(hide yes)
	)
	(fp_text user "c"
		(at -3.991 -2.067 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(fp_text user "d"
		(at -5.991 -2.1 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(fp_text user "b"
		(at -1.991 -2.1 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(fp_text user "PCB"
		(at 0.451125 18.648175 90)
		(layer "Cmts.User")
	)
	(fp_text user "a"
		(at 0.009 -2.067 0)
		(layer "F.Fab")
	)
	(fp_text user "e"
		(at -7.99 -2.067 0)
		(layer "F.Fab")
	)
	(fp_text user "b"
		(at -1.991 -2.1 0)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at -12.1 0.107 90)
		(layer "F.Fab")
	)
	(fp_text user "f"
		(at -10.134 -2.1 0)
		(layer "F.Fab")
	)
	(fp_text user "c"
		(at -3.991 -2.067 0)
		(layer "F.Fab")
	)
	(fp_text user "d"
		(at -5.991 -2.1 0)
		(layer "F.Fab")
	)
	(fp_text user "PRESS-FIT TECHNOLOGY diam. 0.6mm +0.05 -0"
		(at 3.604 17.968 90)
		(layer "F.Fab")
	)
	(fp_text user "19"
		(at -12.1 41.419175 90)
		(layer "F.Fab")
	)
	(pad "A1" thru_hole circle
		(at 0 0)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A2" thru_hole circle
		(at 0 2)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A3" thru_hole circle
		(at 0 4)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A4" thru_hole circle
		(at 0 6)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A5" thru_hole circle
		(at 0 8)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A6" thru_hole circle
		(at 0 10)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A7" thru_hole circle
		(at 0 12)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A8" thru_hole circle
		(at 0 14)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A9" thru_hole circle
		(at 0 16)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A10" thru_hole circle
		(at 0 18)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A11" thru_hole circle
		(at 0 20)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A12" thru_hole circle
		(at 0 22)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A13" thru_hole circle
		(at 0 24)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A14" thru_hole circle
		(at 0 26)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A15" thru_hole circle
		(at 0 28)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A16" thru_hole circle
		(at 0 30)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A17" thru_hole circle
		(at 0 32)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A18" thru_hole circle
		(at 0 34)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A19" thru_hole circle
		(at 0 36)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B1" thru_hole circle
		(at -2 0)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B2" thru_hole circle
		(at -2 2)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B3" thru_hole circle
		(at -2 4)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B4" thru_hole circle
		(at -2 6)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B5" thru_hole circle
		(at -2 8)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B6" thru_hole circle
		(at -2 10)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B7" thru_hole circle
		(at -2 12)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B8" thru_hole circle
		(at -2 14)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B9" thru_hole circle
		(at -2 16)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B10" thru_hole circle
		(at -2 18)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B11" thru_hole circle
		(at -2 20)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B12" thru_hole circle
		(at -2 22)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B13" thru_hole circle
		(at -2 24)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B14" thru_hole circle
		(at -2 26)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B15" thru_hole circle
		(at -2 28)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B16" thru_hole circle
		(at -2 30)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B17" thru_hole circle
		(at -2 32)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B18" thru_hole circle
		(at -2 34)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B19" thru_hole circle
		(at -2 36)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C1" thru_hole circle
		(at -4 0)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C2" thru_hole circle
		(at -4 2)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C3" thru_hole circle
		(at -4 4)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C4" thru_hole circle
		(at -4 6)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C5" thru_hole circle
		(at -4 8)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C6" thru_hole circle
		(at -4 10)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C7" thru_hole circle
		(at -4 12)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C8" thru_hole circle
		(at -4 14)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C9" thru_hole circle
		(at -4 16)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C10" thru_hole circle
		(at -4 18)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C11" thru_hole circle
		(at -4 20)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C12" thru_hole circle
		(at -4 22)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C13" thru_hole circle
		(at -4 24)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C14" thru_hole circle
		(at -4 26)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C15" thru_hole circle
		(at -4 28)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C16" thru_hole circle
		(at -4 30)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C17" thru_hole circle
		(at -4 32)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C18" thru_hole circle
		(at -4 34)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C19" thru_hole circle
		(at -4 36)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D1" thru_hole circle
		(at -6 0)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D2" thru_hole circle
		(at -6 2)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D3" thru_hole circle
		(at -6 4)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D4" thru_hole circle
		(at -6 6)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D5" thru_hole circle
		(at -6 8)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D6" thru_hole circle
		(at -6 10)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D7" thru_hole circle
		(at -6 12)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D8" thru_hole circle
		(at -6 14)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D9" thru_hole circle
		(at -6 16)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D10" thru_hole circle
		(at -6 18)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D11" thru_hole circle
		(at -6 20)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D12" thru_hole circle
		(at -6 22)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D13" thru_hole circle
		(at -6 24)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D14" thru_hole circle
		(at -6 26)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D15" thru_hole circle
		(at -6 28)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D16" thru_hole circle
		(at -6 30)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D17" thru_hole circle
		(at -6 32)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D18" thru_hole circle
		(at -6 34)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D19" thru_hole circle
		(at -6 36)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E1" thru_hole circle
		(at -8 0)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E2" thru_hole circle
		(at -8 2)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E3" thru_hole circle
		(at -8 4)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E4" thru_hole circle
		(at -8 6)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E5" thru_hole circle
		(at -8 8)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E6" thru_hole circle
		(at -8 10)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E7" thru_hole circle
		(at -8 12)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E8" thru_hole circle
		(at -8 14)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E9" thru_hole circle
		(at -8 16)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E10" thru_hole circle
		(at -8 18)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E11" thru_hole circle
		(at -8 20)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E12" thru_hole circle
		(at -8 22)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E13" thru_hole circle
		(at -8 24)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E14" thru_hole circle
		(at -8 26)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E15" thru_hole circle
		(at -8 28)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E16" thru_hole circle
		(at -8 30)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E17" thru_hole circle
		(at -8 32)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E18" thru_hole circle
		(at -8 34)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "E19" thru_hole circle
		(at -8 36)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "F1" thru_hole circle
		(at -10 0)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "F3" thru_hole circle
		(at -10 4)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "F5" thru_hole circle
		(at -10 8)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "F7" thru_hole circle
		(at -10 12)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "F9" thru_hole circle
		(at -10 16)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "F11" thru_hole circle
		(at -10 20)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "F13" thru_hole circle
		(at -10 24)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "F15" thru_hole circle
		(at -10 28)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "F17" thru_hole circle
		(at -10 32)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "F19" thru_hole circle
		(at -10 36)
		(size 1.1 1.1)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "HARTING17250952102.step")
			(type model)
		)
	)
	(model "kicad-embed://HARTING17250952102.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
