(footprint "IND_MURATA_BLM31PG"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Chip Ferrite Bead, 3.20mm L X 1.60mm W, BLM31PG Series")
	(property "Reference" "REF**"
		(at 0 -2.176 180)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "IND1206_MURATA_BLM31PG500SN1"
		(at 0 2.176 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM JLC"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" "1206"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "50R@100MHz"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "1.3mm"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "12/05/13 00:00:00"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "Inductors & Transformers"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "Inductors SMD"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "IND_MURATA_BLM31PG"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "10/25/18 00:00:00"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Inductors SMD"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "Ferrite Bead"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "MURATA"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "BLM31PG500SN1"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "SMD EMIFIL Chip Ferrite Bead"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "IND1206_MURATA_BLM31PG500SN1"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "2"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Power" "3.5A"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Resistance" "0.015R"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Tolerance" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Val" "50R@100MHz"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at -1.675 0)
		(size 1.35 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.675 0)
		(size 1.35 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "IND_MURATA_BLM31PG.step")
			(type model)
		)
	)
	(model "kicad-embed://IND_MURATA_BLM31PG.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
