(footprint "IND_TDK_VLCF5020-1"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMD Inductor, 5mm L X 5mm W X 2mm H, TDK VLCF5020-1 Case")
	(property "Reference" "REF**"
		(at 0 -3.901 0)
		(layer "F.SilkS")
	)
	(property "Value" "IND_10UH_20%_TDK_VLCF5020-1"
		(at 0 3.901 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM JLC"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "10uH"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "2mm"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "07/10/14 00:00:00"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "Inductors & Transformers"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "Inductors SMD"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\Inductors SMD.PcbLib"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "IND_TDK_VLCF5020-1"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "07/10/14 00:00:00"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Inductors SMD"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Inductors & Transformers.SchLib"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "Inductor With Magnetic core"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "TDK"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "VLCF5020T-100M1R1-1"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "SMD Inductor for Power Circuits (Wound/STD , Magnetic Shielded), VLCF series"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "IND_10UH_20%_TDK_VLCF5020-1"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "2"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Power" "1.5A"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Resistance" "0.198R"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Tolerance" "±20%"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Val" "10uH"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd custom
		(at -1.25 0)
		(size 1.2 4.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.6 -0.91) (xy 0 -0.91) (xy 0.019509 -0.908079) (xy 0.055557 -0.893147) (xy 0.083147 -0.865557)
					(xy 0.098079 -0.829509) (xy 0.1 -0.81) (xy 0.1 0) (xy 0.098079 0.019509) (xy 0.083147 0.055557)
					(xy 0.055557 0.083147) (xy 0.019509 0.098079) (xy 0 0.1) (xy -0.6 0.1) (xy -0.6 1.55) (xy -1.5 1.55)
					(xy -1.5 -1.55) (xy -0.6 -1.55)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at 1.25 0)
		(size 1.2 4.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_rect
				(start 0.04 -0.69)
				(end 1.01 0.23)
				(width 0.2)
				(fill no)
			)
			(gr_poly
				(pts
					(xy 1.5 1.55) (xy 0.6 1.55) (xy 0.6 -1.55) (xy 1.5 -1.55)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "IND_TDK_VLCF5020-1.step")
			(type model)
		)
	)
	(model "kicad-embed://IND_TDK_VLCF5020-1.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
