(footprint "INFINEON_PG-VQFN-56-900 (IRPS5401M)"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "INFINEON Package PG-VQFN-56-900 (Version for IRPS5401M), 0.40mm Pitch, Square; 56 Pin, 7.00mm L X 7.00mm W X 1.00mm H Body (w/thermal tab 5.6 X 5.6mm)")
	(property "Reference" "REF**"
		(at 0.75 -5.75 270)
		(layer "F.SilkS")
	)
	(property "Value" "IRPS5401MTRPBF"
		(at 0 5.066 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" "kicad-embed://Infineon-IRPS5401M-DataSheet-v02_08-EN.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM JLC"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Bonding" "No"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" "QFN"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "IRPS5401MTRPBF"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "1mm"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1Description" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1URL" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2Description" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2URL" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "08/21/18 00:00:00"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "ICs And Semiconductors"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Device" "IRPS5401MTRPBF"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "ICs And Semiconductors SMD"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "INFINEON_PG-VQFN-56-900 (IRPS5401M)"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "08/21/18 00:00:00"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Regulators"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Regulators.SchLib"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "IRPS5401M"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "INFINEON"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "IRPS5401MTRPBF"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" "INFINEON Package PG-VQFN-56-900 (Version for IRPS5401M), 0.40mm Pitch, Square; 56 Pin, 7.00mm L X 7.00mm W X 1.00mm H Body (w/Thermal Tab 5.6 X 5.6mm)"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "Flexible Power Management Unit (4A, 4A, 2A and 2A Switching Regulators + 500mA Source/Sink Linear regulator)"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "IRPS5401MTRPBF"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "57"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" "No"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SCEM" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at -3.44 -2.6)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.44 -2.2)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.245 -2.2)
		(size 0.31 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.44 -1.8)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3.44 -1.4)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.44 -1)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.44 -0.6)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.245 -0.6)
		(size 0.31 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -3.44 -0.2)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -3.44 0.2)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -3.44 0.6)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -3.245 0.6)
		(size 0.31 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -3.44 1)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -3.44 1.4)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -3.44 1.8)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -3.44 2.2)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -3.245 2.2)
		(size 0.31 1.02)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -3.44 2.6)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -2.6 3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -2.2 3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -1.8 3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -1.4 3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -1 3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -0.6 3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -0.2 3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 0.2 3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 0.6 3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 1 3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 1.4 3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 1.8 3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 2.2 3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 2.6 3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 3.44 2.6)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 3.44 2.2)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 3.44 1.8)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 3.44 1.4)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 3.44 1)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 3.245 0.4 180)
		(size 0.31 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 3.44 0.6)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 3.44 0.2)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 3.245 -0.4 180)
		(size 0.31 0.62)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 3.44 -0.2)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 3.44 -0.6)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 3.44 -1)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 3.44 -1.4)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 3.44 -1.8)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 3.44 -2.2)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 3.44 -2.6)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at 2.6 -3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 2.2 -3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at 1.8 -3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at 1.4 -3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at 1 -3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at 0.6 -3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at 0.2 -3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at -0.2 -3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at -0.6 -3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at -1 -3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at -1.4 -3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at -1.8 -3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at -2.2 -3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at -2.6 -3.44 90)
		(size 0.7 0.22)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at 0 0)
		(size 5.6 5.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "Infineon-IRPS5401M-DataSheet-v02_08-EN.pdf")
			(type datasheet)
		)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-56-1EP_7x7mm_P0.4mm_EP5.7x5.7mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
