(footprint "INFINEON_TDA21535"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "INFINEON_TDA21535 Package")
	(property "Reference" "REF**"
		(at -4.24156 1.970165 0)
		(layer "F.SilkS")
	)
	(property "Value" "TDA21535AUMA1"
		(at 0 4.176 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" "kicad-embed://TDA21535.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM HF"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Bonding" "No"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" "PQFN28"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "TDA21535AUMA1"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "1.1mm"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1Description" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1URL" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2Description" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2URL" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "03/16/23 00:00:00"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "ICs And Semiconductors"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Device" "TDA21535AUMA1"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "ICs And Semiconductors SMD"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "INFINEON_TDA21535"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "03/16/23 00:00:00"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Regulators"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Regulators.SchLib"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "TDA21535"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "INFINEON"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "TDA21535AUMA1"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" "INFINEON INFINEON_TDA21535 ,PQFN 4 mm x 5 mm X 1.1mm H body"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "25A Half Bridge Driver for Synchronous Buck Converter"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "TDA21535AUMA1"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "27"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" "No"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SCEM" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" "Not Recommended"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" "Solder Paste Deposition Limitation"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at -1.975 -1.86 90)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.975 -1.36 90)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.975 -0.86 90)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.975 -0.36 90)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.975 0.14 90)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -1.975 1.585 90)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -1 2.475 180)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -0.5 2.475 180)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd circle
		(at 0 2.45)
		(size 0.025 0.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 0 2.475 180)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 0.5 2.475 180)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1 2.475 180)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd circle
		(at 0 0.98)
		(size 0.025 0.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 1.975 1.48 270)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 1.975 0.98 270)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 1.975 0.48 270)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 1.975 -0.58 270)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd circle
		(at 1.52 -1.08)
		(size 0.025 0.025)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 1.975 -1.08 270)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 1.975 -1.58 270)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 1.625 -2.475 180)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 1.125 -2.475 180)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 0.625 -2.475 180)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 0.125 -2.475 180)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -0.375 -2.475 180)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at -0.875 -2.475 180)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -1.375 -2.475 180)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at -0.5 -1.005)
		(size 1.78 1.67)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -1.125 0.38)
		(size 0.57 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -1518.485687)
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "INFINEON_TDA21535.step")
			(type model)
		)
		(file
			(name "TDA21535.pdf")
			(type datasheet)
		)
	)
	(model "kicad-embed://INFINEON_TDA21535.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
