(footprint "MOLEX_500075-1517"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Straight, USB Serie Mini-B Type 2 Through Hole Receptacle")
	(property "Reference" "REF**"
		(at 4.020575 -3.824275 270)
		(layer "F.SilkS")
	)
	(property "Value" "MOLEX_500075-1517"
		(at 0 3.501 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" "https://www.molex.com/content/dam/molex/molex-dot-com/products/automated/en-us/salesdrawingpdf/500/500075/5000751517_sd.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM JLC"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "7.7mm"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1Description" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1URL" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2Description" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2URL" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "07/25/12 00:00:00"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "Connectors"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Device" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Family" "USB"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "MOLEX THD"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\MOLEX THD.PcbLib"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "MOLEX_500075-1517"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "07/25/12 00:00:00"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "MOLEX"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Connectors.SchLib"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "Connector USB 5 Pin + 1Shield"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "MOLEX"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "500075-1517"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "USB Mini-B Serie Type 2, Through Hole Straight Receptacle"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "MOLEX_500075-1517"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "6"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" "No"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SCEM" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "No"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" "None"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(pad "1" thru_hole circle
		(at 1.6 -1.3)
		(size 1.25 1.25)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0.8 1.3)
		(size 1.25 1.25)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 -1.3)
		(size 1.25 1.25)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -0.8 1.3)
		(size 1.25 1.25)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -1.6 -1.3)
		(size 1.25 1.25)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole roundrect
		(at -3.65 0 90)
		(size 3.9 1.4)
		(drill oval 2.4 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "6" thru_hole roundrect
		(at 3.65 0 90)
		(size 3.9 1.4)
		(drill oval 2.4 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "5000751517.step")
			(type model)
		)
	)
	(model "kicad-embed://5000751517.step"
		(offset
			(xyz 0 0 7.75)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -180)
		)
	)
)
