(footprint "MOLEX_87832-1420"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Milli-Grid, Pitch 2mm, 14 contacts, Surface Mount Vertical Header With Locking Window And Centre Polarization Slot")
	(property "Reference" "REF**"
		(at -8.249555 -4.988835 0)
		(layer "F.SilkS")
	)
	(property "Value" "MOLEX_87832-1420"
		(at 0 5.351 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" "https://www.molex.com/en-us/products/part-detail-pdf/878321420?display=pdf&download=true"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM JLC"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "7.6mm"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1Description" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1URL" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2Description" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2URL" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "09/09/08 00:00:00"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "Connectors"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Device" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Family" "Milli-Grid™"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "MOLEX SMD"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\MOLEX SMD.PcbLib"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "MOLEX_87832-1420"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "09/09/08 00:00:00"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "MOLEX"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Connectors.SchLib"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "Connector 14 Male"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "MOLEX"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "87832-1420"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "2.00mm (.079\") Pitch Milli-Grid™ Header, Surface Mount, Vertical, Shrouded, 14 Circuits, with Locking Windows and Centre Polarization Slot, PCB Locator"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "MOLEX_87832-1420"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "14"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" "No"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SCEM" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" "None"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "" np_thru_hole circle
		(at -5 0)
		(size 0.5 0.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(solder_mask_margin 0.25)
	)
	(pad "" np_thru_hole circle
		(at 5 0)
		(size 0.5 0.5)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(solder_mask_margin 0.25)
	)
	(pad "1" smd rect
		(at -6 2.125)
		(size 1 2.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -6 -2.125)
		(size 1 2.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4 2.125)
		(size 1 2.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -4 -2.125)
		(size 1 2.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -2 2.125)
		(size 1 2.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2 -2.125)
		(size 1 2.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0 2.125)
		(size 1 2.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0 -2.125)
		(size 1 2.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 2 2.125)
		(size 1 2.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 2 -2.125)
		(size 1 2.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 4 2.125)
		(size 1 2.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 4 -2.125)
		(size 1 2.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 6 2.125)
		(size 1 2.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 6 -2.125)
		(size 1 2.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "878321420.step")
			(type model)
		)
	)
	(model "kicad-embed://878321420.step"
		(offset
			(xyz 0 0 4.4)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 -0 -0)
		)
	)
)
