(footprint "OSC_EPSON_SG-8018CE"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Oscillator, Corner Concave; 4 Pin, 2.50mm L X 3.20mm W X 1.20mm H")
	(property "Reference" "REF**"
		(at -3.312501 -1.050001 270)
		(layer "F.SilkS")
	)
	(property "Value" "OSC_50MHZ_EPSON_SG-8018CE"
		(at 0 3.176 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" "https://download.epsondevice.com/td/pdf/brief/SG-8018CE_en.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM BC"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Bonding" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "50MHz"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "1.2mm"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1Description" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1URL" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2Description" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2URL" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "08/11/21 00:00:00"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "ICs And Semiconductors"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Device" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "ICs And Semiconductors SMD"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "OSC_EPSON_SG-8018CE"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "08/11/21 00:00:00"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Crystals & Oscillators"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Crystals & Oscillators.SchLib"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "Oscillator 1OE 2GND 3OUT 4VCC"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "EPSON SEIKO"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "SG-8018CE 50.0000M-TJHPA3"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" "Oscillator, Corner Concave; 4 Pin, 2.50mm L X 3.20mm W X 1.20mm H"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "1.6 to 3.6V, ±50ppm, 15pF, -40 to 105°C, CMOS Surface Programmable Crystal Oscillator (SG-8018CE Series)"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "OSC_50MHZ_EPSON_SG-8018CE"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "4"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Val" "50MHz"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at -0.95 -1.2)
		(size 1.2 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.95 1.2)
		(size 1.2 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.95 1.2)
		(size 1.2 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.95 -1.2)
		(size 1.2 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "OSC_EPSON_SG-8018CE.step")
			(type model)
		)
	)
	(model "kicad-embed://OSC_EPSON_SG-8018CE.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
