(footprint "OSC_KYOCERA_KV7050B-C3"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Oscillator, Side Concave, 2.54mm Pitch, 6 Pins, 5.00mm L X 7.00mm W X 1.60mm H, KV7050B-C3 Series")
	(property "Reference" "REF**"
		(at 3.729065 -1.131685 90)
		(layer "F.SilkS")
	)
	(property "Value" "OSC_25MHZ_KYOCERA_KV7050B25.0000C3GD00"
		(at 0 4.876 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" "kicad-embed://KV7050B25.0000C3GD00.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM MR"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Bonding" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "25MHz"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "1.6mm"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1Description" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1URL" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2Description" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2URL" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "10/01/19 00:00:00"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "ICs And Semiconductors"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Device" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "ICs And Semiconductors SMD"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "OSC_KYOCERA_KV7050B-C3"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "10/01/19 00:00:00"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Crystals & Oscillators"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Crystals & Oscillators.SchLib"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "Oscillator KYOCERA_KV7050B-C3"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "KYOCERA"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "KV7050B25.0000C3GD00"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" "SMD Oscillator, Side Concave; 2.54mm Pitch, 6 Pins, 5.00mm L X 7.00mm W X 1.60mm H, Crystal Kyocera"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" " ±50ppm, 15pF, Supply Voltage 3.3V, -40°C to +85°C, Surface Mount Crystal Oscillator VCXO, KV7050B-C3 Series"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "OSC_25MHZ_KYOCERA_KV7050B25.0000C3GD00"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "6"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Val" "25MHz"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at -1.8 -2.54)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.8 0)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.8 2.54)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1.8 2.54)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.8 0)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.8 -2.54)
		(size 1.6 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "KV7050B25.0000C3GD00.pdf")
			(type datasheet)
		)
		(file
			(name "OSC_KYOCERA_KV7050B-C3.step")
			(type model)
		)
	)
	(model "kicad-embed://OSC_KYOCERA_KV7050B-C3.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
