(footprint "SON50P200X200X80-9N-R100X170"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SON, 0.50mm Pitch; 8 Pin, 2.00mm W X 2.00mm L X 0.80mm H body (w/thermal tab 1.0 X 1.7 mm), IPC Medium Density")
	(property "Reference" "REF**"
		(at -2.64062 1.500815 270)
		(layer "F.SilkS")
	)
	(property "Value" "TPS62125DSG"
		(at 0 2.326 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM MR"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Bonding" "No"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" "SON8"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "TPS62125DSG"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "0.8mm"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1Description" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1URL" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2Description" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2URL" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "07/05/16 00:00:00"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "ICs And Semiconductors"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Device" "TPS62125DSG"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "ICs And Semiconductors SMD"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "SON50P200X200X80-9N-R100X170"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "07/05/16 00:00:00"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Regulators"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Regulators.SchLib"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "TPS62125"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "TEXAS INSTRUMENTS"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "TPS62125DSG"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" "SON, 0.50mm Pitch; 8 Pin, 2.00mm W X 2.00mm L X 0.80mm H body (w/Thermal Tab 1.00 X 1.70mm), IPC Medium Density"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "3-V to 17-V, 300-mA Step-Down Converter With Adjustable Enable Threshold and Hysteresis"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "TPS62125DSG"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "9"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" "No"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SCEM" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at -1.05 -0.75)
		(size 0.7 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.05 -0.25)
		(size 0.7 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.05 0.25)
		(size 0.7 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.05 0.75)
		(size 0.7 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.05 0.75)
		(size 0.7 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.05 0.25)
		(size 0.7 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.05 -0.25)
		(size 0.7 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.05 -0.75)
		(size 0.7 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0 0 180)
		(size 1 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-8-1EP_2x2mm_P0.5mm_EP0.6x1.2mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
