(footprint "SOP65P400X130-8N"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SOP, 0.65mm, Pitch; 8 Pin, 2.80mm W X 2.95mm L X 1.30mm H Body, PC Medium Density")
	(property "Reference" "REF**"
		(at -1.878075 -2.777825 0)
		(layer "F.SilkS")
	)
	(property "Value" "SN74LVC2G126DCT"
		(at 0 2.876 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM MR"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Bonding" "No"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" "TSSOP8"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "SN74LVC2G126DCT"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "1.3mm"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1Description" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1URL" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2Description" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2URL" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "10/07/16 00:00:00"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "ICs And Semiconductors"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Device" "SN74LVC2G126DCT"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "ICs And Semiconductors SMD"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "SOP65P400X130-8N"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "07/28/20 00:00:00"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Standard Logic"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Standard Logic.SchLib"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "742G126"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "TEXAS INSTRUMENTS"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "SN74LVC2G126DCT"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" "SOP, 0.65mm Pitch; 8 Pin, 2.80mm W X 2.95mm L X 1.30mm H body, IPC Medium Density"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "Dual Bus Buffer Gate With 3-State Outputs"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "SN74LVC2G126DCT"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "8"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" "No"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SCEM" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 90)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at -1.9 -0.975)
		(size 1.1 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.9 -0.325)
		(size 1.1 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.9 0.325)
		(size 1.1 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.9 0.975)
		(size 1.1 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.9 0.975)
		(size 1.1 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.9 0.325)
		(size 1.1 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.9 -0.325)
		(size 1.1 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.9 -0.975)
		(size 1.1 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-8_2.95x2.8mm_P0.65mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
