(footprint "SOT190P230X110-4N"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SOT143, SOT, 1.90mm Pitch; 4 Pin, 1.30mm W X 2.90mm L X 1.10mm H body, IPC Medium Density")
	(property "Reference" "REF**"
		(at 0 -3.001 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "PRTR5V0U2X"
		(at 0 2.776 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "B.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM JLC"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Bonding" "No"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" "SOT143B"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "PRTR5V0U2X"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "1.1mm"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1Description" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1URL" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2Description" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2URL" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "03/22/11 00:00:00"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "ICs And Semiconductors"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Device" "PRTR5V0U2X"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "ICs And Semiconductors SMD"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "SOT190P230X110-4N"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "03/22/11 00:00:00"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Diodes"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Diodes.SchLib"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "PRTR5V0U2X"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "NXP SEMICONDUCTORS"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "PRTR5V0U2X"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" "SOT143B, SOT, 1.90mm Pitch; 4 Pin, 1.30mm W X 2.90mm L X 1.10mm H body, IPC Medium Density"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "Ultra Low Capacitance (1pF) Double Rail-to-Rail ESD Protection Diode (8kV)"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "PRTR5V0U2X"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "4"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Power" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" "No"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Voltage" "5.5V"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at -1.15 -0.75 270)
		(size 1 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.15 0.95 180)
		(size 1 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 1.15 0.95 180)
		(size 1 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1.15 -0.95 180)
		(size 1 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-143.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
