(footprint "SOT95P280X145-6N"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SOT23, 6-Leads, Body 1.6x3.0mm, Pitch 0.95mm, IPC Medium Density")
	(property "Reference" "REF**"
		(at -3.3 1.6 270)
		(layer "F.SilkS")
	)
	(property "Value" "24AA025E48T-I_OT"
		(at 0 2.826 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM BC"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Bonding" "No"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" "SOT23-6"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "24AA025E48T-I/OT"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "1.45mm"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1Description" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1URL" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2Description" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2URL" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "12/06/19 00:00:00"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "ICs And Semiconductors"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Device" "24AA025E48T-I/OT"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "ICs And Semiconductors SMD"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "SOT95P280X145-6N"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "12/06/19 00:00:00"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Logic"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Logic.SchLib"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "24AA025E48T-I/OT"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "MICROCHIP TECHNOLOGY"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "24AA025E48T-I/OT"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" "SOT, 0.95mm pitch; 6 pin, 1.60mm W X 2.90mm L X 1.45mm H body, IPC Medium Density"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "1.7V-5.5V, 2K I2C Serial EEPROM With EUI-48™ Node Identity; Cascadable"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "24AA025E48T-I_OT"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "6"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" "No"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SCEM" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at -1.35 -0.95 90)
		(size 0.6 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.35 0 90)
		(size 0.6 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.35 0.95 90)
		(size 0.6 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 1.35 0.95 90)
		(size 0.6 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.35 0 90)
		(size 0.6 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.35 -0.95 90)
		(size 0.6 1.05)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
