(footprint "TEXAS_DSC (S-PWSON-N10)"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SON, TEXAS Case Style DSC, 0.50mm Pitch, Square, 10 Pin, 3.00mm L X 3.00mm W X 0.80mm H body  (w/Thermal Tab 1.2 X 2.0 mm)")
	(property "Reference" "REF**"
		(at -3.748275 -0.446985 90)
		(layer "F.SilkS")
	)
	(property "Value" "DAC8562SDSC"
		(at 0 2.776 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dac8562.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM HF"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Bonding" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" "SON10"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" "DAC8562SDSC"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "0.8mm"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1Description" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1URL" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2Description" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2URL" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "03/29/23 00:00:00"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "ICs And Semiconductors"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Device" "DAC8562SDSC"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "ICs And Semiconductors SMD"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\ICs And Semiconductors SMD.PcbLib"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "TEXAS_DSC (S-PWSON-N10)"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "03/29/23 00:00:00"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "Analog & Interface"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Analog & Interface.SchLib"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "DAC8562"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "TEXAS INSTRUMENTS"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "DAC8562SDSC"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "Yes"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" "TEXAS Case Style DRC (Formerly DRC (S-PWSON-N10)), SON, 0.50mm Pitch, 10 Pin, 3.00mm W  X 3.00mm L X 0.80mm H body, (w/Thermal Tab 1.05 X 2.55 mm)"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "16-Bit, Low-Power, Buffered, Voltage-Output DACs With 2.5-V, 4-PPM/°C Internal Reference"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "DAC8562SDSC"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "11"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SCEM" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "Yes"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(pad "1" smd rect
		(at -1.475 -1)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.475 -0.5)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.475 0)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.475 0.5)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.475 1)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.475 1)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.475 0.5)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.475 0)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 1.475 -0.5)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.475 -1)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 0 0)
		(size 1.05 2.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "TEXAS_DSC_S-PWSON-N10.step")
			(type model)
		)
	)
	(model "kicad-embed://TEXAS_DSC_S-PWSON-N10.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
