(footprint "TYCO_2149027-1"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "2x4 Press Fit SFP+ Cage and PT Connectors Assembly with EMI Springs")
	(property "Reference" "REF**"
		(at 0 -7.356 0)
		(layer "F.SilkS")
		(hide yes)
	)
	(property "Value" "TYCO_2149027-1"
		(at 0 7.356 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" "Mini-SAS HD"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Number" "TYCO_2149027-1"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Ref" "Mini-SAS HD"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Path" "SchLib\\Connectors.SchLib"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Comment" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Kind" "Standard"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Component Type" "Standard"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PackageDescription" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Pin Count" "36"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Case" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Path" "PcbLib\\TYCO THD.PcbLib"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Ref" "TYCO_2149027-1"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Family" "Mini-SAS HD"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Mounted" "No"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Socket" "No"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SMD" "No"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "PressFit" "Yes"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense" "No"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Sense Comment" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status" "None"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Status Comment" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "SCEM" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Device" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Part Description" "36 Contacts, Through Hole, Right Angle, Mini-SAS High Density"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer" "TYCO ELECTRONICS"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Manufacturer Part Number" "2149027-1"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentHeight" "12.32mm"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1URL" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink1Description" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2URL" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "ComponentLink2Description" " "
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "HelpURL" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Author" "CERN DEM HF"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "CreateDate" "08/21/23 00:00:00"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "LatestRevisionDate" "08/21/23 00:00:00"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Database Table Name" "Connectors"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Library Name" "TYCO"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Footprint Library" "TYCO THD"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "License" "CC-BY-SA 4.0"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "PRESS-FIT TECHNOLOGY"
		(at -14.808 -3.63 0)
		(layer "F.Fab")
	)
	(fp_text user "6x diam. 0.8mm +0.02/-0.08"
		(at -13.486 -2.716 0)
		(layer "F.Fab")
	)
	(fp_text user "PRESS-FIT TECHNOLOGY"
		(at -13.308 3.37 0)
		(layer "F.Fab")
	)
	(fp_text user "36x diam. 0.8mm +0.02/-0.08"
		(at -11.719 4.284 0)
		(layer "F.Fab")
	)
	(pad "A1" thru_hole roundrect
		(at -5 -3)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "A2" thru_hole roundrect
		(at -6.4 -2.25)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "A3" thru_hole roundrect
		(at -5.7 -1.5)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "A4" thru_hole roundrect
		(at -5 -0.75)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "A5" thru_hole roundrect
		(at -6.4 0)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "A6" thru_hole roundrect
		(at -5.7 0.75)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "A7" thru_hole roundrect
		(at -5 1.5)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "A8" thru_hole roundrect
		(at -6.4 2.25)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "A9" thru_hole roundrect
		(at -5.7 3)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "B1" thru_hole roundrect
		(at -1.2 -3)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "B2" thru_hole roundrect
		(at -2.6 -2.25)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "B3" thru_hole roundrect
		(at -1.9 -1.5)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "B4" thru_hole roundrect
		(at -1.2 -0.75)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "B5" thru_hole roundrect
		(at -2.6 0)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "B6" thru_hole roundrect
		(at -1.9 0.75)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "B7" thru_hole roundrect
		(at -1.2 1.5)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "B8" thru_hole roundrect
		(at -2.6 2.25)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "B9" thru_hole roundrect
		(at -1.9 3)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "C1" thru_hole roundrect
		(at 2.6 -3)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "C2" thru_hole roundrect
		(at 1.2 -2.25)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "C3" thru_hole roundrect
		(at 1.9 -1.5)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "C4" thru_hole roundrect
		(at 2.6 -0.75)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "C5" thru_hole roundrect
		(at 1.2 0)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "C6" thru_hole roundrect
		(at 1.9 0.75)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "C7" thru_hole roundrect
		(at 2.6 1.5)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "C8" thru_hole roundrect
		(at 1.2 2.25)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "C9" thru_hole roundrect
		(at 1.9 3)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "D1" thru_hole roundrect
		(at 6.4 -3)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "D2" thru_hole roundrect
		(at 5 -2.25)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "D3" thru_hole roundrect
		(at 5.7 -1.5)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "D4" thru_hole roundrect
		(at 6.4 -0.75)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "D5" thru_hole roundrect
		(at 5 0)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "D6" thru_hole roundrect
		(at 5.7 0.75)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "D7" thru_hole roundrect
		(at 6.4 1.5)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "D8" thru_hole roundrect
		(at 5 2.25)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "D9" thru_hole roundrect
		(at 5.7 3)
		(size 0.9 0.9)
		(drill 0.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.5)
	)
	(pad "SHIELD" thru_hole circle
		(at -9.4 0 90)
		(size 4.4 4.4)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SHIELD" thru_hole circle
		(at -5.7 -5.5 90)
		(size 1.3 1.3)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SHIELD" thru_hole circle
		(at -5.7 5.5 90)
		(size 1.3 1.3)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SHIELD" thru_hole circle
		(at 8.11 -1.5 90)
		(size 1.3 1.3)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SHIELD" thru_hole rect
		(at 8.11 3 90)
		(size 1.7 1.7)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "TYCO_2149027-1.step")
			(type model)
		)
	)
	(model "kicad-embed://TYCO_2149027-1.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
