(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A5")
	(lib_symbols
		(symbol "Resistors:RES"
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 1.27 2.54 0)
			)
			(property "Value" "RES"
				(at -1.27 2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 1.27 2.54 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "val" "Ω"
				(at 1.27 1.27 0)
			)
			(property "tol" ""
				(at 1.27 0 0)
			)
			(property "pkg" ""
				(at 1.27 -1.27 0)
			)
			(property "pwr" ""
				(at 1.27 -2.54 0)
			)
			(property "height" ""
				(at -1.27 -1.27 0)
			)
			(property "Sim.Device" "R"
				(at 0 0 0)
			)
			(property "Sim.Pins" "1=+ 2=-"
				(at 0 -2.54 0)
			)
			(property "Sim.Params" "r=\"${val}\""
				(at 0 -2.54 0)
			)
			(symbol "RES_1_1"
				(polyline
					(pts
						(xy 0 -2.286) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.286) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -0.762) (xy 1.016 -1.143) (xy 0 -1.524) (xy -1.016 -1.905) (xy 0 -2.286)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0.762) (xy 1.016 0.381) (xy 0 0) (xy -1.016 -0.381) (xy 0 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.286) (xy 1.016 1.905) (xy 0 1.524) (xy -1.016 1.143) (xy 0 0.762)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
					(alternate "bidir" bidirectional line)
					(alternate "in" input line)
					(alternate "open_collector" open_collector line)
					(alternate "open_emitter" open_emitter line)
					(alternate "out" output line)
					(alternate "pwr_in" power_in line)
					(alternate "pwr_out" power_out line)
					(alternate "tristate" tri_state line)
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
					(alternate "bidir" bidirectional line)
					(alternate "in" input line)
					(alternate "open_collector" open_collector line)
					(alternate "open_emitter" open_emitter line)
					(alternate "out" output line)
					(alternate "pwr_in" power_in line)
					(alternate "pwr_out" power_out line)
					(alternate "tristate" tri_state line)
				)
			)
		)
	)
	(bus_alias "a"
		(members "a" "b" "c")
	)
	(junction
		(at 78.74 68.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 78.74 71.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 78.74 66.04)
		(diameter 0)
		(color 0 0 0 0)
	)
	(bus_entry
		(at 63.5 68.58)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 63.5 66.04)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 63.5 63.5)
		(size 2.54 2.54)
	)
	(bus_entry
		(at 63.5 60.96)
		(size 2.54 2.54)
	)
	(bus
		(pts
			(xy 57.15 60.96) (xy 63.5 60.96)
		)
	)
	(wire
		(pts
			(xy 78.74 63.5) (xy 78.74 66.04)
		)
	)
	(bus
		(pts
			(xy 63.5 60.96) (xy 63.5 63.5)
		)
	)
	(wire
		(pts
			(xy 66.04 68.58) (xy 78.74 68.58)
		)
	)
	(bus
		(pts
			(xy 63.5 63.5) (xy 63.5 66.04)
		)
	)
	(wire
		(pts
			(xy 66.04 66.04) (xy 78.74 66.04)
		)
	)
	(wire
		(pts
			(xy 78.74 68.58) (xy 78.74 71.12)
		)
	)
	(wire
		(pts
			(xy 78.74 66.04) (xy 78.74 68.58)
		)
	)
	(wire
		(pts
			(xy 78.74 71.12) (xy 78.74 73.66)
		)
	)
	(bus
		(pts
			(xy 63.5 66.04) (xy 63.5 68.58)
		)
	)
	(wire
		(pts
			(xy 66.04 71.12) (xy 78.74 71.12)
		)
	)
	(wire
		(pts
			(xy 66.04 63.5) (xy 78.74 63.5)
		)
	)
	(label "A0"
		(at 67.31 63.5 0)
	)
	(label "A2"
		(at 67.31 68.58 0)
	)
	(label "A1"
		(at 67.31 66.04 0)
	)
	(label "A3"
		(at 67.31 71.12 0)
	)
	(hierarchical_label "A[0..3]"
		(shape input)
		(at 57.15 60.96 180)
		(fields_autoplaced yes)
	)
	(symbol
		(lib_id "Resistors:RES")
		(at 78.74 77.47 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R201"
			(at 80.01 74.93 0)
		)
		(property "Value" "RES"
			(at 77.47 74.93 0)
		)
		(property "Footprint" ""
			(at 78.74 77.47 0)
		)
		(property "Datasheet" "~"
			(at 80.01 74.93 0)
		)
		(property "Description" ""
			(at 78.74 77.47 0)
		)
		(property "val" "Ω"
			(at 80.01 76.2 0)
		)
		(property "tol" ""
			(at 80.01 77.47 0)
		)
		(property "pkg" ""
			(at 80.01 78.74 0)
		)
		(property "pwr" ""
			(at 80.01 80.01 0)
		)
		(property "height" ""
			(at 77.47 78.74 0)
		)
		(property "Sim.Device" "R"
			(at 78.74 77.47 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 78.74 80.01 0)
		)
		(property "Sim.Params" "r=\"${val}\""
			(at 78.74 80.01 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "R201")
					(unit 1)
				)
			)
		)
	)
)
