(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "Device:R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
				(hide yes)
			)
			(property "Datasheet" ""
				(at 0 0 0)
				(hide yes)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
				(hide yes)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
				(hide yes)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
				(hide yes)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "")
					(number "2")
				)
			)
		)
		(symbol "custom:MOLEX_PICOBLADE_8PHOR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J1"
				(at 6.35 0.0001 0)
			)
			(property "Value" "MOLEX"
				(at 6.35 -2.5399 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
				(hide yes)
			)
			(property "Datasheet" ""
				(at 0 0 0)
				(hide yes)
			)
			(property "Description" "1.25mm (.049\") Pitch PicoBlade Header, SMT, Vertical, Lead-free, 8 Circuits"
				(at 0 0 0)
				(hide yes)
			)
			(property "LOCATION" "Front"
				(at 0 0 0)
				(hide yes)
			)
			(property "FUNCTION" "Panel"
				(at 0 0 0)
				(hide yes)
			)
			(symbol "MOLEX_PICOBLADE_8PHOR_1_0"
				(polyline
					(pts
						(xy -2.54 12.7) (xy 5.08 12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 -15.24) (xy -2.54 12.7)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 12.7) (xy 5.08 -15.24)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -15.24) (xy -2.54 -15.24)
					)
					(fill
						(type none)
					)
				)
				(text "${LOCATION}"
					(at 2.286 -2.54 900)
				)
				(text "${FUNCTION}"
					(at 3.81 -2.54 900)
				)
				(pin no_connect line
					(at -5.08 7.62 0)
					(length 2.54)
					(name "1")
					(number "1")
					(alternate "1.bidir" bidirectional line)
					(alternate "1.free" free line)
					(alternate "1.in" input line)
					(alternate "1.oc" open_collector line)
					(alternate "1.oe" open_emitter line)
					(alternate "1.out" output line)
					(alternate "1.pas" passive line)
					(alternate "1.pow" power_in line)
					(alternate "1.sup" power_out line)
					(alternate "1.tristate" tri_state line)
					(alternate "1.unspec" unspecified line)
				)
				(pin no_connect line
					(at -5.08 5.08 0)
					(length 2.54)
					(name "2")
					(number "2")
					(alternate "2.bidir" bidirectional line)
					(alternate "2.free" free line)
					(alternate "2.in" input line)
					(alternate "2.oc" open_collector line)
					(alternate "2.oe" open_emitter line)
					(alternate "2.out" output line)
					(alternate "2.pas" passive line)
					(alternate "2.pow" power_in line)
					(alternate "2.sup" power_out line)
					(alternate "2.tristate" tri_state line)
					(alternate "2.unspec" unspecified line)
				)
				(pin no_connect line
					(at -5.08 2.54 0)
					(length 2.54)
					(name "3")
					(number "3")
					(alternate "3.bidir" bidirectional line)
					(alternate "3.free" free line)
					(alternate "3.in" input line)
					(alternate "3.oc" open_collector line)
					(alternate "3.oe" open_emitter line)
					(alternate "3.out" output line)
					(alternate "3.pas" passive line)
					(alternate "3.pow" power_in line)
					(alternate "3.sup" power_out line)
					(alternate "3.tristate" tri_state line)
					(alternate "3.unspec" unspecified line)
				)
				(pin no_connect line
					(at -5.08 0 0)
					(length 2.54)
					(name "4")
					(number "4")
					(alternate "4.bidir" bidirectional line)
					(alternate "4.free" free line)
					(alternate "4.in" input line)
					(alternate "4.oc" open_collector line)
					(alternate "4.oe" open_emitter line)
					(alternate "4.out" output line)
					(alternate "4.pas" passive line)
					(alternate "4.pow" power_in line)
					(alternate "4.sup" power_out line)
					(alternate "4.tristate" tri_state line)
					(alternate "4.unspec" unspecified line)
				)
				(pin no_connect line
					(at -5.08 -2.54 0)
					(length 2.54)
					(name "5")
					(number "5")
					(alternate "5.bidir" bidirectional line)
					(alternate "5.free" free line)
					(alternate "5.in" input line)
					(alternate "5.oc" open_collector line)
					(alternate "5.oe" open_emitter line)
					(alternate "5.out" output line)
					(alternate "5.pas" passive line)
					(alternate "5.pow" power_in line)
					(alternate "5.sup" power_out line)
					(alternate "5.tristate" tri_state line)
					(alternate "5.unspec" unspecified line)
				)
				(pin no_connect line
					(at -5.08 -5.08 0)
					(length 2.54)
					(name "6")
					(number "6")
					(alternate "6.bidir" bidirectional line)
					(alternate "6.free" free line)
					(alternate "6.in" input line)
					(alternate "6.oc" open_collector line)
					(alternate "6.oe" open_emitter line)
					(alternate "6.out" output line)
					(alternate "6.pas" passive line)
					(alternate "6.pow" power_in line)
					(alternate "6.sup" power_out line)
					(alternate "6.tristate" tri_state line)
					(alternate "6.unspec" unspecified line)
				)
				(pin no_connect line
					(at -5.08 -7.62 0)
					(length 2.54)
					(name "7")
					(number "7")
					(alternate "7.bidir" bidirectional line)
					(alternate "7.free" free line)
					(alternate "7.in" input line)
					(alternate "7.oc" open_collector line)
					(alternate "7.oe" open_emitter line)
					(alternate "7.out" output line)
					(alternate "7.pas" passive line)
					(alternate "7.pow" power_in line)
					(alternate "7.sup" power_out line)
					(alternate "7.tristate" tri_state line)
					(alternate "7.unspec" unspecified line)
				)
				(pin no_connect line
					(at -5.08 -10.16 0)
					(length 2.54)
					(name "8")
					(number "8")
					(alternate "8.bidir" bidirectional line)
					(alternate "8.free" free line)
					(alternate "8.in" input line)
					(alternate "8.oc" open_collector line)
					(alternate "8.oe" open_emitter line)
					(alternate "8.out" output line)
					(alternate "8.pas" passive line)
					(alternate "8.pow" power_in line)
					(alternate "8.sup" power_out line)
					(alternate "8.tristate" tri_state line)
					(alternate "8.unspec" unspecified line)
				)
				(pin passive line
					(at -5.08 -15.24 0)
					(length 2.54)
					(name "G")
					(number "G")
				)
			)
		)
		(symbol "power:+5V"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
				(hide yes)
			)
			(property "Value" "+5V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
				(hide yes)
			)
			(property "Datasheet" ""
				(at 0 0 0)
				(hide yes)
			)
			(property "Description" "Power symbol creates a global label with name \"+5V\""
				(at 0 0 0)
				(hide yes)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
				(hide yes)
			)
			(symbol "+5V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+5V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "")
					(number "1")
				)
			)
		)
		(symbol "power:Earth"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
				(hide yes)
			)
			(property "Value" "Earth"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
				(hide yes)
			)
			(property "Datasheet" ""
				(at 0 0 0)
				(hide yes)
			)
			(property "Description" "Power symbol creates a global label with name \"Earth\""
				(at 0 0 0)
				(hide yes)
			)
			(property "ki_keywords" "global ground gnd"
				(at 0 0 0)
				(hide yes)
			)
			(symbol "Earth_0_1"
				(polyline
					(pts
						(xy -0.635 -1.905) (xy 0.635 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.127 -2.54) (xy 0.127 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.27) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Earth_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "")
					(number "1")
				)
			)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
				(hide yes)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
				(hide yes)
			)
			(property "Datasheet" ""
				(at 0 0 0)
				(hide yes)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
				(hide yes)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
				(hide yes)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "")
					(number "1")
				)
			)
		)
	)
	(junction
		(at 85.09 93.98)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 85.09 76.2) (xy 85.09 93.98)
		)
	)
	(wire
		(pts
			(xy 88.9 78.74) (xy 92.71 78.74)
		)
	)
	(wire
		(pts
			(xy 85.09 93.98) (xy 85.09 102.87)
		)
	)
	(wire
		(pts
			(xy 88.9 72.39) (xy 88.9 78.74)
		)
	)
	(wire
		(pts
			(xy 92.71 93.98) (xy 85.09 93.98)
		)
	)
	(wire
		(pts
			(xy 92.71 76.2) (xy 85.09 76.2)
		)
	)
	(wire
		(pts
			(xy 72.39 91.44) (xy 92.71 91.44)
		)
	)
	(wire
		(pts
			(xy 72.39 90.17) (xy 72.39 91.44)
		)
	)
	(wire
		(pts
			(xy 92.71 99.06) (xy 90.17 99.06)
		)
	)
	(wire
		(pts
			(xy 72.39 81.28) (xy 72.39 82.55)
		)
	)
	(wire
		(pts
			(xy 90.17 99.06) (xy 90.17 102.87)
		)
	)
	(wire
		(pts
			(xy 92.71 81.28) (xy 72.39 81.28)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 85.09 102.87 0)
		(unit 1)
		(convert 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 85.09 109.22 0)
			(hide yes)
		)
		(property "Value" "GND"
			(at 85.09 107.95 0)
		)
		(property "Footprint" ""
			(at 85.09 102.87 0)
			(hide yes)
		)
		(property "Datasheet" ""
			(at 85.09 102.87 0)
			(hide yes)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 85.09 102.87 0)
			(hide yes)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 88.9 72.39 0)
		(unit 1)
		(convert 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 88.9 76.2 0)
			(hide yes)
		)
		(property "Value" "+5V"
			(at 88.9 67.31 0)
		)
		(property "Footprint" ""
			(at 88.9 72.39 0)
			(hide yes)
		)
		(property "Datasheet" ""
			(at 88.9 72.39 0)
			(hide yes)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 88.9 72.39 0)
			(hide yes)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "custom:MOLEX_PICOBLADE_8PHOR")
		(at 97.79 83.82 0)
		(unit 1)
		(convert 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J1"
			(at 104.14 83.8199 0)
		)
		(property "Value" "MOLEX"
			(at 104.14 86.3599 0)
		)
		(property "Footprint" "custom:MOLEX_533980871"
			(at 97.79 83.82 0)
			(hide yes)
		)
		(property "Datasheet" ""
			(at 97.79 83.82 0)
			(hide yes)
		)
		(property "Description" "1.25mm (.049\") Pitch PicoBlade Header, SMT, Vertical, Lead-free, 8 Circuits"
			(at 97.79 83.82 0)
			(hide yes)
		)
		(property "FUNCTION" "Function"
			(at 97.79 83.82 0)
			(hide yes)
		)
		(property "LOCATION" "Location"
			(at 97.79 83.82 0)
			(hide yes)
		)
		(pin "3"
			(alternate "3.out")
		)
		(pin "2"
			(alternate "2.pow")
		)
		(pin "1"
			(alternate "1.pow")
		)
		(pin "G")
		(pin "8"
			(alternate "8.pow")
		)
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7"
			(alternate "7.in")
		)
		(instances
			(project ""
				(path
					(reference "J1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 72.39 86.36 0)
		(unit 1)
		(convert 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 74.93 85.0899 0)
		)
		(property "Value" "R"
			(at 74.93 87.6299 0)
		)
		(property "Footprint" "Resistor_SMD:R_0402_1005Metric"
			(at 70.612 86.36 90)
			(hide yes)
		)
		(property "Datasheet" ""
			(at 72.39 86.36 0)
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 72.39 86.36 0)
			(hide yes)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:Earth")
		(at 90.17 102.87 0)
		(unit 1)
		(convert 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 90.17 109.22 0)
			(hide yes)
		)
		(property "Value" "Earth"
			(at 90.17 107.95 0)
		)
		(property "Footprint" ""
			(at 90.17 102.87 0)
			(hide yes)
		)
		(property "Datasheet" ""
			(at 90.17 102.87 0)
			(hide yes)
		)
		(property "Description" "Power symbol creates a global label with name \"Earth\""
			(at 90.17 102.87 0)
			(hide yes)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)
