(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0.7")
	(paper "A4")
	(lib_symbols
		(symbol "FPGA_Microsemi:A3P060-xVQx100"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U1"
				(at 4.6833 -59.69 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "A3P060-xVQx100"
				(at 4.6833 -62.23 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
				(at 28.194 50.8 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/268/ProASIC_c2_ae3_Flash_Family_FPGAs_with_Optimal_Sof-3082432.pdf"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ProASIC3 Flash Family FPGAs, 512 MCLB / macrocells, TQFP-100 (VQ100)"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "ProASIC3 ACTEL FLASH A3P060-VQ100 A3P060-VQG100 A3P060-2VQG100"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "*TQFP*14x14mm*P0.5mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "A3P060-xVQx100_0_1"
				(rectangle
					(start -26.67 57.15)
					(end 26.67 -57.15)
					(fill
						(type background)
					)
				)
			)
			(symbol "A3P060-xVQx100_1_1"
				(pin input line
					(at -30.48 50.8 0)
					(length 3.81)
					(name "TCK")
					(number "47")
				)
				(pin input line
					(at -30.48 48.26 0)
					(length 3.81)
					(name "TDI")
					(number "48")
				)
				(pin output line
					(at -30.48 45.72 0)
					(length 3.81)
					(name "TDO")
					(number "54")
				)
				(pin input line
					(at -30.48 43.18 0)
					(length 3.81)
					(name "TMS")
					(number "49")
				)
				(pin input line
					(at -30.48 40.64 0)
					(length 3.81)
					(name "TRST")
					(number "55")
				)
				(pin bidirectional line
					(at -30.48 35.56 0)
					(length 3.81)
					(name "IO95RSB1")
					(number "5")
				)
				(pin bidirectional line
					(at -30.48 33.02 0)
					(length 3.81)
					(name "IO94RSB1/GAC2")
					(number "6")
				)
				(pin bidirectional line
					(at -30.48 30.48 0)
					(length 3.81)
					(name "IO93RSB1")
					(number "7")
				)
				(pin bidirectional line
					(at -30.48 27.94 0)
					(length 3.81)
					(name "IO92RSB1")
					(number "8")
				)
				(pin bidirectional line
					(at -30.48 25.4 0)
					(length 3.81)
					(name "IO87RSB1/GFB1")
					(number "10")
				)
				(pin bidirectional line
					(at -30.48 22.86 0)
					(length 3.81)
					(name "IO86RSB1/GFB0")
					(number "11")
				)
				(pin bidirectional line
					(at -30.48 20.32 0)
					(length 3.81)
					(name "IO85RSB1/GFA0")
					(number "13")
				)
				(pin bidirectional line
					(at -30.48 17.78 0)
					(length 3.81)
					(name "IO84RSB1/GFA1")
					(number "15")
				)
				(pin bidirectional line
					(at -30.48 15.24 0)
					(length 3.81)
					(name "IO83RSB1/GFA2")
					(number "16")
				)
				(pin bidirectional line
					(at -30.48 12.7 0)
					(length 3.81)
					(name "IO77RSB1/GEC1")
					(number "19")
				)
				(pin bidirectional line
					(at -30.48 10.16 0)
					(length 3.81)
					(name "IO74RSB1/GEB0")
					(number "21")
				)
				(pin bidirectional line
					(at -30.48 7.62 0)
					(length 3.81)
					(name "IO75RSB1/GEB1")
					(number "20")
				)
				(pin bidirectional line
					(at -30.48 5.08 0)
					(length 3.81)
					(name "IO73RSB1/GEA1")
					(number "22")
				)
				(pin bidirectional line
					(at -30.48 2.54 0)
					(length 3.81)
					(name "IO72RSB1/GEA0")
					(number "23")
				)
				(pin bidirectional line
					(at -30.48 0 0)
					(length 3.81)
					(name "IO71RSB1/GEA2")
					(number "26")
				)
				(pin bidirectional line
					(at -30.48 -2.54 0)
					(length 3.81)
					(name "IO70RSB1/GEB2")
					(number "27")
				)
				(pin bidirectional line
					(at -30.48 -5.08 0)
					(length 3.81)
					(name "IO69RSB1/GEC2")
					(number "28")
				)
				(pin bidirectional line
					(at -30.48 -7.62 0)
					(length 3.81)
					(name "IO68RSB1")
					(number "29")
				)
				(pin bidirectional line
					(at -30.48 -10.16 0)
					(length 3.81)
					(name "IO67RSB1")
					(number "30")
				)
				(pin bidirectional line
					(at -30.48 -12.7 0)
					(length 3.81)
					(name "IO66RSB1")
					(number "31")
				)
				(pin bidirectional line
					(at -30.48 -15.24 0)
					(length 3.81)
					(name "IO65RSB1")
					(number "32")
				)
				(pin bidirectional line
					(at -30.48 -17.78 0)
					(length 3.81)
					(name "IO64RSB1")
					(number "33")
				)
				(pin bidirectional line
					(at -30.48 -20.32 0)
					(length 3.81)
					(name "IO63RSB1")
					(number "34")
				)
				(pin bidirectional line
					(at -30.48 -22.86 0)
					(length 3.81)
					(name "IO62RSB1")
					(number "35")
				)
				(pin bidirectional line
					(at -30.48 -25.4 0)
					(length 3.81)
					(name "IO61RSB1")
					(number "36")
				)
				(pin bidirectional line
					(at -30.48 -27.94 0)
					(length 3.81)
					(name "IO60RSB1")
					(number "40")
				)
				(pin bidirectional line
					(at -30.48 -30.48 0)
					(length 3.81)
					(name "IO59RSB1")
					(number "41")
				)
				(pin bidirectional line
					(at -30.48 -33.02 0)
					(length 3.81)
					(name "IO58RSB1")
					(number "42")
				)
				(pin bidirectional line
					(at -30.48 -35.56 0)
					(length 3.81)
					(name "IO57RSB1")
					(number "43")
				)
				(pin bidirectional line
					(at -30.48 -38.1 0)
					(length 3.81)
					(name "IO56RSB1/GDC2")
					(number "44")
				)
				(pin bidirectional line
					(at -30.48 -40.64 0)
					(length 3.81)
					(name "IO55RSB1/GDB2")
					(number "45")
				)
				(pin bidirectional line
					(at -30.48 -43.18 0)
					(length 3.81)
					(name "IO54RSB1/GDA2")
					(number "46")
				)
				(pin bidirectional line
					(at -30.48 -45.72 0)
					(length 3.81)
					(name "IO53RSB1/GAB2")
					(number "4")
				)
				(pin bidirectional line
					(at -30.48 -48.26 0)
					(length 3.81)
					(name "IO52RSB1")
					(number "3")
				)
				(pin bidirectional line
					(at -30.48 -50.8 0)
					(length 3.81)
					(name "IO51RSB1/GAA2")
					(number "2")
				)
				(pin power_in line
					(at -17.78 60.96 270)
					(length 3.81)
					(name "VJTAG")
					(number "56")
				)
				(pin power_in line
					(at -15.24 60.96 270)
					(length 3.81)
					(name "VPUMP")
					(number "52")
				)
				(pin power_in line
					(at -2.54 60.96 270)
					(length 3.81)
					(name "VCCPLF")
					(number "14")
				)
				(pin power_in line
					(at -2.54 -60.96 90)
					(length 3.81)
					(name "VCOMPLF")
					(number "12")
				)
				(pin power_in line
					(at 0 60.96 270)
					(length 3.81)
					(name "VCC")
					(number "17")
				)
				(pin passive line
					(at 0 60.96 270)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "37")
				)
				(pin passive line
					(at 0 60.96 270)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "68")
				)
				(pin passive line
					(at 0 60.96 270)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "89")
				)
				(pin power_in line
					(at 0 -60.96 90)
					(length 3.81)
					(name "GND")
					(number "1")
				)
				(pin passive line
					(at 0 -60.96 90)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "38")
				)
				(pin passive line
					(at 0 -60.96 90)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "51")
				)
				(pin passive line
					(at 0 -60.96 90)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "67")
				)
				(pin passive line
					(at 0 -60.96 90)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "88")
				)
				(pin passive line
					(at 0 -60.96 90)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "9")
				)
				(pin power_in line
					(at 2.54 -60.96 90)
					(length 3.81)
					(name "GNDQ")
					(number "25")
				)
				(pin passive line
					(at 2.54 -60.96 90)
					(length 3.81)
					(hide yes)
					(name "GNDQ")
					(number "75")
				)
				(pin power_in line
					(at 5.08 60.96 270)
					(length 3.81)
					(name "VCCIB1")
					(number "18")
				)
				(pin passive line
					(at 5.08 60.96 270)
					(length 3.81)
					(hide yes)
					(name "VCCIB1")
					(number "39")
				)
				(pin power_in line
					(at 7.62 60.96 270)
					(length 3.81)
					(name "VMV1")
					(number "24")
				)
				(pin passive line
					(at 7.62 60.96 270)
					(length 3.81)
					(hide yes)
					(name "VMV1")
					(number "50")
				)
				(pin power_in line
					(at 12.7 60.96 270)
					(length 3.81)
					(name "VCCIB0")
					(number "66")
				)
				(pin passive line
					(at 12.7 60.96 270)
					(length 3.81)
					(hide yes)
					(name "VCCIB0")
					(number "87")
				)
				(pin power_in line
					(at 15.24 60.96 270)
					(length 3.81)
					(name "VMV0")
					(number "74")
				)
				(pin no_connect line
					(at 26.67 45.72 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "53")
				)
				(pin bidirectional line
					(at 30.48 38.1 180)
					(length 3.81)
					(name "IO00RSB0")
					(number "100")
				)
				(pin no_connect line
					(at 30.48 35.56 180)
					(length 3.81)
					(name "IO01RSB0")
					(number "99")
				)
				(pin no_connect line
					(at 30.48 33.02 180)
					(length 3.81)
					(name "GAA0/IO02RSB0")
					(number "98")
				)
				(pin no_connect line
					(at 30.48 30.48 180)
					(length 3.81)
					(name "GAA1/IO03RSB0")
					(number "97")
				)
				(pin no_connect line
					(at 30.48 27.94 180)
					(length 3.81)
					(name "GAB0/IO04RSB0")
					(number "96")
				)
				(pin no_connect line
					(at 30.48 25.4 180)
					(length 3.81)
					(name "GAB1/IO05RSB0")
					(number "95")
				)
				(pin no_connect line
					(at 30.48 22.86 180)
					(length 3.81)
					(name "GAC1/IO06RSB0")
					(number "94")
				)
				(pin no_connect line
					(at 30.48 20.32 180)
					(length 3.81)
					(name "GAC1/IO07RSB0")
					(number "93")
				)
				(pin no_connect line
					(at 30.48 27.94 180)
					(length 3.81)
					(name "IO08RSB0")
					(number "92")
				)
				(pin no_connect line
					(at 30.48 25.4 180)
					(length 3.81)
					(name "IO09RSB0")
					(number "91")
				)
				(pin no_connect line
					(at 30.48 22.86 180)
					(length 3.81)
					(name "IO10RSB0")
					(number "90")
				)
				(pin no_connect line
					(at 30.48 20.32 180)
					(length 3.81)
					(name "IO11RSB0")
					(number "86")
				)
				(pin no_connect line
					(at 30.48 20.32 180)
					(length 3.81)
					(name "IO13RSB0")
					(number "85")
				)
				(pin bidirectional line
					(at 30.48 5.08 180)
					(length 3.81)
					(name "IO15RSB0")
					(number "84")
				)
				(pin bidirectional line
					(at 30.48 2.54 180)
					(length 3.81)
					(name "IO17RSB0")
					(number "83")
				)
				(pin bidirectional line
					(at 30.48 0 180)
					(length 3.81)
					(name "IO18RSB0")
					(number "82")
				)
				(pin bidirectional line
					(at 30.48 -2.54 180)
					(length 3.81)
					(name "GBC0/IO19RSB0")
					(number "81")
				)
				(pin bidirectional line
					(at 30.48 -5.08 180)
					(length 3.81)
					(name "GBC1/IO20RSB0")
					(number "80")
				)
				(pin bidirectional line
					(at 30.48 -7.62 180)
					(length 3.81)
					(name "GBB0/IO21RSB0")
					(number "79")
				)
				(pin bidirectional line
					(at 30.48 -10.16 180)
					(length 3.81)
					(name "GBB1/IO22RSB0")
					(number "78")
				)
				(pin bidirectional line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "GBA0/IO23RSB0")
					(number "77")
				)
				(pin bidirectional line
					(at 30.48 -15.24 180)
					(length 3.81)
					(name "GBA1/IO24RSB0")
					(number "76")
				)
				(pin bidirectional line
					(at 30.48 -17.78 180)
					(length 3.81)
					(name "GBA2/IO25RSB0")
					(number "73")
				)
				(pin bidirectional line
					(at 30.48 -20.32 180)
					(length 3.81)
					(name "IO26RSB0")
					(number "72")
				)
				(pin bidirectional line
					(at 30.48 -22.86 180)
					(length 3.81)
					(name "GBB2/IO27RSB0")
					(number "71")
				)
				(pin bidirectional line
					(at 30.48 -25.4 180)
					(length 3.81)
					(name "GBC2/IO29RSB0")
					(number "70")
				)
				(pin bidirectional line
					(at 30.48 -27.94 180)
					(length 3.81)
					(name "IO31RSB0")
					(number "69")
				)
				(pin bidirectional line
					(at 30.48 -30.48 180)
					(length 3.81)
					(name "GCC1/IO35RSB0")
					(number "65")
				)
				(pin bidirectional line
					(at 30.48 -33.02 180)
					(length 3.81)
					(name "GCC0/IO36RSB0")
					(number "64")
				)
				(pin bidirectional line
					(at 30.48 -35.56 180)
					(length 3.81)
					(name "GCA1/IO39RSB0")
					(number "63")
				)
				(pin bidirectional line
					(at 30.48 -38.1 180)
					(length 3.81)
					(name "GCA0/IO40RSB0")
					(number "62")
				)
				(pin bidirectional line
					(at 30.48 -40.64 180)
					(length 3.81)
					(name "GCB2/IO42RSB0")
					(number "61")
				)
				(pin bidirectional line
					(at 30.48 -43.18 180)
					(length 3.81)
					(name "GCC2/IO43RSB0")
					(number "60")
				)
				(pin bidirectional line
					(at 30.48 -45.72 180)
					(length 3.81)
					(name "GDC1/IO45RSB0")
					(number "59")
				)
				(pin bidirectional line
					(at 30.48 -48.26 180)
					(length 3.81)
					(name "GDC0/IO46RSB0")
					(number "58")
				)
				(pin bidirectional line
					(at 30.48 -50.8 180)
					(length 3.81)
					(name "GDA1/IO49RSB0")
					(number "57")
				)
			)
			(embedded_fonts no)
		)
	)
	(no_connect
		(at 179.07 143.51)
	)
	(no_connect
		(at 179.07 95.25)
	)
	(no_connect
		(at 146.05 31.75)
	)
	(no_connect
		(at 118.11 57.15)
	)
	(no_connect
		(at 179.07 107.95)
	)
	(no_connect
		(at 133.35 31.75)
	)
	(no_connect
		(at 118.11 85.09)
	)
	(no_connect
		(at 153.67 31.75)
	)
	(no_connect
		(at 148.59 31.75)
	)
	(no_connect
		(at 179.07 110.49)
	)
	(no_connect
		(at 118.11 62.23)
	)
	(no_connect
		(at 118.11 143.51)
	)
	(no_connect
		(at 118.11 46.99)
	)
	(no_connect
		(at 118.11 105.41)
	)
	(no_connect
		(at 179.07 102.87)
	)
	(no_connect
		(at 179.07 100.33)
	)
	(no_connect
		(at 163.83 31.75)
	)
	(no_connect
		(at 118.11 125.73)
	)
	(no_connect
		(at 130.81 31.75)
	)
	(no_connect
		(at 179.07 118.11)
	)
	(no_connect
		(at 118.11 87.63)
	)
	(no_connect
		(at 118.11 138.43)
	)
	(no_connect
		(at 118.11 82.55)
	)
	(no_connect
		(at 151.13 153.67)
	)
	(no_connect
		(at 179.07 133.35)
	)
	(no_connect
		(at 161.29 31.75)
	)
	(no_connect
		(at 179.07 125.73)
	)
	(no_connect
		(at 118.11 135.89)
	)
	(no_connect
		(at 179.07 140.97)
	)
	(no_connect
		(at 118.11 102.87)
	)
	(no_connect
		(at 118.11 118.11)
	)
	(no_connect
		(at 118.11 115.57)
	)
	(no_connect
		(at 179.07 97.79)
	)
	(no_connect
		(at 118.11 107.95)
	)
	(no_connect
		(at 148.59 153.67)
	)
	(no_connect
		(at 118.11 90.17)
	)
	(no_connect
		(at 179.07 130.81)
	)
	(no_connect
		(at 146.05 153.67)
	)
	(no_connect
		(at 118.11 95.25)
	)
	(no_connect
		(at 118.11 130.81)
	)
	(no_connect
		(at 179.07 128.27)
	)
	(no_connect
		(at 118.11 140.97)
	)
	(no_connect
		(at 179.07 135.89)
	)
	(no_connect
		(at 118.11 97.79)
	)
	(no_connect
		(at 118.11 69.85)
	)
	(no_connect
		(at 179.07 138.43)
	)
	(no_connect
		(at 179.07 115.57)
	)
	(no_connect
		(at 118.11 67.31)
	)
	(no_connect
		(at 118.11 113.03)
	)
	(no_connect
		(at 118.11 133.35)
	)
	(no_connect
		(at 118.11 52.07)
	)
	(no_connect
		(at 179.07 54.61)
	)
	(no_connect
		(at 118.11 59.69)
	)
	(no_connect
		(at 118.11 92.71)
	)
	(no_connect
		(at 118.11 44.45)
	)
	(no_connect
		(at 179.07 92.71)
	)
	(no_connect
		(at 118.11 72.39)
	)
	(no_connect
		(at 118.11 64.77)
	)
	(no_connect
		(at 118.11 80.01)
	)
	(no_connect
		(at 179.07 105.41)
	)
	(no_connect
		(at 179.07 113.03)
	)
	(no_connect
		(at 179.07 120.65)
	)
	(no_connect
		(at 118.11 77.47)
	)
	(no_connect
		(at 118.11 123.19)
	)
	(no_connect
		(at 179.07 87.63)
	)
	(no_connect
		(at 118.11 110.49)
	)
	(no_connect
		(at 179.07 123.19)
	)
	(no_connect
		(at 118.11 41.91)
	)
	(no_connect
		(at 118.11 128.27)
	)
	(no_connect
		(at 118.11 100.33)
	)
	(no_connect
		(at 179.07 90.17)
	)
	(no_connect
		(at 118.11 49.53)
	)
	(no_connect
		(at 118.11 120.65)
	)
	(no_connect
		(at 156.21 31.75)
	)
	(no_connect
		(at 118.11 74.93)
	)
	(symbol
		(lib_id "FPGA_Microsemi:A3P060-xVQx100")
		(at 148.59 92.71 0)
		(unit 1)
		(convert 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 153.2733 152.4 0)
			(show_name no)
			(do_not_autoplace no)
		)
		(property "Value" "A3P060-xVQx100"
			(at 153.2733 154.94 0)
			(show_name no)
			(do_not_autoplace no)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 176.784 41.91 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/268/ProASIC_c2_ae3_Flash_Family_FPGAs_with_Optimal_Sof-3082432.pdf"
			(at 148.59 92.71 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
		)
		(property "Description" "ProASIC3 Flash Family FPGAs, 512 MCLB / macrocells, TQFP-100 (VQ100)"
			(at 148.59 92.71 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
		)
		(pin "86")
		(pin "53")
		(pin "87")
		(pin "40")
		(pin "48")
		(pin "42")
		(pin "50")
		(pin "96")
		(pin "14")
		(pin "2")
		(pin "55")
		(pin "6")
		(pin "41")
		(pin "45")
		(pin "5")
		(pin "7")
		(pin "47")
		(pin "3")
		(pin "36")
		(pin "46")
		(pin "28")
		(pin "49")
		(pin "29")
		(pin "9")
		(pin "56")
		(pin "34")
		(pin "52")
		(pin "10")
		(pin "100")
		(pin "84")
		(pin "98")
		(pin "85")
		(pin "44")
		(pin "35")
		(pin "11")
		(pin "69")
		(pin "38")
		(pin "8")
		(pin "15")
		(pin "4")
		(pin "83")
		(pin "43")
		(pin "93")
		(pin "65")
		(pin "63")
		(pin "31")
		(pin "30")
		(pin "54")
		(pin "99")
		(pin "1")
		(pin "80")
		(pin "64")
		(pin "24")
		(pin "66")
		(pin "51")
		(pin "88")
		(pin "39")
		(pin "73")
		(pin "77")
		(pin "26")
		(pin "18")
		(pin "75")
		(pin "71")
		(pin "76")
		(pin "25")
		(pin "70")
		(pin "27")
		(pin "94")
		(pin "68")
		(pin "78")
		(pin "37")
		(pin "33")
		(pin "12")
		(pin "91")
		(pin "95")
		(pin "74")
		(pin "90")
		(pin "22")
		(pin "79")
		(pin "67")
		(pin "57")
		(pin "62")
		(pin "58")
		(pin "97")
		(pin "13")
		(pin "81")
		(pin "21")
		(pin "89")
		(pin "32")
		(pin "19")
		(pin "16")
		(pin "60")
		(pin "59")
		(pin "82")
		(pin "20")
		(pin "17")
		(pin "72")
		(pin "61")
		(pin "92")
		(pin "23")
		(instances
			(project ""
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
	(embedded_fonts no)
)
