(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_000010fc_ffffffff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "A")
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 125.2 90.9)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(pintype "passive+no_connect")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "D5"
		(layer "F.Cu")
		(at 105.85 65.35)
		(descr "Diode 5 pas")
		(tags "DIODE DEV")
		(property "Reference" "D1"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1N4007"
			(at -0.254 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -6.35 0)
			(size 2.032 2.032)
			(drill 1.143)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 1 "A")
		)
		(pad "2" thru_hole rect
			(at 6.35 0)
			(size 2.032 2.032)
			(drill 1.143)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(solder_mask_margin 0.3)
			(solder_paste_margin 0.3)
			(solder_paste_margin_ratio 0.23)
			(clearance 1)
			(zone_connect 1)
			(thermal_bridge_width 20)
			(thermal_bridge_angle 47)
			(thermal_gap 10)
			(teardrops
				(best_length_ratio 0.45)
				(max_length 2)
				(best_width_ratio 0.95)
				(max_width 3)
				(curved_edges no)
				(filter_ratio 0.8)
				(enabled yes)
				(allow_two_segments no)
				(prefer_zone_connections no)
			)
		)
		(embedded_fonts no)
		(model "discret/diode.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 0.5 0.5 0.5)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "bornier2"
		(layer "F.Cu")
		(at 88.3 68.9 -90)
		(descr "Bornier d'alimentation 2 pins")
		(tags "DEV")
		(property "Reference" "P2"
			(at 0 -5.08 270)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_2"
			(at 0 5.08 270)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CustomField" "CustomValue"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -2.54 0 270)
			(size 2.54 2.54)
			(drill 1.524)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 1 "A")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 2.54 2.54)
			(drill 1.524)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
		(model "device/bornier_2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_poly
		(pts
			(xy 105.25 114.4) (xy 105.25 136.8) (xy 128.7 145.65) (xy 143.05 131.35) (xy 121.65 127.7) (xy 122.15 109.95)
		)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_poly
		(pts
			(xy 215.5 49.5) (xy 106.25 29.4) (xy 35.65 100.85) (xy 76.55 170.7) (xy 187.85 168.1) (xy 258.75 96.9)
			(xy 222 79.2)
		)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 197.75 63.3)
		(end 199.05 65.4)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 224.6 97.7)
		(end 228.25 99.55)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "Text!"
		(at 120.45 49.35 0)
		(layer "B.Fab")
	)
	(gr_text_box "Box\no\nCharacters"
		(start 116.9 49.9)
		(end 127.3 55.45)
		(margins 1.0025 1.0025 1.0025 1.0025)
		(layer "F.SilkS")
		(border yes)
	)
	(dimension
		(type aligned)
		(layer "F.SilkS")
		(pts
			(xy 119.75 76.25) (xy 119.75 82.5)
		)
		(height -5.5)
		(format
			(prefix "")
			(suffix "")
			(units 1)
			(units_format 1)
			(precision 1)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
		)
		(gr_text "246.1 mils"
			(at 126 79 0)
			(layer "F.SilkS")
		)
	)
	(dimension
		(type aligned)
		(layer "F.SilkS")
		(pts
			(xy 119.75 76.25) (xy 93.25 78.75)
		)
		(height 2.5229)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "26.6177 mm"
			(at 106.159728 75 5.38931176)
			(layer "F.SilkS")
		)
	)
	(dimension
		(type leader)
		(layer "F.SilkS")
		(pts
			(xy 109.5 89) (xy 113.25 85.75)
		)
		(format
			(prefix "")
			(suffix "")
			(units 0)
			(units_format 0)
			(precision 4)
			(override_value "Leader")
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(text_frame 1)
			(extension_offset 0.5)
		)
		(gr_text "Leader"
			(at 119 85.75 0)
			(layer "F.SilkS")
		)
	)
	(dimension
		(type center)
		(layer "F.SilkS")
		(pts
			(xy 106.5 90.75) (xy 106.5 87.25)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
	)
	(dimension
		(type radial)
		(layer "F.SilkS")
		(pts
			(xy 115 93.5) (xy 113.25 94.75)
		)
		(leader_length 3.81)
		(format
			(prefix "R ")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "R 2.1506 mm"
			(at 97.449675 96.964518 0)
			(layer "F.SilkS")
		)
	)
	(dimension
		(type orthogonal)
		(layer "F.Cu")
		(pts
			(xy 93.25 78.75) (xy 119.75 76.25)
		)
		(height 3.75)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "26.5000 mm"
			(at 106.5 80.7 0)
			(layer "F.Cu")
		)
	)
	(zone
		(net 0)
		(net_name "")
		(locked yes)
		(layers "F.Cu" "B.Cu")
		(name "MyKeepout")
		(hatch full 0.65)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 81 107.15) (xy 88.35 111.05) (xy 93 100.4) (xy 82.85 91.75) (xy 76.1 98.9)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch edge 1)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 71 106.5) (xy 63.7 111.45) (xy 53.05 106.8) (xy 56.95 99.45) (xy 65.2 94.55)
			)
		)
		(polygon
			(pts
				(xy 62.45 100.8) (xy 62.6 102.35) (xy 65.4 103.05) (xy 65.75 101.35) (xy 64.05 100.15)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch none 0.65)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 67.85 85.1) (xy 63.95 92.45) (xy 74.6 97.1) (xy 83.25 86.95) (xy 76.1 80.2)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.762)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 232.833 116.922) (xy 232.833 38.436) (xy 133.9 38.436) (xy 133.9 116.922)
			)
		)
	)
	(embedded_fonts no)
)
