(kicad_pcb (version 20230620) (generator pcbnew)
  (general
    (thickness 1.6002)
  )
  (paper "A4")
  (title_block
    (title "Actionneur_piezo")
  )
  (layers
    (0 "F.Cu" power "Composant")
    (31 "B.Cu" signal "Cuivre")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
  )
  (setup
    (pad_to_mask_clearance 0.254)
    (pcbplotparams
      (layerselection 0x00000f0_80000001)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (pdf_front_fp_property_popups true)
      (pdf_back_fp_property_popups true)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+12V")
  (net 2 "-VAA")
  (net 3 "/12Vext")
  (net 4 "/ampli_h1")
  (net 5 "/ampli_h2")
  (net 6 "/ampli_h3")
  (net 7 "/ampli_h4")
  (net 8 "/ampli_h5")
  (net 9 "/ampli_h6")
  (net 10 "/ampli_h7")
  (net 11 "/ampli_h8")
  (net 12 "GND")
  (net 13 "HT")
  (net 14 "N-000005")
  (net 15 "N-000010")
  (net 16 "N-000011")
  (net 17 "N-000012")
  (net 18 "N-000013")
  (net 19 "N-000014")
  (net 20 "N-000015")
  (net 21 "N-000016")
  (net 22 "N-000017")
  (net 23 "N-000018")
  (net 24 "N-000019")
  (net 25 "N-000020")
  (net 26 "N-000021")
  (net 27 "N-000022")
  (net 28 "N-000023")
  (net 29 "N-000024")
  (net 30 "N-000025")
  (net 31 "N-000026")
  (net 32 "N-000027")
  (net 33 "N-000032")
  (net 34 "N-000033")
  (net 35 "N-000034")
  (net 36 "N-000035")
  (net 37 "N-000036")
  (net 38 "N-000037")
  (net 39 "N-000038")
  (net 40 "N-000039")
  (net 41 "N-000040")
  (net 42 "N-000041")
  (net 43 "N-000042")
  (net 44 "N-000043")
  (net 45 "N-000044")
  (net 46 "N-000045")
  (net 47 "N-000046")
  (net 48 "N-000047")
  (net 49 "N-000048")
  (net 50 "VCC")
  (footprint "bornier2" (layer "F.Cu")
    (at 95.885 59.436 -90)
    (descr "Bornier d'alimentation 2 pins")
    (tags "DEV")
    (property "Reference" "P1" (at 0 -5.08 -90) (layer "F.SilkS"))
    (property "Value" "CONN_2" (at 0 5.08 -90) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at -2.54 0 270) (size 2.54 2.54) (drill 1.524) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 13 "HT")
    )
    (pad "2" thru_hole circle (at 2.54 0 270) (size 2.54 2.54) (drill 1.524) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "device/bornier_2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "bornier2" (layer "F.Cu")
    (at 182.245 120.396 90)
    (descr "Bornier d'alimentation 2 pins")
    (tags "DEV")
    (property "Reference" "P3" (at 0 -5.08 90) (layer "F.SilkS"))
    (property "Value" "CONN_2" (at 0 5.08 90) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at -2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 6 "/ampli_h3")
    )
    (pad "2" thru_hole circle (at 2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "device/bornier_2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "C2" (layer "F.Cu")
    (at 140.589 104.14)
    (descr "Condensateur = 2 pas")
    (tags "C")
    (property "Reference" "C8" (at 0 0 0) (layer "F.SilkS"))
    (property "Value" "820pF" (at 0 0 0) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 37 "N-000036")
    )
    (pad "2" thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "C2" (layer "F.Cu")
    (at 116.205 112.776)
    (descr "Condensateur = 2 pas")
    (tags "C")
    (property "Reference" "C4" (at 0 0 0) (layer "F.SilkS"))
    (property "Value" "4,7nF" (at 0 0 0) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 29 "N-000024")
    )
    (pad "2" thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CP6" (layer "F.Cu")
    (at 133.985 60.706 180)
    (descr "Condensateur polarise")
    (tags "CP")
    (property "Reference" "C2" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "47uF/20V" (at 0.635 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at -7.62 0 180) (size 2.159 2.159) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 1 "+12V")
    )
    (pad "2" thru_hole circle (at 7.62 0 180) (size 2.159 2.159) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "discret/c_pol.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.6 0.6 0.6))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CP8" (layer "F.Cu")
    (at 112.395 60.706 180)
    (descr "Condensateur polarise")
    (tags "CP")
    (property "Reference" "C9" (at 1.27 1.27 180) (layer "F.SilkS"))
    (property "Value" "47uF/63V" (at 1.27 -1.27 180) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at -10.16 0 180) (size 1.778 1.778) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 13 "HT")
    )
    (pad "2" thru_hole circle (at 10.16 0 180) (size 1.778 1.778) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "discret/c_pol.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "C2" (layer "F.Cu")
    (at 140.716 130.048)
    (descr "Condensateur = 2 pas")
    (tags "C")
    (property "Reference" "C5" (at 0 0 0) (layer "F.SilkS"))
    (property "Value" "820pF" (at 0 0 0) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 20 "N-000015")
    )
    (pad "2" thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "C2" (layer "F.Cu")
    (at 116.205 110.236 180)
    (descr "Condensateur = 2 pas")
    (tags "C")
    (property "Reference" "C3" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "15nF" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 4 "/ampli_h1")
    )
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 18 "N-000013")
    )
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "C2" (layer "F.Cu")
    (at 116.205 81.026 180)
    (descr "Condensateur = 2 pas")
    (tags "C")
    (property "Reference" "C6" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "15nF" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 5 "/ampli_h2")
    )
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 35 "N-000034")
    )
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CP6" (layer "F.Cu")
    (at 109.855 74.676 180)
    (descr "Condensateur polarise")
    (tags "CP")
    (property "Reference" "C1" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "47uF" (at 0.635 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at -7.62 0 180) (size 2.159 2.159) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 50 "VCC")
    )
    (pad "2" thru_hole circle (at 7.62 0 180) (size 2.159 2.159) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "discret/c_pol.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.6 0.6 0.6))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "C2" (layer "F.Cu")
    (at 116.205 84.836)
    (descr "Condensateur = 2 pas")
    (tags "C")
    (property "Reference" "C7" (at 0 0 0) (layer "F.SilkS"))
    (property "Value" "4,7nF" (at 0 0 0) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 46 "N-000045")
    )
    (pad "2" thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "D3" (layer "F.Cu")
    (at 128.905 82.296)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (property "Reference" "D6" (at 0 0 0) (layer "F.SilkS"))
    (property "Value" "1N4148" (at 0 0 0) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 34 "N-000033")
    )
    (pad "2" thru_hole rect (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 41 "N-000040")
    )
    (model "discret/diode.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "D3" (layer "F.Cu")
    (at 140.97 119.761 -90)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (property "Reference" "D4" (at 0 0 -90) (layer "F.SilkS"))
    (property "Value" "1N4148" (at 0 0 -90) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 28 "N-000023")
    )
    (pad "2" thru_hole rect (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 30 "N-000025")
    )
    (model "discret/diode.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "D3" (layer "F.Cu")
    (at 131.445 108.966 180)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (property "Reference" "D3" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "1N4148" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 17 "N-000012")
    )
    (pad "2" thru_hole rect (at 3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 24 "N-000019")
    )
    (model "discret/diode.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "D3" (layer "F.Cu")
    (at 131.445 106.426 180)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (property "Reference" "D2" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "1N4148" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 13 "HT")
    )
    (pad "2" thru_hole rect (at 3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 17 "N-000012")
    )
    (model "discret/diode.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "D5" (layer "F.Cu")
    (at 109.855 68.326)
    (descr "Diode 5 pas")
    (tags "DIODE DEV")
    (property "Reference" "D1" (at 0 0 0) (layer "F.SilkS"))
    (property "Value" "1N4007" (at -0.254 0 0) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -6.35 0) (size 2.032 2.032) (drill 1.143) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 3 "/12Vext")
    )
    (pad "2" thru_hole rect (at 6.35 0) (size 2.032 2.032) (drill 1.143) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 1 "+12V")
    )
    (model "discret/diode.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "D3" (layer "F.Cu")
    (at 141.605 93.726 -90)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (property "Reference" "D7" (at 0 0 -90) (layer "F.SilkS"))
    (property "Value" "1N4148" (at 0 0 -90) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 45 "N-000044")
    )
    (pad "2" thru_hole rect (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 47 "N-000046")
    )
    (model "discret/diode.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "D3" (layer "F.Cu")
    (at 128.905 79.756 180)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (property "Reference" "D5" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "1N4148" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 13 "HT")
    )
    (pad "2" thru_hole rect (at 3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 34 "N-000033")
    )
    (model "discret/diode.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LM78LXX" (layer "F.Cu")
    (at 125.095 69.596 90)
    (descr "Regulateur TO92 serie LM78Lxx")
    (tags "TR TO92")
    (property "Reference" "U2" (at -1.905 3.81 90) (layer "F.SilkS"))
    (property "Value" "78L05" (at -1.27 -5.08 90) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "GND" thru_hole rect (at -1.27 -1.397 90) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (pad "VI" thru_hole circle (at 1.27 -1.27 90) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 1 "+12V")
    )
    (pad "VO" thru_hole circle (at -1.27 1.27 90) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 50 "VCC")
    )
    (model "discret/to98.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 156.21 120.396 -90)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R12" (at 0 0 -90) (layer "F.SilkS"))
    (property "Value" "220K" (at 0 0 -90) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 270) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 10 "/ampli_h7")
    )
    (pad "2" thru_hole circle (at 3.81 0 270) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 22 "N-000017")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 106.045 84.836)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R17" (at 0 0 0) (layer "F.SilkS"))
    (property "Value" "22K" (at 0 0 0) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 46 "N-000045")
    )
    (pad "2" thru_hole circle (at 3.81 0) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 35 "N-000034")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 142.875 108.966 180)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R3" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "470" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 13 "HT")
    )
    (pad "2" thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 32 "N-000027")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 121.793 101.346 180)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R18" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "1K" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 42 "N-000041")
    )
    (pad "2" thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 169.545 119.126 180)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R5" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "47" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 6 "/ampli_h3")
    )
    (pad "2" thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 21 "N-000016")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 122.555 128.016 180)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R8" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "1K" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 25 "N-000020")
    )
    (pad "2" thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 141.605 86.106 180)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R13" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "470" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 13 "HT")
    )
    (pad "2" thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 49 "N-000048")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 156.845 93.726 -90)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R22" (at 0 0 -90) (layer "F.SilkS"))
    (property "Value" "220K" (at 0 0 -90) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 270) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 11 "/ampli_h8")
    )
    (pad "2" thru_hole circle (at 3.81 0 270) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 39 "N-000038")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 102.87 122.936 90)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R11" (at 0 0 90) (layer "F.SilkS"))
    (property "Value" "4,7K" (at 0 0 90) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 90) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 23 "N-000018")
    )
    (pad "2" thru_hole circle (at 3.81 0 90) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 106.045 110.236 180)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R6" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "22K" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 18 "N-000013")
    )
    (pad "2" thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 19 "N-000014")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 102.235 98.806 90)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R21" (at 0 0 90) (layer "F.SilkS"))
    (property "Value" "4,7K" (at 0 0 90) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 90) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 40 "N-000039")
    )
    (pad "2" thru_hole circle (at 3.81 0 90) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 106.045 82.296 180)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R16" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "22K" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 35 "N-000034")
    )
    (pad "2" thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 36 "N-000035")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 122.301 94.996 180)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R19" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "1K" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 33 "N-000032")
    )
    (pad "2" thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 43 "N-000042")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 140.589 127.381 180)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R10" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "5,6K" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 30 "N-000025")
    )
    (pad "2" thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 20 "N-000015")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 137.795 101.346 180)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R20" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "5,6K" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 47 "N-000046")
    )
    (pad "2" thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 37 "N-000036")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 122.555 119.126 -90)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R4" (at 0 0 -90) (layer "F.SilkS"))
    (property "Value" "220K" (at 0 0 -90) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 270) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 24 "N-000019")
    )
    (pad "2" thru_hole circle (at 3.81 0 270) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 106.045 112.776 180)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R7" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "22K" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 29 "N-000024")
    )
    (pad "2" thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 18 "N-000013")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TO92-CBE" (layer "F.Cu")
    (at 149.225 124.206 180)
    (descr "Transistor TO92 brochage type BC237")
    (tags "TR TO92")
    (property "Reference" "Q3" (at 0.762 0.635 180) (layer "F.SilkS"))
    (property "Value" "MPAS92" (at 0.254 -3.048 180) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "B" thru_hole circle (at -1.27 -1.27 180) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 30 "N-000025")
    )
    (pad "C" thru_hole circle (at 1.27 -1.27 180) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (pad "E" thru_hole rect (at -1.27 1.27 180) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 22 "N-000017")
    )
    (model "discret/to98.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TO92-CBE" (layer "F.Cu")
    (at 131.445 88.646)
    (descr "Transistor TO92 brochage type BC237")
    (tags "TR TO92")
    (property "Reference" "Q5" (at 0.762 0.635 0) (layer "F.SilkS"))
    (property "Value" "MPAS92" (at 0.254 -3.048 0) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "B" thru_hole circle (at -1.27 -1.27) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 41 "N-000040")
    )
    (pad "C" thru_hole circle (at 1.27 -1.27) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 48 "N-000047")
    )
    (pad "E" thru_hole rect (at -1.27 1.27) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 49 "N-000048")
    )
    (model "discret/to98.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TO92-CBE" (layer "F.Cu")
    (at 149.225 99.441 180)
    (descr "Transistor TO92 brochage type BC237")
    (tags "TR TO92")
    (property "Reference" "Q7" (at 0.762 0.635 180) (layer "F.SilkS"))
    (property "Value" "MPAS92" (at 0.254 -3.048 180) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "B" thru_hole circle (at -1.27 -1.27 180) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 47 "N-000046")
    )
    (pad "C" thru_hole circle (at 1.27 -1.27 180) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (pad "E" thru_hole rect (at -1.27 1.27 180) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 39 "N-000038")
    )
    (model "discret/to98.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TO92-CBE" (layer "F.Cu")
    (at 150.495 89.916)
    (descr "Transistor TO92 brochage type BC237")
    (tags "TR TO92")
    (property "Reference" "Q6" (at 0.762 0.635 0) (layer "F.SilkS"))
    (property "Value" "MPAS42" (at 0.254 -3.048 0) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "B" thru_hole circle (at -1.27 -1.27) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 48 "N-000047")
    )
    (pad "C" thru_hole circle (at 1.27 -1.27) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 13 "HT")
    )
    (pad "E" thru_hole rect (at -1.27 1.27) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 38 "N-000037")
    )
    (model "discret/to98.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TO92-CBE" (layer "F.Cu")
    (at 131.445 115.316)
    (descr "Transistor TO92 brochage type BC237")
    (tags "TR TO92")
    (property "Reference" "Q1" (at 0.762 0.635 0) (layer "F.SilkS"))
    (property "Value" "MPAS92" (at 0.254 -3.048 0) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "B" thru_hole circle (at -1.27 -1.27) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 24 "N-000019")
    )
    (pad "C" thru_hole circle (at 1.27 -1.27) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 31 "N-000026")
    )
    (pad "E" thru_hole rect (at -1.27 1.27) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 32 "N-000027")
    )
    (model "discret/to98.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TO92-CBE" (layer "F.Cu")
    (at 150.495 116.586)
    (descr "Transistor TO92 brochage type BC237")
    (tags "TR TO92")
    (property "Reference" "Q2" (at 0.762 0.635 0) (layer "F.SilkS"))
    (property "Value" "MPAS42" (at 0.254 -3.048 0) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "B" thru_hole circle (at -1.27 -1.27) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 31 "N-000026")
    )
    (pad "C" thru_hole circle (at 1.27 -1.27) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 13 "HT")
    )
    (pad "E" thru_hole rect (at -1.27 1.27) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 21 "N-000016")
    )
    (model "discret/to98.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TO92-CBE" (layer "F.Cu")
    (at 132.715 125.476)
    (descr "Transistor TO92 brochage type BC237")
    (tags "TR TO92")
    (property "Reference" "Q4" (at 0.762 0.635 0) (layer "F.SilkS"))
    (property "Value" "MPAS42" (at 0.254 -3.048 0) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "B" thru_hole circle (at -1.27 -1.27) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 25 "N-000020")
    )
    (pad "C" thru_hole circle (at 1.27 -1.27) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 30 "N-000025")
    )
    (pad "E" thru_hole rect (at -1.27 1.27) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 16 "N-000011")
    )
    (model "discret/to98.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TO92-CBE" (layer "F.Cu")
    (at 131.445 98.806)
    (descr "Transistor TO92 brochage type BC237")
    (tags "TR TO92")
    (property "Reference" "Q8" (at 0.762 0.635 0) (layer "F.SilkS"))
    (property "Value" "MPAS42" (at 0.254 -3.048 0) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "B" thru_hole circle (at -1.27 -1.27) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 42 "N-000041")
    )
    (pad "C" thru_hole circle (at 1.27 -1.27) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 47 "N-000046")
    )
    (pad "E" thru_hole rect (at -1.27 1.27) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 33 "N-000032")
    )
    (model "discret/to98.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "bornier2" (layer "F.Cu")
    (at 95.885 72.136 -90)
    (descr "Bornier d'alimentation 2 pins")
    (tags "DEV")
    (property "Reference" "P2" (at 0 -5.08 -90) (layer "F.SilkS"))
    (property "Value" "CONN_2" (at 0 5.08 -90) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at -2.54 0 270) (size 2.54 2.54) (drill 1.524) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 3 "/12Vext")
    )
    (pad "2" thru_hole circle (at 2.54 0 270) (size 2.54 2.54) (drill 1.524) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "device/bornier_2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DIP-8__300_ELL" (layer "F.Cu")
    (at 149.225 68.326)
    (descr "8 pins DIL package, elliptical pads")
    (tags "DIL")
    (property "Reference" "U1" (at -6.35 0 90) (layer "F.SilkS"))
    (property "Value" "ICL7660" (at 0 0 0) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at -3.81 3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "2" thru_hole oval (at -1.27 3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 15 "N-000010")
    )
    (pad "3" thru_hole oval (at 1.27 3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (pad "4" thru_hole oval (at 3.81 3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 14 "N-000005")
    )
    (pad "5" thru_hole oval (at 3.81 -3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 2 "-VAA")
    )
    (pad "6" thru_hole oval (at 1.27 -3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "7" thru_hole oval (at -1.27 -3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "8" thru_hole oval (at -3.81 -3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 50 "VCC")
    )
    (model "dil/dil_8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DIP-8__300_ELL" (layer "F.Cu")
    (at 111.125 92.456)
    (descr "8 pins DIL package, elliptical pads")
    (tags "DIL")
    (property "Reference" "U4" (at -6.35 0 90) (layer "F.SilkS"))
    (property "Value" "LM358N" (at 0 0 0) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at -3.81 3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 43 "N-000042")
    )
    (pad "2" thru_hole oval (at -1.27 3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 44 "N-000043")
    )
    (pad "3" thru_hole oval (at 1.27 3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 5 "/ampli_h2")
    )
    (pad "4" thru_hole oval (at 3.81 3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 2 "-VAA")
    )
    (pad "5" thru_hole oval (at 3.81 -3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 46 "N-000045")
    )
    (pad "6" thru_hole oval (at 1.27 -3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 5 "/ampli_h2")
    )
    (pad "7" thru_hole oval (at -1.27 -3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 5 "/ampli_h2")
    )
    (pad "8" thru_hole oval (at -3.81 -3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 1 "+12V")
    )
    (model "dil/dil_8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "bornier2" (layer "F.Cu")
    (at 94.615 114.046 -90)
    (descr "Bornier d'alimentation 2 pins")
    (tags "DEV")
    (property "Reference" "P4" (at 0 -5.08 -90) (layer "F.SilkS"))
    (property "Value" "CONN_2" (at 0 5.08 -90) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at -2.54 0 270) (size 2.54 2.54) (drill 1.524) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 7 "/ampli_h4")
    )
    (pad "2" thru_hole circle (at 2.54 0 270) (size 2.54 2.54) (drill 1.524) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "device/bornier_2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "bornier2" (layer "F.Cu")
    (at 182.245 97.536 90)
    (descr "Bornier d'alimentation 2 pins")
    (tags "DEV")
    (property "Reference" "P5" (at 0 -5.08 90) (layer "F.SilkS"))
    (property "Value" "CONN_2" (at 0 5.08 90) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at -2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 8 "/ampli_h5")
    )
    (pad "2" thru_hole circle (at 2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "device/bornier_2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "bornier2" (layer "F.Cu")
    (at 95.885 87.376 -90)
    (descr "Bornier d'alimentation 2 pins")
    (tags "DEV")
    (property "Reference" "P6" (at 0 -5.08 -90) (layer "F.SilkS"))
    (property "Value" "CONN_2" (at 0 5.08 -90) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at -2.54 0 270) (size 2.54 2.54) (drill 1.524) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 9 "/ampli_h6")
    )
    (pad "2" thru_hole circle (at 2.54 0 270) (size 2.54 2.54) (drill 1.524) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "device/bornier_2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DIP-8__300_ELL" (layer "F.Cu")
    (at 111.125 120.396)
    (descr "8 pins DIL package, elliptical pads")
    (tags "DIL")
    (property "Reference" "U3" (at -6.35 0 90) (layer "F.SilkS"))
    (property "Value" "LM358N" (at 0 0 0) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at -3.81 3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 26 "N-000021")
    )
    (pad "2" thru_hole oval (at -1.27 3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 27 "N-000022")
    )
    (pad "3" thru_hole oval (at 1.27 3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 4 "/ampli_h1")
    )
    (pad "4" thru_hole oval (at 3.81 3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 2 "-VAA")
    )
    (pad "5" thru_hole oval (at 3.81 -3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 29 "N-000024")
    )
    (pad "6" thru_hole oval (at 1.27 -3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 4 "/ampli_h1")
    )
    (pad "7" thru_hole oval (at -1.27 -3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 4 "/ampli_h1")
    )
    (pad "8" thru_hole oval (at -3.81 -3.81) (size 1.5748 2.286) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 1 "+12V")
    )
    (model "dil/dil_8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 130.683 120.142 180)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R9" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "1K" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 16 "N-000011")
    )
    (pad "2" thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 26 "N-000021")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 169.545 91.186 180)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R15" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "47" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 8 "/ampli_h5")
    )
    (pad "2" thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 38 "N-000037")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RV2" (layer "F.Cu")
    (at 95.885 124.206)
    (descr "Resistance variable / potentiometre")
    (tags "R")
    (property "Reference" "RV1" (at 0 -5.08 0) (layer "F.SilkS"))
    (property "Value" "4,7K" (at -0.254 5.207 0) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -2.54 1.27) (size 1.524 1.524) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 23 "N-000018")
    )
    (pad "2" thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 27 "N-000022")
    )
    (pad "3" thru_hole circle (at 2.54 1.27) (size 1.524 1.524) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 10 "/ampli_h7")
    )
    (model "discret/adjustable_rx2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RV2" (layer "F.Cu")
    (at 95.885 98.806)
    (descr "Resistance variable / potentiometre")
    (tags "R")
    (property "Reference" "RV2" (at 0 -5.08 0) (layer "F.SilkS"))
    (property "Value" "4,7K" (at -0.254 5.207 0) (layer "F.SilkS"))
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -2.54 1.27) (size 1.524 1.524) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 40 "N-000039")
    )
    (pad "2" thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 44 "N-000043")
    )
    (pad "3" thru_hole circle (at 2.54 1.27) (size 1.524 1.524) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 11 "/ampli_h8")
    )
    (model "discret/adjustable_rx2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MIRE" (layer "F.Cu")
    (at 188.595 51.816)
    (property "Reference" "MIRE" (at -0.127 4.572 0) (layer "F.SilkS") hide)
    (property "Value" "*" (at 3.302 2.794 0) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "" thru_hole rect (at -1.524 0) (size 2.286 0.254) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "" thru_hole rect (at -1.524 0) (size 2.794 0.254) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "" thru_hole rect (at 0 -1.524) (size 0.254 2.794) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "" thru_hole circle (at 0 0) (size 0.254 0.254) (drill 0.0508) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole rect (at 0 1.524) (size 0.254 2.794) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "" thru_hole rect (at 1.524 0) (size 2.794 0.254) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
  )
  (footprint "MIRE" (layer "F.Cu")
    (at 88.265 51.816)
    (property "Reference" "MIRE" (at -0.127 4.572 0) (layer "F.SilkS") hide)
    (property "Value" "*" (at 3.302 2.794 0) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "" thru_hole rect (at -1.524 0) (size 2.286 0.254) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "" thru_hole rect (at -1.524 0) (size 2.794 0.254) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "" thru_hole rect (at 0 -1.524) (size 0.254 2.794) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "" thru_hole circle (at 0 0) (size 0.254 0.254) (drill 0.0508) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole rect (at 0 1.524) (size 0.254 2.794) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "" thru_hole rect (at 1.524 0) (size 2.794 0.254) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
  )
  (footprint "MIRE" (layer "F.Cu")
    (at 88.265 131.826)
    (property "Reference" "MIRE" (at -0.127 4.572 0) (layer "F.SilkS") hide)
    (property "Value" "*" (at 3.302 2.794 0) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "" thru_hole rect (at -1.524 0) (size 2.286 0.254) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "" thru_hole rect (at -1.524 0) (size 2.794 0.254) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "" thru_hole rect (at 0 -1.524) (size 0.254 2.794) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "" thru_hole circle (at 0 0) (size 0.254 0.254) (drill 0.0508) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole rect (at 0 1.524) (size 0.254 2.794) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "" thru_hole rect (at 1.524 0) (size 2.794 0.254) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
  )
  (footprint "MIRE" (layer "F.Cu")
    (at 188.595 131.826)
    (property "Reference" "MIRE" (at -0.127 4.572 0) (layer "F.SilkS") hide)
    (property "Value" "*" (at 3.302 2.794 0) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "" thru_hole rect (at -1.524 0) (size 2.286 0.254) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "" thru_hole rect (at -1.524 0) (size 2.794 0.254) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "" thru_hole rect (at 0 -1.524) (size 0.254 2.794) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "" thru_hole circle (at 0 0) (size 0.254 0.254) (drill 0.0508) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole rect (at 0 1.524) (size 0.254 2.794) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
    (pad "" thru_hole rect (at 1.524 0) (size 2.794 0.254) (drill 0.762) (layers "*.Cu" "*.Mask" "F.SilkS"))
  )
  (footprint "CP6" (layer "F.Cu")
    (at 147.32 77.216)
    (descr "Condensateur polarise")
    (tags "CP")
    (property "Reference" "C10" (at 0 0 0) (layer "F.SilkS"))
    (property "Value" "10uF" (at 0.635 0 0) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at -7.62 0) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 15 "N-000010")
    )
    (pad "2" thru_hole circle (at 7.62 0) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 14 "N-000005")
    )
    (model "discret/c_pol.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.6 0.6 0.6))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CP6" (layer "F.Cu")
    (at 160.02 70.866 90)
    (descr "Condensateur polarise")
    (tags "CP")
    (property "Reference" "C11" (at 0 0 90) (layer "F.SilkS"))
    (property "Value" "10uF" (at 0.635 0 90) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole rect (at -7.62 0 90) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (pad "2" thru_hole circle (at 7.62 0 90) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 2 "-VAA")
    )
    (model "discret/c_pol.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.6 0.6 0.6))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 141.605 81.026)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R14" (at 0 0 0) (layer "F.SilkS"))
    (property "Value" "220K" (at 0 0 0) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 41 "N-000040")
    )
    (pad "2" thru_hole circle (at 3.81 0) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "C2" (layer "F.Cu")
    (at 116.205 78.486)
    (descr "Condensateur = 2 pas")
    (tags "C")
    (property "Reference" "C14" (at 0 0 0) (layer "F.SilkS"))
    (property "Value" "150nF" (at 0 0 0) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 36 "N-000035")
    )
    (pad "2" thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "C2" (layer "F.Cu")
    (at 116.205 107.061)
    (descr "Condensateur = 2 pas")
    (tags "C")
    (property "Reference" "C12" (at 0 0 0) (layer "F.SilkS"))
    (property "Value" "150nF" (at 0 0 0) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 19 "N-000014")
    )
    (pad "2" thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 12 "GND")
    )
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 106.045 107.061 180)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R23" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "1K" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 19 "N-000014")
    )
    (pad "2" thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 7 "/ampli_h4")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 106.553 78.74 180)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R24" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "1K" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 36 "N-000035")
    )
    (pad "2" thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 9 "/ampli_h6")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "D3" (layer "F.Cu")
    (at 145.415 93.726 -90)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (property "Reference" "D9" (at 0 0 -90) (layer "F.SilkS"))
    (property "Value" "1N4148" (at 0 0 -90) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 48 "N-000047")
    )
    (pad "2" thru_hole rect (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 45 "N-000044")
    )
    (model "discret/diode.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "D3" (layer "F.Cu")
    (at 144.78 119.761 -90)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (property "Reference" "D8" (at 0 0 -90) (layer "F.SilkS"))
    (property "Value" "1N4148" (at 0 0 -90) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 31 "N-000026")
    )
    (pad "2" thru_hole rect (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 28 "N-000023")
    )
    (model "discret/diode.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 169.545 122.936 180)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R25" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "47" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 6 "/ampli_h3")
    )
    (pad "2" thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 22 "N-000017")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 160.02 120.396 -90)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R26" (at 0 0 -90) (layer "F.SilkS"))
    (property "Value" "220K" (at 0 0 -90) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 270) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 10 "/ampli_h7")
    )
    (pad "2" thru_hole circle (at 3.81 0 270) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 21 "N-000016")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 169.545 97.536 180)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R27" (at 0 0 180) (layer "F.SilkS"))
    (property "Value" "47" (at 0 0 180) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 180 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 8 "/ampli_h5")
    )
    (pad "2" thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 39 "N-000038")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "R3-LARGE_PADS" (layer "F.Cu")
    (at 161.29 93.726 -90)
    (descr "Resitance 3 pas")
    (tags "R")
    (property "Reference" "R28" (at 0 0 -90) (layer "F.SilkS"))
    (property "Value" "220K" (at 0 0 -90) (layer "F.SilkS") hide)
    (property "Footprint" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 -90 unlocked) (layer "F.Fab") hide)
    (attr through_hole)
    (pad "1" thru_hole circle (at -3.81 0 270) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 11 "/ampli_h8")
    )
    (pad "2" thru_hole circle (at 3.81 0 270) (size 1.651 1.651) (drill 0.8128) (layers "*.Cu" "*.Mask" "F.SilkS")
      (net 38 "N-000037")
    )
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 88.265 51.816) (end 188.595 51.816)
    (layer "Edge.Cuts"))
  (gr_line (start 88.265 131.826) (end 88.265 51.816)
    (layer "Edge.Cuts"))
  (gr_line (start 188.595 131.826) (end 88.265 131.826)
    (layer "Edge.Cuts"))
  (gr_line (start 188.595 51.816) (end 188.595 131.826)
    (layer "Edge.Cuts"))
  (gr_text "Actionneur\nPiezo New Amp\nV02" (at 173.355 68.453 0) (layer "F.Cu"))
  (gr_text "Actionneur\nPiezo New Amp\nV02" (at 176.149 64.643 0) (layer "B.Cu"))
  (zone (net 12) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.762) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 187.325 131.572)
        (xy 187.325 53.086)
        (xy 88.392 53.086)
        (xy 88.392 131.572)
      )
    )
  )
)
