(kicad_pcb (version 20210108) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad1)")
  (footprint "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical" (layer "F.Cu")
    (tedit 5C28146C)
    (at 52.5 42 90)
    (descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (property "Sheet file" "custom_fields.kicad_sch")
    (property "Sheet name" "")
    (property "myfield" "myvalue")
    (attr through_hole)
    (fp_text reference "J1" (at 1.25 -3.55 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 1.25 4.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 2.7 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (locked) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 "Net-(J1-Pad1)") (pinfunction "Pin_1"))
    (pad "2" thru_hole oval (at 2.5 0 90) (locked) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)") (pinfunction "Pin_2"))
    (model "${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 43 40.5 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheet file" "custom_fields.kicad_sch")
    (property "Sheet name" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4625 0 90) (locked) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 2 "Net-(J1-Pad1)"))
    (pad "2" smd roundrect (at 1.4625 0 90) (locked) (size 1.125 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.222222)
      (net 1 "Net-(J1-Pad2)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 33.5 29.5) (end 63.5 51.5) (layer "Edge.Cuts") (width 0.1) (fill none))
)
