(kicad_pcb (version 20200829) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user)
    (33 "F.Adhes" user)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user)
    (37 "F.SilkS" user)
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user)
    (41 "Cmts.User" user)
    (42 "Eco1.User" user)
    (43 "Eco2.User" user)
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user)
    (47 "F.CrtYd" user)
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (module "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "F.Cu") (tedit 5A64794F)
    (at 55 55)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "SB1" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text value "SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
          (xy -0.5 -0.75)
          (xy 0.5 -0.75)
          (xy 1 0)
          (xy 0.5 0.75)
          (xy -0.5 0.75)
) (width 0))
      ))
    (pad "2" smd custom (at 0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
          (xy -0.65 -0.75)
          (xy 0.5 -0.75)
          (xy 0.5 0.75)
          (xy -0.65 0.75)
          (xy -0.15 0)
) (width 0))
      ))
  )
  (gr_rect (start 50 50) (end 100 100) (layer "Edge.Cuts") (width 0.05))
)
