(kicad_pcb (version 20230620) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (pdf_front_fp_property_popups true)
      (pdf_back_fp_property_popups true)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "A")
  (net 2 "B")
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (at 126.383886 85.958221)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Reference" "REF**" (at 0 -1.448 0 unlocked) (layer "F.SilkS"))
    (property "Value" "TestPoint_Pad_1.0x1.0mm" (at 0 1.55 0 unlocked) (layer "F.Fab"))
    (property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "F.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0 -1.45 0) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 1 "A")
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "B.Cu")
    (at 128.622292 85.304594 180)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Reference" "REF**" (at 0 1.448 0 unlocked) (layer "B.SilkS"))
    (property "Value" "TestPoint_Pad_1.0x1.0mm" (at 0 -1.55 0 unlocked) (layer "B.Fab"))
    (property "Footprint" "TestPoint:TestPoint_Pad_1.0x1.0mm" (at 0 0 0 unlocked) (layer "B.Fab") hide)
    (property "Datasheet" "" (at 0 0 0 unlocked) (layer "B.Fab") hide)
    (property "Description" "" (at 0 0 0 unlocked) (layer "B.Fab") hide)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text user "${REFERENCE}" (at 0 1.45 180) (layer "B.Fab"))
    (pad "1" smd rect (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask")
      (net 2 "B")
    )
  )
  (gr_rect (start 120.188564 80.549407) (end 134.184964 91.096551)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "Without refilling, \nthe inner zone \nis located too close" (at 122.336593 82.233874 0) (layer "Cmts.User"))
  (zone (net 1) (net_name "A") (layer "F.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 122.70769 82.894624)
        (xy 127.682194 82.784966)
        (xy 127.742008 89.07537)
        (xy 122.647877 88.736426)
      )
    )
  )
  (zone (net 2) (net_name "B") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 118.583563 79.871518)
        (xy 118.513781 92.023664)
        (xy 135.590585 92.063539)
        (xy 135.002417 80.190525)
      )
    )
  )
)
