(kicad_pcb (version 20220427) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A")
  (title_block
    (title "Frontend")
    (rev "00")
    (company "Lockwood")
    (comment 1 "This design rejects intellectual property. Do what you want with it. Be gay, do crime.")
    (comment 4 "A05")
  )
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "White"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 0.48) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 0.48) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 0.48) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "White"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/SIG_1XC")
  (net 2 "GND")
  (net 3 "/ATN_IN")
  (net 4 "Net-(C6-Pad2)")
  (net 5 "Net-(C7-Pad1)")
  (net 6 "Net-(C8-Pad1)")
  (net 7 "Net-(C8-Pad2)")
  (net 8 "Net-(C9-Pad1)")
  (net 9 "Net-(C9-Pad2)")
  (net 10 "/SIG_100X")
  (net 11 "Net-(C12-Pad1)")
  (net 12 "Net-(C12-Pad2)")
  (net 13 "Net-(C13-Pad1)")
  (net 14 "Net-(C13-Pad2)")
  (net 15 "/VFILT'")
  (net 16 "Net-(C16-Pad1)")
  (net 17 "Net-(C16-Pad2)")
  (net 18 "/SIG_{2}")
  (net 19 "Net-(C17-Pad2)")
  (net 20 "Net-(C18-Pad1)")
  (net 21 "Net-(C19-Pad1)")
  (net 22 "-5V")
  (net 23 "+5V")
  (net 24 "Net-(D2-Pad1)")
  (net 25 "Net-(D2-Pad2)")
  (net 26 "Net-(D3-Pad2)")
  (net 27 "Net-(FB1-Pad1)")
  (net 28 "/THERM")
  (net 29 "/SIG_IN_{1}")
  (net 30 "/OUT1+")
  (net 31 "/OUT1-")
  (net 32 "/OUT2+")
  (net 33 "/OUT2-")
  (net 34 "/OUT3+")
  (net 35 "/OUT3-")
  (net 36 "/OFFSET1")
  (net 37 "/OFFSET2")
  (net 38 "/VGAIN")
  (net 39 "/VFILTER")
  (net 40 "+12V")
  (net 41 "/EN_BWL")
  (net 42 "Net-(J4-Pad1)")
  (net 43 "/SIG_50_{OPEN}")
  (net 44 "/SIG_50")
  (net 45 "/SIG_IN_{2}")
  (net 46 "/SIG_IN_{3}")
  (net 47 "/SIG_1X")
  (net 48 "/SIG_100XD")
  (net 49 "/SIG_{1}")
  (net 50 "Net-(Q2-Pad3)")
  (net 51 "Net-(Q3-Pad1)")
  (net 52 "Net-(Q4-Pad2)")
  (net 53 "Net-(Q4-Pad3)")
  (net 54 "Net-(Q5-Pad1)")
  (net 55 "Net-(Q5-Pad2)")
  (net 56 "Net-(Q6-Pad2)")
  (net 57 "Net-(Q6-Pad3)")
  (net 58 "Net-(C1-Pad1)")
  (net 59 "Net-(R5-Pad1)")
  (net 60 "Net-(R10-Pad1)")
  (net 61 "Net-(R10-Pad2)")
  (net 62 "Net-(R12-Pad2)")
  (net 63 "Net-(R15-Pad2)")
  (net 64 "Net-(R19-Pad2)")
  (net 65 "Net-(R20-Pad2)")
  (net 66 "Net-(R21-Pad1)")
  (net 67 "Net-(R24-Pad2)")
  (net 68 "Net-(R32-Pad2)")
  (net 69 "Net-(R36-Pad2)")
  (net 70 "Net-(R39-Pad1)")
  (net 71 "Net-(R43-Pad1)")
  (net 72 "Net-(R44-Pad2)")
  (net 73 "Net-(R45-Pad2)")
  (net 74 "Net-(R47-Pad1)")
  (net 75 "Net-(R49-Pad1)")
  (net 76 "Net-(R52-Pad2)")
  (net 77 "Net-(R53-Pad2)")
  (net 78 "Net-(Q1-Pad2)")
  (net 79 "Net-(Q3-Pad3)")
  (net 80 "unconnected-(U2-Pad13)")
  (net 81 "/~{EN_ATN_1X}")
  (net 82 "/~{EN_DC}")
  (net 83 "/~{EN_50}")
  (net 84 "/~{EN_SIG}")
  (net 85 "unconnected-(J3-Pad39)")
  (net 86 "/LMH_EN")
  (net 87 "/SIG_1XC2")
  (net 88 "/SIG_100XC2")
  (net 89 "Net-(R23-Pad2)")
  (net 90 "Net-(R71-Pad2)")
  (net 91 "Net-(R70-Pad1)")
  (net 92 "Net-(R72-Pad1)")
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 94.25 124.5 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R35" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "390k" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(C16-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(R32-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:SOT-23" (layer "F.Cu")
    (at 89 133.5 180)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q3" (at 1.6 -1.1 unlocked) (layer "F.SilkS") hide)
    (fp_text value "2SK3557-7" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 -0.95 180) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(Q3-Pad1)") (pinfunction "S") (pintype "passive"))
    (pad "2" smd roundrect (at -1 0.95 180) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "+5V") (pinfunction "D") (pintype "passive"))
    (pad "3" smd roundrect (at 1 0 180) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "Net-(Q3-Pad3)") (pinfunction "G") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 88.35 141 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R58" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "330" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(Q4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "F.Cu")
    (at 62.25 141.75)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP3" (at -6 0 90) (layer "F.SilkS"))
    (fp_text value "SELG" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab"))
    (pad "1" smd circle locked (at 0 0) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 94.75 130 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R49" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "2k4" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "Net-(R49-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(C16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 82.5 136.75 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R27" (at 0 -1.65 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "330k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 67 "Net-(R24-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 18 "/SIG_{2}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 97.9 134.3 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "18" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(R10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(R10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 93 129.25 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R48" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (fp_text value "12k" (at 0 0.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 180) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(C16-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 180) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(R47-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (at 101 122.75)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (zone_connect 2)
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.8 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Relay_THT:Relay_SPST_StandexMeder_SIL_Form1A" (layer "F.Cu")
    (at 78.4825 138.5 90)
    (descr "Standex-Meder SIL-relais, Form 1A, see https://standexelectronics.com/wp-content/uploads/datasheet_reed_relay_SIL.pdf")
    (tags "Standex Meder SIL reed relais")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "K3" (at -3.25 0.0175 unlocked) (layer "F.SilkS"))
    (fp_text value "Relay-SPST-Reed" (at 7.65 3.55 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.75 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "/SIG_{2}") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 40 "+12V") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 10.16 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 84 "/~{EN_SIG}") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 15.24 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 49 "/SIG_{1}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPST_StandexMeder_SIL_Form1A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SON:WSON-8-1EP_3x2.5mm_P0.5mm_EP1.2x1.5mm_PullBack" (layer "F.Cu")
    (at 112.2 132.2 180)
    (descr "WSON, 8 Pin (http://www.ti.com/lit/ml/mpds400/mpds400.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "WSON NoLead")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 0 -2.2 unlocked) (layer "F.SilkS"))
    (fp_text value "LMH6551MA" (at 0 2.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect locked (at -0.3 -0.375 180) (size 0.48 0.6) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at -0.3 0.375 180) (size 0.48 0.6) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.3 -0.375 180) (size 0.48 0.6) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.3 0.375 180) (size 0.48 0.6) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -1.1375 -0.75 180) (size 0.675 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(R45-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "2" smd roundrect locked (at -1.1375 -0.25 180) (size 0.675 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VCM") (pintype "input"))
    (pad "3" smd roundrect locked (at -1.1375 0.25 180) (size 0.675 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "+5V") (pinfunction "V+") (pintype "power_in"))
    (pad "4" smd roundrect locked (at -1.1375 0.75 180) (size 0.675 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(R53-Pad2)") (pinfunction "+") (pintype "output"))
    (pad "5" smd roundrect locked (at 1.1375 0.75 180) (size 0.675 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(R52-Pad2)") (pinfunction "-") (pintype "output"))
    (pad "6" smd roundrect locked (at 1.1375 0.25 180) (size 0.675 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pinfunction "V-") (pintype "power_in"))
    (pad "7" smd roundrect locked (at 1.1375 -0.25 180) (size 0.675 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "/LMH_EN") (pinfunction "EN") (pintype "input"))
    (pad "8" smd roundrect locked (at 1.1375 -0.75 180) (size 0.675 0.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(R44-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "9" smd rect locked (at 0 0 180) (size 1.2 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "DAP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SON.3dshapes/WSON-8-1EP_3x2.5mm_P0.5mm_EP1.2x1.5mm_PullBack.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 101.75 139.75 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "270" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(R5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 114.6 134.8 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R45" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "30" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(R45-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 110.6 136.8)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at 0 -1.43 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47p" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C13-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(C13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (at 42.8 138.1 160)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "TH1" (at 0 -1.43 -20 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.43 160) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 160) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9125 0 160) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(FB1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 160) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 103 139.75 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "30k" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(R5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "/OFFSET2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 95.25 134.5 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R69" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(Q5-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "Net-(R43-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 113.8 136.8)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at 0 -1.43 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47p" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/VFILT'") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(C12-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 96.9 133 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R43" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "750k" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "Net-(R43-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(R39-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 92.75 141 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R67" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "150" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(Q6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 115.4 133)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R53" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (fp_text value "510" (at 0 0.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(R45-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(R53-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:SOT-23" (layer "F.Cu")
    (at 92.5 138 90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q6" (at 1.25 -1.58 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MMBTH10" (at 0 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 -0.95 90) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(C19-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -1 0.95 90) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(Q6-Pad2)") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 1 0 90) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(Q6-Pad3)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "F.Cu")
    (at 102.25 133.75)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 2 -5.25 unlocked) (layer "F.SilkS"))
    (fp_text value "VCA821ID" (at 0 5.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "+5V") (pinfunction "+V_{CC}") (pintype "power_in"))
    (pad "2" smd roundrect locked (at -2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(C1-Pad1)") (pinfunction "V_{G}") (pintype "input"))
    (pad "3" smd roundrect locked (at -2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "Net-(R43-Pad1)") (pinfunction "+V_{IN}") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(R10-Pad1)") (pinfunction "+R_{G}") (pintype "passive"))
    (pad "5" smd roundrect locked (at -2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(R10-Pad2)") (pinfunction "-R_{G}") (pintype "passive"))
    (pad "6" smd roundrect locked (at -2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(R5-Pad1)") (pinfunction "-V_{IN}") (pintype "input"))
    (pad "7" smd roundrect locked (at -2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pinfunction "-V_{CC}") (pintype "power_in"))
    (pad "8" smd roundrect locked (at 2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pinfunction "-V_{CC}") (pintype "passive"))
    (pad "9" smd roundrect locked (at 2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(R20-Pad2)") (pinfunction "V_{REF}") (pintype "input"))
    (pad "10" smd roundrect locked (at 2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C9-Pad1)") (pinfunction "V_{OUT}") (pintype "output"))
    (pad "11" smd roundrect locked (at 2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "12" smd roundrect locked (at 2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(R21-Pad1)") (pinfunction "FB") (pintype "input"))
    (pad "13" smd roundrect locked (at 2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "unconnected-(U2-Pad13)") (pinfunction "NC") (pintype "no_connect"))
    (pad "14" smd roundrect locked (at 2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "+5V") (pinfunction "+V_{CC}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 114.4 129.4 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R59" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/OUT2+") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(R53-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_THT:Relay_DPDT_Omron_G5V-2" (layer "F.Cu")
    (at 47 121.1425)
    (descr "http://omronfs.omron.com/en_US/ecb/products/pdf/en-g5v2.pdf")
    (tags "Omron G5V-2 Relay DPDT")
    (property "BOM" "J104D2C12VDC.15S")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "K1" (at 3.81 20.6075 unlocked) (layer "F.SilkS"))
    (fp_text value "Relay-DPDT-CIT-J104D" (at 3.81 20.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.94 9.16) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 40 "+12V") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 0 7.62) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 29 "/SIG_IN_{1}") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 0 12.7) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 43 "/SIG_50_{OPEN}") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 0 17.78) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 44 "/SIG_50") (pintype "passive"))
    (pad "9" thru_hole circle locked (at 7.62 17.78) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 44 "/SIG_50") (pintype "passive"))
    (pad "11" thru_hole circle locked (at 7.62 12.7) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 29 "/SIG_IN_{1}") (pintype "passive"))
    (pad "13" thru_hole circle locked (at 7.62 7.62) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 45 "/SIG_IN_{2}") (pintype "passive"))
    (pad "16" thru_hole circle locked (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 83 "/~{EN_50}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_DPDT_Omron_G5V-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 115.4 129.4 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R62" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/OUT1+") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(R53-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (at 44.3 140.6 -30)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "FB1" (at 0 -1.43 -30 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1k" (at 0 1.43 150) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 150) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.875 0 330) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(FB1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.875 0 330) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/THERM") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 110 129.4 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R60" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/OUT2-") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(R52-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder" (layer "F.Cu")
    (at 100.75 128.5 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 0.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.2) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5675 0 180) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5675 0 180) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 86 128.2)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "BOM" "CAP-15NF-630V-1206")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 0 -1.85) (layer "F.SilkS") hide)
    (fp_text value "15n" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 6 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.475 0) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 7 "Net-(C8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 111 129.4 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R56" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/OUT3-") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(R52-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 94.25 122 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R36" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "2k4" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(R32-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(R36-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:C_0204_LowESL" (layer "F.Cu")
    (at 104.75 139.25 -90)
    (property "BOM" "CAP-100N-0204")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "CW6" (at 0 -1.397 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.9 8 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.265 0 270) (size 0.38 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.265 0 270) (size 0.38 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 90.5 135.75)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R63" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (fp_text value "75" (at 0 0.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(Q3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(Q5-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:C-Trim-Vishay-BFC2-809-05" (layer "F.Cu")
    (at 71.25 131)
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C5" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "2-18p" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole oval (at -2.54 0) (size 1.4 1.8) (drill oval 0.8 1.2) (layers *.Cu *.Mask)
      (net 88 "/SIG_100XC2") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.4 1.8) (drill oval 0.8 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 96.75 124.5 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "120k" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 113.4 129.4 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R55" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/OUT3+") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(R53-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:NOC-A-BGDC" (layer "F.Cu")
    (at 116.5 122)
    (descr "Symbol")
    (attr board_only exclude_from_bom)
    (fp_text reference "REF**" (at 0 -0.4 unlocked) (layer "F.SilkS") hide)
    (fp_text value "NOC-A-BGDC" (at 0 0.9 unlocked) (layer "F.Fab"))
    (fp_text user "BGDC" (at 2 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.4 unlocked) (layer "F.Fab") hide)
    (pad "" smd rect (at 0 0.05) (size 2 0.5) (layers "Dwgs.User"))
  )
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "F.Cu")
    (at 65 141.75 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 7.5 0 90) (layer "F.SilkS"))
    (fp_text value "SEL2" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab"))
    (pad "1" smd circle locked (at 0 0 180) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 91 "Net-(R70-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 93 130.5)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R50" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (fp_text value "51" (at 0 0.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "Net-(R49-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 95.2 126.4)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C33" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:C_0204_LowESL" (layer "F.Cu")
    (at 97.5 137 90)
    (property "BOM" "CAP-100N-0204")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "CW5" (at 0 -1.397 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.265 0 90) (size 0.38 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.265 0 90) (size 0.38 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 90 128.25 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R47" (at 0 -1.65 unlocked) (layer "F.SilkS") hide)
    (fp_text value "4M7" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 74 "Net-(R47-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 26 "Net-(D3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 107.5 138)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R25" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (fp_text value "DNS" (at 6.45 4.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.025 4.2 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:C-Trim-Vishay-BFC2-809-05" (layer "F.Cu")
    (at 71.25 139)
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "2-18p" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole oval (at -2.54 0) (size 1.4 1.8) (drill oval 0.8 1.2) (layers *.Cu *.Mask)
      (net 87 "/SIG_1XC2") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.4 1.8) (drill oval 0.8 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "alexisvl:C_0204_LowESL" (layer "F.Cu")
    (at 94 141.25)
    (property "BOM" "CAP-100N-0204")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "CW8" (at 0 -1.397 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.265 0) (size 0.38 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.265 0) (size 0.38 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "Package_SO:SO-4_4.4x4.3mm_P2.54mm" (layer "F.Cu")
    (at 85.75 123.2 -90)
    (descr "4-Lead Plastic Small Outline (SO), see https://docs.broadcom.com/docs/AV02-0173EN")
    (tags "SO SOIC 2.54")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at -1 3.25 90 unlocked) (layer "F.SilkS"))
    (fp_text value "AB30S" (at 0 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -3 -1.27 180) (size 0.8 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "+12V") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect locked (at -3 1.27 180) (size 0.8 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "/~{EN_DC}") (pinfunction "K") (pintype "passive"))
    (pad "3" smd rect locked (at 3 1.27 180) (size 0.8 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(C8-Pad1)") (pinfunction "D1") (pintype "passive"))
    (pad "4" smd rect locked (at 3 -1.27 180) (size 0.8 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(C8-Pad2)") (pinfunction "D2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SO-4_4.4x4.3mm_P2.54mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:C_0204_LowESL" (layer "F.Cu")
    (at 107 130.25 -90)
    (property "BOM" "CAP-100N-0204")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "CW1" (at 0 -1.397 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.265 0 270) (size 0.38 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.265 0 270) (size 0.38 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 108.25 135.5 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 0 -1.43 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "DNS" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C9-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:C_0204_LowESL" (layer "F.Cu")
    (at 109.35 131.75 -90)
    (property "BOM" "CAP-100N-0204")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "CW7" (at 0 -1.397 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.265 0 270) (size 0.38 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.265 0 270) (size 0.38 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 84.5 136.75 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R51" (at 0 -1.65 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "22" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 26 "Net-(D3-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 19 "Net-(C17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3528-15_AVX-H" (layer "F.Cu")
    (at 108.6 126)
    (descr "Tantalum Capacitor SMD AVX-H (3528-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "BOM" "478-1693-1-ND")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C28" (at 0 -2.35 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47µ" (at 0 2.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -1.5375 0) (size 1.325 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 23 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.5375 0) (size 1.325 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-15_AVX-H.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 83.5 139.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "BOM" "CAP-330P-500V-0805")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C17" (at 0 -1.68 unlocked) (layer "F.SilkS") hide)
    (fp_text value "330p" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "/SIG_{2}") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(C17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 114.35 138.1 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R30" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (fp_text value "30" (at 0 0.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 180) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 180) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(C12-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 95.5 124.5 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R32" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "430k" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(C16-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(R32-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 100.5 139.75 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "120k" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(R5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 88 135.75)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R57" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10" (at 0 0.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(Q4-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(Q3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3528-15_AVX-H" (layer "F.Cu")
    (at 108.6 140.4)
    (descr "Tantalum Capacitor SMD AVX-H (3528-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "BOM" "478-1693-1-ND")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C30" (at 0 -2.35 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47µ" (at 0 2.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -1.5375 0) (size 1.325 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.5375 0) (size 1.325 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 22 "-5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-15_AVX-H.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 110 138.1)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R29" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (fp_text value "30" (at 0 0.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C9-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C13-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:C_0204_LowESL" (layer "F.Cu")
    (at 86 141.25 180)
    (property "BOM" "CAP-100N-0204")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "CW9" (at 0 -1.397 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.265 0 180) (size 0.38 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.265 0 180) (size 0.38 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 82.25 126 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at 0 -1.43 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "390k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C8-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 100.75 127.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (fp_text value "30k" (at 0 0.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 180) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 180) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 96 130.5 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R39" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "240k" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(R39-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(C16-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:C_0204_LowESL" (layer "F.Cu")
    (at 115.05 131.75 -90)
    (property "BOM" "CAP-100N-0204")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "CW3" (at 0 -1.397 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.265 0 270) (size 0.38 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.265 0 270) (size 0.38 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 90.55 141.05 -155)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C19" (at 0 -1.43 -335 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100p" (at 0 1.43 -335) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -335) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.775 0 205) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(C19-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 205) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 106.75 133.75 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R21" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "402" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(R21-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C9-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 109.8 134.8 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R44" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "30" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C13-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(R44-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 89 125.5 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R28" (at 0 -1.43 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "390k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Samtec_SMA-J-P-X-ST-EM1_EdgeMount" (layer "F.Cu")
    (at 42.35 130 -90)
    (descr "Connector SMA, 0Hz to 20GHz, 50Ohm, Edge Mount (http://suddendocs.samtec.com/prints/sma-j-p-x-st-em1-mkt.pdf)")
    (tags "SMA Straight Samtec Edge Mount")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at -4.25 -2.25 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Conn_Coaxial" (at 0 13 90) (layer "F.Fab"))
    (fp_text user "PCB Edge" (at 0 2.6 90) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 0 4.79 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at 0 0.2 270) (size 1.27 3.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/SIG_IN_{1}") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect locked (at -2.825 0 270) (size 1.35 4.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect locked (at -2.825 0 270) (size 1.35 4.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect locked (at 2.825 0 270) (size 1.35 4.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect locked (at 2.825 0 270) (size 1.35 4.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Samtec_SMA-J-P-X-ST-EM1_EdgeMount.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 102.5 128 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 0 -270 unlocked) (layer "F.SilkS") hide)
    (fp_text value "3k9" (at 0 0.25 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 -270) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/VGAIN") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(C1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:U.FL_Hirose_U.FL-R-SMT-1_Vertical" (layer "F.Cu")
    (at 97.25 140 -90)
    (descr "Hirose U.FL Coaxial https://www.hirose.com/product/en/products/U.FL/U.FL-R-SMT-1%2810%29/")
    (tags "Hirose U.FL Coaxial")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J4" (at 1.5 -3.25 unlocked) (layer "F.SilkS"))
    (fp_text value "TEST1" (at 0.475 3.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.475 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.05 0 270) (size 1.05 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "Net-(J4-Pad1)") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect locked (at 0.475 -1.475 270) (size 2.2 1.05) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect locked (at 0.475 1.475 270) (size 2.2 1.05) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/U.FL_Hirose_U.FL-R-SMT-1_Vertical.wrl"
      (offset (xyz 0.4749999928 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:R_Susumu_HPT2012" (layer "F.Cu")
    (at 42.6 135.8 180)
    (descr "Resistor, SMT, like 0805, RF high power termination")
    (tags "resistor")
    (property "BOM" "RES-50-RFTerm-5W-SMT")
    (property "MFR" "Susumu")
    (property "MPN" "HPT2012-50-T1")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.65 180) (layer "F.SilkS") hide)
    (fp_text value "50" (at 0 1.65 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1125 0 180) (size 0.625 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 44 "/SIG_50") (pintype "passive"))
    (pad "2" smd roundrect (at 0.4625 0 180) (size 1.925 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.08333333333)
      (net 2 "GND") (pintype "passive") (solder_paste_margin_ratio -0.1))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:SOT-23" (layer "F.Cu")
    (at 88.25 138 90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q4" (at 1.25 -1.75 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MMBTH10" (at 0 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 -0.95 90) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(C19-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -1 0.95 90) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(Q4-Pad2)") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 1 0 90) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(Q4-Pad3)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:TrimCap-Generic" (layer "F.Cu")
    (at 71.25 123)
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C15" (at 0 -1.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "15-60p" (at 0 0 unlocked) (layer "F.Fab"))
    (fp_text user "REF**" (at 0 1.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -2.5 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "/SIG_100X") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 106.75 136.25 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R20" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "22" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(R20-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 93 135.75)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R66" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10" (at 0 0.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(Q6-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(Q5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 82.5 129.75 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R19" (at 0 -1.65 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "330k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 6 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 64 "Net-(R19-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 82.8 120.8 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R73" (at 0 0 270 unlocked) (layer "F.SilkS") hide)
    (fp_text value "220k" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "+12V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "/~{EN_DC}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 108.8 133.1 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R52" (at 0 0 unlocked) (layer "F.SilkS") hide)
    (fp_text value "510" (at 0 0.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 180) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(R44-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 180) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(R52-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 86 139.25 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R64" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1k" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(C19-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "F.Cu")
    (at 59.5 141.75 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 4.5 0 90) (layer "F.SilkS"))
    (fp_text value "SEL1" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab"))
    (pad "1" smd circle locked (at 0 0 180) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 92 "Net-(R72-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "alexisvl:SOT-23" (layer "F.Cu")
    (at 93 133.5 90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q5" (at 0 -2.5 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "MMBTH10" (at 0 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 -0.95 90) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(Q5-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -1 0.95 90) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(Q5-Pad2)") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 1 0 90) (size 1.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "+5V") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:D_MiniMELF" (layer "F.Cu")
    (at 89 130.5 180)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at 0 -2 180) (layer "F.SilkS") hide)
    (fp_text value "LL4448" (at 0 1.75 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.75 0 180) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "+5V") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.75 0 180) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(D3-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:C_0204_LowESL" (layer "F.Cu")
    (at 95.6 132.5 90)
    (property "BOM" "CAP-100N-0204")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "CW4" (at 0 -1.397 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.265 0 90) (size 0.38 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.265 0 90) (size 0.38 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 95.25 136.75 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R68" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(Q5-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J4-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 95.5 122 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R37" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "DNS" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(R36-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 89.2 121.8 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C32" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 87.25 141 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R61" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "1k" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(C19-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 86.75 132.75 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R54" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "22" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "Net-(Q3-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 90) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(D3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 109 129.4 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R65" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "47" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/OUT1-") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(R52-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder" (layer "F.Cu")
    (at 96.75 122 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 0.15 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.2 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5675 0 270) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5675 0 270) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:C_0204_LowESL" (layer "F.Cu")
    (at 97.5 130.25 -90)
    (property "BOM" "CAP-100N-0204")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "CW2" (at 0 -1.397 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "100n" (at 0 1 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 -90 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.265 0 270) (size 0.38 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.265 0 270) (size 0.38 1.1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "fixed_standard:D_MiniMELF" (layer "F.Cu")
    (at 85 132.25 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at 0 -2 90) (layer "F.SilkS") hide)
    (fp_text value "LL4448" (at 0 1.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(D3-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 97.8 126.6 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 0 0 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "30k" (at 0 0.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.175 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/OFFSET1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:MSOP-8_3x3mm_P0.65mm" (layer "F.Cu")
    (at 91.75 123.5 90)
    (descr "MSOP, 8 Pin (https://www.jedec.org/system/files/docs/mo-187F.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "MSOP SO")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 3.45 2.7 unlocked) (layer "F.SilkS"))
    (fp_text value "ADA4177-2" (at 0 2.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.1125 -0.975 90) (size 1.625 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(R47-Pad1)") (pintype "output"))
    (pad "2" smd roundrect locked (at -2.1125 -0.325 90) (size 1.625 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(C16-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect locked (at -2.1125 0.325 90) (size 1.625 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C8-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.1125 0.975 90) (size 1.625 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect locked (at 2.1125 0.975 90) (size 1.625 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C7-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect locked (at 2.1125 0.325 90) (size 1.625 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(R36-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect locked (at 2.1125 -0.325 90) (size 1.625 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(R32-Pad2)") (pintype "output"))
    (pad "8" smd roundrect locked (at 2.1125 -0.975 90) (size 1.625 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "+5V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-8_3x3mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 93.25 128)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C16" (at 0 -1.43 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10n" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(C16-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(C16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_THT:Relay_DPDT_Omron_G5V-2" (layer "F.Cu")
    (at 57.7375 121.1425)
    (descr "http://omronfs.omron.com/en_US/ecb/products/pdf/en-g5v2.pdf")
    (tags "Omron G5V-2 Relay DPDT")
    (property "BOM" "J104D2C12VDC.15S")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "K2" (at 9.7625 -0.8925 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Relay-DPDT-CIT-J104D" (at 3.81 20.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.94 9.16) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 40 "+12V") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 0 7.62) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 46 "/SIG_IN_{3}") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 0 12.7) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "/ATN_IN") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 0 17.78) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 47 "/SIG_1X") (pintype "passive"))
    (pad "9" thru_hole circle locked (at 7.62 17.78) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 47 "/SIG_1X") (pintype "passive"))
    (pad "11" thru_hole circle locked (at 7.62 12.7) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 48 "/SIG_100XD") (pintype "passive"))
    (pad "13" thru_hole circle locked (at 7.62 7.62) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 49 "/SIG_{1}") (pintype "passive"))
    (pad "16" thru_hole circle locked (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 81 "/~{EN_ATN_1X}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_DPDT_Omron_G5V-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 82.5 133.25 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R24" (at 0 -1.65 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "330k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect locked (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 64 "Net-(R19-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 67 "Net-(R24-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 59.9 125.8 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at 0 1.43 -270) (layer "B.SilkS") hide)
    (fp_text value "62p" (at 0 -1.43 -270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "/SIG_100X") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "B.Cu")
    (at 56.75 136.25)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0 1.85) (layer "B.SilkS") hide)
    (fp_text value "6p8" (at 0 -1.85) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.475 0) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.217391)
      (net 3 "/ATN_IN") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.475 0) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.217391)
      (net 4 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "B.Cu")
    (at 114.8 137.8 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R34" (at 0 0 90) (layer "B.SilkS") hide)
    (fp_text value "100k" (at 0 -0.25 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.175 90) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 90) (size 0.715 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "/VFILTER") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 90) (size 0.715 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "/VFILT'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 62 129 -20)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at 0 1.65 160) (layer "B.SilkS") hide)
    (fp_text value "390k" (at 0 -1.65 160) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 160) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.9125 0 340) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 63 "Net-(R15-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 340) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 10 "/SIG_100X") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 115.4 133.7 125)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 0 1.43 125) (layer "B.SilkS") hide)
    (fp_text value "220p" (at 0 -1.43 125) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 125) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.775 0 125) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 125) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 61.6 125.8 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 0 1.43 -270) (layer "B.SilkS") hide)
    (fp_text value "560p" (at 0 -1.43 -270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "/SIG_100X") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:D_SOD-123F" (layer "B.Cu")
    (at 111.8 137.8 180)
    (descr "D_SOD-123F")
    (tags "D_SOD-123F")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at -0.127 1.905) (layer "B.SilkS") hide)
    (fp_text value "1N4007FL" (at 0 -0.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.7) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0 180) (size 1.1 1.1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 15 "/VFILT'") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0 180) (size 1.1 1.1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 14 "Net-(C13-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "B.Cu")
    (at 64 131.75 -165)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 1.85 -345) (layer "B.SilkS") hide)
    (fp_text value "10p" (at 0 -1.85 -345) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -345) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -1.475 0 195) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.217391)
      (net 88 "/SIG_100XC2") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.475 0 195) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.217391)
      (net 3 "/ATN_IN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 53.4 131.4 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R71" (at 0 1.65) (layer "B.SilkS") hide)
    (fp_text value "3M" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 3 "/ATN_IN") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 180) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 90 "Net-(R71-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "B.Cu")
    (at 114.4 129.7)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R38" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "100k" (at 0 -0.25) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.175) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0) (size 0.715 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C12-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0) (size 0.715 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 60.2 131.4 70)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 0 1.65 70) (layer "B.SilkS") hide)
    (fp_text value "390k" (at 0 -1.65 70) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 70) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.9125 0 70) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 62 "Net-(R12-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 70) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 63 "Net-(R15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 57.1 131.4)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0 1.65) (layer "B.SilkS") hide)
    (fp_text value "390k" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 3 "/ATN_IN") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 62 "Net-(R12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:D_SOD-123F" (layer "B.Cu")
    (at 111.8 135.4 180)
    (descr "D_SOD-123F")
    (tags "D_SOD-123F")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at -0.127 1.905) (layer "B.SilkS") hide)
    (fp_text value "1N4007FL" (at 0 -0.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.7) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.4 0 180) (size 1.1 1.1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 15 "/VFILT'") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4 0 180) (size 1.1 1.1) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2)
      (net 14 "Net-(C13-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "B.Cu")
    (at 112.1 129.7)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R42" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "100k" (at 0 -0.25) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.175) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0) (size 0.715 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(C18-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0) (size 0.715 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(Q2-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:BergStak-Lite-40p-Receptacle" (layer "B.Cu")
    (at 118.688351 123.651087 -90)
    (property "BOM" "Mezz-BergStakLite0.8-Receptacle-40p-9,10,11,12mm")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J3" (at 7.599996 -2.199999 90) (layer "B.SilkS") hide)
    (fp_text value "INTERFACE" (at 7.599996 -2.199999 90) (layer "B.Fab"))
    (pad "" np_thru_hole circle (at -2.5 -2.199999 270) (size 1.2192 1.2192) (drill 1.2192) (layers *.Mask))
    (pad "" np_thru_hole circle (at 17.7 -2.199999 270) (size 0.8382 0.8382) (drill 0.8382) (layers F&B.Cu *.Mask))
    (pad "1" smd rect (at 0 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "/~{EN_DC}") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 0.799998 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "/~{EN_ATN_1X}") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at 1.599999 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "/~{EN_50}") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 2.399997 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "/~{EN_SIG}") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at 3.199998 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "/EN_BWL") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 3.999999 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "+12V") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at 4.799998 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "+12V") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 5.599998 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "+12V") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at 6.399997 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "+12V") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 7.199998 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect (at 7.999999 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "+5V") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect (at 8.799997 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "+5V") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect (at 9.599998 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "+5V") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect (at 10.399997 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "+5V") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect (at 11.199997 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect (at 11.999996 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect (at 12.799997 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "-5V") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect (at 13.599998 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "-5V") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect (at 14.399996 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "-5V") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect (at 15.199997 -4.399999 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "-5V") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect (at 0 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect (at 0.799998 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "/OUT1+") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect (at 1.599999 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "/OUT1-") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect (at 2.399997 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect (at 3.199998 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "/OUT2+") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect (at 3.999999 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "/OUT2-") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" smd rect (at 4.799998 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" smd rect (at 5.599998 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "/OUT3+") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" smd rect (at 6.399997 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "/OUT3-") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" smd rect (at 7.199998 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" smd rect (at 7.999999 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" smd rect (at 8.799997 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" smd rect (at 9.599998 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" smd rect (at 10.399997 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "/THERM") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" smd rect (at 11.199997 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" smd rect (at 11.999996 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "/OFFSET1") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" smd rect (at 12.799997 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "/OFFSET2") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" smd rect (at 13.599998 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "/VGAIN") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" smd rect (at 14.399996 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 85 "unconnected-(J3-Pad39)") (pinfunction "Pin_39") (pintype "passive+no_connect"))
    (pad "40" smd rect (at 15.199997 0 270) (size 0.5334 2.0574) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "/VFILTER") (pinfunction "Pin_40") (pintype "passive") (clearance 0.25))
    (model "${ALEXISVL}/3d/Mezz-BergStakLite0.8-Receptacle-40p-5,6,7,8mm.stp"
      (offset (xyz 7.6 -2.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -180))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 60.6 135.75 70)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at 0 1.65 70) (layer "B.SilkS") hide)
    (fp_text value "22" (at 0 -1.65 70) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 70) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.9125 0 70) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(C6-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 70) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 10 "/SIG_100X") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric" (layer "B.Cu")
    (at 56.25 126.8)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 0 1.82 180) (layer "B.SilkS") hide)
    (fp_text value "4R7" (at 0 -1.82 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 45 "/SIG_IN_{2}") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.4625 0) (size 1.125 1.75) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.222222)
      (net 46 "/SIG_IN_{3}") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 72.6 136 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R70" (at 3.9 1.2 unlocked) (layer "B.SilkS"))
    (fp_text value "SEL2" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 270) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 91 "Net-(R70-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 270) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:SOT-23" (layer "B.Cu")
    (at 112.2 132 90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q2" (at 0 2.5 90) (layer "B.SilkS") hide)
    (fp_text value "MMBFJ211" (at 0 -2.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0.95 90) (size 1.2 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C12-Pad2)") (pinfunction "S") (pintype "passive"))
    (pad "2" smd roundrect (at -1 -0.95 90) (size 1.2 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(C18-Pad1)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd roundrect (at 1 0 90) (size 1.2 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(Q2-Pad3)") (pinfunction "G") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "B.Cu")
    (at 108.8 137.8 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R33" (at 0 0 90) (layer "B.SilkS") hide)
    (fp_text value "100k" (at 0 -0.25 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.175 90) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 90) (size 0.715 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 90) (size 0.715 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(C13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "B.Cu")
    (at 109.8 129.7)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R46" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "100k" (at 0 -0.25) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.175) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0) (size 0.715 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0) (size 0.715 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(C18-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "B.Cu")
    (at 104.4 130.2 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R31" (at 0 0 90) (layer "B.SilkS") hide)
    (fp_text value "3k3" (at 0 -0.25 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.175 90) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 270) (size 0.715 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "/EN_BWL") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 270) (size 0.715 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 78 "Net-(Q1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "B.Cu")
    (at 107.5 127.7 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R40" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "10k" (at 0 -0.25) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.175) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 180) (size 0.715 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(Q2-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 180) (size 0.715 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(D2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 61.9 138.1 -110)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 0 1.65 70) (layer "B.SilkS") hide)
    (fp_text value "18" (at 0 -1.65 70) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 70) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.9125 0 250) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 1 "/SIG_1XC") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 250) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 47 "/SIG_1X") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 51.3 136.7 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R72" (at 0.4 -1.7 unlocked) (layer "B.SilkS"))
    (fp_text value "SEL1" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 92 "Net-(R72-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 52 134.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R75" (at 0 1.65 90) (layer "B.SilkS") hide)
    (fp_text value "3M" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 90 "Net-(R71-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 92 "Net-(R72-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 109 133.7 -125)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C18" (at 0 1.43 55) (layer "B.SilkS") hide)
    (fp_text value "220p" (at 0 -1.43 55) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 55) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.775 0 235) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(C18-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 235) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C13-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "alexisvl:SOT-23" (layer "B.Cu")
    (at 103.4 133.4 -90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 0 2.5 90) (layer "B.SilkS") hide)
    (fp_text value "MMBT3906" (at 0 -2.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0.95 270) (size 1.2 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -1 -0.95 270) (size 1.2 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 78 "Net-(Q1-Pad2)") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 1 0 270) (size 1.2 0.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(D2-Pad1)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "B.Cu")
    (at 63.7 127.1 -160)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R22" (at 0 0 -340) (layer "B.SilkS") hide)
    (fp_text value "11k8" (at 0 -0.25 -340) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.175 -340) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 200) (size 0.715 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 200) (size 0.715 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "/SIG_100X") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 106.8 129 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C31" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 86 "/LMH_EN") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 180) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "B.Cu")
    (at 68.2 136.6 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 1.85) (layer "B.SilkS") hide)
    (fp_text value "10p" (at 0 -1.85) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -1.475 0 180) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.217391)
      (net 87 "/SIG_1XC2") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.475 0 180) (size 1.15 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.217391)
      (net 1 "/SIG_1XC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 63.75 135.25 -30)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R26" (at 0 1.65 150) (layer "B.SilkS") hide)
    (fp_text value "100" (at 0 -1.65 150) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 150) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.9125 0 330) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 10 "/SIG_100X") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 330) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 48 "/SIG_100XD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:D_MiniMELF" (layer "B.Cu")
    (at 106.4 132.6 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 0 2 90) (layer "B.SilkS") hide)
    (fp_text value "LL4448" (at 0 -1.75 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(D2-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.75 0 90) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 74.8 135.8 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R74" (at 0 1.65 90) (layer "B.SilkS") hide)
    (fp_text value "3M" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 89 "Net-(R23-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 91 "Net-(R70-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (at 77.8 136 150)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R23" (at 0 1.65 150) (layer "B.SilkS") hide)
    (fp_text value "3M" (at 0 -1.65 150) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 150) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.9125 0 150) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 18 "/SIG_{2}") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.9125 0 150) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902)
      (net 89 "Net-(R23-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "fixed_standard:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "B.Cu")
    (at 104 135.75 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "A05-attenuator.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R41" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "10k" (at 0 -0.25) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.175) (layer "B.Fab") hide)
    (pad "1" smd roundrect locked (at -0.5975 0 180) (size 0.715 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(D2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.5975 0 180) (size 0.715 0.64) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "-5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 40 124.35) (end 40 143)
    (layer "Edge.Cuts"))
  (gr_line (start 40 143) (end 125 143)
    (layer "Edge.Cuts"))
  (gr_arc (start 40 121.15) (mid 41.6 122.75) (end 40 124.35)
    (layer "Edge.Cuts"))
  (gr_line (start 40 119) (end 40 121.15)
    (layer "Edge.Cuts"))
  (gr_line (start 125 119) (end 40 119)
    (layer "Edge.Cuts"))
  (gr_line (start 125 143) (end 125 119)
    (layer "Edge.Cuts"))
  (gr_text "P${COMMENT4}-${REVISION}\nFRONTEND\n(2022)" (at 48.6 124.2) (layer "B.Cu"))
  (gr_text "${COMMENT4}-${REVISION}" (at 106.25 123.75) (layer "F.SilkS"))
  (gr_text "100X BAL" (at 74.75 120) (layer "F.SilkS"))
  (gr_text "+" (at 105.5 126.5) (layer "F.SilkS"))
  (gr_text "2022 LOCKWOOD" (at 106.25 120.25) (layer "F.SilkS"))
  (gr_text "${TITLE}" (at 106.25 122) (layer "F.SilkS"))
  (gr_text "+" (at 105.5 141.3) (layer "F.SilkS"))
  (gr_text "JLC 2313 controlled impedance\n50 ohm single: 5.78mil\n100 ohm diff: 4.35mil/6mil sp" (at 40 112.5) (layer "Cmts.User"))
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.125))
    (polygon
      (pts
        (xy 112.8 133.6)
        (xy 113.6 133.6)
        (xy 113.6 135)
        (xy 110.6 135)
        (xy 110.6 133.6)
        (xy 111.6 133.6)
        (xy 111.6 131.4)
        (xy 112.8 131.4)
      )
    )
  )
  (zone (net 86) (net_name "/LMH_EN") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.739242 132.397634)
        (xy 110.688377 132.399205)
        (xy 110.645461 132.396938)
        (xy 110.608798 132.391255)
        (xy 110.576689 132.382583)
        (xy 110.547437 132.371344)
        (xy 110.519344 132.357963)
        (xy 110.490713 132.342866)
        (xy 110.459846 132.326476)
        (xy 110.425046 132.309218)
        (xy 110.384615 132.291517)
        (xy 110.187742 132.507361)
        (xy 110.411115 132.695648)
        (xy 110.448888 132.672818)
        (xy 110.481137 132.651163)
        (xy 110.509599 132.630883)
        (xy 110.536013 132.612176)
        (xy 110.562118 132.595242)
        (xy 110.589653 132.58028)
        (xy 110.620354 132.567488)
        (xy 110.655962 132.557067)
        (xy 110.698214 132.549214)
        (xy 110.748849 132.544131)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (name "Conformal2") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.25 141.25)
        (xy 81.5 141.25)
        (xy 81.5 128)
        (xy 85.25 128)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.939397 131.9048)
        (xy 108.889889 131.906333)
        (xy 108.846955 131.906475)
        (xy 108.80934 131.90511)
        (xy 108.77579 131.902121)
        (xy 108.745053 131.897394)
        (xy 108.715873 131.890813)
        (xy 108.686998 131.882262)
        (xy 108.657173 131.871626)
        (xy 108.625145 131.85879)
        (xy 108.589661 131.843637)
        (xy 108.387596 132.054628)
        (xy 108.606323 132.248293)
        (xy 108.640441 132.230273)
        (xy 108.671305 132.214847)
        (xy 108.700155 132.201795)
        (xy 108.728229 132.190899)
        (xy 108.756769 132.181941)
        (xy 108.787014 132.174703)
        (xy 108.820205 132.168967)
        (xy 108.85758 132.164514)
        (xy 108.900381 132.161125)
        (xy 108.949847 132.158584)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.560895 125.641583)
        (xy 109.514863 125.623295)
        (xy 109.475416 125.606345)
        (xy 109.441448 125.590129)
        (xy 109.411857 125.57404)
        (xy 109.385536 125.557476)
        (xy 109.361383 125.53983)
        (xy 109.338292 125.520498)
        (xy 109.31516 125.498875)
        (xy 109.290882 125.474356)
        (xy 109.264355 125.446338)
        (xy 108.995032 125.559531)
        (xy 109.118663 125.824224)
        (xy 109.157134 125.821265)
        (xy 109.191587 125.81939)
        (xy 109.223248 125.818892)
        (xy 109.25334 125.820064)
        (xy 109.283088 125.823199)
        (xy 109.313716 125.82859)
        (xy 109.34645 125.83653)
        (xy 109.382512 125.847313)
        (xy 109.423128 125.861231)
        (xy 109.469523 125.878578)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.655 130.6516)
        (xy 100.705022 130.652686)
        (xy 100.747687 130.655912)
        (xy 100.784476 130.661225)
        (xy 100.816871 130.668573)
        (xy 100.846353 130.677905)
        (xy 100.874404 130.689168)
        (xy 100.902505 130.702311)
        (xy 100.932138 130.717282)
        (xy 100.964784 130.734029)
        (xy 101.001925 130.7525)
        (xy 101.2125 130.55)
        (xy 101.001925 130.3475)
        (xy 100.964784 130.36597)
        (xy 100.932138 130.382717)
        (xy 100.902505 130.397688)
        (xy 100.874404 130.410831)
        (xy 100.846353 130.422094)
        (xy 100.816871 130.431426)
        (xy 100.784476 130.438774)
        (xy 100.747687 130.444087)
        (xy 100.705022 130.447313)
        (xy 100.655 130.4484)
      )
    )
  )
  (zone (net 23) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.577295 131.538344)
        (xy 115.626401 131.531875)
        (xy 115.669107 131.527447)
        (xy 115.70667 131.52505)
        (xy 115.740351 131.524674)
        (xy 115.771407 131.526309)
        (xy 115.801098 131.529944)
        (xy 115.830683 131.535569)
        (xy 115.861421 131.543174)
        (xy 115.89457 131.552749)
        (xy 115.931391 131.564284)
        (xy 116.111381 131.334173)
        (xy 115.874411 131.163313)
        (xy 115.842261 131.184648)
        (xy 115.813092 131.203079)
        (xy 115.78569 131.218946)
        (xy 115.758843 131.23259)
        (xy 115.73134 131.244352)
        (xy 115.701969 131.254574)
        (xy 115.669517 131.263596)
        (xy 115.632773 131.271758)
        (xy 115.590524 131.279403)
        (xy 115.54156 131.286871)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.705 137.0516)
        (xy 100.755022 137.052686)
        (xy 100.797687 137.055912)
        (xy 100.834476 137.061225)
        (xy 100.866871 137.068573)
        (xy 100.896353 137.077905)
        (xy 100.924404 137.089168)
        (xy 100.952505 137.102311)
        (xy 100.982138 137.117282)
        (xy 101.014784 137.134029)
        (xy 101.051925 137.1525)
        (xy 101.2625 136.95)
        (xy 101.051925 136.7475)
        (xy 101.014784 136.76597)
        (xy 100.982138 136.782717)
        (xy 100.952505 136.797688)
        (xy 100.924404 136.810831)
        (xy 100.896353 136.822094)
        (xy 100.866871 136.831426)
        (xy 100.834476 136.838774)
        (xy 100.797687 136.844087)
        (xy 100.755022 136.847313)
        (xy 100.705 136.8484)
      )
    )
  )
  (zone (net 29) (net_name "/SIG_IN_{1}") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.197267 129.472455)
        (xy 48.064784 129.373063)
        (xy 47.967068 129.276655)
        (xy 47.897171 129.18152)
        (xy 47.848147 129.085948)
        (xy 47.81305 128.988229)
        (xy 47.784933 128.886653)
        (xy 47.75685 128.779508)
        (xy 47.721854 128.665084)
        (xy 47.672999 128.541672)
        (xy 47.603338 128.407561)
        (xy 46.708783 128.568355)
        (xy 46.904417 129.455943)
        (xy 47.055005 129.468664)
        (xy 47.187714 129.466295)
        (xy 47.306796 129.45459)
        (xy 47.4165 129.439303)
        (xy 47.521077 129.426189)
        (xy 47.624778 129.421002)
        (xy 47.731853 129.429496)
        (xy 47.846553 129.457426)
        (xy 47.973128 129.510546)
        (xy 48.11583 129.59461)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.995 136.8484)
        (xy 98.944977 136.847313)
        (xy 98.902312 136.844087)
        (xy 98.865523 136.838774)
        (xy 98.833128 136.831426)
        (xy 98.803646 136.822094)
        (xy 98.775595 136.810831)
        (xy 98.747494 136.797688)
        (xy 98.717861 136.782717)
        (xy 98.685215 136.76597)
        (xy 98.648075 136.7475)
        (xy 98.4375 136.95)
        (xy 98.648075 137.1525)
        (xy 98.685215 137.134029)
        (xy 98.717861 137.117282)
        (xy 98.747494 137.102311)
        (xy 98.775595 137.089168)
        (xy 98.803646 137.077905)
        (xy 98.833128 137.068573)
        (xy 98.865523 137.061225)
        (xy 98.902312 137.055912)
        (xy 98.944977 137.052686)
        (xy 98.995 137.0516)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.695 128.3984)
        (xy 99.644977 128.397313)
        (xy 99.602312 128.394087)
        (xy 99.565523 128.388774)
        (xy 99.533128 128.381426)
        (xy 99.503646 128.372094)
        (xy 99.475595 128.360831)
        (xy 99.447494 128.347688)
        (xy 99.417861 128.332717)
        (xy 99.385215 128.31597)
        (xy 99.348075 128.2975)
        (xy 99.1375 128.5)
        (xy 99.348075 128.7025)
        (xy 99.385215 128.684029)
        (xy 99.417861 128.667282)
        (xy 99.447494 128.652311)
        (xy 99.475595 128.639168)
        (xy 99.503646 128.627905)
        (xy 99.533128 128.618573)
        (xy 99.565523 128.611225)
        (xy 99.602312 128.605912)
        (xy 99.644977 128.602686)
        (xy 99.695 128.6016)
      )
    )
  )
  (zone (net 36) (net_name "/OFFSET1") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.673 127.855)
        (xy 97.672495 127.904528)
        (xy 97.67087 127.947432)
        (xy 97.667959 127.984959)
        (xy 97.663592 128.018357)
        (xy 97.657605 128.048875)
        (xy 97.649829 128.077759)
        (xy 97.640097 128.106258)
        (xy 97.628243 128.135621)
        (xy 97.6141 128.167093)
        (xy 97.5975 128.201925)
        (xy 97.8 128.4125)
        (xy 98.0025 128.201925)
        (xy 97.985899 128.167093)
        (xy 97.971756 128.135621)
        (xy 97.959902 128.106258)
        (xy 97.95017 128.077759)
        (xy 97.942394 128.048875)
        (xy 97.936407 128.018357)
        (xy 97.93204 127.984959)
        (xy 97.929129 127.947432)
        (xy 97.927504 127.904528)
        (xy 97.927 127.855)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.748785 125.833268)
        (xy 96.756756 125.882153)
        (xy 96.762491 125.924703)
        (xy 96.766038 125.962175)
        (xy 96.767447 125.995828)
        (xy 96.766765 126.02692)
        (xy 96.764043 126.056708)
        (xy 96.759327 126.086451)
        (xy 96.752668 126.117408)
        (xy 96.744114 126.150835)
        (xy 96.733714 126.187992)
        (xy 96.969234 126.360843)
        (xy 97.132749 126.118746)
        (xy 97.110437 126.087266)
        (xy 97.091121 126.058675)
        (xy 97.074421 126.031772)
        (xy 97.05996 126.005356)
        (xy 97.04736 125.978227)
        (xy 97.036243 125.949182)
        (xy 97.026231 125.917022)
        (xy 97.016945 125.880546)
        (xy 97.008009 125.838551)
        (xy 96.999044 125.789839)
      )
    )
  )
  (zone (net 15) (net_name "/VFILT'") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.614665 135.81519)
        (xy 112.593494 135.768913)
        (xy 112.578944 135.728476)
        (xy 112.569967 135.692477)
        (xy 112.565512 135.659518)
        (xy 112.56453 135.628196)
        (xy 112.565971 135.597113)
        (xy 112.568786 135.564868)
        (xy 112.571926 135.530061)
        (xy 112.574341 135.491292)
        (xy 112.574982 135.447161)
        (xy 112.299689 135.349377)
        (xy 112.212739 135.628281)
        (xy 112.248428 135.654247)
        (xy 112.280892 135.675577)
        (xy 112.310621 135.69395)
        (xy 112.338106 135.711045)
        (xy 112.363838 135.728542)
        (xy 112.388305 135.74812)
        (xy 112.412 135.771461)
        (xy 112.435413 135.800242)
        (xy 112.459033 135.836144)
        (xy 112.483352 135.880847)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (name "PadsNearEdge1") (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.2) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.75 133.75)
        (xy 39.75 133.75)
        (xy 39.75 126)
        (xy 44.75 126)
      )
    )
  )
  (zone (net 14) (net_name "Net-(C13-Pad2)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.397105 135.840434)
        (xy 111.396141 135.789553)
        (xy 111.398922 135.746668)
        (xy 111.405042 135.710075)
        (xy 111.414099 135.678073)
        (xy 111.425687 135.648957)
        (xy 111.439402 135.621026)
        (xy 111.454841 135.592578)
        (xy 111.471599 135.561909)
        (xy 111.489272 135.527318)
        (xy 111.507456 135.487102)
        (xy 111.293983 135.287662)
        (xy 111.103037 135.508766)
        (xy 111.125412 135.546809)
        (xy 111.14668 135.579315)
        (xy 111.166618 135.608017)
        (xy 111.185008 135.634654)
        (xy 111.201628 135.66096)
        (xy 111.216261 135.688671)
        (xy 111.228684 135.719523)
        (xy 111.238679 135.755253)
        (xy 111.246026 135.797596)
        (xy 111.250504 135.848288)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.765307 140.307224)
        (xy 107.812608 140.29253)
        (xy 107.853946 140.280932)
        (xy 107.890561 140.272207)
        (xy 107.923691 140.266132)
        (xy 107.954575 140.262482)
        (xy 107.984453 140.261035)
        (xy 108.014563 140.261567)
        (xy 108.046144 140.263856)
        (xy 108.080437 140.267677)
        (xy 108.118679 140.272809)
        (xy 108.25709 140.015535)
        (xy 107.994603 139.887284)
        (xy 107.966532 139.913756)
        (xy 107.940906 139.936862)
        (xy 107.916587 139.957141)
        (xy 107.89244 139.975136)
        (xy 107.867327 139.991387)
        (xy 107.840111 140.006436)
        (xy 107.809656 140.020824)
        (xy 107.774826 140.035093)
        (xy 107.734483 140.049784)
        (xy 107.687491 140.065438)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.163276 136.849054)
        (xy 98.199923 136.852518)
        (xy 98.229627 136.861035)
        (xy 98.253468 136.874071)
        (xy 98.272526 136.891089)
        (xy 98.287881 136.911555)
        (xy 98.300613 136.934933)
        (xy 98.311802 136.960688)
        (xy 98.322529 136.988284)
        (xy 98.333874 137.017186)
        (xy 98.346916 137.046859)
        (xy 98.637847 137.020277)
        (xy 98.554218 136.72504)
        (xy 98.509462 136.722187)
        (xy 98.470896 136.716001)
        (xy 98.436702 136.707308)
        (xy 98.405061 136.696937)
        (xy 98.374158 136.685718)
        (xy 98.342174 136.674478)
        (xy 98.307292 136.664047)
        (xy 98.267694 136.655253)
        (xy 98.221564 136.648924)
        (xy 98.167085 136.64589)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.845 130.4984)
        (xy 103.794977 130.497313)
        (xy 103.752312 130.494087)
        (xy 103.715523 130.488774)
        (xy 103.683128 130.481426)
        (xy 103.653646 130.472094)
        (xy 103.625595 130.460831)
        (xy 103.597494 130.447688)
        (xy 103.567861 130.432717)
        (xy 103.535215 130.41597)
        (xy 103.498075 130.3975)
        (xy 103.2875 130.6)
        (xy 103.498075 130.8025)
        (xy 103.535215 130.784029)
        (xy 103.567861 130.767282)
        (xy 103.597494 130.752311)
        (xy 103.625595 130.739168)
        (xy 103.653646 130.727905)
        (xy 103.683128 130.718573)
        (xy 103.715523 130.711225)
        (xy 103.752312 130.705912)
        (xy 103.794977 130.702686)
        (xy 103.845 130.7016)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.051719 130.635972)
        (xy 98.101672 130.638807)
        (xy 98.144198 130.643524)
        (xy 98.180779 130.65012)
        (xy 98.212897 130.658597)
        (xy 98.242035 130.668954)
        (xy 98.269674 130.681191)
        (xy 98.297299 130.695309)
        (xy 98.326389 130.711307)
        (xy 98.35843 130.729186)
        (xy 98.394902 130.748945)
        (xy 98.612431 130.553934)
        (xy 98.409068 130.344194)
        (xy 98.371304 130.361354)
        (xy 98.338092 130.376949)
        (xy 98.307954 130.390874)
        (xy 98.27941 130.403026)
        (xy 98.250983 130.413301)
        (xy 98.221192 130.421595)
        (xy 98.18856 130.427806)
        (xy 98.151608 130.431829)
        (xy 98.108856 130.43356)
        (xy 98.058827 130.432897)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63.051348 140.910955)
        (xy 63.083445 140.872573)
        (xy 63.112616 140.841272)
        (xy 63.139747 140.815863)
        (xy 63.165722 140.795158)
        (xy 63.191426 140.777965)
        (xy 63.217744 140.763097)
        (xy 63.245561 140.749365)
        (xy 63.275763 140.735578)
        (xy 63.309234 140.720547)
        (xy 63.346859 140.703084)
        (xy 63.320277 140.412153)
        (xy 63.030607 140.450084)
        (xy 63.021828 140.490624)
        (xy 63.014512 140.526578)
        (xy 63.007691 140.559069)
        (xy 63.000399 140.589223)
        (xy 62.991671 140.618162)
        (xy 62.980541 140.647013)
        (xy 62.966042 140.6769)
        (xy 62.947209 140.708946)
        (xy 62.923075 140.744277)
        (xy 62.892676 140.784017)
      )
    )
  )
  (zone (net 23) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.632201 122.152477)
        (xy 90.630675 122.201984)
        (xy 90.628166 122.244845)
        (xy 90.624482 122.282305)
        (xy 90.619428 122.315606)
        (xy 90.612812 122.345993)
        (xy 90.604442 122.374711)
        (xy 90.594125 122.403004)
        (xy 90.581669 122.432115)
        (xy 90.566879 122.46329)
        (xy 90.549565 122.497772)
        (xy 90.747681 122.712476)
        (xy 90.954478 122.50612)
        (xy 90.938599 122.470954)
        (xy 90.925107 122.439196)
        (xy 90.913861 122.409596)
        (xy 90.904719 122.380902)
        (xy 90.89754 122.351864)
        (xy 90.892183 122.321229)
        (xy 90.888506 122.287748)
        (xy 90.886369 122.250169)
        (xy 90.885629 122.207241)
        (xy 90.886146 122.157713)
      )
    )
  )
  (zone (net 28) (net_name "/THERM") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.844828 134.479265)
        (xy 116.872792 134.437774)
        (xy 116.898577 134.40363)
        (xy 116.92294 134.375556)
        (xy 116.946639 134.35228)
        (xy 116.970431 134.332527)
        (xy 116.995074 134.315021)
        (xy 117.021325 134.29849)
        (xy 117.049942 134.28166)
        (xy 117.081682 134.263254)
        (xy 117.117304 134.242001)
        (xy 117.060835 133.955368)
        (xy 116.776627 134.022996)
        (xy 116.77208 134.064226)
        (xy 116.768513 134.100743)
        (xy 116.765082 134.133764)
        (xy 116.760942 134.164509)
        (xy 116.755248 134.194196)
        (xy 116.747155 134.224041)
        (xy 116.735818 134.255265)
        (xy 116.720393 134.289084)
        (xy 116.700035 134.326717)
        (xy 116.6739 134.369383)
      )
    )
  )
  (zone (net 28) (net_name "/THERM") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45.776832 141.54265)
        (xy 45.819895 141.569583)
        (xy 45.854349 141.595215)
        (xy 45.881807 141.620151)
        (xy 45.903882 141.644995)
        (xy 45.922185 141.670351)
        (xy 45.938329 141.696823)
        (xy 45.953926 141.725015)
        (xy 45.970589 141.755533)
        (xy 45.989931 141.788981)
        (xy 46.013564 141.825962)
        (xy 46.297315 141.756443)
        (xy 46.21676 141.475626)
        (xy 46.172925 141.473475)
        (xy 46.134289 141.473295)
        (xy 46.099525 141.473985)
        (xy 46.067308 141.474446)
        (xy 46.036314 141.473577)
        (xy 46.005217 141.470281)
        (xy 45.972691 141.463456)
        (xy 45.937412 141.452004)
        (xy 45.898055 141.434825)
        (xy 45.853294 141.41082)
      )
    )
  )
  (zone (net 91) (net_name "Net-(R70-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.571039 141.65601)
        (xy 66.620809 141.650883)
        (xy 66.663545 141.648792)
        (xy 66.700709 141.649501)
        (xy 66.733765 141.652774)
        (xy 66.764177 141.658377)
        (xy 66.793408 141.666074)
        (xy 66.822922 141.67563)
        (xy 66.854183 141.68681)
        (xy 66.888654 141.699378)
        (xy 66.927799 141.7131)
        (xy 67.111631 141.486047)
        (xy 66.877566 141.311229)
        (xy 66.843003 141.334163)
        (xy 66.812686 141.35483)
        (xy 66.785139 141.373361)
        (xy 66.758885 141.389887)
        (xy 66.732448 141.404543)
        (xy 66.704351 141.417459)
        (xy 66.673118 141.428769)
        (xy 66.637271 141.438604)
        (xy 66.595336 141.447097)
        (xy 66.545835 141.45438)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.129045 127.300594)
        (xy 96.141865 127.348957)
        (xy 96.15059 127.390845)
        (xy 96.155682 127.427665)
        (xy 96.1576 127.460828)
        (xy 96.156805 127.491741)
        (xy 96.153757 127.521814)
        (xy 96.148918 127.552457)
        (xy 96.142746 127.585078)
        (xy 96.135704 127.621086)
        (xy 96.128251 127.661892)
        (xy 96.38118 127.808092)
        (xy 96.517384 127.549643)
        (xy 96.489342 127.519076)
        (xy 96.464204 127.492351)
        (xy 96.441606 127.468028)
        (xy 96.42119 127.444671)
        (xy 96.402593 127.420841)
        (xy 96.385456 127.3951)
        (xy 96.369417 127.366011)
        (xy 96.354116 127.332136)
        (xy 96.339191 127.292036)
        (xy 96.324283 127.244275)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.566284 131.271983)
        (xy 84.551479 131.319491)
        (xy 84.538511 131.362836)
        (xy 84.526848 131.402311)
        (xy 84.515958 131.438208)
        (xy 84.505307 131.47082)
        (xy 84.494364 131.500441)
        (xy 84.482596 131.527364)
        (xy 84.469472 131.551882)
        (xy 84.454459 131.574288)
        (xy 84.437025 131.594875)
        (xy 84.565713 131.857147)
        (xy 84.822756 131.718308)
        (xy 84.820512 131.691424)
        (xy 84.821295 131.664464)
        (xy 84.824843 131.636882)
        (xy 84.830891 131.60813)
        (xy 84.839178 131.577658)
        (xy 84.849439 131.544921)
        (xy 84.861411 131.509371)
        (xy 84.874832 131.470459)
        (xy 84.889437 131.427638)
        (xy 84.904965 131.380361)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.541422 138.148689)
        (xy 106.501055 138.178251)
        (xy 106.465228 138.201641)
        (xy 106.432795 138.219801)
        (xy 106.402612 138.233672)
        (xy 106.373535 138.244197)
        (xy 106.344419 138.252319)
        (xy 106.31412 138.258978)
        (xy 106.281493 138.265119)
        (xy 106.245395 138.271683)
        (xy 106.20468 138.279612)
        (xy 106.160703 138.568426)
        (xy 106.451016 138.601081)
        (xy 106.469261 138.563829)
        (xy 106.484988 138.53068)
        (xy 106.499403 138.500773)
        (xy 106.513714 138.473249)
        (xy 106.529129 138.447247)
        (xy 106.546854 138.421908)
        (xy 106.568098 138.396372)
        (xy 106.594068 138.369778)
        (xy 106.625971 138.341268)
        (xy 106.665016 138.30998)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.907565 138.870858)
        (xy 100.940114 138.833524)
        (xy 100.969214 138.801955)
        (xy 100.9958 138.77531)
        (xy 101.020811 138.75275)
        (xy 101.045183 138.733433)
        (xy 101.069855 138.716519)
        (xy 101.095764 138.701169)
        (xy 101.123847 138.68654)
        (xy 101.155042 138.671794)
        (xy 101.190286 138.65609)
        (xy 101.173063 138.364455)
        (xy 100.882324 138.393063)
        (xy 100.872325 138.430329)
        (xy 100.86264 138.463446)
        (xy 100.852585 138.493472)
        (xy 100.841476 138.521463)
        (xy 100.828629 138.548476)
        (xy 100.813363 138.57557)
        (xy 100.794992 138.603802)
        (xy 100.772834 138.634228)
        (xy 100.746205 138.667908)
        (xy 100.714423 138.705897)
      )
    )
  )
  (zone (net 44) (net_name "/SIG_50") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53.286844 138.522275)
        (xy 53.439387 138.586779)
        (xy 53.557471 138.656772)
        (xy 53.64825 138.73224)
        (xy 53.718878 138.813166)
        (xy 53.776508 138.899535)
        (xy 53.828294 138.991331)
        (xy 53.88139 139.08854)
        (xy 53.942951 139.191144)
        (xy 54.02013 139.29913)
        (xy 54.120082 139.412481)
        (xy 54.949446 139.040674)
        (xy 54.54551 138.226475)
        (xy 54.396299 138.250449)
        (xy 54.268078 138.284757)
        (xy 54.155335 138.324838)
        (xy 54.052557 138.366133)
        (xy 53.954229 138.404083)
        (xy 53.854841 138.434128)
        (xy 53.748878 138.451711)
        (xy 53.630828 138.45227)
        (xy 53.495177 138.431247)
        (xy 53.336414 138.384084)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.154475 139.975145)
        (xy 86.204001 139.975855)
        (xy 86.246897 139.977659)
        (xy 86.284412 139.980727)
        (xy 86.317792 139.985232)
        (xy 86.348284 139.991347)
        (xy 86.377136 139.999243)
        (xy 86.405595 140.009093)
        (xy 86.434907 140.021069)
        (xy 86.466321 140.035343)
        (xy 86.501083 140.052089)
        (xy 86.712499 139.850468)
        (xy 86.502769 139.647094)
        (xy 86.467869 139.663549)
        (xy 86.436337 139.677561)
        (xy 86.406926 139.689293)
        (xy 86.378387 139.698905)
        (xy 86.349471 139.706561)
        (xy 86.318929 139.712421)
        (xy 86.285512 139.716648)
        (xy 86.247974 139.719404)
        (xy 86.205063 139.72085)
        (xy 86.155534 139.721148)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.899598 131.340389)
        (xy 108.850126 131.33796)
        (xy 108.807318 131.334669)
        (xy 108.769932 131.330301)
        (xy 108.736729 131.324641)
        (xy 108.706467 131.317472)
        (xy 108.677907 131.308579)
        (xy 108.649807 131.297748)
        (xy 108.620928 131.284762)
        (xy 108.590029 131.269406)
        (xy 108.55587 131.251465)
        (xy 108.337585 131.445629)
        (xy 108.540132 131.656158)
        (xy 108.575581 131.640923)
        (xy 108.60758 131.628013)
        (xy 108.63738 131.617309)
        (xy 108.666236 131.608693)
        (xy 108.6954 131.602045)
        (xy 108.726127 131.597248)
        (xy 108.75967 131.594183)
        (xy 108.797282 131.592731)
        (xy 108.840216 131.592775)
        (xy 108.889727 131.594196)
      )
    )
  )
  (zone (net 92) (net_name "Net-(R72-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.454292 141.294336)
        (xy 58.40718 141.277486)
        (xy 58.367724 141.260934)
        (xy 58.334503 141.24426)
        (xy 58.306094 141.227044)
        (xy 58.281076 141.208868)
        (xy 58.258027 141.189313)
        (xy 58.235524 141.167958)
        (xy 58.212146 141.144385)
        (xy 58.186471 141.118174)
        (xy 58.157078 141.088906)
        (xy 57.893274 141.214425)
        (xy 58.029006 141.473122)
        (xy 58.070081 141.467343)
        (xy 58.106348 141.46178)
        (xy 58.139194 141.456948)
        (xy 58.170009 141.453366)
        (xy 58.200182 141.451551)
        (xy 58.231102 141.452021)
        (xy 58.264158 141.455294)
        (xy 58.30074 141.461887)
        (xy 58.342235 141.472319)
        (xy 58.390035 141.487107)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.25) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 100.8 137.8)
        (xy 96.7 137.8)
        (xy 96.7 137.1)
        (xy 100.8 137.1)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.127 124.195)
        (xy 89.127504 124.145471)
        (xy 89.129129 124.102567)
        (xy 89.13204 124.06504)
        (xy 89.136407 124.031642)
        (xy 89.142394 124.001124)
        (xy 89.15017 123.97224)
        (xy 89.159902 123.943741)
        (xy 89.171756 123.914378)
        (xy 89.185899 123.882906)
        (xy 89.2025 123.848075)
        (xy 89 123.6375)
        (xy 88.7975 123.848075)
        (xy 88.8141 123.882906)
        (xy 88.828243 123.914378)
        (xy 88.840097 123.943741)
        (xy 88.849829 123.97224)
        (xy 88.857605 124.001124)
        (xy 88.863592 124.031642)
        (xy 88.867959 124.06504)
        (xy 88.87087 124.102567)
        (xy 88.872495 124.145471)
        (xy 88.873 124.195)
      )
    )
  )
  (zone (net 32) (net_name "/OUT2+") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.662976 126.047984)
        (xy 112.609849 126.038821)
        (xy 112.565357 126.028557)
        (xy 112.527676 126.017118)
        (xy 112.494985 126.004431)
        (xy 112.465461 125.990424)
        (xy 112.437283 125.975024)
        (xy 112.408629 125.958158)
        (xy 112.377676 125.939754)
        (xy 112.342603 125.919739)
        (xy 112.301588 125.89804)
        (xy 112.087518 126.09684)
        (xy 112.294531 126.302978)
        (xy 112.333542 126.283366)
        (xy 112.367308 126.264)
        (xy 112.397434 126.245506)
        (xy 112.425528 126.228512)
        (xy 112.453195 126.213645)
        (xy 112.482043 126.201534)
        (xy 112.513679 126.192806)
        (xy 112.549708 126.188089)
        (xy 112.591738 126.18801)
        (xy 112.641376 126.193198)
      )
    )
  )
  (zone (net 34) (net_name "/OUT3+") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.671166 127.660287)
        (xy 112.617441 127.64542)
        (xy 112.572355 127.631208)
        (xy 112.53406 127.617291)
        (xy 112.500711 127.603307)
        (xy 112.470462 127.588895)
        (xy 112.441467 127.573696)
        (xy 112.41188 127.557347)
        (xy 112.379854 127.539488)
        (xy 112.343544 127.519758)
        (xy 112.301104 127.497796)
        (xy 112.087513 127.697111)
        (xy 112.295023 127.902749)
        (xy 112.333061 127.883279)
        (xy 112.366269 127.8636)
        (xy 112.396113 127.844576)
        (xy 112.42406 127.82707)
        (xy 112.451578 127.811948)
        (xy 112.480134 127.800073)
        (xy 112.511195 127.79231)
        (xy 112.546228 127.789524)
        (xy 112.5867 127.792578)
        (xy 112.63408 127.802337)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.25) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 93.85 141.95)
        (xy 92.45 141.95)
        (xy 92.45 141.25)
        (xy 93.45 140.55)
        (xy 93.85 140.55)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.045 133.676594)
        (xy 102.994141 133.674834)
        (xy 102.951465 133.669763)
        (xy 102.915252 133.661694)
        (xy 102.883779 133.650938)
        (xy 102.855325 133.63781)
        (xy 102.828168 133.62262)
        (xy 102.800586 133.605681)
        (xy 102.770858 133.587307)
        (xy 102.737261 133.567809)
        (xy 102.698075 133.5475)
        (xy 102.4875 133.75)
        (xy 102.698075 133.9525)
        (xy 102.737261 133.93219)
        (xy 102.770858 133.912692)
        (xy 102.800586 133.894318)
        (xy 102.828168 133.877379)
        (xy 102.855325 133.862189)
        (xy 102.883779 133.849061)
        (xy 102.915252 133.838305)
        (xy 102.951465 133.830236)
        (xy 102.994141 133.825165)
        (xy 103.045 133.823406)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.25) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 105.9 138.1)
        (xy 105.3 139.1)
        (xy 104.2 139.1)
        (xy 103.6 138.1)
        (xy 103.6 137.1)
        (xy 105.9 137.1)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.25) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 85.9 141.95)
        (xy 81.5 141.95)
        (xy 81.5 140.65)
        (xy 85.9 140.65)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.091789 130.735798)
        (xy 92.060334 130.774708)
        (xy 92.031687 130.806489)
        (xy 92.004983 130.832346)
        (xy 91.979356 130.853481)
        (xy 91.953942 130.871098)
        (xy 91.927875 130.886402)
        (xy 91.90029 130.900595)
        (xy 91.870322 130.914883)
        (xy 91.837106 130.930468)
        (xy 91.799777 130.948555)
        (xy 91.831193 131.239004)
        (xy 92.120193 131.19626)
        (xy 92.128295 131.155578)
        (xy 92.135013 131.119508)
        (xy 92.141292 131.086908)
        (xy 92.148081 131.056637)
        (xy 92.156327 131.027556)
        (xy 92.166976 130.998524)
        (xy 92.180975 130.968401)
        (xy 92.199273 130.936046)
        (xy 92.222816 130.900318)
        (xy 92.252551 130.860079)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.763963 123.006439)
        (xy 95.798496 123.042644)
        (xy 95.826321 123.075147)
        (xy 95.848521 123.104961)
        (xy 95.866177 123.133097)
        (xy 95.880373 123.16057)
        (xy 95.89219 123.188391)
        (xy 95.902711 123.217575)
        (xy 95.913018 123.249135)
        (xy 95.924194 123.284082)
        (xy 95.93732 123.323431)
        (xy 96.229396 123.329702)
        (xy 96.224247 123.037604)
        (xy 96.184949 123.024327)
        (xy 96.150045 123.013017)
        (xy 96.118525 123.002589)
        (xy 96.089382 122.991956)
        (xy 96.061606 122.980032)
        (xy 96.034188 122.965731)
        (xy 96.006119 122.947967)
        (xy 95.976392 122.925652)
        (xy 95.943996 122.897702)
        (xy 95.907923 122.863031)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.945 130.4484)
        (xy 98.894977 130.447313)
        (xy 98.852312 130.444087)
        (xy 98.815523 130.438774)
        (xy 98.783128 130.431426)
        (xy 98.753646 130.422094)
        (xy 98.725595 130.410831)
        (xy 98.697494 130.397688)
        (xy 98.667861 130.382717)
        (xy 98.635215 130.36597)
        (xy 98.598075 130.3475)
        (xy 98.3875 130.55)
        (xy 98.598075 130.7525)
        (xy 98.635215 130.734029)
        (xy 98.667861 130.717282)
        (xy 98.697494 130.702311)
        (xy 98.725595 130.689168)
        (xy 98.753646 130.677905)
        (xy 98.783128 130.668573)
        (xy 98.815523 130.661225)
        (xy 98.852312 130.655912)
        (xy 98.894977 130.652686)
        (xy 98.945 130.6516)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.500402 132.159611)
        (xy 115.549873 132.162039)
        (xy 115.592681 132.16533)
        (xy 115.630067 132.169698)
        (xy 115.66327 132.175358)
        (xy 115.693532 132.182527)
        (xy 115.722092 132.19142)
        (xy 115.750192 132.202251)
        (xy 115.779071 132.215237)
        (xy 115.80997 132.230593)
        (xy 115.84413 132.248535)
        (xy 116.062415 132.054371)
        (xy 115.859868 131.843842)
        (xy 115.824418 131.859076)
        (xy 115.792419 131.871986)
        (xy 115.762619 131.88269)
        (xy 115.733763 131.891306)
        (xy 115.704599 131.897954)
        (xy 115.673872 131.902751)
        (xy 115.640329 131.905816)
        (xy 115.602717 131.907268)
        (xy 115.559783 131.907224)
        (xy 115.510273 131.905804)
      )
    )
  )
  (zone (net 35) (net_name "/OUT3-") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.709788 128.397128)
        (xy 111.764662 128.387141)
        (xy 111.811624 128.383671)
        (xy 111.852331 128.385993)
        (xy 111.888443 128.393383)
        (xy 111.921621 128.405115)
        (xy 111.953524 128.420463)
        (xy 111.985812 128.438704)
        (xy 112.020143 128.459112)
        (xy 112.058179 128.480963)
        (xy 112.101578 128.503531)
        (xy 112.312499 128.301392)
        (xy 112.102272 128.098533)
        (xy 112.054155 128.121868)
        (xy 112.012608 128.142024)
        (xy 111.975636 128.159542)
        (xy 111.941242 128.174966)
        (xy 111.907431 128.188839)
        (xy 111.872207 128.201705)
        (xy 111.833575 128.214107)
        (xy 111.78954 128.226589)
        (xy 111.738104 128.239692)
        (xy 111.677274 128.253962)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.25) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 87.45 141.3)
        (xy 87.45 141.95)
        (xy 86.1 141.95)
        (xy 86.1 140.65)
        (xy 86.55 140.65)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.651869 140.650754)
        (xy 89.631561 140.605577)
        (xy 89.615048 140.565944)
        (xy 89.601958 140.530654)
        (xy 89.59192 140.498502)
        (xy 89.584561 140.468286)
        (xy 89.57951 140.438802)
        (xy 89.576396 140.408849)
        (xy 89.574848 140.377222)
        (xy 89.574493 140.342719)
        (xy 89.574961 140.304138)
        (xy 89.302834 140.197866)
        (xy 89.207277 140.473939)
        (xy 89.236951 140.498601)
        (xy 89.262986 140.521244)
        (xy 89.286058 140.54293)
        (xy 89.306842 140.564724)
        (xy 89.326011 140.587687)
        (xy 89.344242 140.612882)
        (xy 89.362208 140.641372)
        (xy 89.380586 140.674221)
        (xy 89.400048 140.712491)
        (xy 89.421272 140.757245)
      )
    )
  )
  (zone (net 11) (net_name "Net-(C12-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.88641 135.215968)
        (xy 114.923695 135.181334)
        (xy 114.957517 135.154821)
        (xy 114.988875 135.134991)
        (xy 115.018767 135.12041)
        (xy 115.048196 135.10964)
        (xy 115.078159 135.101246)
        (xy 115.109656 135.093792)
        (xy 115.143688 135.085841)
        (xy 115.181254 135.075958)
        (xy 115.223354 135.062706)
        (xy 115.22973 134.770632)
        (xy 114.937631 134.775677)
        (xy 114.924187 134.817715)
        (xy 114.914132 134.855236)
        (xy 114.906026 134.889231)
        (xy 114.898428 134.920695)
        (xy 114.889898 134.950619)
        (xy 114.878994 134.979998)
        (xy 114.864277 135.009824)
        (xy 114.844305 135.041091)
        (xy 114.817637 135.074792)
        (xy 114.782835 135.11192)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.25) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 99.35 141.95)
        (xy 94.1 141.95)
        (xy 94.1 140.55)
        (xy 95.2 139.75)
        (xy 99.35 139.75)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.377 124.595)
        (xy 82.377504 124.545471)
        (xy 82.379129 124.502567)
        (xy 82.38204 124.46504)
        (xy 82.386407 124.431642)
        (xy 82.392394 124.401124)
        (xy 82.40017 124.37224)
        (xy 82.409902 124.343741)
        (xy 82.421756 124.314378)
        (xy 82.435899 124.282906)
        (xy 82.4525 124.248075)
        (xy 82.25 124.0375)
        (xy 82.0475 124.248075)
        (xy 82.0641 124.282906)
        (xy 82.078243 124.314378)
        (xy 82.090097 124.343741)
        (xy 82.099829 124.37224)
        (xy 82.107605 124.401124)
        (xy 82.113592 124.431642)
        (xy 82.117959 124.46504)
        (xy 82.12087 124.502567)
        (xy 82.122495 124.545471)
        (xy 82.123 124.595)
      )
    )
  )
  (zone (net 30) (net_name "/OUT1+") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.665531 124.494667)
        (xy 112.612049 124.487812)
        (xy 112.56722 124.479185)
        (xy 112.529227 124.468809)
        (xy 112.496252 124.456711)
        (xy 112.466479 124.442915)
        (xy 112.438092 124.427448)
        (xy 112.409272 124.410333)
        (xy 112.378205 124.391598)
        (xy 112.343072 124.371265)
        (xy 112.302057 124.349363)
        (xy 112.087522 124.547662)
        (xy 112.294054 124.754283)
        (xy 112.334186 124.734404)
        (xy 112.368852 124.715072)
        (xy 112.399728 124.69679)
        (xy 112.428491 124.680064)
        (xy 112.456819 124.665401)
        (xy 112.486388 124.653306)
        (xy 112.518877 124.644285)
        (xy 112.555962 124.638842)
        (xy 112.599321 124.637485)
        (xy 112.650631 124.640719)
      )
    )
  )
  (zone (net 23) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.504918 129.698105)
        (xy 97.484217 129.653107)
        (xy 97.467359 129.613621)
        (xy 97.453961 129.578446)
        (xy 97.443642 129.546383)
        (xy 97.43602 129.516232)
        (xy 97.430713 129.486794)
        (xy 97.427338 129.456869)
        (xy 97.425514 129.425257)
        (xy 97.424858 129.390759)
        (xy 97.424989 129.352175)
        (xy 97.151944 129.248281)
        (xy 97.0588 129.525178)
        (xy 97.088688 129.54958)
        (xy 97.11492 129.571995)
        (xy 97.138181 129.593479)
        (xy 97.159153 129.615091)
        (xy 97.178523 129.637885)
        (xy 97.196973 129.662921)
        (xy 97.215187 129.691253)
        (xy 97.23385 129.72394)
        (xy 97.253646 129.762039)
        (xy 97.27526 129.806606)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.058801 131.369422)
        (xy 85.072583 131.417237)
        (xy 85.085607 131.460564)
        (xy 85.097591 131.499942)
        (xy 85.108251 131.535908)
        (xy 85.117304 131.569)
        (xy 85.124467 131.599754)
        (xy 85.129457 131.62871)
        (xy 85.13199 131.656403)
        (xy 85.131784 131.683373)
        (xy 85.128556 131.710157)
        (xy 85.380333 131.858333)
        (xy 85.518556 131.600958)
        (xy 85.501888 131.579745)
        (xy 85.487707 131.556803)
        (xy 85.475491 131.531821)
        (xy 85.464719 131.504484)
        (xy 85.45487 131.474482)
        (xy 85.445423 131.4415)
        (xy 85.435857 131.405228)
        (xy 85.42565 131.365352)
        (xy 85.414281 131.321561)
        (xy 85.40123 131.273541)
      )
    )
  )
  (zone (net 29) (net_name "/SIG_IN_{1}") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45.283185 129.984749)
        (xy 45.536392 129.90646)
        (xy 45.749109 129.837784)
        (xy 45.93084 129.777181)
        (xy 46.091093 129.723109)
        (xy 46.239373 129.674028)
        (xy 46.385187 129.628398)
        (xy 46.53804 129.584678)
        (xy 46.707439 129.541327)
        (xy 46.90289 129.496806)
        (xy 47.1339 129.449573)
        (xy 47.28 128.552501)
        (xy 46.377903 128.441574)
        (xy 46.280048 128.646991)
        (xy 46.20141 128.836064)
        (xy 46.133461 129.009493)
        (xy 46.067672 129.167978)
        (xy 45.995516 129.312217)
        (xy 45.908462 129.44291)
        (xy 45.797983 129.560757)
        (xy 45.655551 129.666458)
        (xy 45.472636 129.760711)
        (xy 45.240711 129.844217)
      )
    )
  )
  (zone (net 23) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.092748 129.16271)
        (xy 105.107567 129.115447)
        (xy 105.121542 129.074851)
        (xy 105.135192 129.039773)
        (xy 105.149039 129.009068)
        (xy 105.163604 128.981591)
        (xy 105.179409 128.956194)
        (xy 105.196973 128.931732)
        (xy 105.216819 128.907058)
        (xy 105.239467 128.881027)
        (xy 105.26544 128.852493)
        (xy 105.132565 128.592317)
        (xy 104.87778 128.735259)
        (xy 104.883587 128.773404)
        (xy 104.888014 128.807623)
        (xy 104.890862 128.839159)
        (xy 104.891927 128.869255)
        (xy 104.891009 128.899153)
        (xy 104.887906 128.930097)
        (xy 104.882418 128.963329)
        (xy 104.874342 129.000093)
        (xy 104.863478 129.04163)
        (xy 104.849624 129.089184)
      )
    )
  )
  (zone (net 82) (net_name "/~{EN_DC}") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.855 120.3016)
        (xy 84.905022 120.302686)
        (xy 84.947687 120.305912)
        (xy 84.984476 120.311225)
        (xy 85.016871 120.318573)
        (xy 85.046353 120.327905)
        (xy 85.074404 120.339168)
        (xy 85.102505 120.352311)
        (xy 85.132138 120.367282)
        (xy 85.164784 120.384029)
        (xy 85.201925 120.4025)
        (xy 85.4125 120.2)
        (xy 85.201925 119.9975)
        (xy 85.164784 120.01597)
        (xy 85.132138 120.032717)
        (xy 85.102505 120.047688)
        (xy 85.074404 120.060831)
        (xy 85.046353 120.072094)
        (xy 85.016871 120.081426)
        (xy 84.984476 120.088774)
        (xy 84.947687 120.094087)
        (xy 84.905022 120.097313)
        (xy 84.855 120.0984)
      )
    )
  )
  (zone (net 23) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.746417 129.801025)
        (xy 97.770766 129.757892)
        (xy 97.792899 129.721102)
        (xy 97.813564 129.689642)
        (xy 97.83351 129.6625)
        (xy 97.853485 129.638664)
        (xy 97.874238 129.617122)
        (xy 97.896517 129.59686)
        (xy 97.921072 129.576868)
        (xy 97.948651 129.556132)
        (xy 97.980003 129.533641)
        (xy 97.904304 129.251475)
        (xy 97.625313 129.338144)
        (xy 97.623037 129.376661)
        (xy 97.620232 129.411051)
        (xy 97.61644 129.442488)
        (xy 97.611206 129.472144)
        (xy 97.604073 129.501194)
        (xy 97.594586 129.53081)
        (xy 97.582288 129.562167)
        (xy 97.566723 129.596438)
        (xy 97.547436 129.634796)
        (xy 97.52397 129.678416)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 44 133.4)
        (xy 42.4 134.4)
        (xy 42.5 142.2)
        (xy 40.8 142.2)
        (xy 40.8 132.2)
        (xy 44 132.2)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.750714 122.919448)
        (xy 89.796326 122.940014)
        (xy 89.83433 122.95967)
        (xy 89.86611 122.97895)
        (xy 89.89305 122.998384)
        (xy 89.916533 123.018504)
        (xy 89.937943 123.039841)
        (xy 89.958664 123.062929)
        (xy 89.980081 123.088297)
        (xy 90.003575 123.116479)
        (xy 90.030533 123.148006)
        (xy 90.303537 123.044003)
        (xy 90.188944 122.775272)
        (xy 90.147537 122.777744)
        (xy 90.110942 122.780387)
        (xy 90.077814 122.782575)
        (xy 90.046812 122.783679)
        (xy 90.01659 122.783074)
        (xy 89.985807 122.78013)
        (xy 89.953119 122.774222)
        (xy 89.917183 122.764722)
        (xy 89.876656 122.751003)
        (xy 89.830194 122.732438)
      )
    )
  )
  (zone (net 38) (net_name "/VGAIN") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.967018 127.805526)
        (xy 103.009188 127.832452)
        (xy 103.043962 127.857381)
        (xy 103.072631 127.88104)
        (xy 103.096488 127.904154)
        (xy 103.116826 127.927449)
        (xy 103.134937 127.95165)
        (xy 103.152114 127.977483)
        (xy 103.16965 128.005674)
        (xy 103.188837 128.036947)
        (xy 103.210968 128.072031)
        (xy 103.496112 128.008468)
        (xy 103.421454 127.726026)
        (xy 103.380123 127.722503)
        (xy 103.343529 127.719844)
        (xy 103.310433 127.717233)
        (xy 103.279595 127.713857)
        (xy 103.249776 127.708901)
        (xy 103.219739 127.701551)
        (xy 103.188244 127.690993)
        (xy 103.154053 127.676412)
        (xy 103.115926 127.656994)
        (xy 103.072626 127.631925)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.481056 126.087419)
        (xy 109.433964 126.102772)
        (xy 109.392792 126.114947)
        (xy 109.356303 126.124184)
        (xy 109.323262 126.130722)
        (xy 109.292431 126.134804)
        (xy 109.262577 126.136669)
        (xy 109.232462 126.136558)
        (xy 109.200852 126.134711)
        (xy 109.166509 126.13137)
        (xy 109.1282 126.126775)
        (xy 108.993403 126.38596)
        (xy 109.257659 126.510526)
        (xy 109.285356 126.483662)
        (xy 109.310656 126.4602)
        (xy 109.334689 126.439583)
        (xy 109.358582 126.421252)
        (xy 109.383465 126.404651)
        (xy 109.410468 126.389223)
        (xy 109.440718 126.37441)
        (xy 109.475345 126.359655)
        (xy 109.515479 126.344401)
        (xy 109.562248 126.328092)
      )
    )
  )
  (zone (net 33) (net_name "/OUT2-") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.017739 127.113745)
        (xy 112.047061 127.072153)
        (xy 112.074673 127.039221)
        (xy 112.101256 127.013339)
        (xy 112.12749 126.992894)
        (xy 112.154057 126.976275)
        (xy 112.181638 126.96187)
        (xy 112.210915 126.948066)
        (xy 112.242569 126.933253)
        (xy 112.277281 126.915819)
        (xy 112.315733 126.894152)
        (xy 112.261605 126.607067)
        (xy 111.976855 126.672375)
        (xy 111.97239 126.716284)
        (xy 111.970307 126.755073)
        (xy 111.969402 126.790009)
        (xy 111.968471 126.822363)
        (xy 111.96631 126.853405)
        (xy 111.961714 126.884403)
        (xy 111.953478 126.916627)
        (xy 111.9404 126.951346)
        (xy 111.921274 126.989831)
        (xy 111.894896 127.03335)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.645 120.0984)
        (xy 86.594977 120.097313)
        (xy 86.552312 120.094087)
        (xy 86.515523 120.088774)
        (xy 86.483128 120.081426)
        (xy 86.453646 120.072094)
        (xy 86.425595 120.060831)
        (xy 86.397494 120.047688)
        (xy 86.367861 120.032717)
        (xy 86.335215 120.01597)
        (xy 86.298075 119.9975)
        (xy 86.0875 120.2)
        (xy 86.298075 120.4025)
        (xy 86.335215 120.384029)
        (xy 86.367861 120.367282)
        (xy 86.397494 120.352311)
        (xy 86.425595 120.339168)
        (xy 86.453646 120.327905)
        (xy 86.483128 120.318573)
        (xy 86.515523 120.311225)
        (xy 86.552312 120.305912)
        (xy 86.594977 120.302686)
        (xy 86.645 120.3016)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.847545 138.955197)
        (xy 114.846554 139.005221)
        (xy 114.84341 139.047892)
        (xy 114.838168 139.084691)
        (xy 114.830882 139.1171)
        (xy 114.821607 139.1466)
        (xy 114.810398 139.174673)
        (xy 114.797309 139.202799)
        (xy 114.782395 139.23246)
        (xy 114.765711 139.265138)
        (xy 114.747312 139.302315)
        (xy 114.950216 139.512499)
        (xy 115.152311 139.301536)
        (xy 115.133768 139.26443)
        (xy 115.116959 139.231817)
        (xy 115.101931 139.202213)
        (xy 115.088734 139.174137)
        (xy 115.077417 139.146109)
        (xy 115.068029 139.116645)
        (xy 115.060618 139.084264)
        (xy 115.055234 139.047485)
        (xy 115.051926 139.004827)
        (xy 115.050744 138.954807)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.695 127.3984)
        (xy 99.644977 127.397313)
        (xy 99.602312 127.394087)
        (xy 99.565523 127.388774)
        (xy 99.533128 127.381426)
        (xy 99.503646 127.372094)
        (xy 99.475595 127.360831)
        (xy 99.447494 127.347688)
        (xy 99.417861 127.332717)
        (xy 99.385215 127.31597)
        (xy 99.348075 127.2975)
        (xy 99.1375 127.5)
        (xy 99.348075 127.7025)
        (xy 99.385215 127.684029)
        (xy 99.417861 127.667282)
        (xy 99.447494 127.652311)
        (xy 99.475595 127.639168)
        (xy 99.503646 127.627905)
        (xy 99.533128 127.618573)
        (xy 99.565523 127.611225)
        (xy 99.602312 127.605912)
        (xy 99.644977 127.602686)
        (xy 99.695 127.6016)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.836146 124.842287)
        (xy 92.835629 124.792758)
        (xy 92.836369 124.74983)
        (xy 92.838506 124.712251)
        (xy 92.842183 124.67877)
        (xy 92.84754 124.648135)
        (xy 92.854719 124.619097)
        (xy 92.863861 124.590403)
        (xy 92.875107 124.560803)
        (xy 92.888599 124.529045)
        (xy 92.904478 124.49388)
        (xy 92.697681 124.287524)
        (xy 92.499565 124.502228)
        (xy 92.516879 124.536709)
        (xy 92.531669 124.567884)
        (xy 92.544125 124.596995)
        (xy 92.554442 124.625288)
        (xy 92.562812 124.654006)
        (xy 92.569428 124.684393)
        (xy 92.574482 124.717694)
        (xy 92.578166 124.755154)
        (xy 92.580675 124.798015)
        (xy 92.582201 124.847523)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.676594 140.805)
        (xy 101.674834 140.855858)
        (xy 101.669763 140.898534)
        (xy 101.661694 140.934747)
        (xy 101.650938 140.96622)
        (xy 101.63781 140.994674)
        (xy 101.62262 141.021831)
        (xy 101.605681 141.049413)
        (xy 101.587307 141.079141)
        (xy 101.567809 141.112738)
        (xy 101.5475 141.151925)
        (xy 101.75 141.3625)
        (xy 101.9525 141.151925)
        (xy 101.93219 141.112738)
        (xy 101.912692 141.079141)
        (xy 101.894318 141.049413)
        (xy 101.877379 141.021831)
        (xy 101.862189 140.994674)
        (xy 101.849061 140.96622)
        (xy 101.838305 140.934747)
        (xy 101.830236 140.898534)
        (xy 101.825165 140.855858)
        (xy 101.823406 140.805)
      )
    )
  )
  (zone (net 31) (net_name "/OUT1-") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.03343 125.571411)
        (xy 112.061162 125.528742)
        (xy 112.087512 125.494793)
        (xy 112.113099 125.467927)
        (xy 112.138543 125.446507)
        (xy 112.164464 125.428897)
        (xy 112.191483 125.413462)
        (xy 112.220218 125.398564)
        (xy 112.251291 125.382568)
        (xy 112.28532 125.363837)
        (xy 112.322928 125.340735)
        (xy 112.25801 125.055896)
        (xy 111.975926 125.131897)
        (xy 111.97312 125.175944)
        (xy 111.972502 125.214783)
        (xy 111.972916 125.249729)
        (xy 111.973206 125.282095)
        (xy 111.972217 125.313196)
        (xy 111.968793 125.344346)
        (xy 111.96178 125.376857)
        (xy 111.95002 125.412046)
        (xy 111.932359 125.451224)
        (xy 111.907642 125.495708)
      )
    )
  )
  (zone (net 28) (net_name "/THERM") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 72.95575 141.775274)
        (xy 72.907973 141.760411)
        (xy 72.867859 141.745526)
        (xy 72.833969 141.730257)
        (xy 72.804864 141.714247)
        (xy 72.779107 141.697134)
        (xy 72.755259 141.678561)
        (xy 72.731882 141.658167)
        (xy 72.707537 141.635594)
        (xy 72.680787 141.610481)
        (xy 72.650194 141.58247)
        (xy 72.391877 141.718925)
        (xy 72.538324 141.971712)
        (xy 72.579121 141.964218)
        (xy 72.615123 141.957141)
        (xy 72.647738 141.950938)
        (xy 72.678376 141.946068)
        (xy 72.708446 141.942992)
        (xy 72.739359 141.942167)
        (xy 72.772523 141.944053)
        (xy 72.809348 141.949109)
        (xy 72.851244 141.957793)
        (xy 72.899621 141.970567)
      )
    )
  )
  (zone (net 44) (net_name "/SIG_50") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.094729 137.86516)
        (xy 46.188199 138.001884)
        (xy 46.249711 138.1246)
        (xy 46.285292 138.237162)
        (xy 46.300969 138.343423)
        (xy 46.302768 138.447238)
        (xy 46.296717 138.552461)
        (xy 46.288843 138.662944)
        (xy 46.285174 138.782544)
        (xy 46.291735 138.915112)
        (xy 46.314556 139.064504)
        (xy 47.213291 139.200001)
        (xy 47.313558 138.296656)
        (xy 47.175064 138.236172)
        (xy 47.048646 138.195727)
        (xy 46.932128 138.168506)
        (xy 46.823337 138.147693)
        (xy 46.720099 138.126471)
        (xy 46.620241 138.098025)
        (xy 46.521588 138.05554)
        (xy 46.421968 137.9922)
        (xy 46.319206 137.901189)
        (xy 46.21113 137.775692)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.556575 130.608262)
        (xy 107.606607 130.608598)
        (xy 107.649316 130.611183)
        (xy 107.686181 130.615944)
        (xy 107.718682 130.622805)
        (xy 107.748301 130.631694)
        (xy 107.776517 130.642535)
        (xy 107.804812 130.655255)
        (xy 107.834666 130.669779)
        (xy 107.867559 130.686035)
        (xy 107.904973 130.703947)
        (xy 108.112487 130.498314)
        (xy 107.8989 130.298994)
        (xy 107.86204 130.318019)
        (xy 107.829649 130.335254)
        (xy 107.800244 130.350667)
        (xy 107.772343 130.36423)
        (xy 107.744464 130.375913)
        (xy 107.715126 130.385686)
        (xy 107.682844 130.393519)
        (xy 107.646139 130.399383)
        (xy 107.603527 130.403249)
        (xy 107.553527 130.405086)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.963773 138.02807)
        (xy 100.978217 138.071227)
        (xy 100.985779 138.109133)
        (xy 100.987286 138.14286)
        (xy 100.98356 138.173478)
        (xy 100.975426 138.20206)
        (xy 100.963709 138.229677)
        (xy 100.949234 138.2574)
        (xy 100.932824 138.286302)
        (xy 100.915304 138.317453)
        (xy 100.8975 138.351925)
        (xy 101.1 138.5625)
        (xy 101.3025 138.351925)
        (xy 101.281989 138.308077)
        (xy 101.265301 138.269393)
        (xy 101.251465 138.234273)
        (xy 101.239508 138.201114)
        (xy 101.22846 138.168315)
        (xy 101.21735 138.134273)
        (xy 101.205205 138.097388)
        (xy 101.191055 138.056058)
        (xy 101.173929 138.00868)
        (xy 101.152855 137.953654)
      )
    )
  )
  (zone (net 23) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.25) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 91.5 131.25)
        (xy 94.8 131.25)
        (xy 94.8 132.6)
        (xy 95.5 132.6)
        (xy 95.5 133)
        (xy 89.5 133)
        (xy 89.5 129.5)
        (xy 91.5 129.5)
      )
    )
  )
  (zone (net 23) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.868824 125.862407)
        (xy 107.915922 125.847074)
        (xy 107.957099 125.834918)
        (xy 107.993593 125.825698)
        (xy 108.026637 125.819175)
        (xy 108.057469 125.815107)
        (xy 108.087325 125.813256)
        (xy 108.117439 125.813381)
        (xy 108.149049 125.815242)
        (xy 108.18339 125.818599)
        (xy 108.221698 125.823212)
        (xy 108.356614 125.564088)
        (xy 108.092415 125.439403)
        (xy 108.064705 125.466253)
        (xy 108.039394 125.489703)
        (xy 108.015352 125.51031)
        (xy 107.99145 125.528629)
        (xy 107.966559 125.545219)
        (xy 107.93955 125.560635)
        (xy 107.909293 125.575434)
        (xy 107.874658 125.590173)
        (xy 107.834518 125.605408)
        (xy 107.787742 125.621697)
      )
    )
  )
  (zone (net 23) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.673933 129.154977)
        (xy 104.663272 129.106606)
        (xy 104.655195 129.064438)
        (xy 104.649583 129.027219)
        (xy 104.646317 128.993696)
        (xy 104.64528 128.962614)
        (xy 104.646352 128.93272)
        (xy 104.649417 128.902762)
        (xy 104.654356 128.871485)
        (xy 104.66105 128.837636)
        (xy 104.669382 128.799962)
        (xy 104.42467 128.640389)
        (xy 104.274782 128.89115)
        (xy 104.298798 128.921349)
        (xy 104.319664 128.948829)
        (xy 104.337825 128.974768)
        (xy 104.353724 129.000344)
        (xy 104.367803 129.026736)
        (xy 104.380508 129.055122)
        (xy 104.392282 129.086679)
        (xy 104.403569 129.122587)
        (xy 104.414812 129.164023)
        (xy 104.426456 129.212167)
      )
    )
  )
  (zone (net 37) (net_name "/OFFSET2") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.8984 140.805)
        (xy 102.897313 140.855022)
        (xy 102.894087 140.897687)
        (xy 102.888774 140.934476)
        (xy 102.881426 140.966871)
        (xy 102.872094 140.996353)
        (xy 102.860831 141.024404)
        (xy 102.847688 141.052505)
        (xy 102.832717 141.082138)
        (xy 102.81597 141.114784)
        (xy 102.7975 141.151925)
        (xy 103 141.3625)
        (xy 103.2025 141.151925)
        (xy 103.184029 141.114784)
        (xy 103.167282 141.082138)
        (xy 103.152311 141.052505)
        (xy 103.139168 141.024404)
        (xy 103.127905 140.996353)
        (xy 103.118573 140.966871)
        (xy 103.111225 140.934476)
        (xy 103.105912 140.897687)
        (xy 103.102686 140.855022)
        (xy 103.1016 140.805)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.290714 139.431185)
        (xy 104.240687 139.432042)
        (xy 104.197929 139.430477)
        (xy 104.160961 139.426598)
        (xy 104.128305 139.420514)
        (xy 104.098483 139.412335)
        (xy 104.070016 139.40217)
        (xy 104.041426 139.390129)
        (xy 104.011234 139.376321)
        (xy 103.977962 139.360855)
        (xy 103.940132 139.343842)
        (xy 103.737585 139.554371)
        (xy 103.95587 139.748535)
        (xy 103.992264 139.728634)
        (xy 104.024235 139.710632)
        (xy 104.053263 139.694521)
        (xy 104.080832 139.680296)
        (xy 104.108424 139.667951)
        (xy 104.137521 139.657481)
        (xy 104.169606 139.648879)
        (xy 104.206161 139.642141)
        (xy 104.248668 139.637259)
        (xy 104.298611 139.63423)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.512509 140.065438)
        (xy 109.465516 140.049784)
        (xy 109.425173 140.035093)
        (xy 109.390343 140.020824)
        (xy 109.359888 140.006436)
        (xy 109.332672 139.991387)
        (xy 109.307559 139.975136)
        (xy 109.283412 139.957141)
        (xy 109.259093 139.936862)
        (xy 109.233467 139.913756)
        (xy 109.205397 139.887284)
        (xy 108.94291 140.015535)
        (xy 109.081321 140.272809)
        (xy 109.119562 140.267677)
        (xy 109.153855 140.263856)
        (xy 109.185436 140.261567)
        (xy 109.215546 140.261035)
        (xy 109.245424 140.262482)
        (xy 109.276308 140.266132)
        (xy 109.309438 140.272207)
        (xy 109.346053 140.280932)
        (xy 109.387391 140.29253)
        (xy 109.434693 140.307224)
      )
    )
  )
  (zone (net 13) (net_name "Net-(C13-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.578193 135.095728)
        (xy 109.54181 135.060146)
        (xy 109.513705 135.027636)
        (xy 109.492394 134.997266)
        (xy 109.476395 134.968107)
        (xy 109.464226 134.939229)
        (xy 109.454404 134.909703)
        (xy 109.445447 134.8786)
        (xy 109.435873 134.844988)
        (xy 109.424198 134.80794)
        (xy 109.408942 134.766525)
        (xy 109.116899 134.77417)
        (xy 109.135952 135.065691)
        (xy 109.178587 135.077102)
        (xy 109.216547 135.085345)
        (xy 109.250892 135.09181)
        (xy 109.282684 135.09789)
        (xy 109.312983 135.104975)
        (xy 109.342851 135.114456)
        (xy 109.373349 135.127726)
        (xy 109.405538 135.146174)
        (xy 109.44048 135.171194)
        (xy 109.479235 135.204176)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.306575 139.608262)
        (xy 105.356607 139.608598)
        (xy 105.399316 139.611183)
        (xy 105.436181 139.615944)
        (xy 105.468682 139.622805)
        (xy 105.498301 139.631694)
        (xy 105.526517 139.642535)
        (xy 105.554812 139.655255)
        (xy 105.584666 139.669779)
        (xy 105.617559 139.686035)
        (xy 105.654973 139.703947)
        (xy 105.862487 139.498314)
        (xy 105.6489 139.298994)
        (xy 105.61204 139.318019)
        (xy 105.579649 139.335254)
        (xy 105.550244 139.350667)
        (xy 105.522343 139.36423)
        (xy 105.494464 139.375913)
        (xy 105.465126 139.385686)
        (xy 105.432844 139.393519)
        (xy 105.396139 139.399383)
        (xy 105.353527 139.403249)
        (xy 105.303527 139.405086)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.87063 140.646768)
        (xy 93.871841 140.597251)
        (xy 93.874079 140.554375)
        (xy 93.877526 140.516893)
        (xy 93.882369 140.483561)
        (xy 93.888792 140.453132)
        (xy 93.89698 140.424361)
        (xy 93.907118 140.396004)
        (xy 93.91939 140.366814)
        (xy 93.933981 140.335547)
        (xy 93.951078 140.300957)
        (xy 93.751606 140.087512)
        (xy 93.54612 140.295173)
        (xy 93.562221 140.330237)
        (xy 93.575913 140.361908)
        (xy 93.587347 140.391437)
        (xy 93.59667 140.420072)
        (xy 93.604033 140.449064)
        (xy 93.609584 140.479664)
        (xy 93.613472 140.513121)
        (xy 93.615848 140.550686)
        (xy 93.61686 140.593608)
        (xy 93.616657 140.643139)
      )
    )
  )
  (zone (net 18) (net_name "/SIG_{2}") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.871957 138.416972)
        (xy 79.706532 138.408906)
        (xy 79.571573 138.383827)
        (xy 79.460367 138.34421)
        (xy 79.366203 138.292534)
        (xy 79.28237 138.231274)
        (xy 79.202155 138.162907)
        (xy 79.118848 138.08991)
        (xy 79.025736 138.014759)
        (xy 78.916109 137.939931)
        (xy 78.783254 137.867903)
        (xy 78.132509 138.502423)
        (xy 78.791977 139.127872)
        (xy 78.923822 139.05401)
        (xy 79.032403 138.977671)
        (xy 79.124465 138.901238)
        (xy 79.206754 138.827094)
        (xy 79.286014 138.757623)
        (xy 79.368991 138.695208)
        (xy 79.46243 138.642233)
        (xy 79.573077 138.60108)
        (xy 79.707676 138.574134)
        (xy 79.872974 138.563779)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.303884 131.940239)
        (xy 95.260052 131.917171)
        (xy 95.222625 131.896133)
        (xy 95.190569 131.876404)
        (xy 95.162851 131.857268)
        (xy 95.138436 131.838004)
        (xy 95.116291 131.817896)
        (xy 95.095381 131.796223)
        (xy 95.074673 131.772269)
        (xy 95.053133 131.745313)
        (xy 95.029728 131.714639)
        (xy 94.749917 131.798624)
        (xy 94.844774 132.074939)
        (xy 94.883341 132.076077)
        (xy 94.917799 132.077867)
        (xy 94.949334 132.08073)
        (xy 94.979132 132.085088)
        (xy 95.00838 132.091361)
        (xy 95.038263 132.099971)
        (xy 95.069969 132.111339)
        (xy 95.104685 132.125886)
        (xy 95.143595 132.144034)
        (xy 95.187888 132.166204)
      )
    )
  )
  (zone (net 29) (net_name "/SIG_IN_{1}") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53.422733 133.132545)
        (xy 53.555215 133.231936)
        (xy 53.652931 133.328344)
        (xy 53.722828 133.423479)
        (xy 53.771852 133.519051)
        (xy 53.806949 133.61677)
        (xy 53.835066 133.718346)
        (xy 53.863149 133.825491)
        (xy 53.898145 133.939915)
        (xy 53.947 134.063327)
        (xy 54.016662 134.197439)
        (xy 54.911217 134.036645)
        (xy 54.715583 133.149057)
        (xy 54.564994 133.136335)
        (xy 54.432285 133.138704)
        (xy 54.313203 133.150409)
        (xy 54.203499 133.165696)
        (xy 54.098922 133.17881)
        (xy 53.995221 133.183997)
        (xy 53.888146 133.175503)
        (xy 53.773446 133.147573)
        (xy 53.646871 133.094453)
        (xy 53.50417 133.01039)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.445203 140.459235)
        (xy 109.397323 140.471919)
        (xy 109.355532 140.481763)
        (xy 109.318582 140.488935)
        (xy 109.285225 140.493608)
        (xy 109.254215 140.495951)
        (xy 109.224302 140.496136)
        (xy 109.194241 140.494334)
        (xy 109.162784 140.490715)
        (xy 109.128684 140.48545)
        (xy 109.090693 140.478711)
        (xy 108.941551 140.729916)
        (xy 109.198394 140.869127)
        (xy 109.227556 140.843861)
        (xy 109.254134 140.821858)
        (xy 109.279287 140.802622)
        (xy 109.304172 140.785662)
        (xy 109.329948 140.770485)
        (xy 109.357774 140.756598)
        (xy 109.388809 140.743507)
        (xy 109.424211 140.73072)
        (xy 109.465138 140.717745)
        (xy 109.512749 140.704088)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.426594 137.355)
        (xy 97.424834 137.405858)
        (xy 97.419763 137.448534)
        (xy 97.411694 137.484747)
        (xy 97.400938 137.51622)
        (xy 97.38781 137.544674)
        (xy 97.37262 137.571831)
        (xy 97.355681 137.599413)
        (xy 97.337307 137.629141)
        (xy 97.317809 137.662738)
        (xy 97.2975 137.701925)
        (xy 97.5 137.9125)
        (xy 97.7025 137.701925)
        (xy 97.68219 137.662738)
        (xy 97.662692 137.629141)
        (xy 97.644318 137.599413)
        (xy 97.627379 137.571831)
        (xy 97.612189 137.544674)
        (xy 97.599061 137.51622)
        (xy 97.588305 137.484747)
        (xy 97.580236 137.448534)
        (xy 97.575165 137.405858)
        (xy 97.573406 137.355)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.367507 122.848706)
        (xy 96.333663 122.885557)
        (xy 96.303071 122.91547)
        (xy 96.27479 122.939592)
        (xy 96.247883 122.95907)
        (xy 96.221409 122.975051)
        (xy 96.194429 122.988682)
        (xy 96.166005 123.001109)
        (xy 96.135196 123.01348)
        (xy 96.101064 123.026941)
        (xy 96.06267 123.04264)
        (xy 96.075722 123.334491)
        (xy 96.36684 123.310043)
        (xy 96.377489 123.269953)
        (xy 96.386467 123.234377)
        (xy 96.394788 123.202238)
        (xy 96.403471 123.172455)
        (xy 96.413533 123.143951)
        (xy 96.42599 123.115648)
        (xy 96.44186 123.086467)
        (xy 96.46216 123.055329)
        (xy 96.487907 123.021156)
        (xy 96.520119 122.98287)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.687251 140.704088)
        (xy 107.734861 140.717745)
        (xy 107.775788 140.73072)
        (xy 107.81119 140.743507)
        (xy 107.842225 140.756598)
        (xy 107.870051 140.770485)
        (xy 107.895827 140.785662)
        (xy 107.920712 140.802622)
        (xy 107.945865 140.821858)
        (xy 107.972443 140.843861)
        (xy 108.001606 140.869127)
        (xy 108.258449 140.729916)
        (xy 108.109307 140.478711)
        (xy 108.071315 140.48545)
        (xy 108.037215 140.490715)
        (xy 108.005758 140.494334)
        (xy 107.975697 140.496136)
        (xy 107.945784 140.495951)
        (xy 107.914774 140.493608)
        (xy 107.881417 140.488935)
        (xy 107.844467 140.481763)
        (xy 107.802676 140.471919)
        (xy 107.754797 140.459235)
      )
    )
  )
  (zone (net 23) (net_name "+5V") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.787449 126.314135)
        (xy 107.835345 126.326755)
        (xy 107.876544 126.338839)
        (xy 107.912215 126.350854)
        (xy 107.943526 126.363268)
        (xy 107.971648 126.376548)
        (xy 107.997748 126.391162)
        (xy 108.022995 126.407577)
        (xy 108.048559 126.426262)
        (xy 108.075609 126.447684)
        (xy 108.105314 126.47231)
        (xy 108.359073 126.327554)
        (xy 108.204512 126.079647)
        (xy 108.166675 126.08721)
        (xy 108.132697 126.093214)
        (xy 108.101326 126.097515)
        (xy 108.071312 126.099969)
        (xy 108.041403 126.100434)
        (xy 108.010348 126.098764)
        (xy 107.976898 126.094817)
        (xy 107.939801 126.088448)
        (xy 107.897806 126.079515)
        (xy 107.849663 126.067873)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 44 126.75)
        (xy 40 126.75)
        (xy 40 119)
        (xy 44 119)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "In1.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43.9 131.1)
        (xy 40 131.1)
        (xy 40 128.9)
        (xy 43.9 128.9)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "In1.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125 143)
        (xy 82 143)
        (xy 82 125)
        (xy 82 119)
        (xy 125 119)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "In1.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (mode hatch) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.2)
      (hatch_thickness 0.4) (hatch_gap 3.5) (hatch_orientation 45)
      (hatch_border_algorithm hatch_thickness) (hatch_min_hole_area 0.3))
    (polygon
      (pts
        (xy 82.5 143)
        (xy 40 143)
        (xy 40 119)
        (xy 82.5 119)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layers "In1.Cu" "In2.Cu" "B.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56.75 125)
        (xy 45.25 125)
        (xy 45.25 135.5)
        (xy 54.5 138.9)
        (xy 54.5 143)
        (xy 40 143)
        (xy 40 119)
        (xy 56.75 119)
      )
    )
  )
  (zone (net 23) (net_name "+5V") (layer "In2.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 97 122.5)
        (xy 124.75 122.5)
        (xy 124.75 135.75)
        (xy 120.75 135.5)
        (xy 117.75 133)
        (xy 113 133)
        (xy 113 131)
        (xy 108 131)
        (xy 108 134)
        (xy 89 134)
        (xy 89 127.5)
        (xy 93.5 127.5)
        (xy 93.5 123.5)
        (xy 89 123.5)
        (xy 89 120.5)
        (xy 97 120.5)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "In2.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56.805408 122.277825)
        (xy 56.949344 122.186906)
        (xy 57.074595 122.11451)
        (xy 57.185682 122.057373)
        (xy 57.287128 122.012231)
        (xy 57.383454 121.975822)
        (xy 57.479184 121.944882)
        (xy 57.578839 121.916147)
        (xy 57.686943 121.886355)
        (xy 57.808017 121.852241)
        (xy 57.946584 121.810544)
        (xy 57.992551 120.902816)
        (xy 57.083719 120.89236)
        (xy 57.040051 121.017229)
        (xy 57.006233 121.130864)
        (xy 56.977573 121.235076)
        (xy 56.949379 121.331673)
        (xy 56.916959 121.422467)
        (xy 56.875624 121.509266)
        (xy 56.82068 121.593882)
        (xy 56.747438 121.678122)
        (xy 56.651204 121.763799)
        (xy 56.52729 121.852721)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "In2.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.431621 120.61951)
        (xy 86.425072 120.57018)
        (xy 86.418608 120.525401)
        (xy 86.412588 120.484683)
        (xy 86.407373 120.447534)
        (xy 86.40332 120.413467)
        (xy 86.400791 120.381991)
        (xy 86.400145 120.352616)
        (xy 86.401741 120.324852)
        (xy 86.40594 120.29821)
        (xy 86.4131 120.272201)
        (xy 86.186047 120.088369)
        (xy 86.011229 120.322434)
        (xy 86.02457 120.345881)
        (xy 86.035197 120.370669)
        (xy 86.043578 120.397186)
        (xy 86.050183 120.425816)
        (xy 86.055479 120.456946)
        (xy 86.059937 120.490963)
        (xy 86.064026 120.528252)
        (xy 86.068214 120.5692)
        (xy 86.072972 120.614192)
        (xy 86.078768 120.663616)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "In2.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.25) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 93.25 127.25)
        (xy 88.75 127.25)
        (xy 88.75 134.25)
        (xy 108.25 134.25)
        (xy 108.25 131.25)
        (xy 112.75 131.25)
        (xy 112.75 133.25)
        (xy 117.25 133.25)
        (xy 120.75 136)
        (xy 124.75 136)
        (xy 124.75 142.5)
        (xy 85.75 142.5)
        (xy 83.75 131.75)
        (xy 83.75 123.75)
        (xy 93.25 123.75)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (mode hatch) (thermal_gap 0.508) (thermal_bridge_width 0.508)
      (hatch_thickness 0.4) (hatch_gap 3.5) (hatch_orientation 0)
      (hatch_border_algorithm hatch_thickness) (hatch_min_hole_area 0.3))
    (polygon
      (pts
        (xy 88.5 123.5)
        (xy 83.25 123.5)
        (xy 83.25 131.75)
        (xy 85.25 143)
        (xy 40 143)
        (xy 40 119)
        (xy 88.5 119)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "In2.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.3222 131.755)
        (xy 78.322579 131.80476)
        (xy 78.323439 131.849995)
        (xy 78.324361 131.891146)
        (xy 78.324929 131.928654)
        (xy 78.324725 131.962961)
        (xy 78.32333 131.994508)
        (xy 78.320328 132.023737)
        (xy 78.315301 132.051088)
        (xy 78.30783 132.077003)
        (xy 78.2975 132.101925)
        (xy 78.5 132.3125)
        (xy 78.7025 132.101925)
        (xy 78.692169 132.077003)
        (xy 78.684698 132.051088)
        (xy 78.679671 132.023737)
        (xy 78.676669 131.994508)
        (xy 78.675274 131.962961)
        (xy 78.67507 131.928654)
        (xy 78.675638 131.891146)
        (xy 78.67656 131.849995)
        (xy 78.67742 131.80476)
        (xy 78.6778 131.755)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "In2.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59.123096 120.865485)
        (xy 58.964917 120.863275)
        (xy 58.83136 120.851469)
        (xy 58.717283 120.830866)
        (xy 58.617542 120.802265)
        (xy 58.526994 120.766468)
        (xy 58.440496 120.724274)
        (xy 58.352903 120.676482)
        (xy 58.259074 120.623894)
        (xy 58.153865 120.567309)
        (xy 58.032133 120.507527)
        (xy 57.387549 121.148303)
        (xy 58.053028 121.767353)
        (xy 58.172711 121.703566)
        (xy 58.275985 121.643523)
        (xy 58.368019 121.587852)
        (xy 58.453978 121.537183)
        (xy 58.53903 121.492143)
        (xy 58.628341 121.453363)
        (xy 58.727079 121.421471)
        (xy 58.84041 121.397096)
        (xy 58.973501 121.380867)
        (xy 59.13152 121.373414)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65.074795 126.844566)
        (xy 65.124918 126.838388)
        (xy 65.167571 126.836638)
        (xy 65.204381 126.838761)
        (xy 65.236973 126.8442)
        (xy 65.266975 126.852402)
        (xy 65.296012 126.862811)
        (xy 65.32571 126.874872)
        (xy 65.357697 126.88803)
        (xy 65.393598 126.90173)
        (xy 65.43504 126.915418)
        (xy 65.611096 126.682283)
        (xy 65.371258 126.515473)
        (xy 65.336174 126.541335)
        (xy 65.306341 126.565488)
        (xy 65.280045 126.587905)
        (xy 65.255573 126.608561)
        (xy 65.231211 126.627429)
        (xy 65.205244 126.644483)
        (xy 65.17596 126.659696)
        (xy 65.141644 126.673041)
        (xy 65.100583 126.684493)
        (xy 65.051063 126.694026)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.845 120.9984)
        (xy 48.794977 120.997313)
        (xy 48.752312 120.994087)
        (xy 48.715523 120.988774)
        (xy 48.683128 120.981426)
        (xy 48.653646 120.972094)
        (xy 48.625595 120.960831)
        (xy 48.597494 120.947688)
        (xy 48.567861 120.932717)
        (xy 48.535215 120.91597)
        (xy 48.498075 120.8975)
        (xy 48.2875 121.1)
        (xy 48.498075 121.3025)
        (xy 48.535215 121.284029)
        (xy 48.567861 121.267282)
        (xy 48.597494 121.252311)
        (xy 48.625595 121.239168)
        (xy 48.653646 121.227905)
        (xy 48.683128 121.218573)
        (xy 48.715523 121.211225)
        (xy 48.752312 121.205912)
        (xy 48.794977 121.202686)
        (xy 48.845 121.2016)
      )
    )
  )
  (zone (net 30) (net_name "/OUT1+") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.584685 124.664396)
        (xy 112.549842 124.661944)
        (xy 112.521276 124.654843)
        (xy 112.498101 124.643471)
        (xy 112.479433 124.628205)
        (xy 112.464387 124.609424)
        (xy 112.452079 124.587507)
        (xy 112.441625 124.562833)
        (xy 112.43214 124.535779)
        (xy 112.422739 124.506723)
        (xy 112.412538 124.476046)
        (xy 112.120451 124.470336)
        (xy 112.2 124.774884)
        (xy 112.246121 124.774884)
        (xy 112.285611 124.774884)
        (xy 112.320319 124.774884)
        (xy 112.352092 124.774884)
        (xy 112.382782 124.774884)
        (xy 112.414236 124.774884)
        (xy 112.448304 124.774884)
        (xy 112.486835 124.774884)
        (xy 112.531679 124.774884)
        (xy 112.584685 124.774885)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.726594 138.805)
        (xy 108.724834 138.855858)
        (xy 108.719763 138.898534)
        (xy 108.711694 138.934747)
        (xy 108.700938 138.96622)
        (xy 108.68781 138.994674)
        (xy 108.67262 139.021831)
        (xy 108.655681 139.049413)
        (xy 108.637307 139.079141)
        (xy 108.617809 139.112738)
        (xy 108.5975 139.151925)
        (xy 108.8 139.3625)
        (xy 109.0025 139.151925)
        (xy 108.98219 139.112738)
        (xy 108.962692 139.079141)
        (xy 108.944318 139.049413)
        (xy 108.927379 139.021831)
        (xy 108.912189 138.994674)
        (xy 108.899061 138.96622)
        (xy 108.888305 138.934747)
        (xy 108.880236 138.898534)
        (xy 108.875165 138.855858)
        (xy 108.873406 138.805)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.423 135.66)
        (xy 121.422856 135.66884)
        (xy 121.422459 135.677433)
        (xy 121.421859 135.685626)
        (xy 121.421108 135.693269)
        (xy 121.420258 135.700208)
        (xy 121.419358 135.706292)
        (xy 121.41846 135.71137)
        (xy 121.417615 135.715288)
        (xy 121.416874 135.717896)
        (xy 121.416289 135.719041)
        (xy 121.55 136.0125)
        (xy 121.683711 135.719041)
        (xy 121.683125 135.717896)
        (xy 121.682384 135.715288)
        (xy 121.681539 135.71137)
        (xy 121.680641 135.706292)
        (xy 121.679741 135.700208)
        (xy 121.678891 135.693269)
        (xy 121.67814 135.685626)
        (xy 121.67754 135.677433)
        (xy 121.677143 135.66884)
        (xy 121.677 135.66)
      )
    )
  )
  (zone (net 23) (net_name "+5V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.996086 131.524086)
        (xy 121.946522 131.523582)
        (xy 121.90358 131.521955)
        (xy 121.866016 131.519036)
        (xy 121.832584 131.514651)
        (xy 121.80204 131.508631)
        (xy 121.773139 131.500802)
        (xy 121.744636 131.490995)
        (xy 121.715287 131.479037)
        (xy 121.683845 131.464757)
        (xy 121.649068 131.447985)
        (xy 121.437502 131.649448)
        (xy 121.647079 131.852979)
        (xy 121.682174 131.836465)
        (xy 121.713874 131.822409)
        (xy 121.743435 131.810639)
        (xy 121.772114 131.800987)
        (xy 121.801169 131.793285)
        (xy 121.831858 131.787362)
        (xy 121.865436 131.78305)
        (xy 121.903162 131.780179)
        (xy 121.946293 131.778581)
        (xy 121.996086 131.778086)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.945 135.6484)
        (xy 102.894977 135.647313)
        (xy 102.852312 135.644087)
        (xy 102.815523 135.638774)
        (xy 102.783128 135.631426)
        (xy 102.753646 135.622094)
        (xy 102.725595 135.610831)
        (xy 102.697494 135.597688)
        (xy 102.667861 135.582717)
        (xy 102.635215 135.56597)
        (xy 102.598075 135.5475)
        (xy 102.3875 135.75)
        (xy 102.598075 135.9525)
        (xy 102.635215 135.934029)
        (xy 102.667861 135.917282)
        (xy 102.697494 135.902311)
        (xy 102.725595 135.889168)
        (xy 102.753646 135.877905)
        (xy 102.783128 135.868573)
        (xy 102.815523 135.861225)
        (xy 102.852312 135.855912)
        (xy 102.894977 135.852686)
        (xy 102.945 135.8516)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.3984 132.020126)
        (xy 78.389729 132.185014)
        (xy 78.365165 132.320035)
        (xy 78.326877 132.431697)
        (xy 78.277037 132.526507)
        (xy 78.217814 132.610972)
        (xy 78.15138 132.691599)
        (xy 78.079905 132.774896)
        (xy 78.00556 132.867369)
        (xy 77.930515 132.975525)
        (xy 77.856941 133.105873)
        (xy 78.477481 133.769964)
        (xy 79.116811 133.123944)
        (xy 79.047111 132.991055)
        (xy 78.975882 132.880474)
        (xy 78.905213 132.785711)
        (xy 78.837192 132.700276)
        (xy 78.773906 132.617679)
        (xy 78.717444 132.53143)
        (xy 78.669894 132.43504)
        (xy 78.633345 132.322019)
        (xy 78.609884 132.185878)
        (xy 78.6016 132.020126)
      )
    )
  )
  (zone (net 23) (net_name "+5V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.996085 133.124085)
        (xy 121.946521 133.123581)
        (xy 121.903579 133.121954)
        (xy 121.866015 133.119035)
        (xy 121.832584 133.11465)
        (xy 121.80204 133.108629)
        (xy 121.773139 133.100801)
        (xy 121.744636 133.090994)
        (xy 121.715286 133.079036)
        (xy 121.683844 133.064756)
        (xy 121.649067 133.047984)
        (xy 121.437502 133.249448)
        (xy 121.64708 133.452978)
        (xy 121.682175 133.436464)
        (xy 121.713874 133.422407)
        (xy 121.743435 133.410638)
        (xy 121.772114 133.400986)
        (xy 121.801169 133.393284)
        (xy 121.831857 133.387361)
        (xy 121.865436 133.383049)
        (xy 121.903161 133.380178)
        (xy 121.946292 133.37858)
        (xy 121.996085 133.378085)
      )
    )
  )
  (zone (net 28) (net_name "/THERM") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.445064 133.948686)
        (xy 117.395042 133.947567)
        (xy 117.352379 133.944313)
        (xy 117.315593 133.938977)
        (xy 117.283203 133.931608)
        (xy 117.253727 133.922257)
        (xy 117.225683 133.910976)
        (xy 117.197591 133.897815)
        (xy 117.167968 133.882825)
        (xy 117.135332 133.866057)
        (xy 117.098204 133.847563)
        (xy 116.887501 134.049928)
        (xy 117.097945 134.252562)
        (xy 117.135097 134.234114)
        (xy 117.167753 134.217389)
        (xy 117.197396 134.202437)
        (xy 117.225505 134.189312)
        (xy 117.253563 134.178067)
        (xy 117.283051 134.168754)
        (xy 117.31545 134.161427)
        (xy 117.352243 134.156138)
        (xy 117.39491 134.152939)
        (xy 117.444933 134.151885)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.386276 120.99877)
        (xy 48.222046 120.995226)
        (xy 48.086937 120.975183)
        (xy 47.974544 120.940994)
        (xy 47.878462 120.895017)
        (xy 47.792287 120.839608)
        (xy 47.709615 120.777121)
        (xy 47.624041 120.709915)
        (xy 47.529161 120.640344)
        (xy 47.418571 120.570764)
        (xy 47.285866 120.503533)
        (xy 46.650162 121.153119)
        (xy 47.324097 121.762951)
        (xy 47.45248 121.687793)
        (xy 47.558646 121.611633)
        (xy 47.649131 121.536435)
        (xy 47.730471 121.464162)
        (xy 47.809201 121.396776)
        (xy 47.891856 121.336241)
        (xy 47.984972 121.28452)
        (xy 48.095085 121.243577)
        (xy 48.22873 121.215374)
        (xy 48.392442 121.201876)
      )
    )
  )
  (zone (net 37) (net_name "/OFFSET2") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.45596 141.22884)
        (xy 103.406921 141.218908)
        (xy 103.365502 141.208175)
        (xy 103.330236 141.196429)
        (xy 103.299655 141.183458)
        (xy 103.272292 141.169051)
        (xy 103.24668 141.152997)
        (xy 103.221352 141.135083)
        (xy 103.19484 141.1151)
        (xy 103.165677 141.092835)
        (xy 103.132396 141.068077)
        (xy 102.88928 141.230071)
        (xy 103.060651 141.466671)
        (xy 103.100476 141.455071)
        (xy 103.135572 141.444373)
        (xy 103.167388 141.434888)
        (xy 103.197373 141.426931)
        (xy 103.226975 141.420815)
        (xy 103.257644 141.416854)
        (xy 103.290828 141.415361)
        (xy 103.327976 141.416649)
        (xy 103.370538 141.421032)
        (xy 103.419962 141.428825)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.996085 128.324085)
        (xy 121.946521 128.323581)
        (xy 121.903579 128.321954)
        (xy 121.866015 128.319035)
        (xy 121.832584 128.31465)
        (xy 121.80204 128.308629)
        (xy 121.773139 128.300801)
        (xy 121.744636 128.290994)
        (xy 121.715286 128.279036)
        (xy 121.683844 128.264756)
        (xy 121.649067 128.247984)
        (xy 121.437502 128.449448)
        (xy 121.64708 128.652978)
        (xy 121.682175 128.636464)
        (xy 121.713874 128.622407)
        (xy 121.743435 128.610638)
        (xy 121.772114 128.600986)
        (xy 121.801169 128.593284)
        (xy 121.831857 128.587361)
        (xy 121.865436 128.583049)
        (xy 121.903161 128.580178)
        (xy 121.946292 128.57858)
        (xy 121.996085 128.578085)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.623 139.455)
        (xy 123.622495 139.504528)
        (xy 123.62087 139.547432)
        (xy 123.617959 139.584959)
        (xy 123.613592 139.618357)
        (xy 123.607605 139.648875)
        (xy 123.599829 139.677759)
        (xy 123.590097 139.706258)
        (xy 123.578243 139.735621)
        (xy 123.5641 139.767093)
        (xy 123.5475 139.801925)
        (xy 123.75 140.0125)
        (xy 123.9525 139.801925)
        (xy 123.935899 139.767093)
        (xy 123.921756 139.735621)
        (xy 123.909902 139.706258)
        (xy 123.90017 139.677759)
        (xy 123.892394 139.648875)
        (xy 123.886407 139.618357)
        (xy 123.88204 139.584959)
        (xy 123.879129 139.547432)
        (xy 123.877504 139.504528)
        (xy 123.877 139.455)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.409614 135.453923)
        (xy 121.364089 135.434408)
        (xy 121.32511 135.416406)
        (xy 121.29159 135.399285)
        (xy 121.26244 135.382409)
        (xy 121.236573 135.365145)
        (xy 121.212901 135.346858)
        (xy 121.190337 135.326914)
        (xy 121.167793 135.304679)
        (xy 121.144181 135.279518)
        (xy 121.118415 135.250799)
        (xy 120.846154 135.356731)
        (xy 120.962646 135.624644)
        (xy 121.001182 135.622717)
        (xy 121.035673 135.621766)
        (xy 121.067336 135.622117)
        (xy 121.097386 135.624095)
        (xy 121.127039 135.628027)
        (xy 121.157512 135.634237)
        (xy 121.19002 135.643052)
        (xy 121.225781 135.654798)
        (xy 121.266009 135.6698)
        (xy 121.311922 135.688384)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.595207 132.646411)
        (xy 78.597011 132.596409)
        (xy 78.600848 132.553794)
        (xy 78.606688 132.517085)
        (xy 78.6145 132.484799)
        (xy 78.624254 132.455454)
        (xy 78.635918 132.427567)
        (xy 78.649462 132.399658)
        (xy 78.664857 132.370243)
        (xy 78.68207 132.33784)
        (xy 78.701072 132.300969)
        (xy 78.501613 132.087512)
        (xy 78.296115 132.295161)
        (xy 78.314051 132.332562)
        (xy 78.330328 132.365445)
        (xy 78.344872 132.395289)
        (xy 78.357611 132.423576)
        (xy 78.36847 132.451785)
        (xy 78.377378 132.481398)
        (xy 78.384261 132.513894)
        (xy 78.389046 132.550756)
        (xy 78.391659 132.593463)
        (xy 78.392029 132.643496)
      )
    )
  )
  (zone (net 88) (net_name "/SIG_100XC2") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67.33714 131.230559)
        (xy 67.502361 131.221239)
        (xy 67.639146 131.231896)
        (xy 67.753888 131.259393)
        (xy 67.852982 131.300596)
        (xy 67.94282 131.35237)
        (xy 68.029796 131.411579)
        (xy 68.120303 131.475088)
        (xy 68.220736 131.539762)
        (xy 68.337488 131.602467)
        (xy 68.476953 131.660067)
        (xy 69.057821 130.961013)
        (xy 68.3366 130.407909)
        (xy 68.213348 130.494956)
        (xy 68.113376 130.581952)
        (xy 68.029754 130.667257)
        (xy 67.955553 130.749228)
        (xy 67.883845 130.826224)
        (xy 67.807699 130.896602)
        (xy 67.720186 130.958722)
        (xy 67.614379 131.01094)
        (xy 67.483348 131.051616)
        (xy 67.320164 131.079108)
      )
    )
  )
  (zone (net 49) (net_name "/SIG_{1}") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77.228979 123.865119)
        (xy 77.385045 123.809677)
        (xy 77.519403 123.781556)
        (xy 77.63732 123.775912)
        (xy 77.74406 123.787901)
        (xy 77.84489 123.812683)
        (xy 77.945075 123.845414)
        (xy 78.049882 123.881251)
        (xy 78.164575 123.915353)
        (xy 78.294421 123.942875)
        (xy 78.444686 123.958977)
        (xy 78.805281 123.124678)
        (xy 77.957526 122.796965)
        (xy 77.863669 122.915411)
        (xy 77.79227 123.027303)
        (xy 77.736186 123.133)
        (xy 77.688271 123.232864)
        (xy 77.64138 123.327255)
        (xy 77.588368 123.416533)
        (xy 77.52209 123.501059)
        (xy 77.435402 123.581192)
        (xy 77.321159 123.657294)
        (xy 77.172216 123.729725)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.996085 129.124085)
        (xy 121.946521 129.123581)
        (xy 121.903579 129.121954)
        (xy 121.866015 129.119035)
        (xy 121.832584 129.11465)
        (xy 121.80204 129.108629)
        (xy 121.773139 129.100801)
        (xy 121.744636 129.090994)
        (xy 121.715286 129.079036)
        (xy 121.683844 129.064756)
        (xy 121.649067 129.047984)
        (xy 121.437502 129.249448)
        (xy 121.64708 129.452978)
        (xy 121.682175 129.436464)
        (xy 121.713874 129.422407)
        (xy 121.743435 129.410638)
        (xy 121.772114 129.400986)
        (xy 121.801169 129.393284)
        (xy 121.831857 129.387361)
        (xy 121.865436 129.383049)
        (xy 121.903161 129.380178)
        (xy 121.946292 129.37858)
        (xy 121.996085 129.378085)
      )
    )
  )
  (zone (net 18) (net_name "/SIG_{2}") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.479586 137.107917)
        (xy 78.461756 137.272437)
        (xy 78.428871 137.405638)
        (xy 78.382977 137.514338)
        (xy 78.326121 137.605358)
        (xy 78.260351 137.685518)
        (xy 78.187714 137.761639)
        (xy 78.110257 137.84054)
        (xy 78.030027 137.929043)
        (xy 77.949072 138.033967)
        (xy 77.869438 138.162133)
        (xy 78.464074 138.849514)
        (xy 79.127689 138.228468)
        (xy 79.061972 138.092639)
        (xy 78.992498 137.979785)
        (xy 78.922019 137.883336)
        (xy 78.853287 137.796728)
        (xy 78.789057 137.713391)
        (xy 78.732081 137.62676)
        (xy 78.685111 137.530266)
        (xy 78.650902 137.417343)
        (xy 78.632205 137.281423)
        (xy 78.631774 137.11594)
      )
    )
  )
  (zone (net 28) (net_name "/THERM") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 72.077759 141.923374)
        (xy 72.127279 141.916222)
        (xy 72.169894 141.91239)
        (xy 72.207055 141.911582)
        (xy 72.240217 141.913505)
        (xy 72.270832 141.917863)
        (xy 72.300353 141.924362)
        (xy 72.330232 141.932706)
        (xy 72.361923 141.942602)
        (xy 72.396878 141.953754)
        (xy 72.43655 141.965868)
        (xy 72.610969 141.731506)
        (xy 72.369969 141.566379)
        (xy 72.33637 141.590704)
        (xy 72.306921 141.61259)
        (xy 72.280153 141.632228)
        (xy 72.254595 141.649812)
        (xy 72.228778 141.665534)
        (xy 72.201231 141.679585)
        (xy 72.170485 141.692159)
        (xy 72.13507 141.703448)
        (xy 72.093516 141.713644)
        (xy 72.044353 141.72294)
      )
    )
  )
  (zone (net 81) (net_name "/~{EN_ATN_1X}") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.724194 120.86943)
        (xy 66.560356 120.881299)
        (xy 66.423962 120.874011)
        (xy 66.308859 120.850511)
        (xy 66.20889 120.813745)
        (xy 66.117899 120.766659)
        (xy 66.029733 120.712199)
        (xy 65.938235 120.653311)
        (xy 65.83725 120.592943)
        (xy 65.720623 120.534038)
        (xy 65.582199 120.479545)
        (xy 65.010198 121.185873)
        (xy 65.738342 121.729832)
        (xy 65.859112 121.642968)
        (xy 65.957671 121.55719)
        (xy 66.040707 121.473839)
        (xy 66.114912 121.394258)
        (xy 66.186977 121.319787)
        (xy 66.263593 121.251769)
        (xy 66.351449 121.191546)
        (xy 66.457238 121.140459)
        (xy 66.587649 121.099851)
        (xy 66.749375 121.071063)
      )
    )
  )
  (zone (net 15) (net_name "/VFILT'") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.789921 135.35059)
        (xy 112.739046 135.351819)
        (xy 112.696147 135.349263)
        (xy 112.659522 135.343335)
        (xy 112.627472 135.334446)
        (xy 112.598296 135.323011)
        (xy 112.570294 135.309442)
        (xy 112.541765 135.294152)
        (xy 112.511009 135.277555)
        (xy 112.476326 135.260063)
        (xy 112.436015 135.242091)
        (xy 112.237695 135.456605)
        (xy 112.459796 135.646391)
        (xy 112.497722 135.623816)
        (xy 112.530115 135.602378)
        (xy 112.558713 135.58229)
        (xy 112.585253 135.563761)
        (xy 112.611472 135.547003)
        (xy 112.639106 135.532226)
        (xy 112.669893 135.519641)
        (xy 112.70557 135.509459)
        (xy 112.747874 135.501891)
        (xy 112.798542 135.497148)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.996085 130.724085)
        (xy 121.946521 130.723581)
        (xy 121.903579 130.721954)
        (xy 121.866015 130.719035)
        (xy 121.832584 130.71465)
        (xy 121.80204 130.708629)
        (xy 121.773139 130.700801)
        (xy 121.744636 130.690994)
        (xy 121.715286 130.679036)
        (xy 121.683844 130.664756)
        (xy 121.649067 130.647984)
        (xy 121.437502 130.849448)
        (xy 121.64708 131.052978)
        (xy 121.682175 131.036464)
        (xy 121.713874 131.022407)
        (xy 121.743435 131.010638)
        (xy 121.772114 131.000986)
        (xy 121.801169 130.993284)
        (xy 121.831857 130.987361)
        (xy 121.865436 130.983049)
        (xy 121.903161 130.980178)
        (xy 121.946292 130.97858)
        (xy 121.996085 130.978085)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47.958289 121.215055)
        (xy 48.008321 121.214623)
        (xy 48.051064 121.216553)
        (xy 48.087997 121.220747)
        (xy 48.1206 121.227109)
        (xy 48.150351 121.235542)
        (xy 48.178731 121.245948)
        (xy 48.207218 121.258233)
        (xy 48.237291 121.272297)
        (xy 48.27043 121.288046)
        (xy 48.308114 121.305382)
        (xy 48.512448 121.096587)
        (xy 48.295826 120.900569)
        (xy 48.259262 120.920158)
        (xy 48.227139 120.937888)
        (xy 48.197975 120.953751)
        (xy 48.170285 120.96774)
        (xy 48.142589 120.97985)
        (xy 48.113404 120.990072)
        (xy 48.081247 120.998399)
        (xy 48.044636 121.004826)
        (xy 48.002089 121.009345)
        (xy 47.952123 121.01195)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.755093 131.777319)
        (xy 119.804621 131.777787)
        (xy 119.847526 131.779381)
        (xy 119.885055 131.782266)
        (xy 119.918457 131.786608)
        (xy 119.948978 131.792574)
        (xy 119.977868 131.800329)
        (xy 120.006374 131.81004)
        (xy 120.035745 131.821873)
        (xy 120.067227 131.835994)
        (xy 120.102071 131.85257)
        (xy 120.312499 131.64992)
        (xy 120.10178 131.447571)
        (xy 120.06696 131.464196)
        (xy 120.035498 131.478362)
        (xy 120.006144 131.490237)
        (xy 119.977652 131.499989)
        (xy 119.948773 131.507786)
        (xy 119.91826 131.513795)
        (xy 119.884865 131.518185)
        (xy 119.84734 131.521124)
        (xy 119.804438 131.522779)
        (xy 119.75491 131.52332)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59.255 121.2016)
        (xy 59.305022 121.202686)
        (xy 59.347687 121.205912)
        (xy 59.384476 121.211225)
        (xy 59.416871 121.218573)
        (xy 59.446353 121.227905)
        (xy 59.474404 121.239168)
        (xy 59.502505 121.252311)
        (xy 59.532138 121.267282)
        (xy 59.564784 121.284029)
        (xy 59.601925 121.3025)
        (xy 59.8125 121.1)
        (xy 59.601925 120.8975)
        (xy 59.564784 120.91597)
        (xy 59.532138 120.932717)
        (xy 59.502505 120.947688)
        (xy 59.474404 120.960831)
        (xy 59.446353 120.972094)
        (xy 59.416871 120.981426)
        (xy 59.384476 120.988774)
        (xy 59.347687 120.994087)
        (xy 59.305022 120.997313)
        (xy 59.255 120.9984)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.098711 132.304496)
        (xy 102.04806 132.299567)
        (xy 102.005785 132.291844)
        (xy 101.970145 132.281531)
        (xy 101.939405 132.268834)
        (xy 101.911825 132.253955)
        (xy 101.885668 132.237101)
        (xy 101.859197 132.218475)
        (xy 101.830672 132.198282)
        (xy 101.798358 132.176726)
        (xy 101.760515 132.154013)
        (xy 101.53772 132.342983)
        (xy 101.735252 132.558223)
        (xy 101.775628 132.540397)
        (xy 101.810376 132.523033)
        (xy 101.841192 132.506549)
        (xy 101.869777 132.491364)
        (xy 101.897829 132.477898)
        (xy 101.927046 132.466569)
        (xy 101.959129 132.457798)
        (xy 101.995775 132.452003)
        (xy 102.038683 132.449604)
        (xy 102.089553 132.451021)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.595088 123.523315)
        (xy 117.545559 123.522775)
        (xy 117.502657 123.52112)
        (xy 117.465132 123.518182)
        (xy 117.431736 123.513792)
        (xy 117.401223 123.507783)
        (xy 117.372344 123.499986)
        (xy 117.343852 123.490235)
        (xy 117.314498 123.47836)
        (xy 117.283036 123.464194)
        (xy 117.248217 123.44757)
        (xy 117.037501 123.649921)
        (xy 117.247932 123.852569)
        (xy 117.282774 123.835993)
        (xy 117.314257 123.821871)
        (xy 117.343627 123.810038)
        (xy 117.372133 123.800327)
        (xy 117.401023 123.792571)
        (xy 117.431545 123.786605)
        (xy 117.464946 123.782263)
        (xy 117.502475 123.779377)
        (xy 117.54538 123.777783)
        (xy 117.594909 123.777314)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.755093 133.377318)
        (xy 119.804621 133.377786)
        (xy 119.847526 133.37938)
        (xy 119.885055 133.382265)
        (xy 119.918456 133.386607)
        (xy 119.948978 133.392573)
        (xy 119.977868 133.400328)
        (xy 120.006374 133.410039)
        (xy 120.035744 133.421872)
        (xy 120.067227 133.435993)
        (xy 120.10207 133.452569)
        (xy 120.312499 133.24992)
        (xy 120.101781 133.047571)
        (xy 120.066961 133.064196)
        (xy 120.035499 133.078362)
        (xy 120.006145 133.090236)
        (xy 119.977653 133.099988)
        (xy 119.948774 133.107785)
        (xy 119.918261 133.113794)
        (xy 119.884866 133.118184)
        (xy 119.84734 133.121123)
        (xy 119.804438 133.122779)
        (xy 119.75491 133.123319)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59.545 120.9984)
        (xy 59.494977 120.997313)
        (xy 59.452312 120.994087)
        (xy 59.415523 120.988774)
        (xy 59.383128 120.981426)
        (xy 59.353646 120.972094)
        (xy 59.325595 120.960831)
        (xy 59.297494 120.947688)
        (xy 59.267861 120.932717)
        (xy 59.235215 120.91597)
        (xy 59.198075 120.8975)
        (xy 58.9875 121.1)
        (xy 59.198075 121.3025)
        (xy 59.235215 121.284029)
        (xy 59.267861 121.267282)
        (xy 59.297494 121.252311)
        (xy 59.325595 121.239168)
        (xy 59.353646 121.227905)
        (xy 59.383128 121.218573)
        (xy 59.415523 121.211225)
        (xy 59.452312 121.205912)
        (xy 59.494977 121.202686)
        (xy 59.545 121.2016)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61.673406 124.345)
        (xy 61.675165 124.294141)
        (xy 61.680236 124.251465)
        (xy 61.688305 124.215252)
        (xy 61.699061 124.183779)
        (xy 61.712189 124.155325)
        (xy 61.727379 124.128168)
        (xy 61.744318 124.100586)
        (xy 61.762692 124.070858)
        (xy 61.78219 124.037261)
        (xy 61.8025 123.998075)
        (xy 61.6 123.7875)
        (xy 61.3975 123.998075)
        (xy 61.417809 124.037261)
        (xy 61.437307 124.070858)
        (xy 61.455681 124.100586)
        (xy 61.47262 124.128168)
        (xy 61.48781 124.155325)
        (xy 61.500938 124.183779)
        (xy 61.511694 124.215252)
        (xy 61.519763 124.251465)
        (xy 61.524834 124.294141)
        (xy 61.526594 124.345)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.595088 125.923314)
        (xy 117.545559 125.922774)
        (xy 117.502657 125.921119)
        (xy 117.465132 125.918181)
        (xy 117.431736 125.913791)
        (xy 117.401223 125.907782)
        (xy 117.372344 125.899986)
        (xy 117.343852 125.890234)
        (xy 117.314498 125.87836)
        (xy 117.283036 125.864194)
        (xy 117.248217 125.84757)
        (xy 117.037501 126.049921)
        (xy 117.247932 126.252569)
        (xy 117.282774 126.235993)
        (xy 117.314257 126.221871)
        (xy 117.343627 126.210038)
        (xy 117.372133 126.200327)
        (xy 117.401023 126.192571)
        (xy 117.431544 126.186605)
        (xy 117.464946 126.182262)
        (xy 117.502475 126.179376)
        (xy 117.54538 126.177782)
        (xy 117.594909 126.177313)
      )
    )
  )
  (zone (net 47) (net_name "/SIG_1X") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63.968242 139.008796)
        (xy 64.133685 139.016472)
        (xy 64.268702 139.041234)
        (xy 64.380001 139.080588)
        (xy 64.474286 139.132043)
        (xy 64.558263 139.193106)
        (xy 64.638639 139.261284)
        (xy 64.722117 139.334085)
        (xy 64.815406 139.409017)
        (xy 64.925209 139.483587)
        (xy 65.058234 139.555303)
        (xy 65.707484 138.919254)
        (xy 65.046547 138.295358)
        (xy 64.914875 138.369529)
        (xy 64.806474 138.446123)
        (xy 64.714592 138.522772)
        (xy 64.632478 138.597109)
        (xy 64.553381 138.666766)
        (xy 64.470551 138.729376)
        (xy 64.377237 138.782571)
        (xy 64.266687 138.823983)
        (xy 64.132152 138.851246)
        (xy 63.96688 138.861991)
      )
    )
  )
  (zone (net 33) (net_name "/OUT2-") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.584685 126.4762)
        (xy 112.531679 126.4762)
        (xy 112.486835 126.4762)
        (xy 112.448304 126.476199)
        (xy 112.414236 126.476199)
        (xy 112.382782 126.4762)
        (xy 112.352093 126.4762)
        (xy 112.320319 126.4762)
        (xy 112.285612 126.4762)
        (xy 112.246122 126.4762)
        (xy 112.2 126.4762)
        (xy 112.120451 126.780749)
        (xy 112.412538 126.775039)
        (xy 112.422739 126.744361)
        (xy 112.43214 126.715306)
        (xy 112.441625 126.688252)
        (xy 112.452079 126.663577)
        (xy 112.464387 126.64166)
        (xy 112.479433 126.62288)
        (xy 112.498101 126.607614)
        (xy 112.521276 126.596242)
        (xy 112.549842 126.589141)
        (xy 112.584685 126.58669)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.12796 136.11028)
        (xy 50.098855 136.068653)
        (xy 50.077165 136.031589)
        (xy 50.061642 135.997903)
        (xy 50.051039 135.966406)
        (xy 50.044106 135.935912)
        (xy 50.039598 135.905236)
        (xy 50.036265 135.873189)
        (xy 50.032861 135.838585)
        (xy 50.028136 135.800238)
        (xy 50.020845 135.756961)
        (xy 49.7325 135.71)
        (xy 49.696846 135.99996)
        (xy 49.73635 136.019077)
        (xy 49.77184 136.03435)
        (xy 49.804107 136.047307)
        (xy 49.833939 136.05948)
        (xy 49.862126 136.072398)
        (xy 49.889459 136.087591)
        (xy 49.916727 136.106589)
        (xy 49.944719 136.130924)
        (xy 49.974227 136.162124)
        (xy 50.00604 136.20172)
      )
    )
  )
  (zone (net 92) (net_name "Net-(R72-Pad1)") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57.544225 141.225175)
        (xy 57.592015 141.239989)
        (xy 57.632144 141.254836)
        (xy 57.666049 141.270071)
        (xy 57.69517 141.286053)
        (xy 57.720944 141.303139)
        (xy 57.744811 141.321689)
        (xy 57.768208 141.34206)
        (xy 57.792575 141.36461)
        (xy 57.819349 141.389696)
        (xy 57.849971 141.417678)
        (xy 58.108153 141.280968)
        (xy 57.961458 141.028326)
        (xy 57.920667 141.035859)
        (xy 57.884672 141.042972)
        (xy 57.852064 141.049207)
        (xy 57.82143 141.054107)
        (xy 57.791363 141.057213)
        (xy 57.760451 141.058068)
        (xy 57.727285 141.056215)
        (xy 57.690455 141.051195)
        (xy 57.64855 141.042552)
        (xy 57.600162 141.029827)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.596084 134.724084)
        (xy 117.54652 134.72358)
        (xy 117.503578 134.721953)
        (xy 117.466014 134.719034)
        (xy 117.432583 134.714649)
        (xy 117.402039 134.708629)
        (xy 117.373138 134.7008)
        (xy 117.344635 134.690993)
        (xy 117.315285 134.679035)
        (xy 117.283843 134.664756)
        (xy 117.249066 134.647984)
        (xy 117.037502 134.849449)
        (xy 117.247081 135.052978)
        (xy 117.282176 135.036464)
        (xy 117.313875 135.022407)
        (xy 117.343435 135.010637)
        (xy 117.372114 135.000986)
        (xy 117.401169 134.993283)
        (xy 117.431857 134.98736)
        (xy 117.465435 134.983048)
        (xy 117.503161 134.980177)
        (xy 117.546291 134.978579)
        (xy 117.596084 134.978084)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.755093 132.577318)
        (xy 119.804621 132.577786)
        (xy 119.847526 132.57938)
        (xy 119.885055 132.582265)
        (xy 119.918456 132.586607)
        (xy 119.948978 132.592573)
        (xy 119.977868 132.600328)
        (xy 120.006374 132.610039)
        (xy 120.035744 132.621872)
        (xy 120.067227 132.635993)
        (xy 120.10207 132.652569)
        (xy 120.312499 132.44992)
        (xy 120.101781 132.247571)
        (xy 120.066961 132.264196)
        (xy 120.035499 132.278362)
        (xy 120.006145 132.290237)
        (xy 119.977653 132.299988)
        (xy 119.948774 132.307785)
        (xy 119.918261 132.313794)
        (xy 119.884866 132.318184)
        (xy 119.84734 132.321123)
        (xy 119.804438 132.322779)
        (xy 119.75491 132.323319)
      )
    )
  )
  (zone (net 23) (net_name "+5V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.996084 132.324084)
        (xy 121.94652 132.32358)
        (xy 121.903578 132.321953)
        (xy 121.866014 132.319034)
        (xy 121.832583 132.314649)
        (xy 121.802039 132.308629)
        (xy 121.773138 132.3008)
        (xy 121.744635 132.290993)
        (xy 121.715285 132.279035)
        (xy 121.683843 132.264756)
        (xy 121.649066 132.247984)
        (xy 121.437502 132.449449)
        (xy 121.647081 132.652978)
        (xy 121.682176 132.636464)
        (xy 121.713875 132.622407)
        (xy 121.743435 132.610637)
        (xy 121.772114 132.600986)
        (xy 121.801169 132.593283)
        (xy 121.831857 132.58736)
        (xy 121.865435 132.583048)
        (xy 121.903161 132.580177)
        (xy 121.946291 132.578579)
        (xy 121.996084 132.578084)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.645 139.773)
        (xy 123.595471 139.772495)
        (xy 123.552567 139.77087)
        (xy 123.51504 139.767959)
        (xy 123.481642 139.763592)
        (xy 123.451124 139.757605)
        (xy 123.42224 139.749829)
        (xy 123.393741 139.740097)
        (xy 123.364378 139.728243)
        (xy 123.332906 139.7141)
        (xy 123.298075 139.6975)
        (xy 123.0875 139.9)
        (xy 123.298075 140.1025)
        (xy 123.332906 140.085899)
        (xy 123.364378 140.071756)
        (xy 123.393741 140.059902)
        (xy 123.42224 140.05017)
        (xy 123.451124 140.042394)
        (xy 123.481642 140.036407)
        (xy 123.51504 140.03204)
        (xy 123.552567 140.029129)
        (xy 123.595471 140.027504)
        (xy 123.645 140.027)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.3984 131.755)
        (xy 78.397313 131.805022)
        (xy 78.394087 131.847687)
        (xy 78.388774 131.884476)
        (xy 78.381426 131.916871)
        (xy 78.372094 131.946353)
        (xy 78.360831 131.974404)
        (xy 78.347688 132.002505)
        (xy 78.332717 132.032138)
        (xy 78.31597 132.064784)
        (xy 78.2975 132.101925)
        (xy 78.5 132.3125)
        (xy 78.7025 132.101925)
        (xy 78.684029 132.064784)
        (xy 78.667282 132.032138)
        (xy 78.652311 132.002505)
        (xy 78.639168 131.974404)
        (xy 78.627905 131.946353)
        (xy 78.618573 131.916871)
        (xy 78.611225 131.884476)
        (xy 78.605912 131.847687)
        (xy 78.602686 131.805022)
        (xy 78.6016 131.755)
      )
    )
  )
  (zone (net 45) (net_name "/SIG_IN_{2}") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.665067 127.371294)
        (xy 54.641826 127.535276)
        (xy 54.604445 127.667358)
        (xy 54.554773 127.774451)
        (xy 54.494658 127.863465)
        (xy 54.42595 127.941311)
        (xy 54.350498 128.014901)
        (xy 54.270151 128.091144)
        (xy 54.186758 128.176952)
        (xy 54.102168 128.279236)
        (xy 54.018231 128.404907)
        (xy 54.590236 129.111232)
        (xy 55.273665 128.512058)
        (xy 55.212238 128.37398)
        (xy 55.146205 128.258841)
        (xy 55.078559 128.160141)
        (xy 55.012295 128.071385)
        (xy 54.950405 127.986073)
        (xy 54.895884 127.897709)
        (xy 54.851723 127.799795)
        (xy 54.820918 127.685834)
        (xy 54.806461 127.549327)
        (xy 54.811347 127.383779)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.148569 124.484452)
        (xy 93.103137 124.46349)
        (xy 93.065305 124.443504)
        (xy 93.033693 124.423949)
        (xy 93.006923 124.404282)
        (xy 92.983616 124.383959)
        (xy 92.962392 124.362436)
        (xy 92.941872 124.339169)
        (xy 92.920677 124.313616)
        (xy 92.897428 124.285231)
        (xy 92.870746 124.253472)
        (xy 92.596849 124.3551)
        (xy 92.709103 124.624815)
        (xy 92.750529 124.622702)
        (xy 92.787146 124.620377)
        (xy 92.820291 124.618477)
        (xy 92.851302 124.617642)
        (xy 92.881517 124.618511)
        (xy 92.912274 124.621721)
        (xy 92.944909 124.627913)
        (xy 92.980761 124.637725)
        (xy 93.021168 124.651796)
        (xy 93.067468 124.670765)
      )
    )
  )
  (zone (net 3) (net_name "/ATN_IN") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56.930742 132.708205)
        (xy 57.011569 132.852763)
        (xy 57.061823 132.980503)
        (xy 57.087161 133.095803)
        (xy 57.093241 133.203043)
        (xy 57.085719 133.3066)
        (xy 57.070252 133.410856)
        (xy 57.052497 133.520188)
        (xy 57.038112 133.638975)
        (xy 57.032754 133.771598)
        (xy 57.042079 133.922435)
        (xy 57.925034 134.138018)
        (xy 58.105943 133.247312)
        (xy 57.973434 133.174646)
        (xy 57.851154 133.123023)
        (xy 57.737548 133.085458)
        (xy 57.631063 133.054968)
        (xy 57.530146 133.024569)
        (xy 57.433243 132.987279)
        (xy 57.3388 132.936115)
        (xy 57.245264 132.864092)
        (xy 57.151082 132.764229)
        (xy 57.054701 132.629541)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.655 140.027)
        (xy 121.704528 140.027504)
        (xy 121.747432 140.029129)
        (xy 121.784959 140.03204)
        (xy 121.818357 140.036407)
        (xy 121.848875 140.042394)
        (xy 121.877759 140.05017)
        (xy 121.906258 140.059902)
        (xy 121.935621 140.071756)
        (xy 121.967093 140.085899)
        (xy 122.001925 140.1025)
        (xy 122.2125 139.9)
        (xy 122.001925 139.6975)
        (xy 121.967093 139.7141)
        (xy 121.935621 139.728243)
        (xy 121.906258 139.740097)
        (xy 121.877759 139.749829)
        (xy 121.848875 139.757605)
        (xy 121.818357 139.763592)
        (xy 121.784959 139.767959)
        (xy 121.747432 139.77087)
        (xy 121.704528 139.772495)
        (xy 121.655 139.773)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73.055977 137.817158)
        (xy 73.127264 137.9665)
        (xy 73.169282 138.097107)
        (xy 73.187358 138.213705)
        (xy 73.186818 138.321022)
        (xy 73.172986 138.423784)
        (xy 73.151189 138.526718)
        (xy 73.126752 138.63455)
        (xy 73.105001 138.752009)
        (xy 73.091263 138.883819)
        (xy 73.090862 139.03471)
        (xy 73.957993 139.307047)
        (xy 74.196232 138.429934)
        (xy 74.068942 138.348906)
        (xy 73.950529 138.289399)
        (xy 73.839882 138.244378)
        (xy 73.735893 138.206811)
        (xy 73.637452 138.169662)
        (xy 73.543452 138.125898)
        (xy 73.452783 138.068485)
        (xy 73.364336 137.990388)
        (xy 73.277003 137.884574)
        (xy 73.189674 137.744009)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.658385 121.215424)
        (xy 58.708416 121.21495)
        (xy 58.751161 121.216844)
        (xy 58.788098 121.221008)
        (xy 58.820706 121.227342)
        (xy 58.850465 121.23575)
        (xy 58.878853 121.246134)
        (xy 58.90735 121.258394)
        (xy 58.937435 121.272434)
        (xy 58.970587 121.288155)
        (xy 59.008286 121.305459)
        (xy 59.212445 121.096493)
        (xy 58.99566 120.900657)
        (xy 58.959113 120.920276)
        (xy 58.927005 120.938033)
        (xy 58.897853 120.95392)
        (xy 58.870175 120.967933)
        (xy 58.842489 120.980065)
        (xy 58.813313 120.990311)
        (xy 58.781162 120.998666)
        (xy 58.744557 121.005123)
        (xy 58.702013 121.009678)
        (xy 58.652049 121.012324)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.996084 129.924084)
        (xy 121.94652 129.92358)
        (xy 121.903578 129.921953)
        (xy 121.866014 129.919034)
        (xy 121.832583 129.914649)
        (xy 121.802039 129.908629)
        (xy 121.773138 129.9008)
        (xy 121.744635 129.890993)
        (xy 121.715285 129.879035)
        (xy 121.683843 129.864756)
        (xy 121.649066 129.847984)
        (xy 121.437502 130.049449)
        (xy 121.647081 130.252978)
        (xy 121.682176 130.236464)
        (xy 121.713875 130.222407)
        (xy 121.743435 130.210637)
        (xy 121.772114 130.200986)
        (xy 121.801169 130.193283)
        (xy 121.831857 130.18736)
        (xy 121.865435 130.183048)
        (xy 121.903161 130.180177)
        (xy 121.946291 130.178579)
        (xy 121.996084 130.178084)
      )
    )
  )
  (zone (net 46) (net_name "/SIG_IN_{3}") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57.646395 127.373548)
        (xy 57.639291 127.539016)
        (xy 57.614996 127.674119)
        (xy 57.576027 127.785554)
        (xy 57.524899 127.880017)
        (xy 57.464128 127.964205)
        (xy 57.396229 128.044816)
        (xy 57.323717 128.128546)
        (xy 57.249109 128.222093)
        (xy 57.174919 128.332155)
        (xy 57.103665 128.465427)
        (xy 57.741958 129.112471)
        (xy 58.363562 128.449378)
        (xy 58.288935 128.317964)
        (xy 58.211966 128.209828)
        (xy 58.134999 128.118212)
        (xy 58.060378 128.036356)
        (xy 57.990447 127.9575)
        (xy 57.927551 127.874888)
        (xy 57.874033 127.781758)
        (xy 57.832238 127.671352)
        (xy 57.80451 127.536912)
        (xy 57.793194 127.371678)
      )
    )
  )
  (zone (net 48) (net_name "/SIG_100XD") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 64.869081 135.146091)
        (xy 64.943809 134.99844)
        (xy 65.021574 134.885408)
        (xy 65.102867 134.79989)
        (xy 65.18818 134.734783)
        (xy 65.278002 134.682982)
        (xy 65.372824 134.637383)
        (xy 65.473138 134.590884)
        (xy 65.579433 134.536378)
        (xy 65.692202 134.466764)
        (xy 65.811934 134.374937)
        (xy 65.498055 133.521963)
        (xy 64.658 133.868938)
        (xy 64.671568 134.019217)
        (xy 64.696758 134.149326)
        (xy 64.728676 134.264438)
        (xy 64.762431 134.369726)
        (xy 64.793129 134.470365)
        (xy 64.815876 134.571528)
        (xy 64.825781 134.678388)
        (xy 64.81795 134.796119)
        (xy 64.787491 134.929895)
        (xy 64.72951 135.084889)
      )
    )
  )
  (zone (net 10) (net_name "/SIG_100X") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.872966 123.665317)
        (xy 67.104451 123.607604)
        (xy 67.300711 123.58726)
        (xy 67.470073 123.597778)
        (xy 67.620863 123.632652)
        (xy 67.761408 123.685373)
        (xy 67.900034 123.749437)
        (xy 68.045068 123.818335)
        (xy 68.204836 123.885561)
        (xy 68.387665 123.944607)
        (xy 68.601883 123.988969)
        (xy 69.227317 122.851113)
        (xy 68.065886 122.270626)
        (xy 67.914879 122.42891)
        (xy 67.798043 122.58143)
        (xy 67.704828 122.727568)
        (xy 67.624686 122.866704)
        (xy 67.547066 122.99822)
        (xy 67.46142 123.121497)
        (xy 67.357198 123.235915)
        (xy 67.223851 123.340856)
        (xy 67.05083 123.435701)
        (xy 66.827585 123.519831)
      )
    )
  )
  (zone (net 86) (net_name "/LMH_EN") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.968703 132.19397)
        (xy 109.998558 132.23518)
        (xy 110.020774 132.271968)
        (xy 110.036653 132.305499)
        (xy 110.047501 132.33694)
        (xy 110.054622 132.367457)
        (xy 110.05932 132.398217)
        (xy 110.062899 132.430386)
        (xy 110.066664 132.465131)
        (xy 110.071918 132.503618)
        (xy 110.079967 132.547015)
        (xy 110.369112 132.588768)
        (xy 110.399531 132.298212)
        (xy 110.359432 132.279768)
        (xy 110.323408 132.265237)
        (xy 110.290647 132.253068)
        (xy 110.260338 132.241711)
        (xy 110.231669 132.229614)
        (xy 110.203829 132.215228)
        (xy 110.176008 132.197002)
        (xy 110.147395 132.173385)
        (xy 110.117177 132.142827)
        (xy 110.084545 132.103779)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 96.501431 126.165548)
        (xy 96.546862 126.186509)
        (xy 96.584694 126.206495)
        (xy 96.616306 126.22605)
        (xy 96.643076 126.245717)
        (xy 96.666383 126.26604)
        (xy 96.687607 126.287563)
        (xy 96.708127 126.31083)
        (xy 96.729322 126.336383)
        (xy 96.752571 126.364768)
        (xy 96.779254 126.396528)
        (xy 97.053151 126.2949)
        (xy 96.940897 126.025185)
        (xy 96.89947 126.027297)
        (xy 96.862853 126.029622)
        (xy 96.829708 126.031522)
        (xy 96.798697 126.032357)
        (xy 96.768482 126.031488)
        (xy 96.737725 126.028278)
        (xy 96.70509 126.022086)
        (xy 96.669238 126.012274)
        (xy 96.628831 125.998203)
        (xy 96.582532 125.979235)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.305 140.027)
        (xy 123.354528 140.027504)
        (xy 123.397432 140.029129)
        (xy 123.434959 140.03204)
        (xy 123.468357 140.036407)
        (xy 123.498875 140.042394)
        (xy 123.527759 140.05017)
        (xy 123.556258 140.059902)
        (xy 123.585621 140.071756)
        (xy 123.617093 140.085899)
        (xy 123.651925 140.1025)
        (xy 123.8625 139.9)
        (xy 123.651925 139.6975)
        (xy 123.617093 139.7141)
        (xy 123.585621 139.728243)
        (xy 123.556258 139.740097)
        (xy 123.527759 139.749829)
        (xy 123.498875 139.757605)
        (xy 123.468357 139.763592)
        (xy 123.434959 139.767959)
        (xy 123.397432 139.77087)
        (xy 123.354528 139.772495)
        (xy 123.305 139.773)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59.136837 120.9984)
        (xy 58.970797 120.99046)
        (xy 58.834101 120.96797)
        (xy 58.720298 120.932922)
        (xy 58.622936 120.887308)
        (xy 58.535567 120.833119)
        (xy 58.451739 120.772349)
        (xy 58.365001 120.706989)
        (xy 58.268905 120.639032)
        (xy 58.156999 120.570469)
        (xy 58.022833 120.503294)
        (xy 57.387671 121.153411)
        (xy 58.062116 121.76268)
        (xy 58.19108 121.68665)
        (xy 58.2978 121.609008)
        (xy 58.388825 121.532018)
        (xy 58.470707 121.457946)
        (xy 58.549996 121.389055)
        (xy 58.633243 121.327611)
        (xy 58.727 121.275878)
        (xy 58.837818 121.236122)
        (xy 58.972246 121.210608)
        (xy 59.136837 121.2016)
      )
    )
  )
  (zone (net 32) (net_name "/OUT2+") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.584685 126.21331)
        (xy 112.549842 126.210858)
        (xy 112.521276 126.203757)
        (xy 112.498101 126.192385)
        (xy 112.479433 126.177119)
        (xy 112.464387 126.158339)
        (xy 112.452079 126.136422)
        (xy 112.441625 126.111747)
        (xy 112.43214 126.084693)
        (xy 112.422739 126.055638)
        (xy 112.412538 126.024961)
        (xy 112.120451 126.019251)
        (xy 112.2 126.3238)
        (xy 112.246122 126.3238)
        (xy 112.285612 126.3238)
        (xy 112.320319 126.323799)
        (xy 112.352093 126.3238)
        (xy 112.382782 126.3238)
        (xy 112.414236 126.3238)
        (xy 112.448304 126.323799)
        (xy 112.486835 126.3238)
        (xy 112.531679 126.3238)
        (xy 112.584685 126.3238)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.109925 128.434254)
        (xy 106.106723 128.384826)
        (xy 106.105134 128.341921)
        (xy 106.105232 128.304282)
        (xy 106.107088 128.27065)
        (xy 106.110776 128.239771)
        (xy 106.11637 128.210386)
        (xy 106.123943 128.181239)
        (xy 106.133568 128.151073)
        (xy 106.145318 128.11863)
        (xy 106.159267 128.082656)
        (xy 105.941587 127.887816)
        (xy 105.755402 128.112944)
        (xy 105.77456 128.146436)
        (xy 105.791018 128.176763)
        (xy 105.805035 128.205156)
        (xy 105.81687 128.232847)
        (xy 105.826785 128.261069)
        (xy 105.835038 128.291054)
        (xy 105.84189 128.324032)
        (xy 105.8476 128.361236)
        (xy 105.852429 128.403898)
        (xy 105.856637 128.453251)
      )
    )
  )
  (zone (net 91) (net_name "Net-(R70-Pad1)") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67.437795 141.37084)
        (xy 67.387802 141.372875)
        (xy 67.345019 141.372317)
        (xy 67.30797 141.369309)
        (xy 67.275179 141.363996)
        (xy 67.245173 141.356522)
        (xy 67.216474 141.34703)
        (xy 67.187608 141.335666)
        (xy 67.157099 141.322572)
        (xy 67.123472 141.307895)
        (xy 67.085252 141.291777)
        (xy 66.88772 141.507017)
        (xy 67.110515 141.695987)
        (xy 67.146431 141.675235)
        (xy 67.177968 141.656484)
        (xy 67.206609 141.639694)
        (xy 67.233836 141.624824)
        (xy 67.261129 141.611833)
        (xy 67.289972 141.600681)
        (xy 67.321845 141.591326)
        (xy 67.358232 141.583728)
        (xy 67.400612 141.577847)
        (xy 67.45047 141.573643)
      )
    )
  )
  (zone (net 82) (net_name "/~{EN_DC}") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.721164 120.375975)
        (xy 85.68109 120.346015)
        (xy 85.648247 120.318592)
        (xy 85.621399 120.292885)
        (xy 85.599309 120.268077)
        (xy 85.580743 120.243347)
        (xy 85.564463 120.217878)
        (xy 85.549236 120.19085)
        (xy 85.533824 120.161444)
        (xy 85.516993 120.128841)
        (xy 85.497507 120.092224)
        (xy 85.208455 120.134611)
        (xy 85.262107 120.421786)
        (xy 85.303065 120.428343)
        (xy 85.339364 120.43369)
        (xy 85.372179 120.438731)
        (xy 85.402684 120.44437)
        (xy 85.432057 120.451509)
        (xy 85.461471 120.461051)
        (xy 85.492103 120.473901)
        (xy 85.525127 120.490961)
        (xy 85.56172 120.513134)
        (xy 85.603057 120.541325)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (name "Conformal1") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67.5 134)
        (xy 81 134)
        (xy 81 141.5)
        (xy 51 141.5)
        (xy 51 124.5)
        (xy 67.5 124.5)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.095 139.773)
        (xy 123.045471 139.772495)
        (xy 123.002567 139.77087)
        (xy 122.96504 139.767959)
        (xy 122.931642 139.763592)
        (xy 122.901124 139.757605)
        (xy 122.87224 139.749829)
        (xy 122.843741 139.740097)
        (xy 122.814378 139.728243)
        (xy 122.782906 139.7141)
        (xy 122.748075 139.6975)
        (xy 122.5375 139.9)
        (xy 122.748075 140.1025)
        (xy 122.782906 140.085899)
        (xy 122.814378 140.071756)
        (xy 122.843741 140.059902)
        (xy 122.87224 140.05017)
        (xy 122.901124 140.042394)
        (xy 122.931642 140.036407)
        (xy 122.96504 140.03204)
        (xy 123.002567 140.029129)
        (xy 123.045471 140.027504)
        (xy 123.095 140.027)
      )
    )
  )
  (zone (net 84) (net_name "/~{EN_SIG}") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.863043 128.148896)
        (xy 79.698788 128.150977)
        (xy 79.563072 128.13557)
        (xy 79.449575 128.105249)
        (xy 79.351975 128.062588)
        (xy 79.263954 128.010161)
        (xy 79.179191 127.950542)
        (xy 79.091367 127.886304)
        (xy 78.994161 127.820022)
        (xy 78.881253 127.754269)
        (xy 78.746324 127.69162)
        (xy 78.13323 128.36259)
        (xy 78.827649 128.948992)
        (xy 78.953383 128.869483)
        (xy 79.05688 128.789733)
        (xy 79.144738 128.711481)
        (xy 79.223556 128.636465)
        (xy 79.299933 128.566423)
        (xy 79.380467 128.503094)
        (xy 79.471758 128.448216)
        (xy 79.580404 128.403527)
        (xy 79.713005 128.370766)
        (xy 79.876159 128.351671)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.545 139.773)
        (xy 122.495471 139.772495)
        (xy 122.452567 139.77087)
        (xy 122.41504 139.767959)
        (xy 122.381642 139.763592)
        (xy 122.351124 139.757605)
        (xy 122.32224 139.749829)
        (xy 122.293741 139.740097)
        (xy 122.264378 139.728243)
        (xy 122.232906 139.7141)
        (xy 122.198075 139.6975)
        (xy 121.9875 139.9)
        (xy 122.198075 140.1025)
        (xy 122.232906 140.085899)
        (xy 122.264378 140.071756)
        (xy 122.293741 140.059902)
        (xy 122.32224 140.05017)
        (xy 122.351124 140.042394)
        (xy 122.381642 140.036407)
        (xy 122.41504 140.03204)
        (xy 122.452567 140.029129)
        (xy 122.495471 140.027504)
        (xy 122.545 140.027)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.27786 130.275711)
        (xy 109.2944 130.322398)
        (xy 109.307613 130.363249)
        (xy 109.31777 130.399492)
        (xy 109.325143 130.432358)
        (xy 109.330003 130.463075)
        (xy 109.332623 130.492873)
        (xy 109.333274 130.522981)
        (xy 109.332228 130.554628)
        (xy 109.329757 130.589044)
        (xy 109.326133 130.627458)
        (xy 109.588646 130.755653)
        (xy 109.706484 130.488329)
        (xy 109.678928 130.46132)
        (xy 109.654833 130.436621)
        (xy 109.633614 130.413118)
        (xy 109.614685 130.389697)
        (xy 109.59746 130.365241)
        (xy 109.581353 130.338638)
        (xy 109.565779 130.308772)
        (xy 109.550153 130.274529)
        (xy 109.533889 130.234794)
        (xy 109.516401 130.188454)
      )
    )
  )
  (zone (net 34) (net_name "/OUT3+") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.584685 127.81331)
        (xy 112.549842 127.810858)
        (xy 112.521276 127.803757)
        (xy 112.498101 127.792385)
        (xy 112.479433 127.777119)
        (xy 112.464387 127.758339)
        (xy 112.452079 127.736422)
        (xy 112.441625 127.711747)
        (xy 112.43214 127.684693)
        (xy 112.422739 127.655638)
        (xy 112.412538 127.624961)
        (xy 112.120451 127.619251)
        (xy 112.2 127.9238)
        (xy 112.246122 127.9238)
        (xy 112.285612 127.9238)
        (xy 112.320319 127.923799)
        (xy 112.352093 127.9238)
        (xy 112.382782 127.9238)
        (xy 112.414236 127.9238)
        (xy 112.448304 127.923799)
        (xy 112.486835 127.9238)
        (xy 112.531679 127.9238)
        (xy 112.584685 127.9238)
      )
    )
  )
  (zone (net 3) (net_name "/ATN_IN") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59.124505 133.723677)
        (xy 58.959071 133.719609)
        (xy 58.823595 133.69793)
        (xy 58.711451 133.661246)
        (xy 58.616012 133.612168)
        (xy 58.530654 133.553301)
        (xy 58.448749 133.487255)
        (xy 58.363672 133.416637)
        (xy 58.268796 133.344055)
        (xy 58.157495 133.272118)
        (xy 58.023144 133.203433)
        (xy 57.387665 133.853241)
        (xy 58.061813 134.462839)
        (xy 58.191697 134.38604)
        (xy 58.298375 134.30741)
        (xy 58.388619 134.229144)
        (xy 58.469204 134.153439)
        (xy 58.546902 134.082492)
        (xy 58.628488 134.0185)
        (xy 58.720736 133.963658)
        (xy 58.830418 133.920164)
        (xy 58.964309 133.890213)
        (xy 59.129182 133.876004)
      )
    )
  )
  (zone (net 87) (net_name "/SIG_1XC2") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69.16044 137.682963)
        (xy 69.090203 137.832953)
        (xy 69.015786 137.948301)
        (xy 68.936934 138.036156)
        (xy 68.853391 138.103667)
        (xy 68.7649 138.157984)
        (xy 68.671208 138.206255)
        (xy 68.572058 138.255631)
        (xy 68.467196 138.313261)
        (xy 68.356364 138.386294)
        (xy 68.239309 138.48188)
        (xy 68.579431 139.324733)
        (xy 69.408347 138.95193)
        (xy 69.390041 138.801918)
        (xy 69.360616 138.67249)
        (xy 69.324834 138.558309)
        (xy 69.287462 138.45404)
        (xy 69.253265 138.354346)
        (xy 69.227005 138.253891)
        (xy 69.21345 138.147338)
        (xy 69.217363 138.029351)
        (xy 69.243509 137.894595)
        (xy 69.296654 137.737732)
      )
    )
  )
  (zone (net 14) (net_name "Net-(C13-Pad2)") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.855 135.473406)
        (xy 110.905858 135.475165)
        (xy 110.948534 135.480236)
        (xy 110.984747 135.488305)
        (xy 111.01622 135.499061)
        (xy 111.044674 135.512189)
        (xy 111.071831 135.527379)
        (xy 111.099413 135.544318)
        (xy 111.129141 135.562692)
        (xy 111.162738 135.58219)
        (xy 111.201925 135.6025)
        (xy 111.4125 135.4)
        (xy 111.201925 135.1975)
        (xy 111.162738 135.217809)
        (xy 111.129141 135.237307)
        (xy 111.099413 135.255681)
        (xy 111.071831 135.27262)
        (xy 111.044674 135.28781)
        (xy 111.01622 135.300938)
        (xy 110.984747 135.311694)
        (xy 110.948534 135.319763)
        (xy 110.905858 135.324834)
        (xy 110.855 135.326594)
      )
    )
  )
  (zone (net 3) (net_name "/ATN_IN") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56.701884 134.77277)
        (xy 56.836392 134.676373)
        (xy 56.957595 134.612079)
        (xy 57.069209 134.573815)
        (xy 57.174954 134.555508)
        (xy 57.278548 134.551086)
        (xy 57.38371 134.554474)
        (xy 57.494158 134.559602)
        (xy 57.613611 134.560395)
        (xy 57.745786 134.550781)
        (xy 57.894404 134.524688)
        (xy 58.010288 133.623214)
        (xy 57.104974 133.542651)
        (xy 57.04755 133.682187)
        (xy 57.009754 133.809208)
        (xy 56.984857 133.92604)
        (xy 56.966128 134.035009)
        (xy 56.946837 134.138442)
        (xy 56.920253 134.238665)
        (xy 56.879648 134.338005)
        (xy 56.818291 134.438788)
        (xy 56.729451 134.543341)
        (xy 56.6064 134.65399)
      )
    )
  )
  (zone (net 13) (net_name "Net-(C13-Pad1)") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.806561 134.629503)
        (xy 108.84519 134.662631)
        (xy 108.875359 134.693236)
        (xy 108.898609 134.722149)
        (xy 108.916478 134.750201)
        (xy 108.930508 134.778222)
        (xy 108.942238 134.807043)
        (xy 108.953208 134.837495)
        (xy 108.964958 134.870409)
        (xy 108.979028 134.906616)
        (xy 108.996958 134.946947)
        (xy 109.287878 134.920239)
        (xy 109.249821 134.630586)
        (xy 109.20653 134.621984)
        (xy 109.168113 134.616238)
        (xy 109.133419 134.61203)
        (xy 109.101298 134.60804)
        (xy 109.070601 134.60295)
        (xy 109.040177 134.59544)
        (xy 109.008877 134.584191)
        (xy 108.975551 134.567884)
        (xy 108.93905 134.545201)
        (xy 108.898224 134.514822)
      )
    )
  )
  (zone (net 49) (net_name "/SIG_{1}") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.611021 128.157381)
        (xy 66.454954 128.212822)
        (xy 66.320596 128.240943)
        (xy 66.202679 128.246587)
        (xy 66.095939 128.234598)
        (xy 65.995109 128.209816)
        (xy 65.894924 128.177085)
        (xy 65.790117 128.141248)
        (xy 65.675424 128.107146)
        (xy 65.545578 128.079624)
        (xy 65.395314 128.063523)
        (xy 65.034719 128.897822)
        (xy 65.882474 129.225535)
        (xy 65.97633 129.107088)
        (xy 66.047729 128.995196)
        (xy 66.103813 128.889499)
        (xy 66.151728 128.789635)
        (xy 66.198619 128.695244)
        (xy 66.251631 128.605966)
        (xy 66.317909 128.52144)
        (xy 66.404597 128.441307)
        (xy 66.51884 128.365205)
        (xy 66.667784 128.292775)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.595088 130.723314)
        (xy 117.545559 130.722774)
        (xy 117.502657 130.721119)
        (xy 117.465132 130.718181)
        (xy 117.431736 130.713791)
        (xy 117.401223 130.707782)
        (xy 117.372344 130.699986)
        (xy 117.343852 130.690234)
        (xy 117.314498 130.67836)
        (xy 117.283036 130.664194)
        (xy 117.248217 130.64757)
        (xy 117.037501 130.849921)
        (xy 117.247932 131.052569)
        (xy 117.282774 131.035993)
        (xy 117.314257 131.021871)
        (xy 117.343627 131.010038)
        (xy 117.372133 131.000327)
        (xy 117.401023 130.992571)
        (xy 117.431544 130.986605)
        (xy 117.464946 130.982262)
        (xy 117.502475 130.979376)
        (xy 117.54538 130.977782)
        (xy 117.594909 130.977313)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.996086 127.524086)
        (xy 121.946522 127.523582)
        (xy 121.90358 127.521955)
        (xy 121.866016 127.519036)
        (xy 121.832584 127.514651)
        (xy 121.80204 127.508631)
        (xy 121.773139 127.500802)
        (xy 121.744636 127.490995)
        (xy 121.715287 127.479037)
        (xy 121.683845 127.464757)
        (xy 121.649068 127.447985)
        (xy 121.437502 127.649448)
        (xy 121.647079 127.852979)
        (xy 121.682174 127.836465)
        (xy 121.713874 127.822409)
        (xy 121.743435 127.810639)
        (xy 121.772114 127.800987)
        (xy 121.801169 127.793285)
        (xy 121.831858 127.787362)
        (xy 121.865436 127.78305)
        (xy 121.903162 127.780179)
        (xy 121.946293 127.778581)
        (xy 121.996086 127.778086)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.595088 128.323314)
        (xy 117.545559 128.322774)
        (xy 117.502657 128.321119)
        (xy 117.465132 128.318181)
        (xy 117.431736 128.313791)
        (xy 117.401223 128.307782)
        (xy 117.372344 128.299986)
        (xy 117.343852 128.290234)
        (xy 117.314498 128.27836)
        (xy 117.283036 128.264194)
        (xy 117.248217 128.24757)
        (xy 117.037501 128.449921)
        (xy 117.247932 128.652569)
        (xy 117.282774 128.635993)
        (xy 117.314257 128.621871)
        (xy 117.343627 128.610038)
        (xy 117.372133 128.600327)
        (xy 117.401023 128.592571)
        (xy 117.431544 128.586605)
        (xy 117.464946 128.582262)
        (xy 117.502475 128.579376)
        (xy 117.54538 128.577782)
        (xy 117.594909 128.577313)
      )
    )
  )
  (zone (net 23) (net_name "+5V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.996084 133.924084)
        (xy 121.94652 133.92358)
        (xy 121.903578 133.921953)
        (xy 121.866014 133.919034)
        (xy 121.832583 133.914649)
        (xy 121.802039 133.908629)
        (xy 121.773138 133.9008)
        (xy 121.744635 133.890993)
        (xy 121.715285 133.879035)
        (xy 121.683843 133.864756)
        (xy 121.649066 133.847984)
        (xy 121.437502 134.049449)
        (xy 121.647081 134.252978)
        (xy 121.682176 134.236464)
        (xy 121.713875 134.222407)
        (xy 121.743435 134.210637)
        (xy 121.772114 134.200986)
        (xy 121.801169 134.193283)
        (xy 121.831857 134.18736)
        (xy 121.865435 134.183048)
        (xy 121.903161 134.180177)
        (xy 121.946291 134.178579)
        (xy 121.996084 134.178084)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.555 121.2016)
        (xy 48.605022 121.202686)
        (xy 48.647687 121.205912)
        (xy 48.684476 121.211225)
        (xy 48.716871 121.218573)
        (xy 48.746353 121.227905)
        (xy 48.774404 121.239168)
        (xy 48.802505 121.252311)
        (xy 48.832138 121.267282)
        (xy 48.864784 121.284029)
        (xy 48.901925 121.3025)
        (xy 49.1125 121.1)
        (xy 48.901925 120.8975)
        (xy 48.864784 120.91597)
        (xy 48.832138 120.932717)
        (xy 48.802505 120.947688)
        (xy 48.774404 120.960831)
        (xy 48.746353 120.972094)
        (xy 48.716871 120.981426)
        (xy 48.684476 120.988774)
        (xy 48.647687 120.994087)
        (xy 48.605022 120.997313)
        (xy 48.555 120.9984)
      )
    )
  )
  (zone (net 38) (net_name "/VGAIN") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.120248 128.310674)
        (xy 103.159623 128.279803)
        (xy 103.194665 128.255252)
        (xy 103.226485 128.236039)
        (xy 103.256197 128.221186)
        (xy 103.284914 128.209713)
        (xy 103.313748 128.200642)
        (xy 103.343813 128.192993)
        (xy 103.376221 128.185786)
        (xy 103.412085 128.178043)
        (xy 103.452519 128.168784)
        (xy 103.487006 127.878684)
        (xy 103.195779 127.855561)
        (xy 103.178763 127.89339)
        (xy 103.164132 127.927037)
        (xy 103.150704 127.957401)
        (xy 103.137303 127.985379)
        (xy 103.122749 128.011872)
        (xy 103.105863 128.037779)
        (xy 103.085468 128.063998)
        (xy 103.060383 128.091428)
        (xy 103.029431 128.120969)
        (xy 102.991434 128.153521)
      )
    )
  )
  (zone (net 11) (net_name "Net-(C12-Pad1)") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.463679 134.525936)
        (xy 115.421782 134.554821)
        (xy 115.384486 134.576172)
        (xy 115.350593 134.591265)
        (xy 115.318908 134.601376)
        (xy 115.288233 134.607783)
        (xy 115.257372 134.611761)
        (xy 115.225128 134.614589)
        (xy 115.190304 134.617541)
        (xy 115.151705 134.621896)
        (xy 115.108133 134.62893)
        (xy 115.059644 134.917021)
        (xy 115.34941 134.954214)
        (xy 115.368784 134.914557)
        (xy 115.384152 134.878882)
        (xy 115.397082 134.846413)
        (xy 115.409144 134.816377)
        (xy 115.421906 134.787998)
        (xy 115.436938 134.760502)
        (xy 115.455809 134.733114)
        (xy 115.480087 134.705059)
        (xy 115.511341 134.675563)
        (xy 115.551142 134.643851)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.755 140.027)
        (xy 122.804528 140.027504)
        (xy 122.847432 140.029129)
        (xy 122.884959 140.03204)
        (xy 122.918357 140.036407)
        (xy 122.948875 140.042394)
        (xy 122.977759 140.05017)
        (xy 123.006258 140.059902)
        (xy 123.035621 140.071756)
        (xy 123.067093 140.085899)
        (xy 123.101925 140.1025)
        (xy 123.3125 139.9)
        (xy 123.101925 139.6975)
        (xy 123.067093 139.7141)
        (xy 123.035621 139.728243)
        (xy 123.006258 139.740097)
        (xy 122.977759 139.749829)
        (xy 122.948875 139.757605)
        (xy 122.918357 139.763592)
        (xy 122.884959 139.767959)
        (xy 122.847432 139.77087)
        (xy 122.804528 139.772495)
        (xy 122.755 139.773)
      )
    )
  )
  (zone (net 28) (net_name "/THERM") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.648391 141.614607)
        (xy 46.598441 141.611706)
        (xy 46.555921 141.606935)
        (xy 46.519348 141.600291)
        (xy 46.487241 141.591773)
        (xy 46.458117 141.581378)
        (xy 46.430494 141.569105)
        (xy 46.402888 141.554952)
        (xy 46.373818 141.538916)
        (xy 46.341801 141.520996)
        (xy 46.305355 141.501191)
        (xy 46.087575 141.69592)
        (xy 46.290666 141.905923)
        (xy 46.328452 141.888811)
        (xy 46.361683 141.873259)
        (xy 46.391839 141.859373)
        (xy 46.420398 141.847258)
        (xy 46.448839 141.837019)
        (xy 46.47864 141.828763)
        (xy 46.51128 141.822595)
        (xy 46.548238 141.818619)
        (xy 46.590992 141.816943)
        (xy 46.641021 141.817672)
      )
    )
  )
  (zone (net 83) (net_name "/~{EN_50}") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55.755206 121.951033)
        (xy 55.634318 121.839812)
        (xy 55.546189 121.73546)
        (xy 55.484454 121.63551)
        (xy 55.442751 121.537498)
        (xy 55.414718 121.438956)
        (xy 55.39399 121.33742)
        (xy 55.374206 121.230424)
        (xy 55.349001 121.115502)
        (xy 55.312014 120.990188)
        (xy 55.256882 120.852018)
        (xy 54.350478 120.919212)
        (xy 54.453046 121.822298)
        (xy 54.59906 121.850769)
        (xy 54.729066 121.863802)
        (xy 54.846671 121.867191)
        (xy 54.95548 121.866729)
        (xy 55.0591 121.868209)
        (xy 55.161136 121.877425)
        (xy 55.265195 121.90017)
        (xy 55.374883 121.942236)
        (xy 55.493806 122.009419)
        (xy 55.625571 122.10751)
      )
    )
  )
  (zone (net 22) (net_name "-5V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.205 140.027)
        (xy 122.254528 140.027504)
        (xy 122.297432 140.029129)
        (xy 122.334959 140.03204)
        (xy 122.368357 140.036407)
        (xy 122.398875 140.042394)
        (xy 122.427759 140.05017)
        (xy 122.456258 140.059902)
        (xy 122.485621 140.071756)
        (xy 122.517093 140.085899)
        (xy 122.551925 140.1025)
        (xy 122.7625 139.9)
        (xy 122.551925 139.6975)
        (xy 122.517093 139.7141)
        (xy 122.485621 139.728243)
        (xy 122.456258 139.740097)
        (xy 122.427759 139.749829)
        (xy 122.398875 139.757605)
        (xy 122.368357 139.763592)
        (xy 122.334959 139.767959)
        (xy 122.297432 139.77087)
        (xy 122.254528 139.772495)
        (xy 122.205 139.773)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.207671 135.015606)
        (xy 121.169535 135.047213)
        (xy 121.135734 135.073686)
        (xy 121.105205 135.095704)
        (xy 121.076889 135.113944)
        (xy 121.049725 135.129086)
        (xy 121.022653 135.141807)
        (xy 120.994611 135.152787)
        (xy 120.964539 135.162704)
        (xy 120.931378 135.172237)
        (xy 120.894066 135.182064)
        (xy 120.86412 135.472668)
        (xy 121.155672 135.491234)
        (xy 121.171538 135.456062)
        (xy 121.186428 135.424936)
        (xy 121.201185 135.396921)
        (xy 121.216655 135.371083)
        (xy 121.233682 135.34649)
        (xy 121.253111 135.322207)
        (xy 121.275787 135.2973)
        (xy 121.302553 135.270837)
        (xy 121.334256 135.241884)
        (xy 121.37174 135.209507)
      )
    )
  )
  (zone (net 31) (net_name "/OUT1-") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.584685 124.927285)
        (xy 112.531679 124.927285)
        (xy 112.486835 124.927285)
        (xy 112.448304 124.927284)
        (xy 112.414236 124.927285)
        (xy 112.382782 124.927285)
        (xy 112.352093 124.927285)
        (xy 112.320319 124.927285)
        (xy 112.285612 124.927285)
        (xy 112.246122 124.927285)
        (xy 112.2 124.927285)
        (xy 112.120451 125.231834)
        (xy 112.412538 125.226124)
        (xy 112.422739 125.195446)
        (xy 112.43214 125.166391)
        (xy 112.441625 125.139337)
        (xy 112.452079 125.114662)
        (xy 112.464387 125.092745)
        (xy 112.479433 125.073965)
        (xy 112.498101 125.058699)
        (xy 112.521276 125.047327)
        (xy 112.549842 125.040226)
        (xy 112.584685 125.037775)
      )
    )
  )
  (zone (net 40) (net_name "+12V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.6016 132.045)
        (xy 78.602686 131.994977)
        (xy 78.605912 131.952312)
        (xy 78.611225 131.915523)
        (xy 78.618573 131.883128)
        (xy 78.627905 131.853646)
        (xy 78.639168 131.825595)
        (xy 78.652311 131.797494)
        (xy 78.667282 131.767861)
        (xy 78.684029 131.735215)
        (xy 78.7025 131.698075)
        (xy 78.5 131.4875)
        (xy 78.2975 131.698075)
        (xy 78.31597 131.735215)
        (xy 78.332717 131.767861)
        (xy 78.347688 131.797494)
        (xy 78.360831 131.825595)
        (xy 78.372094 131.853646)
        (xy 78.381426 131.883128)
        (xy 78.388774 131.915523)
        (xy 78.394087 131.952312)
        (xy 78.397313 131.994977)
        (xy 78.3984 132.045)
      )
    )
  )
  (zone (net 36) (net_name "/OFFSET1") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.214325 128.491522)
        (xy 98.175394 128.460092)
        (xy 98.143594 128.431466)
        (xy 98.117721 128.404779)
        (xy 98.096569 128.379166)
        (xy 98.078936 128.353763)
        (xy 98.063615 128.327705)
        (xy 98.049404 128.30013)
        (xy 98.035097 128.270171)
        (xy 98.019491 128.236965)
        (xy 98.001381 128.199648)
        (xy 97.710952 128.23125)
        (xy 97.753881 128.520222)
        (xy 97.794567 128.528298)
        (xy 97.830641 128.534992)
        (xy 97.863246 128.541251)
        (xy 97.89352 128.548021)
        (xy 97.922607 128.556248)
        (xy 97.951646 128.566878)
        (xy 97.981778 128.580858)
        (xy 98.014145 128.599135)
        (xy 98.049888 128.622655)
        (xy 98.090147 128.652364)
      )
    )
  )
  (zone (net 23) (net_name "+5V") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.871942 130.305305)
        (xy 114.871555 130.354834)
        (xy 114.870033 130.397741)
        (xy 114.86721 130.435275)
        (xy 114.862923 130.468684)
        (xy 114.857008 130.499215)
        (xy 114.849301 130.528118)
        (xy 114.839638 130.55664)
        (xy 114.827853 130.58603)
        (xy 114.813785 130.617536)
        (xy 114.797268 130.652407)
        (xy 115.000267 130.862499)
        (xy 115.202266 130.651444)
        (xy 115.185582 130.616652)
        (xy 115.171364 130.585213)
        (xy 115.15944 130.555879)
        (xy 115.149641 130.527403)
        (xy 115.141796 130.498537)
        (xy 115.135736 130.468034)
        (xy 115.13129 130.434647)
        (xy 115.128289 130.397127)
        (xy 115.126562 130.354227)
        (xy 115.12594 130.3047)
      )
    )
  )
  (zone (net 47) (net_name "/SIG_1X") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59.128108 138.861721)
        (xy 58.962833 138.851008)
        (xy 58.828292 138.823772)
        (xy 58.717735 138.782381)
        (xy 58.62441 138.729204)
        (xy 58.541568 138.66661)
        (xy 58.462458 138.596968)
        (xy 58.380329 138.522647)
        (xy 58.288432 138.446015)
        (xy 58.180016 138.369442)
        (xy 58.048331 138.295297)
        (xy 57.387515 138.919322)
        (xy 58.036889 139.555244)
        (xy 58.169899 139.483502)
        (xy 58.279688 139.408911)
        (xy 58.372961 139.333961)
        (xy 58.456426 139.261144)
        (xy 58.536788 139.19295)
        (xy 58.620754 139.131871)
        (xy 58.715029 139.080398)
        (xy 58.82632 139.041022)
        (xy 58.961333 139.016234)
        (xy 59.126775 139.008526)
      )
    )
  )
  (zone (net 35) (net_name "/OUT3-") (layer "B.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.584685 128.0762)
        (xy 112.531679 128.0762)
        (xy 112.486835 128.0762)
        (xy 112.448304 128.076199)
        (xy 112.414236 128.076199)
        (xy 112.382782 128.0762)
        (xy 112.352093 128.0762)
        (xy 112.320319 128.0762)
        (xy 112.285612 128.0762)
        (xy 112.246122 128.0762)
        (xy 112.2 128.0762)
        (xy 112.120451 128.380749)
        (xy 112.412538 128.375039)
        (xy 112.422739 128.344361)
        (xy 112.43214 128.315306)
        (xy 112.441625 128.288252)
        (xy 112.452079 128.263577)
        (xy 112.464387 128.24166)
        (xy 112.479433 128.22288)
        (xy 112.498101 128.207614)
        (xy 112.521276 128.196242)
        (xy 112.549842 128.189141)
        (xy 112.584685 128.18669)
      )
    )
  )
)
