(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/BATT_+")
	(net 2 "GND")
	(net 3 "/BATT_PROT")
	(net 4 "GNDD")
	(footprint "Package_TO_SOT_SMD:SOT-23-Alpha"
		(layer "F.Cu")
		(at 139 67 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 2.5 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "DMP3098L-7-ALPHA"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "MOSFET P-Channel 1.25W"
			(at 206 -72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Cost_1" "0.662"
			(at 206 -72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Cost_100" "0.426"
			(at 206 -72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Cost_1000" "0.27"
			(at 206 -72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "DMP3098L-7"
			(at 206 -72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Diodes Inc."
			(at 206 -72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "SOT-23-3"
			(at 206 -72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" "MO"
			(at 206 -72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor PN" "621-DMP3098L-7"
			(at 206 -72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Tie_DRC_error.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "D" smd roundrect
			(at 1 0 90)
			(size 1.1 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "/BATT_+")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "G" smd roundrect
			(at -1 -0.915 90)
			(size 1.1 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "S" smd roundrect
			(at -1 0.915 90)
			(size 1.1 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/BATT_PROT")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset (xyz 0 0 0))
			(scale (xyz 1 1 1))
			(rotate (xyz 0 0 0))
		)
	)
	(footprint "User_1:TestPoint_THTPad_1.0mm_Drill_0.6mm"
		(layer "F.Cu")
		(at 135.495 65.835)
		(descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
		(tags "test point THT pad")
		(property "Reference" "H1"
			(at -2.495 -0.575 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Tie_DRC_error.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/BATT_+")
			(pinfunction "1")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "User_1:TestPoint_THTPad_1.0mm_Drill_0.6mm"
		(layer "F.Cu")
		(at 135.495 70.075)
		(descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
		(tags "test point THT pad")
		(property "Reference" "H3"
			(at -2.495 -0.575 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Tie_DRC_error.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/BATT_PROT")
			(pinfunction "1")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "NetTie:NetTie-2_SMD_Pad2.0mm"
		(layer "F.Cu")
		(at 139 57)
		(descr "Net tie, 2 pin, 2.0mm square SMD pads")
		(tags "net tie")
		(property "Reference" "NT1"
			(at 0 -2 0)
			(layer "F.SilkS")
		)
		(property "Value" "Net-Tie_2"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Net tie, 2 pins"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "exclude_from_bom" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Tie_DRC_error.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(net_tie_pad_groups "1, 2")
		(pad "1" smd circle
			(at -2 0)
			(size 2 2)
			(layers "F.Cu")
			(net 4 "GNDD")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd circle
			(at 2 0)
			(size 2 2)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "User_1:TestPoint_THTPad_1.0mm_Drill_0.6mm"
		(layer "F.Cu")
		(at 135.495 67.955)
		(descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
		(tags "test point THT pad")
		(property "Reference" "H2"
			(at -2.495 -0.575 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Tie_DRC_error.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(gr_rect
		(start 97 40)
		(end 169 92)
		(fill no)
		(layer "Edge.Cuts")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
		(polygon
			(pts
				(xy 139.5 51) (xy 139.5 62) (xy 148 62) (xy 148 51)
			)
		)
	)
	(zone
		(net 4)
		(net_name "GNDD")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
		(polygon
			(pts
				(xy 138.5 51) (xy 138.5 62) (xy 124 62) (xy 124 51)
			)
		)
	)
	(embedded_fonts no)
)
